<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Coaxial Connectors - WR-SMP &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="60124102122403">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, SMT</description>
</package>
<package name="60123002122501">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Right Angle Plug, THT</description>
</package>
<package name="60114202122305">
<description>&lt;B&gt;WR-SMP PCB End Launch

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, End Launch</description>
</package>
<package name="60114002122502">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, THT</description>
</package>
<package name="60114602122404">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, THR</description>
</package>
<package name="60114102122403">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, SMT</description>
</package>
<package name="60124002122502">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, THT</description>
</package>
<package name="60124602122404">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, THR</description>
</package>
<package name="60124202122305">
<description>&lt;B&gt;WR-SMP PCB End Launch

&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Plug, End Launch</description>
</package>
</packages>
<symbols>
<symbol name="PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="60124102122403" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124102122403">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="0.4"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60124102122403?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60124102122403"/>
<attribute name="RETENTION-TYPE" value="Limited Detent"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60124102122403"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60123002122501" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60123002122501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="D0.7"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60123002122501?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60123002122501"/>
<attribute name="RETENTION-TYPE" value="Limited Detent"/>
<attribute name="SIZE" value="Right Angle Plug"/>
<attribute name="VALUE" value="60123002122501"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114202122305" prefix="J">
<description>&lt;b&gt;WR-SMP PCB End Launch&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms (min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779218v209%20Multi-WR-SMP-60114202122305.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779218v209%20Multi-WR-SMP-60114202122305.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-04-11&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114202122305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="D0.38"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60114202122305?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60114202122305"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="RETENTION-TYPE" value="Smooth Bore"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60114202122305"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114002122502" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114002122502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="D0.7"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60114002122502?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60114002122502"/>
<attribute name="RETENTION-TYPE" value="Smooth Bore"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60114002122502"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114102122403" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114102122403">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="0.4"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60114102122403?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60114102122403"/>
<attribute name="RETENTION-TYPE" value="Smooth Bore"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60114102122403"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114602122404" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114602122404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="0.4"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60114602122404?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60114602122404"/>
<attribute name="RETENTION-TYPE" value="Smooth Bore"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60114602122404"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124002122502" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124002122502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="D0.7"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60124002122502?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60124002122502"/>
<attribute name="RETENTION-TYPE" value="Limited Detent"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60124002122502"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124602122404" prefix="J">
<description>&lt;b&gt;WR-SMP PCB THT/ THR/ SMT Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms(min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779196v209%20Family-WR-SMP%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124602122404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="0.4"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60124602122404?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60124602122404"/>
<attribute name="RETENTION-TYPE" value="Limited Detent"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60124602122404"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124202122305" prefix="J">
<description>&lt;b&gt;WR-SMP PCB End Launch&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles(Limited Detent), 1000 Cycles(Smooth Bore)
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 500Vrms (min.)
&lt;br&gt;Mating: Snap on
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o779218v209%20Multi-WR-SMP-60114202122305.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o779218v209%20Multi-WR-SMP-60114202122305.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMP_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/COAX_SMP_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-04-11&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124202122305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="D0.38"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60124202122305?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60124202122305"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="RETENTION-TYPE" value="Limited Detent"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60124202122305"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
