<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Terminal Blocks - WR-TBL Pluggable Connector &lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-07-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691328310010">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691357300006B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm ,6pins</description>
</package>
<package name="691330300006">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691701320002B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691356310004B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305130006">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691382010007">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 7pins</description>
</package>
<package name="691322310007">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691305330003">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691357300010B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm ,10pins</description>
</package>
<package name="691321300008">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691309310003">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691325110008">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691309310008">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691356310006B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691308330006">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691322110004">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691321300023">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 23pins</description>
</package>
<package name="691310340007">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691357300012B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm ,12pins</description>
</package>
<package name="691322310019">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 19pins</description>
</package>
<package name="691327310008">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691305330005">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691327310016">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691356300006B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691328310006">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691307300007">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691323100003">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691328310016">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691382040008">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 8pins</description>
</package>
<package name="691356310012B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691322310002">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691305340002">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691321300019">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 19pins</description>
</package>
<package name="691308330002">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691325110003">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691329300016">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691308330005">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691321300016">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691322310015">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 15pins</description>
</package>
<package name="691309310007">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691321300014">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 14pins</description>
</package>
<package name="691322310006">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691321100012">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691305140012">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691308330012">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691325310012">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691325110012">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691309310006">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691305340012">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691321100005">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691305140008">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691701320006B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691321300011">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 11pins</description>
</package>
<package name="691701310006B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691305340003">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691701320005B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691329300012">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701310003B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691310340006">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691323100012">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691308330007">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691357310012B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691327310012">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691382000005">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 5pins</description>
</package>
<package name="691357310008B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691305140005">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691310340008">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691382010005">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 5pins</description>
</package>
<package name="691357300008B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm ,8pins</description>
</package>
<package name="691307300012">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691327310004">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691321300012">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691305130003">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691322310021">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 21pins</description>
</package>
<package name="691305140006">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691310340004">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305340004">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691701310005B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691323300005">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691305340005">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691321300009">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 9pins</description>
</package>
<package name="691321100008">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691325310008">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691382040012">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 12pins</description>
</package>
<package name="691701310010B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691305340008">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691701340004B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691321300021">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 21pins</description>
</package>
<package name="691322310017">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 17pins</description>
</package>
<package name="691305130002">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691322110008">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691321300004">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305130005">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691305140004">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691323300004">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691382010008">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 8pins</description>
</package>
<package name="691701320010B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691308330004">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691322310013">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 13pins</description>
</package>
<package name="691329300010">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691305330004">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691321300002">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691322310010">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691305140003">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691323300012">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691325310007">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691382030005">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 5pins</description>
</package>
<package name="691322110002">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691325110007">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691322110005">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691328310004">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305140002">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691307300002">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691325110005">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691356300010B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691305130008">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691325310002">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691305330007">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691307300003">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691321100006">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691305330008">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691701310002B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691357310010B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691330300010">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691356300008B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691327310010">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691325310006">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691305130004">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691321300007">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691307500006">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691305340007">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691321100004">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691322310024">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 24pins</description>
</package>
<package name="691323300008">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691327310006">
<description>&lt;b&gt;WR-TBL Serie 3273 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691329300008">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691321300015">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 15pins</description>
</package>
<package name="691325310004">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691307300006">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691322310018">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 18pins</description>
</package>
<package name="691330300016">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691322110012">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691356310008B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691356300004B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691322310005">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691305140007">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691328310008">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691357300004B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm ,4pins</description>
</package>
<package name="691322310020">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 20pins</description>
</package>
<package name="691356300012B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 21.9mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691382040007">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 7pins</description>
</package>
<package name="691330300012">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691382000006">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 6pins</description>
</package>
<package name="691328310012">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 22.7mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691308330008">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691357310004B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691322310003">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691321300006">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691356310010B">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691305330006">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691325310005">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691330300008">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691330300004">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691325310003">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691382040005">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 5pins</description>
</package>
<package name="691382030004">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 4pins</description>
</package>
<package name="691321100002">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691382040002">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 2pins</description>
</package>
<package name="691382000002">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 2pins</description>
</package>
<package name="691382010003">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 3pins</description>
</package>
<package name="691322310011">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 11pins</description>
</package>
<package name="691305130007">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691382040006">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 6pins</description>
</package>
<package name="691322310008">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691325110006">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691321300005">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691382030002">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 2pins</description>
</package>
<package name="691322310023">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 23pins</description>
</package>
<package name="691310340002">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691321100007">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691310340012">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691321300010">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691321300018">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 18pins</description>
</package>
<package name="691382030012">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 12pins</description>
</package>
<package name="691701320012B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691321300022">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 22pins</description>
</package>
<package name="691310340005">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691701340002B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691701340003B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691701320008B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691325110004">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691382010012">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 12pins</description>
</package>
<package name="691322310009">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 9pins</description>
</package>
<package name="691323300003">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691701320004B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691382040004">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 4pins</description>
</package>
<package name="691323100005">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691322110006">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691321300017">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 17pins</description>
</package>
<package name="691325110002">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691382040003">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 3pins</description>
</package>
<package name="691322310012">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691322110007">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691321300020">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 20pins</description>
</package>
<package name="691701340005B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691701310008B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691701310004B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305340006">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691701310012B">
<description>&lt;b&gt;WR-TBL Serie 7013B - 3.81 mm Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701340012B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701350002B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691323100008">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691382010006">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 6pins</description>
</package>
<package name="691323100007">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691305330002">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691701340006B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691309310004">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691305330012">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701350008B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691329300006">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691309310005">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691701350006B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691323300002">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691309310012">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701350005B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691382010004">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 4pins</description>
</package>
<package name="691323100004">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691701340008B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691382030006">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 6pins</description>
</package>
<package name="691382030008">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 8pins</description>
</package>
<package name="691321300003">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691322110003">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691382000012">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 12pins</description>
</package>
<package name="691300700024">
<description>&lt;b&gt;WR-TBL Serie 300 - 5.00 mm Pin Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.95mm , Pitch 5mm , 24pins</description>
</package>
<package name="691701350012B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691701350004B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691311700102">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 2pins</description>
</package>
<package name="691311700005">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 5pins</description>
</package>
<package name="691701340010B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691311700107">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 7pins</description>
</package>
<package name="691311700103">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 3pins</description>
</package>
<package name="691321100003">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691701320003B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Vertical PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691701350003B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691701350010B">
<description>&lt;b&gt;WR-TBL Serie 7013 - 3.81 mm Horizontal PCB Header THR Type with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 7.3mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691311700104">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 4pins</description>
</package>
<package name="691311700002">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 2pins</description>
</package>
<package name="691311700004">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 4pins</description>
</package>
<package name="691311700108">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 8pins</description>
</package>
<package name="691318700002">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 2pins</description>
</package>
<package name="691318700003">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 3pins</description>
</package>
<package name="691311700106">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 6pins</description>
</package>
<package name="691313710007">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 7pins</description>
</package>
<package name="691313710002">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 2pins</description>
</package>
<package name="691318700004">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 4pins</description>
</package>
<package name="691311700012">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 12pins</description>
</package>
<package name="691313710008">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 8pins</description>
</package>
<package name="691311700105">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 5pins</description>
</package>
<package name="691318700005">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 5pins</description>
</package>
<package name="691313710003">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 3pins</description>
</package>
<package name="691311700006">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 6pins</description>
</package>
<package name="691318700008">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 8pins</description>
</package>
<package name="691313710005">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 5pins</description>
</package>
<package name="691305130012">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691311700112">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 12pins</description>
</package>
<package name="691313710006">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 6pins</description>
</package>
<package name="691312710007">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 7pins</description>
</package>
<package name="691311700008">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 8pins</description>
</package>
<package name="691312710008">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 8pins</description>
</package>
<package name="691312710002">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 2pins</description>
</package>
<package name="691382000003">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 3pins</description>
</package>
<package name="691386700002">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 2pins</description>
</package>
<package name="691311700003">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 3pins</description>
</package>
<package name="691318700007">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 7pins</description>
</package>
<package name="691311700007">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 7pins</description>
</package>
<package name="691308330003">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691382030007">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 7pins</description>
</package>
<package name="691309310002">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.6mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691382030003">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 3pins</description>
</package>
<package name="691322310014">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 14pins</description>
</package>
<package name="691357310006B">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22.4mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691322310022">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 22pins</description>
</package>
<package name="691322310016">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 16pins</description>
</package>
<package name="691323300007">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691323100002">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691310340003">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 6.8mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691321300013">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 13pins</description>
</package>
<package name="691307300004">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691321300024">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 24pins</description>
</package>
<package name="691323300006">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691382000008">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 8pins</description>
</package>
<package name="691382000004">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 10.1mm , Pitch 2.5mm , 4pins</description>
</package>
<package name="691318700006">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 6pins</description>
</package>
<package name="691323100006">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 9.2mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691329300004">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691386700004">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 4pins</description>
</package>
<package name="691312710003">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 3pins</description>
</package>
<package name="691307300008">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691386700008">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 8pins</description>
</package>
<package name="691386700003">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 3pins</description>
</package>
<package name="691318700012">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 12pins</description>
</package>
<package name="691307300005">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691322310004">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 7mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691382010002">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 8.1mm , Pitch 2.5mm , 2pins</description>
</package>
<package name="691312710004">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 4pins</description>
</package>
<package name="691386700005">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 5pins</description>
</package>
<package name="691312710006">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 6pins</description>
</package>
<package name="691312710005">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 5pins</description>
</package>
<package name="691386700006">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 6pins</description>
</package>
<package name="691386700018">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 18pins</description>
</package>
<package name="691371700008B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 8pins</description>
</package>
<package name="691386700014">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 14pins</description>
</package>
<package name="691371700007B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 7pins</description>
</package>
<package name="691313710012">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 12pins</description>
</package>
<package name="691386700011">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 11pins</description>
</package>
<package name="691386700013">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 13pins</description>
</package>
<package name="691386700007">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 7pins</description>
</package>
<package name="691371700003B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 3pins</description>
</package>
<package name="691386700010">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 10pins</description>
</package>
<package name="691313710004">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 4pins</description>
</package>
<package name="691386700015">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 15pins</description>
</package>
<package name="691386700009">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 9pins</description>
</package>
<package name="691371700006B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 6pins</description>
</package>
<package name="691371700005B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 5pins</description>
</package>
<package name="691371700012B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 12pins</description>
</package>
<package name="691317710005">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 5pins</description>
</package>
<package name="691312710012">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 8pins</description>
</package>
<package name="691370710007B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 7pins</description>
</package>
<package name="691370710012B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 12pins</description>
</package>
<package name="691371700004B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 4pins</description>
</package>
<package name="691370710003B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 3pins</description>
</package>
<package name="691386700017">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 17pins</description>
</package>
<package name="691317710012">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 12pins</description>
</package>
<package name="691317710008">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 8pins</description>
</package>
<package name="691370710006B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 6pins</description>
</package>
<package name="691370710002B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 2pins</description>
</package>
<package name="691371700002B">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5mm , 2pins</description>
</package>
<package name="691317710002">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 2pins</description>
</package>
<package name="691370710005B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 5pins</description>
</package>
<package name="691311500108">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691311500110">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691386700016">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 16pins</description>
</package>
<package name="691370710004B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 4pins</description>
</package>
<package name="691317710004">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 4pins</description>
</package>
<package name="691370710008B">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 8pins</description>
</package>
<package name="691311500105">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691311500112">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691311500107">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691311500113">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 13pins</description>
</package>
<package name="691317710006">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 6pins</description>
</package>
<package name="691317710003">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 3pins</description>
</package>
<package name="691317710007">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5mm , 7pins</description>
</package>
<package name="691311500114">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691311500102">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311500106">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691311500117">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 17pins</description>
</package>
<package name="691311500104">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691311500111">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691311500103">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701510005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691311500123">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 23pins</description>
</package>
<package name="691311500119">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 19pins</description>
</package>
<package name="691311500116">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691311500118">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 18pins</description>
</package>
<package name="691311500109">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691311500120">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 20pins</description>
</package>
<package name="691701510012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701510002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311500115">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 15pins</description>
</package>
<package name="691701510003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701510010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691701510004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm ,4pins</description>
</package>
<package name="691336500006">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701510008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701510006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691333500008">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691311500122">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 22pins</description>
</package>
<package name="691336500016">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691311500004">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691333500010">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691311500121">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 21pins</description>
</package>
<package name="691311500124">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 24pins</description>
</package>
<package name="691311500009">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691333500016">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691333500004">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691386700012">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.9mm , Pitch 5mm , 12pins</description>
</package>
<package name="691333500006">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691311500005">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691311500014">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691311500002">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311500019">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 19pins</description>
</package>
<package name="691336500010">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691311500007">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691336500012">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691333500012">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691311500008">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691311500003">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691338500010">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691336500004">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691318500005">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691311500010">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691311500015">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691336500008">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691338500012">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691311500013">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 13pins</description>
</package>
<package name="691311500016">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691311500021">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 21pins</description>
</package>
<package name="691318500002">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311500011">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691311500020">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 20pins</description>
</package>
<package name="691338500008">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691338500004">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691311500018">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 18pins</description>
</package>
<package name="691338500006">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691334500008">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691311500012">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691318500007">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691334500012">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691318500006">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691318500003">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691311500006">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691311500024">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 24pins</description>
</package>
<package name="691318500008">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691311500022">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 22pins</description>
</package>
<package name="691334500016">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691334500004">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691338500016">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691311500023">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 23pins</description>
</package>
<package name="691334500014">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691313510009">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691334500020">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691337500006">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691334500006">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691337500008">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691318500004">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691334500010">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691337500004">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691313510006">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691311500017">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 17pins</description>
</package>
<package name="691334500018">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691313510002">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691337500012">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691313510003">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691331510004">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691313510007">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691337500014">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691313510004">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691313510020">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 20pins</description>
</package>
<package name="691313510005">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691331510008">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691313510008">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691313510017">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 17pins</description>
</package>
<package name="691337500016">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691313510018">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 18pins</description>
</package>
<package name="691313510010">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691313510016">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691318500012">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691313510021">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 21pins</description>
</package>
<package name="691337500010">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 22mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691313510023">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 23pins</description>
</package>
<package name="691313510013">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 13pins</description>
</package>
<package name="691313510011">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691312510009">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691313510019">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 19pins</description>
</package>
<package name="691319510012">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691319510008">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691313510024">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 24pins</description>
</package>
<package name="691313510014">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691331510012">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691312510003">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691331510006">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691312510006">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691312510004">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691319510004">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691319510010">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691319510016">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691312510011">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691312510008">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691319510006">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm ,6pins</description>
</package>
<package name="691312510007">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691312510012">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691312510019">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 19pins</description>
</package>
<package name="691312510014">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691312510013">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 13pins</description>
</package>
<package name="691313510022">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 22pins</description>
</package>
<package name="691312510021">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 21pins</description>
</package>
<package name="691312510005">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691312510015">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 15pins</description>
</package>
<package name="691313510012">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691312510016">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691313510015">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 15pins</description>
</package>
<package name="691331510010">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691312510020">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 20pins</description>
</package>
<package name="691335510008">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691312510024">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 24pins</description>
</package>
<package name="691317510003">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691335510006">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691335510016">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691312510002">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691312510022">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 22pins</description>
</package>
<package name="691312510018">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 18pins</description>
</package>
<package name="691317510004">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691335510010">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691317510006">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691312510023">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 23pins</description>
</package>
<package name="691317510002">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691335510012">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691317510007">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691332510008">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691312510010">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691332510012">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691314520102">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691317510012">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691332510006">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691332510010">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691317510008">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691320510008">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691317510005">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691332510004">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691314520113">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 13pins</description>
</package>
<package name="691314520103">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691332510016">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691331510016">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 28.8mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691314520114">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 14pins</description>
</package>
<package name="691314520109">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691314520112">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691320510004">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691320510006">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691314520117">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 17pins</description>
</package>
<package name="691320510010">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691314520107">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691314520118">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 18pins</description>
</package>
<package name="691314520108">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691314520106">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691314520123">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 23pins</description>
</package>
<package name="691314520110">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691320510012">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691314520105">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691320510016">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691314520121">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 21pins</description>
</package>
<package name="691314520115">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 15pins</description>
</package>
<package name="691314520111">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691335510004">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 23.7mm , Pitch 5.08mm , 4pin</description>
</package>
<package name="691307500003">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691312510017">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 17pins</description>
</package>
<package name="691314520116">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 16pins</description>
</package>
<package name="691314520119">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 19pins</description>
</package>
<package name="691309510002">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691307500007">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691307500002">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691314520120">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 20pins</description>
</package>
<package name="691314520124">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 24pins</description>
</package>
<package name="691309510012">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691309510003">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691307500005">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691701500008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691307500008">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701500006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701500004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701500012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701520002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691309510006">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701520006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701520004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701500010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691307500004">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701520005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691309510005">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691701500002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691701500005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691314520104">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691309510008">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701530002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691307500012">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701530004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701540002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691701530008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701500003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Vertical PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691309510004">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701550003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691309510007">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691701520012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701540003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701530005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691701530003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701530006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701530012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701540010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691701520003B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701550006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701520010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691701550004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691701540006B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701520008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Vertical PCB Header THR Type w. Flanges
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701530010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Open Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691701540005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691701550002B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691701540012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691305540006">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691701540008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701550012B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691701550010B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691305540003">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691701550008B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691701550005B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Closed Horizontal PCB Header THR Type with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691305530007">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691305540007">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691305540010">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691305530010">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691305540004">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691305540005">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691305530002">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691305530003">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691311400112">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691318400003">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691305540009">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691311400007">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691305530005">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691311400106">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691311400102">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691701540004B">
<description>&lt;b&gt;WR-TBL Serie 7015B - 5.08 mm Close Horizontal PCB Header THR Type 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691311400104">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691311400003">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691311400105">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691305530004">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691305530008">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691305540002">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311400103">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691305530009">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691313410008">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691318400008">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691311400108">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691305530006">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691311400004">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691313410005">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691311400002">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691318400004">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691318400002">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691311400005">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691318400005">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691313410006">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691305540008">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches
&lt;br&gt;&lt;/b&gt;Max Height = 8.6mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691313410012">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691311400006">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691318400006">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691318400012">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691311400008">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691313410003">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691311400107">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691318400007">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691312410005">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691312410002">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691317410005">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691312410007">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691317410003">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691311400012">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691312410003">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691317410002">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691313410002">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691313410007">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691312410004">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691312410008">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691313410004">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691307400007">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691375400002">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;2pins</description>
</package>
<package name="691312410006">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691307400004">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691317410008">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691317410012">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691307400005">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691312410012">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header  
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691317410006">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691307400006">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691307400012">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691309410002">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691347000002B">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 3470B, Pitch 2.5mm,THT, 2pins</description>
</package>
<package name="691317410004">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691317410007">
<description>&lt;b&gt;WR-TBL Serie 3174 - 7.62 mm Close Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.5mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691309410006">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691375400004">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4pins</description>
</package>
<package name="691307400003">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691309410012">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691307400002">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691375400003">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;3pins</description>
</package>
<package name="691309410007">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691309410005">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691309410003">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691307400008">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header
&lt;br&gt;&lt;/b&gt;Max Height = 19mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691375400006">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;6pins</description>
</package>
<package name="691375410002">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;2pins</description>
</package>
<package name="691347000004B">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 3470B, Pitch 2.5mm,THT, 4pins</description>
</package>
<package name="691300100002">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;&lt;br&gt;2pins</description>
</package>
<package name="691347000003B">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 3470B, Pitch 2.5mm,THT, 3pins</description>
</package>
<package name="691375400005">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;5pins</description>
</package>
<package name="691300300003">
<description>&lt;B&gt;WR-TBL Series 3003 - Pin Header 3.81mm pitch - Vertical cable entry - THT
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;3pins</description>
</package>
<package name="691375460003">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;3pins</description>
</package>
<package name="691309410004">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691300100003">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;&lt;br&gt;3pins</description>
</package>
<package name="691375410004">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4pins</description>
</package>
<package name="691375410003">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;3pins</description>
</package>
<package name="691375460005">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;5pins</description>
</package>
<package name="691309410008">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 8.3mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691375410006">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;6pins</description>
</package>
<package name="691701140003B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 3pins</description>
</package>
<package name="691347000005B">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 3470B, Pitch 2.5mm,THT, 5pins</description>
</package>
<package name="691701100002B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 2pins</description>
</package>
<package name="691300300002">
<description>&lt;B&gt;WR-TBL Series 3003 - Pin Header 3.81mm pitch - Vertical cable entry - THT
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;2pins</description>
</package>
<package name="691701130012B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 12pins</description>
</package>
<package name="691347000006B">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 3470B, Pitch 2.5mm,THT, 6pins</description>
</package>
<package name="691701100003B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 3pins</description>
</package>
<package name="691375410005">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;5pins</description>
</package>
<package name="691300100024">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;&lt;br&gt;24pins</description>
</package>
<package name="691701100004B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 4pins</description>
</package>
<package name="691701100008B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 8pins</description>
</package>
<package name="691375460006">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;6pins</description>
</package>
<package name="691375460004">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4pins</description>
</package>
<package name="691314520122">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 14.5mm , Pitch 5.08mm , 22pins</description>
</package>
<package name="691701110012B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 12pins</description>
</package>
<package name="691701140010B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 10pins</description>
</package>
<package name="691701110006B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 6pins</description>
</package>
<package name="691701110002B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 2pins</description>
</package>
<package name="691701140012B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 12pins</description>
</package>
<package name="691701100005B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 5pins</description>
</package>
<package name="691701130010B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 10pins</description>
</package>
<package name="691701130003B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 3pins</description>
</package>
<package name="691701140008B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 8pins</description>
</package>
<package name="691701110003B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 3pins</description>
</package>
<package name="691701130008B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 8pins</description>
</package>
<package name="691701110004B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 4pins</description>
</package>
<package name="691701140002B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 2pins</description>
</package>
<package name="691701130006B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 6pins</description>
</package>
<package name="691701110005B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 5pins</description>
</package>
<package name="691701140006B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 6pins</description>
</package>
<package name="691701140005B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 5pins</description>
</package>
<package name="691701700105B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 5pins</description>
</package>
<package name="691701110010B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 10pins</description>
</package>
<package name="691701140004B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Horizontal cable entry with flanges, Max Height = 7.3mm, 4pins</description>
</package>
<package name="691701100006B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 6pins</description>
</package>
<package name="691701100010B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 10pins</description>
</package>
<package name="691701110008B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry, Max Height = 7.3mm, 8pins</description>
</package>
<package name="691701130004B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 4pins</description>
</package>
<package name="691375460002">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT
&lt;/b&gt;&lt;br&gt;&lt;br&gt;2pins</description>
</package>
<package name="691701100012B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry, Max Height = 9.5mm, 12pins</description>
</package>
<package name="691701730008B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 8pins</description>
</package>
<package name="691701700108B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 8pins</description>
</package>
<package name="691701130005B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 5pins</description>
</package>
<package name="691701710002B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 2pins</description>
</package>
<package name="691701130002B">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Vertical cable entry with flanges, Max Height = 9.5mm, 2pins</description>
</package>
<package name="691701700103B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 3pins</description>
</package>
<package name="691701740004B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 4pins</description>
</package>
<package name="691701700106B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 6pins</description>
</package>
<package name="691701710108B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 8pins</description>
</package>
<package name="691701700004B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 4pins</description>
</package>
<package name="691701700110B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 10pins</description>
</package>
<package name="691701710005B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 5pins</description>
</package>
<package name="691701700104B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 4pins</description>
</package>
<package name="691701730004B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 4pins</description>
</package>
<package name="691701710105B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 5pins</description>
</package>
<package name="691701740008B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 8pins</description>
</package>
<package name="691701700010B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 10pins</description>
</package>
<package name="691701730012B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 12pins</description>
</package>
<package name="691701730006B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 6pins</description>
</package>
<package name="691701710110B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 10pins</description>
</package>
<package name="691701740012B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 12pins</description>
</package>
<package name="691701730005B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 5pins</description>
</package>
<package name="691701740006B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 6pins</description>
</package>
<package name="691701700005B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 5pins</description>
</package>
<package name="691701700002B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 2pins</description>
</package>
<package name="691701700003B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 3pins</description>
</package>
<package name="691701700006B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 6pins</description>
</package>
<package name="691701710006B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 6pins</description>
</package>
<package name="691701710103B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 3pins</description>
</package>
<package name="691701730002B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 2pins</description>
</package>
<package name="691701710104B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 4pins</description>
</package>
<package name="691701700012B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 12pins</description>
</package>
<package name="691701740002B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 2pins</description>
</package>
<package name="691701710004B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 4pins</description>
</package>
<package name="691701700008B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Open Vertical cable entry, Max Height = 12.3mm, 8pins</description>
</package>
<package name="691701700112B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 12pins</description>
</package>
<package name="691701730010B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 10pins</description>
</package>
<package name="691378110004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 4pins</description>
</package>
<package name="691701710012B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 12pins</description>
</package>
<package name="691701710008B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 8pins</description>
</package>
<package name="691701710010B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 10pins</description>
</package>
<package name="691701710102B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 2pins</description>
</package>
<package name="691701710003B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Open Horizontal cable entry, Max Height = 8.8mm, 3pins</description>
</package>
<package name="691378140006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 6pins</description>
</package>
<package name="691701740005B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 5pins</description>
</package>
<package name="691378100004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 4pins</description>
</package>
<package name="691378100008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 8pins</description>
</package>
<package name="691701740010B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 10pins</description>
</package>
<package name="691378140008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 8pins</description>
</package>
<package name="691701710112B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 12pins</description>
</package>
<package name="691701740003B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Horizontal cable entry with flanges, Max Height = 8.8mm, 3pins</description>
</package>
<package name="691378110008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 8pins</description>
</package>
<package name="691378110018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 18pins</description>
</package>
<package name="691378110020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 20pins</description>
</package>
<package name="691378100014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 14pins</description>
</package>
<package name="691378130006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 6pins</description>
</package>
<package name="691701700102B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Vertical cable entry, Max Height = 12.3mm, 2pins</description>
</package>
<package name="691701730003B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Vertical cable entry with flanges, Max Height = 12.3mm, 3pins</description>
</package>
<package name="691378140016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 16pins</description>
</package>
<package name="691701710106B">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Closed Horizontal cable entry, Max Height = 8.8mm, 6pins</description>
</package>
<package name="691378100020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 20pins</description>
</package>
<package name="691378130018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 18pins</description>
</package>
<package name="691378130004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 4pins</description>
</package>
<package name="691378110006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 6pins</description>
</package>
<package name="691378140024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 24pins</description>
</package>
<package name="691378130008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 8pins</description>
</package>
<package name="691378110014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 14pins</description>
</package>
<package name="691378110012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 12pins</description>
</package>
<package name="691378100016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 16pins</description>
</package>
<package name="691378140010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 10pins</description>
</package>
<package name="691378130012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 12pins</description>
</package>
<package name="691378110016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 16pins</description>
</package>
<package name="691378140020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 20pins</description>
</package>
<package name="691378130020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 20pins</description>
</package>
<package name="691378100010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 10pins</description>
</package>
<package name="691378140014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 14pins</description>
</package>
<package name="691378100024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 24pins</description>
</package>
<package name="691378140012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 12pins</description>
</package>
<package name="691378130010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 10pins</description>
</package>
<package name="691378100012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 12pins</description>
</package>
<package name="691378100006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 6pins</description>
</package>
<package name="691378140018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 18pins</description>
</package>
<package name="691378140004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 4pins</description>
</package>
<package name="691378130014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 14pins</description>
</package>
<package name="691378110024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 24pins</description>
</package>
<package name="691378110010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=11.1mm, 10pins</description>
</package>
<package name="691378130024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 24pins</description>
</package>
<package name="691378130016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 16pins</description>
</package>
<package name="691778140006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 6pins</description>
</package>
<package name="691378100018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max height=10.3mm, 18pins</description>
</package>
<package name="691778110020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 20pins</description>
</package>
<package name="691778130014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 14pins</description>
</package>
<package name="691778110024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 24pins</description>
</package>
<package name="691778130006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 6pins</description>
</package>
<package name="691778110018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 18pins</description>
</package>
<package name="691778100016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 16pins</description>
</package>
<package name="691778140010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 10pins</description>
</package>
<package name="691778140004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 4pins</description>
</package>
<package name="691778100008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 8pins</description>
</package>
<package name="691778130012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 12pins</description>
</package>
<package name="691778110004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 4pins</description>
</package>
<package name="691778110010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 10pins</description>
</package>
<package name="691778140024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 24pins</description>
</package>
<package name="691778140018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 18pins</description>
</package>
<package name="691778130020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 20pins</description>
</package>
<package name="691778100006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 6pins</description>
</package>
<package name="691778140012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 12pins</description>
</package>
<package name="691778100004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 4pins</description>
</package>
<package name="691778130018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 18pins</description>
</package>
<package name="691778140016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 16pins</description>
</package>
<package name="691778140020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 20pins</description>
</package>
<package name="691778130024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 24pins</description>
</package>
<package name="691778110012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 12pins</description>
</package>
<package name="691778130008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 8pins</description>
</package>
<package name="691778100020">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 20pins</description>
</package>
<package name="691778100012">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 12pins</description>
</package>
<package name="691778110008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 8pins</description>
</package>
<package name="691778130016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 16pins</description>
</package>
<package name="691778100024">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 24pins</description>
</package>
<package name="691778130004">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 4pins</description>
</package>
<package name="691778130010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 10pins</description>
</package>
<package name="691778110006">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 6pins</description>
</package>
<package name="691778140014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 14pins</description>
</package>
<package name="691778110016">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 16pins</description>
</package>
<package name="691778140008">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 8pins</description>
</package>
<package name="691778100018">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 18pins</description>
</package>
<package name="691778100014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 14pins</description>
</package>
<package name="691778110014">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 11.1mm, 14pins</description>
</package>
<package name="691778100010">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm, 10pins</description>
</package>
</packages>
<symbols>
<symbol name="1PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="10PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="9PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="11X2PT">
<description>11x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="8PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="7PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="6PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="3X2MT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2MT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5X2MT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="7ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="19PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
</symbol>
<symbol name="4X2MT">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6X2MT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="15PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="5PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="23PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
</symbol>
<symbol name="8X2MT">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="2ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="11PT">
<description>Socket Header THT,11Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="12PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="12ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="14PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="5ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="16PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="21PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
</symbol>
<symbol name="4ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="9PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="10PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="17PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
</symbol>
<symbol name="13PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="24PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="18PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="20PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="22PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="3X2MT_1">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8X2MT_1">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="5X2MT_1">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6X2MT_1">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2X2MT_1">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2MT_1">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="7X2MT">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10X2MT">
<description>10x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="9X2MT">
<description>9x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="7X2MT_1">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="2PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="3PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="3PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="12PT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="12PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="10PT-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="3PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="3PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8PT-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="10PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="10PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12PT-4">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4PT-12">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12PT-5">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5PT-13">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="10PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2PT-12">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="12PT-6">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5PT-12">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT-12">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-12">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6PT-13">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2PT-14">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PT-13">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT-13">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PT-13">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12PT-7">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4PT-14">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12PT-8">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-11">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2X2PT">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12PT-9">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2PT-15">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PT-14">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="3X2PT">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT-14">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2X2PT-1">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2PT">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2PT-1">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12PT-10">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT-15">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4X2PT-2">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2PT-16">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7X2PT">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10X2PT">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="9X2PT">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="3X2PT-1">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT-16">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="8X2PT">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="9X2PT-1">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="6PT-14">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10X2PT-1">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="2X2PT-2">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2PT-3">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2PT-2">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="12X2PT">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="6X2PT">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="7X2PT-1">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="8X2PT-1">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="5X2PT">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6X2PT-1">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8X2PT-2">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="10X2PT-3">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="10X2PT-2">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="5X2PT-1">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7X2PT-2">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="12X2PT-1">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="6X2PT-3">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6X2PT-2">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5X2PT-2">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7X2PT-3">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="9X2PT-2">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="3X2PT-3">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2PT-3">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12X2PT-2">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="5X2PT-3">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8X2PT-3">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="12X2PT-3">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="9X2PT-3">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="3X2PT-4">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10X2PT-4">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="7X2PT-4">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="3X2PT-5">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="12X2PT-4">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="8X2PT-4">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="9X2PT-4">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="2X2PT-4">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5X2PT-4">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2PT-4">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6X2PT-4">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2X2PT-5">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5X2PT-5">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12X2PT-5">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="9X2PT-5">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="6X2PT-5">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10X2PT-5">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="3X2PT-6">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2PT-6">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8X2PT-5">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="9X2PT-6">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="10X2PT-6">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="12X2PT-6">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="6X2PT-6">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8X2PT-6">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="4X2PT-5">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10X2PT-7">
<description>10x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="6X2PT-7">
<description>6x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4X2PT-6">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12X2PT-7">
<description>12x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="2X2PT-7">
<description>2x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5X2PT-6">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="3X2PT-7">
<description>3x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8X2PT-7">
<description>8x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="7X2PT-5">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="4X2PT-7">
<description>4x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="9X2PT-7">
<description>9x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="5X2PT-7">
<description>5x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7X2PT-7">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="7X2PT-6">
<description>7x2Rows Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="691328310010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691328310010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357300006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691357300006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357300006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357300006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691357300006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691330300006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701320002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356310004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691356310004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356310004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356310004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691356310004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305130006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691382010007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691382010007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691322310007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305330003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357300010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691357300010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357300010B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357300010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691357300010B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691321300008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691309310003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691325110008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691309310008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356310006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691356310006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356310006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356310006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691356310006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691308330006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691322110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300023" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691321300023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300023?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300023"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300023"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691310340007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357300012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691357300012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357300012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357300012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691357300012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310019" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691322310019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310019?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310019"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691327310008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305330005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691327310016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356300006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691356300006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356300006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356300006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691356300006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691328310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691328310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691323100003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691307300007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691382040008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356310012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691356310012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356310012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356310012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691356310012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691322310002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691328310016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691328310016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305340002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300019" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691321300019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300019?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300019"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691325110003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691329300016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691308330005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691322310015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691308330002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691309310007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691321300016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691321300014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691322310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691321100012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691305140012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691325310012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691308330012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2" route="any"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691325110012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691309310006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691305340012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691321100005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305140008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701320006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691321300011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305340003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701310006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701320005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701310003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691310340006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691329300012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691323100012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357310012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Horizontal Male PCB Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691357310012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357310012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357310012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691357310012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691308330007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691327310012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357310008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Horizontal Male PCB Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691357310008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357310008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357310008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691357310008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691382000005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305140005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691310340008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691382010005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357300008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691357300008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357300008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357300008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691357300008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691307300012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691327310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691321300012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305140006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310021" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691322310021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310021"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305130003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305340004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701310005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691310340004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305340005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691323300005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691321300009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691321100008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691325310008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701310010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691382040012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701340004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305340008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300021" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691321300021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300021"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691322310017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305130002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-10-30&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691321300004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691322110008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305130005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305140004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691323300004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691382010008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701320010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691322310013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691308330004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691329300010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305330004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691321300002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691322310010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305140003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691325310007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691323300012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691382030005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691322110002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691325110007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691322110005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691328310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691328310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305140002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691307300002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691325110005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356300010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691356300010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356300010B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356300010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691356300010B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691325310002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305330007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305130008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691321100006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305330008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691307300003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701310002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357310010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Horizontal Male PCB Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691357310010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357310010B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357310010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691357310010B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691330300010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356300008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691356300008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356300008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356300008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691356300008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691327310010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 m�� 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691325310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305130004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691321300007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691307500006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305340007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691321100004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691322310024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691323300008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691327310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33343v209%20Family_WR-TL_6913273100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3273_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913273100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691327310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691327310006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691327310006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Dual Horizontal"/>
<attribute name="VALUE" value="691327310006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691329300008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691321300015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691325310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691307300006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691322310018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691330300016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691322110012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356310008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691356310008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356310008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356310008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691356310008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356300004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691356300004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356300004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356300004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691356300004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691322310005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305140007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84264v209%20Family_WR-TBL3_6913051400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3051_HORIZONTAL_PCB_HEADER_6913051400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305140007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305140007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305140007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305140007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691328310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691328310008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357300004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60706v209%20Family_WR-TBL_Serie_357B_6913573000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913573000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691357300004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357300004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357300004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691357300004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691322310020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356300012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60701v209%20WR-TBL_356B_6913563000xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913563000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691356300012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356300012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356300012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691356300012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691382040007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691330300012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691382000006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691328310012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3283 - 3.81 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33281v209%20Family_WR-TBL_6913283100xx.jpg width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3283_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913283100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691328310012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691328310012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691328310012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691328310012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357310004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Horizontal Male PCB Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691357310004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357310004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357310004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691357310004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691322310003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691308330008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691321300006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691356310010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 356B - 3.81 mm Double Level Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60704v209%20Family_WR-TBL_Serie_356B_6913563100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_356B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913563100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691356310010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691356310010B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691356310010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691356310010B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305330006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691325310005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691330300008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691330300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3303 - 3.81 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33283v209%20Family_WR-TBL_6913303000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3303_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913303000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691330300004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691330300004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691330300004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691330300004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325310003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3253 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33280v209%20Family_WR-TBL_69132531000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3253_HORIZONTAL_PCB_HEADER_W_FLANGES_69132531000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691325310003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325310003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325310003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691325310003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691382040005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691382030004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691321100002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691382000002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691382040002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691322310011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305130007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691382010003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691382040006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691322310008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691325110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691321300005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691382030002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691310340002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310023" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691322310023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310023?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310023"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310023"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691321100007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691310340012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691321300018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691321300010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691382030012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691310340005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701320012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300022" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691321300022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300022?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300022"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701340002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701340003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701320008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691325110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691382010012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691322310009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691323300003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701320004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691382040004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691323100005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691322110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691321300017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691325110002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3251 - 3.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33340v209%20Family_WR-TLB_69132511000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3251_HORIZONTAL_PCB_HEADER_W_FLANGES_69132511000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691325110002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691325110002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691325110002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691325110002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382040003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55406v209%20Family_WR-TBL_Serie_382_6913820400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_W_FLANGES_69138204000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691382040003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382040003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382040003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382040003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691322310012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691321300020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691322110007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701340005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701310008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701310004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701310012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701310012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701310012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701310012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701310012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305340006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84290v209%20Family_WR-TBL3_6913053400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_HORIZONTAL_PCB_HEADER_6913053400xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305340006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305340006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305340006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305340006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701340012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701350002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691323100008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691382010006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691323100007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305330002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701340006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691309310004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305330012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3053 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84288v209%20Family_WR-TBL_6913053300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3053_VERTICAL_PCB_HEADER_6913053300xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691305330012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305330012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305330012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305330012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701350008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691329300006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691309310005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701350006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691323300002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691309310012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701350005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691323100004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691382010004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701340008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691382030006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691382030008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691321300003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322110003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3221 - 3.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33276v209%20Family_WR-TBL_69132211000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691322110003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322110003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322110003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322110003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691382000012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300700024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 300 - 5.00 mm Pin Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;IR VDE 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33250v209%20Family_WR-TBL_691300700024.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33250v209%20Family_WR-TBL_691300700024.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_300_PIN_HEADER_691300700024/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_300_PIN_HEADER_691300700024/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691300700024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300700024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300700024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300700024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701350012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311700102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700102?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700102"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701350004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701340010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701340010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701340010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701340010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701340010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700103" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311700103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700103?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700103"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321100003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3211 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33274v209%20Family_WR-TBL_69132110000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3211_VERTICAL_PCB_HEADER_69132110000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="691321100003" package="691321100003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321100003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321100003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321100003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700107" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311700107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700107?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700107"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701320003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701320003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701320003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701320003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical THR"/>
<attribute name="VALUE" value="691701320003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701350003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701350010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7013B - PCB Header - 3.81mm pitch - THR
&lt;br&gt;Series 7013B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33328v209%20Multi-WR-TBL-691701310004B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7013B_TERMINAL_BLOCKS_PCB_HEADER_3_81_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701350010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701350010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="IR-VDE" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701350010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701350010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WITHSTANDING-VOLTAGE-VDE" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700104" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311700104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700104?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700104"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700108" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311700108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700108?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700108"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691318700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691318700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700106" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311700106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700106?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700106"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691313710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691313710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691318700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311700012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700105" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311700105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700105?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700105"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691313710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691318700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691313710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691318700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691313710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305130012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3051 - 3.50 mm Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 12 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84262v209%20Family_WR-TBL3_6913051300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_3051_VERTICAL_PCB_HEADER_6913051300xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691305130012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305130012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305130012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305130012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700112" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33260v209%20Family_WR-TBL_69131170010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_CLOSE_VERTICAL_PCB_HEADER_69131170010X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311700112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700112?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700112"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700112"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691313710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691312710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691312710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691382000003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691312710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691386700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691318700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691382030007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691308330003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3083 - 3.81 mm Vertical Reserved PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60784v209%20WR-TBL_6913083300xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3083_VERTICAL_RESERVED_PCB_HEADER_W_FLANGES_6913083300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691308330003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2" route="any"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691308330003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691308330003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical PCB Header"/>
<attribute name="VALUE" value="691308330003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3117 - 5.00 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46; PA66
&lt;br&gt;Insulator Flammability Rating UL94 V-0
&lt;br&gt;Contact Material Brass
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33259v209%20Family_WR-TBL_69131170000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_00_3117_OPEN_VERTICAL_PCB_HEADER_69131170000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311700007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311700007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311700007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309310002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3093 - 3.81 mm Horizontal Reserved PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86366v209%20Family_WR-TBL_6913093100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3093_HORIZONTAL_RESERVED_PCB_HEADER_W_FLANGES_6913093100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691309310002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309310002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309310002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691309310002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691322310014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382030003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55404v209%20Family_WR-TBL_Serie_382_6913820300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_W_FLANGES_69138203000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691382030003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382030003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382030003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382030003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310022" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691322310022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310022?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310022"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691357310006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 357B - 3.81 mm Double Level Horizontal Male PCB Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60711v209%20Family_WR-TBL_Serie_357B_6913573100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_357B_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913573100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-23&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691357310006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691357310006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691357310006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691357310006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691322310016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691323300007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691323100002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691310340003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3103 - 3.81 mm Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60781v209%20Family_TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3103_HORIZONTAL_PCB_HEADER_W_FLANGES_6913103400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-19&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691310340003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691310340003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691310340003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal PCB Header"/>
<attribute name="VALUE" value="691310340003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691307300004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2" route="any"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691321300013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691321300024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 321 - 3.81 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33275v209%20Family_WR-TBL_6913213000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_321_VERTICAL_PCB_HEADER_6913213000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691321300024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691321300024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691321300024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691321300024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3233 - 3.81 mm Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33279v209%20Family_WR-TBL_69132330000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3233_VERTICAL_PCB_HEADER_W_FLANGES_69132330000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691323300006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323300006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323300006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323300006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691382000008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382000004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55400v209%20Family_WR-TBL_Serie_382_6913820000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_VERTICAL_PCB_HEADER_69138200000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691382000004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382000004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382000004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691382000004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691318700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691323100006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3231 - 3.50 mm Vertical PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33278v209%20Family_WR-TBL_69132310000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_3231_VERTICAL_PCB_HEADER_W_FLANGES_69132310000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-18&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691323100006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691323100006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691323100006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691323100006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691386700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691312710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691329300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3293 - 3.81 mm Double Level Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33282v209%20Family_WR-TBL_6913293000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3293_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913293000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691329300004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691329300004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691329300004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691329300004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691307300008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691386700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691386700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318700012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3187 - 5.00 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33272v209%20Family_WR-TBL_69131870000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3187_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131870000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691318700012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318700012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318700012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318700012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307300005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3073 - 3.81 mm Vertical Reversed PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 8 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
Wire Strip Length 7 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60791v209%20Family_TBL_3_81_3073_VERTICAL_RESERVED_PCB_HEADER_6913073000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_3073_VERTICAL_REVERSED_PCB_HEADER_6913073000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691307300005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307300005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307300005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307300005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691322310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 322 - 3.81 mm Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 10.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33277v209%20Family_WR-TBL_6913223100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_322_HORIZONTAL_PCB_HEADER_6913223100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691322310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691322310004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691322310004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691322310004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691382010002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 382 - 2.50 mm Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 12 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55402v209%20Family_WR-TBL_Serie_382_6913820100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_382_HORIZONTAL_PCB_HEADER_69138201000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-13&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691382010002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691382010002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691382010002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691382010002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691312710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691386700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691312710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691312710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691386700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691371700008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691386700018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691386700014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691371700007B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700007B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700007B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691313710012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691386700011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691386700013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691386700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691371700003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700003B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700003B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691386700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3137 - 5.00 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33266v209%20Family_WR-TBL_69131371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3137_CLOSE_HORIZONTAL_PCB_HEADER_69131371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691313710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313710004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313710004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313710004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691386700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691386700015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691371700006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691371700005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700005B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700005B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312710012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3127 - 5.00 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33263v209%20Family_WR-TBL_69131271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3127_OPEN_HORIZONTAL_PCB_HEADER_69131271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691312710012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312710012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312710012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312710012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691371700012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691370710007B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710007B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710007B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691317710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691370710012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710012B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710012B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691370710003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710003B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710003B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691371700004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691386700017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691317710012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691317710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691370710006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691370710002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710002B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710002B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691317710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691370710005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710005B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710005B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500108" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311500108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500108?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500108"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691371700002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 371B - 5.00 mm Vertical Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60725v209%20Family_Con_TBL_Pluggable_5.00_PCB_V_6913717000xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_371B_VERTICAL_MALE_PCB_HEADER_69137170000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691371700002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691371700002B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691371700002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691371700002B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500110" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691311500110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500110?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500110"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691317710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691386700016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691370710004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691370710008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 370B - 5.00 mm Horizontal Male PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55394v209%20Family_Con_TBL_Pluggable_5_PCB_H_6913707100xxB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_370B_HORIZONTAL_MALE_PCB_HEADER_69137071000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691370710008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691370710008B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691370710008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691370710008B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500112" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311500112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500112?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500112"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500112"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500105" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311500105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500105?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500105"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500107" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311500107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500107?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500107"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500113" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691311500113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500113?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500113"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500113"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691317710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691317710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3177 - 5.00 mm Close Horizontal PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33269v209%20Family_WR-TBL_69131771000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_3177_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131771000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691317710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317710007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317710007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317710007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500114" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691311500114">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500114?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500114"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500114"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500106" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311500106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500106?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500106"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311500102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500102?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500102"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500104" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311500104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500104?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500104"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500117" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691311500117">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500117?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500117"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500117"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500111" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691311500111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500111?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500111"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500111"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701510005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500123" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691311500123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500123?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500123"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500123"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500119" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691311500119">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500119?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500119"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500119"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500103" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311500103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500103?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500103"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500116" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691311500116">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500116?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500116"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500116"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500118" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691311500118">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500118?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500118"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500109" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691311500109">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500109?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500109"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500120" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691311500120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500120?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500120"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500120"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701510012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701510002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701510010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500115" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691311500115">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500115?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500115"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701510003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701510004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701510008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701510006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701510006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701510006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701510006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701510006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691333500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500122" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691311500122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500122?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500122"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691333500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500121" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691311500121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500121"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500124" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66; PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33258v209%20Family_WR-TBL_6913115001xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX//?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_CLOSE_VERTICAL_PCB_HEADER_6913115001XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691311500124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500124?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500124"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500124"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691311500009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691333500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691333500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691333500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691386700012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 386 - 5.00 mm Male PCB Header-Horizontal/Vertical Header Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55398v209%20Family_WR-TBL_Serie_386_6913867000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_386_HORIZONTAL_VERTICAL_HEADER_DIVISIBLE_MALE_PCB_HEADER_6913867000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691386700012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691386700012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691386700012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal/Vertical PCB Header"/>
<attribute name="VALUE" value="691386700012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691311500014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311500002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500019" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691311500019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500019?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500019"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691333500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3335 - 5.08 mm Double Level Vertical Male PCB Header with Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33285v209%20Family_WR-TBL_6913335000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3335_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_6913335000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691333500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691333500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691333500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691333500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311500003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691318500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691311500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691311500015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691336500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3365 - 5.08 mm Double Level Vertical Header with Flanges  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33288v209%20Family_WR-TBL_6913365000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3365_DOUBLE_LEVEL_VERTICAL_HEADER_W_FLANGES_6913365000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691336500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691336500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691336500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691336500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691311500013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691311500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500021" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691311500021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500021"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691318500002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691311500011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691311500020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691311500018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691334500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691334500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691318500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691318500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691318500003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691311500024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691318500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500022" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691311500022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500022?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500022"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691334500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691334500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691338500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3385 - 5.08 mm Double Level Vertical Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33290v209%20Family_WR-TBL_6913385000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3385_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_6913385000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691338500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691338500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691338500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691338500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="691334500014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500023" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691311500023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500023?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500023"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500023"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691313510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="691334500020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691334500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691318500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691313510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691334500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311500017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Open Vertical PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33257v209%20Family_WR-TBL_6913115000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_5_08_311_OPEN_VERTICAL_PCB_HEADER_6913115000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691311500017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311500017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311500017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311500017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691334500018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3345 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33286v209%20Family_WR-TBL_6913345000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3345_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913345000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT"/>
</gates>
<devices>
<device name="" package="691334500018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691334500018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691334500018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691334500018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691313510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691313510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691331510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691313510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691313510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691313510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691331510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691313510020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691313510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691313510017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691313510018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691313510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3185 - 5.08 mm Close Vertical PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33271v209%20Family_WR-TBL_69131850000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3185_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131850000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691318500012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510021" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691313510021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510021"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691313510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691337500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3375 - 5.08 mm Double Level Vertical Male PCB Header w. Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33289v209%20Family_WR-TBL_6913375000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3375_DOUBLE_LEVEL_VERTICAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913375000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691337500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691337500010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691337500010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="VALUE" value="691337500010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510023" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691313510023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510023?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510023"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510023"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691313510013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691313510011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691312510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510019" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691313510019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510019?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510019"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691331510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691313510014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691313510024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691312510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691331510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691312510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691312510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691312510011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510011?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510011"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691312510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691312510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691319510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3195 - 5.08 mm Double Level Horizontal Male PCB Header w. closed Flanges &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33273v209%20Family_WR-TBL_6913195100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3195_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_6913195100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691319510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691319510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691319510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691319510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691312510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510019" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691312510019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510019?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510019"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510014" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691312510014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510014?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510014"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510022" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691313510022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510022?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510022"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510021" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691312510021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510021"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510013" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691312510013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510013?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510013"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691312510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691312510015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691312510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691313510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313510015" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 313 - 5.08 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 [Model number 313] 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33265v209%20Family_WR-TBL_6913135100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_5_08_313_CLOSE_HORIZONTAL_PCB_HEADER_6913135100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691313510015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313510015?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313510015"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313510015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691331510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510020" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691312510020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510020?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510020"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510024" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691312510024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691317510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691312510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510022" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691312510022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510022?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510022"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510018" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691312510018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510018?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691317510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691317510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691317510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510023" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691312510023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510023?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510023"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510023"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691317510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="691332510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691312510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="691332510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691317510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691314520102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520102?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520102"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="691332510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="691332510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691317510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3175 - 5.08 mm Close Horizontal PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33268v209%20Family_WR-TBL_69131751000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3175_CLOSE_HORIZONTAL_PCB_HEADER_W_FLANGES_69131751000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691317510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317510005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317510005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317510005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="691332510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520113" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="691314520113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520113?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520113"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520113"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520103" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691314520103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520103?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520103"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691332510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3325 - 5.08 mm Double Level Horizontal Male PCB Header with Flanges &amp; Nut Type&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60739v209%20Family_WR-TBL_3325_691332510004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3325_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_AND_NUT_6913325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691332510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691332510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691332510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691332510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691331510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3315 - 5.08 mm Double Level Horizontal Male PCB Header w. Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33284v209%20Family_WR-TBL_6913315100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3315_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_FLANGES_6913315100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="691331510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691331510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691331510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691331510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520114" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="691314520114">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520114?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520114"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520114"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520109" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691314520109">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520109?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520109"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520112" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691314520112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520112?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520112"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520112"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520117" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691314520117">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520117?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520117"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520117"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520107" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691314520107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520107?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520107"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520118" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="691314520118">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520118?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520118"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520108" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691314520108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520108?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520108"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520106" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691314520106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520106?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520106"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520123" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23PT"/>
</gates>
<devices>
<device name="" package="691314520123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520123?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520123"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520123"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520110" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691314520110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520110?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520110"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520105" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691314520105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520105?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520105"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691320510016" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3205 - 5.08 mm Double Level Horizontal Male PCB Header with closed Flanges &amp; Nut Type &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33339v209%20Family_WR-TLB_6913205100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3205_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_W_CLOSED_FLANGES_AND_NUT_6913205100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="691320510016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691320510016?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691320510016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691320510016"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520121" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21PT"/>
</gates>
<devices>
<device name="" package="691314520121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520121"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520111" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PT"/>
</gates>
<devices>
<device name="" package="691314520111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520111?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520111"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520111"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691307500003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312510017" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 312 - 5.08 mm Open Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33262v209%20Family_WR-TBL_6913125100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_312_OPEN_HORIZONTAL_PCB_HEADER_6913125100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="17PT"/>
</gates>
<devices>
<device name="" package="691312510017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312510017?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312510017"/>
<attribute name="PINS" value=" 17 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312510017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691335510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3355 - 5.08 mm Double Level Modular Horizontal Male PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33287v209%20Family_WR-TBL_6913355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3355_DOUBLE_LEVEL_HORIZONTAL_MALE_PCB_HEADER_6913355100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_1"/>
</gates>
<devices>
<device name="" package="691335510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691335510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691335510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="VALUE" value="691335510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520115" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="691314520115">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520115?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520115"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520116" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="691314520116">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520116?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520116"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520116"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520119" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19PT"/>
</gates>
<devices>
<device name="" package="691314520119">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520119?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520119"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520119"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691309510002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691307500007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691307500002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520120" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="691314520120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520120?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520120"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520120"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520124" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691314520124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520124?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520124"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520124"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691309510012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691309510003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691307500005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701500008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691307500008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701500006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701500004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701500012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701520002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691309510006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701520006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701520004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701500010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701520005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691307500004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691309510005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701500002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701500005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520104" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691314520104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520104?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520104"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691309510008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307500012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3075 - 5.08 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33112v209%20Family_WR-LTB_69130750000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3075_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130750000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691307500012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307500012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307500012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307500012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701530002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701530004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701530008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701500003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701500003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701500003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701500003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701500003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701540002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691309510004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701550003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3095 - 5.08 mm Reversed Gender Horizontal PCB Header  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33254v209%20Family_WR-TBL_69130951000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3095_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130951000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-27&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691309510007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309510007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309510007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309510007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701520012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701540003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701530005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701530003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701530006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701530012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701540010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691701520003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520003B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701550006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701550004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701520008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701530010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701530010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701530010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701530010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701530010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691701540006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540006B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701520010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701520010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701520010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701520010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691701520010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691701540005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691701550002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550002B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701540012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305540006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701540008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691701550012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550012B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691701550010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550010B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305540003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691701550008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550008B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701550005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701550005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701550005B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701550005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701550005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305530007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691305540007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691305540010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691305530010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530010?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305540004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305540005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305530002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691305530003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400112" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311400112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400112?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400112"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400112"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691305540009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311400007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691305530005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691318400003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400106" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311400106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400106?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400106"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311400102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400102?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400102"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701540004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7015B - PCB Header - 5.08mm pitch - THR
&lt;br&gt;Series 7015B
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Industrial
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33333v209%20Family-WR-TBL-6917015100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;https://www.we-online.com/components/products/WR_TBL_SERIES_7015B_TERMINAL_BLOCKS_PCB_HEADER_5_08_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-12-16&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691701540004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701540004B?ae"/>
<attribute name="IR-CULUS" value="10A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701540004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691701540004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="4000V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400104" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311400104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400104?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400104"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311400003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400105" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311400105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400105?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400105"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305530008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691305540002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400103" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691311400103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400103?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400103"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691305530004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691313410008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="691305530009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530009?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530009"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400108" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311400108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400108?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400108"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691318400008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305530006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5,08 mm - PCB Header Vertical Entry with Plastic Latches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135349v209%20Family_WR-TBL3_6913055300xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055300XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691305530006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305530006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305530006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691305530006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691311400004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691311400002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691318400004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691313410005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691318400002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691311400005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691318400005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691313410006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691305540008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3055 - 5.08 mm - PCB Header Horizontal Entry with Plastic Latches &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Tin-plated surface 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135351v209%20Family_WR-TBL3_6913055400xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_3055_6913055400XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691305540008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691305540008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691305540008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691305540008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691313410012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691311400006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691318400006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691318400012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691311400008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691313410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400107" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Close Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33256v209%20Family_WR-TBL_69131140010x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_CLOSE_VERTICAL_PCB_HEADER_69131140010X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691311400107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400107?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400107"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691318400007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3184 - 7.62 mm Close Vertical PCB Header with Flanges&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33270v209%20Family_WR-TBL_69131840000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3184_CLOSE_VERTICAL_PCB_HEADER_W_FLANGES_69131840000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691318400007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691318400007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691318400007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691318400007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691312410005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691312410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410005" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691317410005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691312410007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410003" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691317410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691311400012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3114 - 7.62 mm Open Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33255v209%20Family_WR-TBL_69131140000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/TBL_7_62_3114_OPEN_VERTICAL_PCB_HEADER_69131140000X&lt;a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2022-07-25&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691311400012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691311400012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691311400012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691311400012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691312410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410002" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691317410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691313410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691313410007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691312410004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691312410008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691313410004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3134 - 7.62 mm Close Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33264v209%20Family_WR-TBL_69131341000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3134_CLOSE_HORIZONTAL_PCB_HEADER_69131341000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691313410004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691313410004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691313410004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691313410004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691307400007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375400002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-2"/>
</gates>
<devices>
<device name="" package="691375400002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375400002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375400002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691375400002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691312410006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691307400004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410008" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691317410008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410012" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691317410012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691307400005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691312410012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3124 - 7.62 mm Open Horizontal PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33261v209%20Family_WR-TBL_69131241000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3124_OPEN_HORIZONTAL_PCB_HEADER_69131241000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691312410012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691312410012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691312410012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691312410012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410006" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691317410006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691307400006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691307400012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691309410002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691347000002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage 150 V 
&lt;br&gt;Working Voltage [cULus] 150 V 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-22&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-1"/>
</gates>
<devices>
<device name="" package="691347000002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691347000002B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691347000002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.50mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value="691347000002B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410004" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691317410004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691317410007" prefix="J">
<description>&lt;b&gt;WL-SMSW SMT Mono-color Side View Waterclear&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33342v209%20Family_WR-TL_69131741000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3174_CLOSE_HORIZONTAL_PCB_HEADER_69131741000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691317410007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691317410007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691317410007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691317410007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691309410006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375400004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-2"/>
</gates>
<devices>
<device name="" package="691375400004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375400004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375400004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691375400004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691307400003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691309410012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410012?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691307400002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="691309410007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410007?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410007"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410007"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375400003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-2"/>
</gates>
<devices>
<device name="" package="691375400003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375400003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375400003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691375400003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691309410005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691309410003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691307400008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3074 - 7.62 mm Reversed Gender Vertical PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33252v209%20Family_WR-TBL_69130740000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3074_REVERSED_GENDER_VERTICAL_PCB_HEADER_69130740000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691307400008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691307400008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691307400008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691307400008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375400006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-2"/>
</gates>
<devices>
<device name="" package="691375400006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
<connect gate="G$1" pin="6" pad="6 A6 B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375400006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375400006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691375400006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375410002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-3"/>
</gates>
<devices>
<device name="" package="691375410002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375410002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375410002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375410002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691347000004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage 150 V 
&lt;br&gt;Working Voltage [cULus] 150 V 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-02-22&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-1"/>
</gates>
<devices>
<device name="" package="691347000004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691347000004B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691347000004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.50mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value="691347000004B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300100002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-24 &lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-5"/>
</gates>
<devices>
<device name="" package="691300100002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300100002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300100002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.50mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300100002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691347000003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage 150 V 
&lt;br&gt;Working Voltage [cULus] 150 V 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-02-22&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-1"/>
</gates>
<devices>
<device name="" package="691347000003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691347000003B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691347000003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.50mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value="691347000003B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375400005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Vertical cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761981v209%20Multi-WR-TBL3-6913754000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TBL_SERIES_3754_PCB_HEADER_7_62_MM_PITCH_VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-2"/>
</gates>
<devices>
<device name="" package="691375400005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375400005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375400005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691375400005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300300003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3003 - Pin Header 3.81mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.81 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-24 &lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-6"/>
</gates>
<devices>
<device name="" package="691300300003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300300003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300300003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300300003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300300024" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3003 - Pin Header 3.81mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.81 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-12-17 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-6"/>
</gates>
<devices>
<device name="" package="691300300003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300300024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300300024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300300024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375460003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-4"/>
</gates>
<devices>
<device name="" package="691375460003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375460003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375460003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375460003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691309410004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300100003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-24 &lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-5"/>
</gates>
<devices>
<device name="" package="691300100003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300100003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300100003"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.50mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300100003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375410004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-3"/>
</gates>
<devices>
<device name="" package="691375410004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375410004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375410004"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375410004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375410003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-3"/>
</gates>
<devices>
<device name="" package="691375410003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375410003?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375410003"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375410003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375460005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-4"/>
</gates>
<devices>
<device name="" package="691375460005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375460005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375460005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375460005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691309410008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 3094 - 7.62 mm Reversed Gender Horizontal PCB Header &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33253v209%20Family_WR-TBL_69130941000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_3094_REVERSED_GENDER_HORIZONTAL_PCB_HEADER_69130941000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691309410008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691309410008?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691309410008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691309410008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375410006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-3"/>
</gates>
<devices>
<device name="" package="691375410006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
<connect gate="G$1" pin="6" pad="6 A6 B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375410006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375410006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375410006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-8"/>
</gates>
<devices>
<device name="" package="691701140003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-7"/>
</gates>
<devices>
<device name="" package="691701100002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691347000005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage 150 V 
&lt;br&gt;Working Voltage [cULus] 150 V 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-02-22&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-1"/>
</gates>
<devices>
<device name="" package="691347000005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691347000005B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691347000005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.50mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value="691347000005B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300300002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3003 - Pin Header 3.81mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.81 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767394v209%20Multi-WR-TBL3-6913003000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3003_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-24 &lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-6"/>
</gates>
<devices>
<device name="" package="691300300002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300300002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300300002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300300002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691347000006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3470B - PCB Header 2.50mm pitch - Vertical cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage 150 V 
&lt;br&gt;Working Voltage [cULus] 150 V 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257307v209%206913470000xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_THR_7015B_CLOSE_VERTICAL_PCB_HEADER_6917015100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-02-22&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-1"/>
</gates>
<devices>
<device name="" package="691347000006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691347000006B?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691347000006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.50mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value="691347000006B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-7"/>
</gates>
<devices>
<device name="" package="691701100003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-1"/>
</gates>
<devices>
<device name="" package="691701130012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375410005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761474v209%20Multi-WR-TBL3-6913754100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754__PCB_HEADER_7_62_MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-3"/>
</gates>
<devices>
<device name="" package="691375410005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375410005?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375410005"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375410005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691300100024" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3001 - Pin Header 3.50mm pitch - Vertical cable entry - THT&lt;br&gt;
&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature -40 up to +115 °C
&lt;br&gt;Pitch 3.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	10 A
&lt;br&gt;Working Voltage	300 V (AC)
&lt;br&gt;Withstanding Voltage	1600 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA46
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Pin Material	Brass
&lt;br&gt;Pin Plating	Tin over Nickel

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;cULus Approval	E315414
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o767396v209%20Multi-WR-TBL3-6913001000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3001_PIN_HEADER_3_81_MM_PITCH&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-12-17 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="691300100024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691300100024?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691300100024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.50mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691300100024"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-5"/>
</gates>
<devices>
<device name="" package="691701100004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375460006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-4"/>
</gates>
<devices>
<device name="" package="691375460006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
<connect gate="G$1" pin="5" pad="5 A5 B5"/>
<connect gate="G$1" pin="6" pad="6 A6 B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375460006?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375460006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375460006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375460004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-4"/>
</gates>
<devices>
<device name="" package="691375460004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
<connect gate="G$1" pin="3" pad="3 A3 B3"/>
<connect gate="G$1" pin="4" pad="4 A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375460004?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375460004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375460004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-2"/>
</gates>
<devices>
<device name="" package="691701100008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691314520122" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 314 - 5.08 mm Close PCB Header&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023195 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33267v209%20Family_WR-TBL_6913145201xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_314_CLOSE_PCB_HEADER_6913145201XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-26&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="691314520122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691314520122?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691314520122"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691314520122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-2"/>
</gates>
<devices>
<device name="" package="691701110012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-3"/>
</gates>
<devices>
<device name="" package="691701140010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-5"/>
</gates>
<devices>
<device name="" package="691701110006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-9"/>
</gates>
<devices>
<device name="" package="691701110002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-3"/>
</gates>
<devices>
<device name="" package="691701140012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-5"/>
</gates>
<devices>
<device name="" package="691701100005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-2"/>
</gates>
<devices>
<device name="" package="691701130010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-10"/>
</gates>
<devices>
<device name="" package="691701130003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-3"/>
</gates>
<devices>
<device name="" package="691701140008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-9"/>
</gates>
<devices>
<device name="" package="691701110003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-4"/>
</gates>
<devices>
<device name="" package="691701130008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-6"/>
</gates>
<devices>
<device name="" package="691701110004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-8"/>
</gates>
<devices>
<device name="" package="691701140002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-6"/>
</gates>
<devices>
<device name="" package="691701130006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-7"/>
</gates>
<devices>
<device name="" package="691701110005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-7"/>
</gates>
<devices>
<device name="" package="691701140006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-6"/>
</gates>
<devices>
<device name="" package="691701140005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700105B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-9"/>
</gates>
<devices>
<device name="" package="691701700105B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700105B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700105B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700105B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701140004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-8"/>
</gates>
<devices>
<device name="" package="691701140004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701140004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701140004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701140004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-4"/>
</gates>
<devices>
<device name="" package="691701110010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-8"/>
</gates>
<devices>
<device name="" package="691701100006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-5"/>
</gates>
<devices>
<device name="" package="691701100010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-7"/>
</gates>
<devices>
<device name="" package="691701130004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701110008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-5"/>
</gates>
<devices>
<device name="" package="691701110008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701110008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701110008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701110008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691375460002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 3754 - PCB Header 7.62mm pitch - Upsidedown Horizontal cable entry - THT&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 7.62 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -30 up to +160 °C 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 41 A 
&lt;BR&gt;Working Voltage 300 V (AC) 
&lt;BR&gt;Withstanding Voltage 1600 V (AC) 
&lt;BR&gt;Contact Resistance 5 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA66 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Green 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E150931 
&lt;BR&gt;Glow Wire Approval Conform [IEC 60335-1] 

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o761472v209%20Multi-WR-TBL3-6913754600xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/SERIES_3754_PCB_HEADER_7_62_MM_PITCH_UPSIDEDOWN_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-10-16&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-4"/>
</gates>
<devices>
<device name="" package="691375460002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1 B1"/>
<connect gate="G$1" pin="2" pad="2 A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691375460002?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691375460002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691375460002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701100012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-4"/>
</gates>
<devices>
<device name="" package="691701100012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701100012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701100012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701100012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700108B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-7"/>
</gates>
<devices>
<device name="" package="691701700108B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700108B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700108B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700108B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730008B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-6"/>
</gates>
<devices>
<device name="" package="691701730008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-8"/>
</gates>
<devices>
<device name="" package="691701130005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-11"/>
</gates>
<devices>
<device name="" package="691701710002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710002B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701130002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7011B - PCB Header - 3.5mm pitch - THR&lt;br&gt;
Series 7011B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 10A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;VDE approval: 40058871
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806674v209%20Family-WR-TBL-6917011100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7011B_PCB_HEADER_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-10"/>
</gates>
<devices>
<device name="" package="691701130002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701130002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701130002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691701130002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700103B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-11"/>
</gates>
<devices>
<device name="" package="691701700103B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700103B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700103B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700103B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740004B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-9"/>
</gates>
<devices>
<device name="" package="691701740004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700106B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-9"/>
</gates>
<devices>
<device name="" package="691701700106B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700106B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700106B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700106B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710108B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-8"/>
</gates>
<devices>
<device name="" package="691701710108B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710108B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710108B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710108B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700004B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-10"/>
</gates>
<devices>
<device name="" package="691701700004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700004B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700110B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-6"/>
</gates>
<devices>
<device name="" package="691701700110B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700110B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700110B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700110B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700104B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-11"/>
</gates>
<devices>
<device name="" package="691701700104B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700104B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700104B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700104B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730004B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-12"/>
</gates>
<devices>
<device name="" package="691701730004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730004B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-10"/>
</gates>
<devices>
<device name="" package="691701710005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710005B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710105B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-13"/>
</gates>
<devices>
<device name="" package="691701710105B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710105B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710105B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710105B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740008B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-9"/>
</gates>
<devices>
<device name="" package="691701740008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740008B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700010B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-8"/>
</gates>
<devices>
<device name="" package="691701700010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700010B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730012B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-5"/>
</gates>
<devices>
<device name="" package="691701730012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730006B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-10"/>
</gates>
<devices>
<device name="" package="691701730006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710110B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-7"/>
</gates>
<devices>
<device name="" package="691701710110B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710110B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710110B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710110B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740012B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-6"/>
</gates>
<devices>
<device name="" package="691701740012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740012B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730005B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-12"/>
</gates>
<devices>
<device name="" package="691701730005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700005B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-11"/>
</gates>
<devices>
<device name="" package="691701700005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700005B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700002B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-12"/>
</gates>
<devices>
<device name="" package="691701700002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700002B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740006B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-11"/>
</gates>
<devices>
<device name="" package="691701740006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740006B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700006B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-12"/>
</gates>
<devices>
<device name="" package="691701700006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700006B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-13"/>
</gates>
<devices>
<device name="" package="691701710006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710006B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710006B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700003B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-12"/>
</gates>
<devices>
<device name="" package="691701700003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700003B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710103B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-13"/>
</gates>
<devices>
<device name="" package="691701710103B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710103B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710103B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710103B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730002B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-13"/>
</gates>
<devices>
<device name="" package="691701730002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710104B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-13"/>
</gates>
<devices>
<device name="" package="691701710104B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710104B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710104B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710104B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700012B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-7"/>
</gates>
<devices>
<device name="" package="691701700012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700012B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740002B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-14"/>
</gates>
<devices>
<device name="" package="691701740002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740002B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740002B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-14"/>
</gates>
<devices>
<device name="" package="691701710004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710004B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710004B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700008B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-11"/>
</gates>
<devices>
<device name="" package="691701700008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700008B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700112B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-8"/>
</gates>
<devices>
<device name="" package="691701700112B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700112B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700112B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700112B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730010B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-11"/>
</gates>
<devices>
<device name="" package="691701730010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710012B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-9"/>
</gates>
<devices>
<device name="" package="691701710012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710012B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710012B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT"/>
</gates>
<devices>
<device name="" package="691378110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710010B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-9"/>
</gates>
<devices>
<device name="" package="691701710010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710010B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710102B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-15"/>
</gates>
<devices>
<device name="" package="691701710102B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710102B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710102B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710102B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710008B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-10"/>
</gates>
<devices>
<device name="" package="691701710008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710008B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710008B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-14"/>
</gates>
<devices>
<device name="" package="691701710003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710003B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT"/>
</gates>
<devices>
<device name="" package="691378140006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740005B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-14"/>
</gates>
<devices>
<device name="" package="691701740005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740005B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740005B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-1"/>
</gates>
<devices>
<device name="" package="691378100004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT"/>
</gates>
<devices>
<device name="" package="691378100008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740010B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-10"/>
</gates>
<devices>
<device name="" package="691701740010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740010B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740010B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710112B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-10"/>
</gates>
<devices>
<device name="" package="691701710112B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710112B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710112B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710112B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-1"/>
</gates>
<devices>
<device name="" package="691378140008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701740003B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-15"/>
</gates>
<devices>
<device name="" package="691701740003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701740003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701740003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701740003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-2"/>
</gates>
<devices>
<device name="" package="691378110008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT"/>
</gates>
<devices>
<device name="" package="691378110018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT"/>
</gates>
<devices>
<device name="" package="691378110020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT"/>
</gates>
<devices>
<device name="" package="691378100014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-1"/>
</gates>
<devices>
<device name="" package="691378130006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701700102B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-16"/>
</gates>
<devices>
<device name="" package="691701700102B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701700102B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701700102B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701700102B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701730003B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-16"/>
</gates>
<devices>
<device name="" package="691701730003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701730003B?ae"/>
<attribute name="IR-CULUS" value="15A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701730003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701730003B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT"/>
</gates>
<devices>
<device name="" package="691378140016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691701710106B" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header - 5mm pitch - THR&lt;br&gt;
Series 7017B
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 15A
&lt;br&gt;Working Voltage: 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o806699v209%20Family-WR-TBL-6917017300xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_7017B_PCB_HEADER_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-01-07 &lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-14"/>
</gates>
<devices>
<device name="" package="691701710106B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691701710106B?ae"/>
<attribute name="IR-CULUS" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691701710106B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="691701710106B"/>
<attribute name="WITHSTANDING-VOLTAGE-CULUS" value="1400V(AC)"/>
<attribute name="WORKING-VOLTAGE-CULUS" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-1"/>
</gates>
<devices>
<device name="" package="691378100020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-1"/>
</gates>
<devices>
<device name="" package="691378130018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-2"/>
</gates>
<devices>
<device name="" package="691378130004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-2"/>
</gates>
<devices>
<device name="" package="691378110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT"/>
</gates>
<devices>
<device name="" package="691378140024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-3"/>
</gates>
<devices>
<device name="" package="691378130008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-1"/>
</gates>
<devices>
<device name="" package="691378110014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-1"/>
</gates>
<devices>
<device name="" package="691378100016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT"/>
</gates>
<devices>
<device name="" package="691378140010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT"/>
</gates>
<devices>
<device name="" package="691378110012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-1"/>
</gates>
<devices>
<device name="" package="691378130012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-2"/>
</gates>
<devices>
<device name="" package="691378110016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-3"/>
</gates>
<devices>
<device name="" package="691378140020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-2"/>
</gates>
<devices>
<device name="" package="691378130020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-1"/>
</gates>
<devices>
<device name="" package="691378100010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-2"/>
</gates>
<devices>
<device name="" package="691378140014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-1"/>
</gates>
<devices>
<device name="" package="691378100024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-2"/>
</gates>
<devices>
<device name="" package="691378140012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-2"/>
</gates>
<devices>
<device name="" package="691378130010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-3"/>
</gates>
<devices>
<device name="" package="691378100012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-3"/>
</gates>
<devices>
<device name="" package="691378100006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-2"/>
</gates>
<devices>
<device name="" package="691378140018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378140004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-3"/>
</gates>
<devices>
<device name="" package="691378140004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378140004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378140004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378140004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-2"/>
</gates>
<devices>
<device name="" package="691378110024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378110010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-3"/>
</gates>
<devices>
<device name="" package="691378110010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378110010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378110010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378110010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-3"/>
</gates>
<devices>
<device name="" package="691378130016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-3"/>
</gates>
<devices>
<device name="" package="691378130014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-4"/>
</gates>
<devices>
<device name="" package="691778140006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-4"/>
</gates>
<devices>
<device name="" package="691778110020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378100018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-3"/>
</gates>
<devices>
<device name="" package="691378100018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378100018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378100018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378100018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691378130024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THT&lt;br&gt;
&lt;/b&gt;Series 3781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +115°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863051v209%20Family-WR-TBL3-6913781100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_SERIES_3781_3_50_MM_PITCH_PCB_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-3"/>
</gates>
<devices>
<device name="" package="691378130024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691378130024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691378130024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691378130024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-4"/>
</gates>
<devices>
<device name="" package="691778130014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-5"/>
</gates>
<devices>
<device name="" package="691778130006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-4"/>
</gates>
<devices>
<device name="" package="691778110024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-4"/>
</gates>
<devices>
<device name="" package="691778110018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-4"/>
</gates>
<devices>
<device name="" package="691778100016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-4"/>
</gates>
<devices>
<device name="" package="691778140010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-4"/>
</gates>
<devices>
<device name="" package="691778140004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-4"/>
</gates>
<devices>
<device name="" package="691778100008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-4"/>
</gates>
<devices>
<device name="" package="691778130012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-5"/>
</gates>
<devices>
<device name="" package="691778110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-5"/>
</gates>
<devices>
<device name="" package="691778110010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-5"/>
</gates>
<devices>
<device name="" package="691778140024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-5"/>
</gates>
<devices>
<device name="" package="691778130020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-5"/>
</gates>
<devices>
<device name="" package="691778140018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-6"/>
</gates>
<devices>
<device name="" package="691778100006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-5"/>
</gates>
<devices>
<device name="" package="691778140012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-6"/>
</gates>
<devices>
<device name="" package="691778100004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-6"/>
</gates>
<devices>
<device name="" package="691778130018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-5"/>
</gates>
<devices>
<device name="" package="691778140016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-6"/>
</gates>
<devices>
<device name="" package="691778140020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-6"/>
</gates>
<devices>
<device name="" package="691778130024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-6"/>
</gates>
<devices>
<device name="" package="691778110012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-5"/>
</gates>
<devices>
<device name="" package="691778130008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100020" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT-7"/>
</gates>
<devices>
<device name="" package="691778100020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100020?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100020"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100020"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100012" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT-7"/>
</gates>
<devices>
<device name="" package="691778100012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100012?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100012"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100012"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-6"/>
</gates>
<devices>
<device name="" package="691778110008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100024" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT-7"/>
</gates>
<devices>
<device name="" package="691778100024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100024?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100024"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100024"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-6"/>
</gates>
<devices>
<device name="" package="691778130016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-6"/>
</gates>
<devices>
<device name="" package="691778130010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110006" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT-7"/>
</gates>
<devices>
<device name="" package="691778110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110006?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110006"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110006"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778130004" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT-7"/>
</gates>
<devices>
<device name="" package="691778130004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778130004?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778130004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778130004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110016" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT-7"/>
</gates>
<devices>
<device name="" package="691778110016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110016?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110016"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110016"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-5"/>
</gates>
<devices>
<device name="" package="691778140014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778140008" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT-7"/>
</gates>
<devices>
<device name="" package="691778140008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778140008?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778140008"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778140008"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100018" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT-7"/>
</gates>
<devices>
<device name="" package="691778100018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100018?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100018"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100018"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778110014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-7"/>
</gates>
<devices>
<device name="" package="691778110014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778110014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778110014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778110014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1300V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100010" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT-7"/>
</gates>
<devices>
<device name="" package="691778100010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100010?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100010"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100010"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691778100014" prefix="J">
<description>&lt;b&gt;WR-TBL Terminal Blocks - PCB Header Dual Row - 3.5mm pitch - THR&lt;br&gt;
&lt;/b&gt;Series 7781
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 8A
&lt;br&gt;Working Voltage: 150V / 300V
&lt;br&gt;Operating temperature: -40°C up to +130°C
&lt;br&gt;UL approval: E315414
&lt;br&gt;UL 94-V0

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o863127v209%20Family-WR-TBL7-6917781000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_TBL_TERMINAL_BLOCKS_PCB_HEADER_DUAL_ROW_3_5_MM_PITCH_THR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT-6"/>
</gates>
<devices>
<device name="" package="691778100014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691778100014?ae"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="691778100014"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="691778100014"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1600V(AC)"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
