<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Terminal Blocks - WR-TBL Rising Cage Clamp &lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-08-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691216700003">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691233510004">
<description>&lt;b&gt;WR-TBL Serie 2335 – 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=31.5mm
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691241510004">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691253710002">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691214310003">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 3.81mm , 2 Pins</description>
</package>
<package name="691211720002">
<description>&lt;b&gt;WR-TBL Serie 211 - 5.00 mm 45° Entry Modular H=15.5mm 
&lt;br&gt;&lt;/b&gt;Max Height =15.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691216510003S">
<description>&lt;b&gt;WR-TBL Serie 2165S - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691241510006">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691243310010">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 10 Pins</description>
</package>
<package name="691243300006">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 6 Pins</description>
</package>
<package name="691233710006">
<description>&lt;b&gt;WR-TBL Serie 2337 - 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691244710005">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691213710002">
<description>&lt;b&gt;WR-TBL Serie 213 - 5.00 mm Horiz.l Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691252700002">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =6mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691243310009">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 9 Pins</description>
</package>
<package name="691243310007">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 7 Pins</description>
</package>
<package name="691709710303">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691221320005">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 5 Pins</description>
</package>
<package name="691242710005">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691243300008">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 8 Pins</description>
</package>
<package name="691508110304">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 4 Pins</description>
</package>
<package name="691242710010">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691244700007">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691241700009">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691215700002">
<description>&lt;b&gt;WR-TBL Serie 2157 - 5.00 mm Vertical Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =19mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691244700004">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691230110004">
<description>&lt;b&gt;WR-TBL Serie 2301 – 3.50 mm Double Level Horiz. Entry Modular w. Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =16.2mm , Pitch 3.5mm , 4 Pins</description>
</package>
<package name="691201520002">
<description>&lt;b&gt;WR-TBL Serie 2015 - 5.08 mm 45° Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691214100002">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691242500004">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691241710010">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691213510003">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691201720002S">
<description>&lt;b&gt;WR-TBL Serie 201S - 5.00 mm 45° Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691241510007">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691252700003">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =6mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691242510007">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691241700006">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691244710008">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691241710006">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691214100003">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.5mm , 3 Pins</description>
</package>
<package name="691242710007">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691241510008">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691243310006">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 6 Pins</description>
</package>
<package name="691221120002">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691221120005">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 5 Pins</description>
</package>
<package name="691210910002">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 2 Pins</description>
</package>
<package name="691241510005">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691231710004">
<description>&lt;b&gt;WR-TBL Serie 2317 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =19.1mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691232510006">
<description>&lt;b&gt;WR-TBL Serie 2325 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=25.3 mm 
&lt;br&gt;&lt;/b&gt;Max Height =25.3mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691214110002S">
<description>&lt;b&gt;WR-TBL Serie 2141S - 3.50 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691214110003">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 3.5mm , 3 Pins</description>
</package>
<package name="691241700010">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691244510005">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691242700007">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691241700008">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691243300005">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 5 Pins</description>
</package>
<package name="691213510002">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691236510003">
<description>&lt;b&gt;WR-TBL Serie 2365 - 5.08 mm Horiz. Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691231710006">
<description>&lt;b&gt;WR-TBL Serie 2317 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =19.1mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691243110009">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 9 Pins</description>
</package>
<package name="691230110006">
<description>&lt;b&gt;WR-TBL Serie 2301 – 3.50 mm Double Level Horiz. Entry Modular w. Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =16.2mm , Pitch 3.5mm , 6 Pins</description>
</package>
<package name="691709710308">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691201520003">
<description>&lt;b&gt;WR-TBL Serie 2015 - 5.08 mm 45° Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691242510006">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691242700010">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691242510004">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691244710006">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691214300002">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 2 Pins</description>
</package>
<package name="691213500002">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691243300004">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 4 Pins</description>
</package>
<package name="691243110008">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 8 Pins</description>
</package>
<package name="691241510009">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691242510010">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691244710009">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691221120003">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 3 Pins</description>
</package>
<package name="691254710003">
<description>&lt;b&gt;WR-TBL Serie 2547 - 5.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691242510005">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691243300009">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 9 Pins</description>
</package>
<package name="691216510002S">
<description>&lt;b&gt;WR-TBL Serie 2165S - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691233510006">
<description>&lt;b&gt;WR-TBL Serie 2335 – 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=31.5mm
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691232710006">
<description>&lt;b&gt;WR-TBL Serie 2327 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =25.3mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691249510002">
<description>&lt;b&gt;WR-TBL Serie 2495 - 5.08 mm Horiz.Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691216710002">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691241700005">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691233710004">
<description>&lt;b&gt;WR-TBL Serie 2337 - 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691253700003">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691244510008">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691242700009">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691241710005">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691241700007">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691244700008">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691243300010">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 10 Pins</description>
</package>
<package name="691232510004">
<description>&lt;b&gt;WR-TBL Serie 2325 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=25.3 mm 
&lt;br&gt;&lt;/b&gt;Max Height =25.3mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691242700008">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691242710009">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691236510002">
<description>&lt;b&gt;WR-TBL Serie 2365 - 5.08 mm Horiz. Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691242700006">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691231510004">
<description>&lt;b&gt;WR-TBL Serie 2315 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=19.1 mm 
&lt;br&gt;&lt;/b&gt;Max Height =19.1mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691210910005">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 5 Pins</description>
</package>
<package name="691508110308">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 8 Pins</description>
</package>
<package name="691244510010">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691244500009">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691244510007">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691244510009">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691231510006">
<description>&lt;b&gt;WR-TBL Serie 2315 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=19.1 mm 
&lt;br&gt;&lt;/b&gt;Max Height =19.1mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691210910008">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 8 Pins</description>
</package>
<package name="691244500004">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691244500005">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691244500008">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691243100006">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 6 Pins</description>
</package>
<package name="691244710010">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691242710006">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691241710009">
</package>
<package name="691242510008">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691241710004">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691243100007">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 7 Pins</description>
</package>
<package name="691244700005">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691243100008">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 8 Pins</description>
</package>
<package name="691254710002">
<description>&lt;b&gt;WR-TBL Serie 2547 - 5.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691232710004">
<description>&lt;b&gt;WR-TBL Serie 2327 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =25.3mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691213710003">
<description>&lt;b&gt;WR-TBL Serie 213 - 5.00 mm Horiz.l Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691243310005">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 5 Pins</description>
</package>
<package name="691241510010">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691252710003">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =17.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691244500006">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691244500007">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691242500007">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691241710007">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691242500010">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691253510003">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691244510006">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691245510004">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691242500006">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691242500008">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691242500009">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691253510002">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691241500004">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691234510006">
<description>&lt;b&gt;WR-TBL Series 2345 - 5.08 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691241500005">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691241500007">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691508110303">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 3 Pins</description>
</package>
<package name="691234510004">
<description>&lt;b&gt;WR-TBL Series 2345 - 5.08 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691241500006">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691241500009">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691254510002">
<description>&lt;b&gt;WR-TBL Serie 2545 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691245510008">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691253700002">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691242500005">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691235510002">
<description>&lt;b&gt;WR-TBL Serie 2355 - 5.08 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691253710003">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691709710306">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691243110010">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 10 Pins</description>
</package>
<package name="691242510009">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691242700005">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691244700006">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691242700004">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691216700002">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691244510004">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 4 Pins</description>
</package>
<package name="691252710002">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =17.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691213500003">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691210910004">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 4 Pins</description>
</package>
<package name="691508110302">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691249510003">
<description>&lt;b&gt;WR-TBL Serie 2495 - 5.08 mm Horiz.Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691221120006">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 6 Pins</description>
</package>
<package name="691214310002">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 3.81mm , 2 Pins</description>
</package>
<package name="691221320004">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 4 Pins</description>
</package>
<package name="691241700004">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691241710008">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691253500002">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 2 Pins</description>
</package>
<package name="691210910006">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 6 Pins</description>
</package>
<package name="691508110306">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 6 Pins</description>
</package>
<package name="691230310006">
<description>&lt;b&gt;WR-TBL Serie 2303 - 3.81 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =16.2mm , Pitch 3.81mm , 6 Pins</description>
</package>
<package name="691243310008">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 8 Pins</description>
</package>
<package name="691245510006">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691253500003">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691243100005">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 5 Pins</description>
</package>
<package name="691243100004">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 4 Pins</description>
</package>
<package name="691216710003">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691243110004">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 4 Pins</description>
</package>
<package name="691230310004">
<description>&lt;b&gt;WR-TBL Serie 2303 - 3.81 mm Double Level Horiz. Entry Modular w. Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =16.2mm , Pitch 3.81mm , 4 Pins</description>
</package>
<package name="691221320003">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 3 Pins</description>
</package>
<package name="691235510003">
<description>&lt;b&gt;WR-TBL Serie 2355 - 5.08 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691245510009">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691243110005">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 5 Pins</description>
</package>
<package name="691244700009">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691709710304">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691250610002">
<description>&lt;b&gt;WR-TBL Serie 2506 - 6.35 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 6.35mm , 2 Pins</description>
</package>
<package name="691211720003">
<description>&lt;b&gt;WR-TBL Serie 211 - 5.00 mm 45° Entry Modular H=15.5mm 
&lt;br&gt;&lt;/b&gt;Max Height =15.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691243200003">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 3 Pins</description>
</package>
<package name="691245510007">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 7 Pins</description>
</package>
<package name="691201720003S">
<description>&lt;b&gt;WR-TBL Serie 201S - 5.00 mm 45° Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691242710008">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691241500010">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691508110305">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12.2mm , Pitch 3.5mm , 5 Pins</description>
</package>
<package name="691247510009">
<description>&lt;b&gt;WR-TBL Serie 2475 - 5.08 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 9 Pins</description>
</package>
<package name="691244500010">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691243100010">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 10 Pins</description>
</package>
<package name="691243210009">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 9 Pins</description>
</package>
<package name="691243200006">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 6 Pins</description>
</package>
<package name="691245510010">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 10 Pins</description>
</package>
<package name="691243200007">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 7 Pins</description>
</package>
<package name="691243200009">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 9 Pins</description>
</package>
<package name="691243200010">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 10 Pins</description>
</package>
<package name="691247510006">
<description>&lt;b&gt;WR-TBL Serie 2475 - 5.08 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 5.08mm , 6 Pins</description>
</package>
<package name="691243200008">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 8 Pins</description>
</package>
<package name="691250610003">
<description>&lt;b&gt;WR-TBL Serie 2506 - 6.35 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 6.35mm , 3 Pins</description>
</package>
<package name="691212200101">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 1 Pins</description>
</package>
<package name="691243200005">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 5 Pins</description>
</package>
<package name="691243210010">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 10 Pins</description>
</package>
<package name="691243210008">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 8 Pins</description>
</package>
<package name="691212200001">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 1 Pins</description>
</package>
<package name="691243210003">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 3 Pins</description>
</package>
<package name="691243210007">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 7 Pins</description>
</package>
<package name="691243210006">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 6 Pins</description>
</package>
<package name="691253900003">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 7.5mm , 3 Pins</description>
</package>
<package name="691245510005">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 5 Pins</description>
</package>
<package name="691214210002">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 2 Pins</description>
</package>
<package name="691243300007">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 7 Pins</description>
</package>
<package name="691243210005">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 5 Pins</description>
</package>
<package name="691216910003">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691244700010">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691244710004">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691212200002">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 2 Pins</description>
</package>
<package name="691243200004">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7mm , 4 Pins</description>
</package>
<package name="691214210101">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 1 Pins</description>
</package>
<package name="691242910006">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 6 Pins</description>
</package>
<package name="691214210001">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 1 Pins</description>
</package>
<package name="691241500008">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 5.08mm , 8 Pins</description>
</package>
<package name="691242910007">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 7 Pins</description>
</package>
<package name="691243410004">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 4 Pins</description>
</package>
<package name="691216910002">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691242910009">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 9 Pins</description>
</package>
<package name="691221320008">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 8 Pins</description>
</package>
<package name="691214110002">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691253910002">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691243310004">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.81mm , 4 Pins</description>
</package>
<package name="691221120008">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 8 Pins</description>
</package>
<package name="691242910005">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 5 Pins</description>
</package>
<package name="691709710305">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691242910004">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 4 Pins</description>
</package>
<package name="691221320002">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 2 Pins</description>
</package>
<package name="691242710004">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691214110003S">
<description>&lt;b&gt;WR-TBL Serie 2141S - 3.50 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691709710302">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Max Height =10.9mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691243100009">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 9 Pins</description>
</package>
<package name="691243210004">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7mm , 4 Pins</description>
</package>
<package name="691210910003">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 2.54mm , 3 Pins</description>
</package>
<package name="691221120004">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.47mm , Pitch 3.5mm , 4 Pins</description>
</package>
<package name="691221320006">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =9.5mm , Pitch 3.81mm , 6 Pins</description>
</package>
<package name="691215700003">
<description>&lt;b&gt;WR-TBL Serie 2157 - 5.00 mm Vertical Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =19mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691243110007">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 7 Pins</description>
</package>
<package name="691242910008">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 8 Pins</description>
</package>
<package name="691244710007">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691254910002">
<description>&lt;b&gt;WR-TBL Serie 2549 - 7.50 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691214300003">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 3.81mm , 2 Pins</description>
</package>
<package name="691216400003">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Vertical Entry Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691216410002">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Horizon. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691216900003">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 7.5mm , 3 Pins</description>
</package>
<package name="691254910003">
<description>&lt;b&gt;WR-TBL Serie 2549 - 7.50 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.5mm , 3 Pins</description>
</package>
<package name="691253910003">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.5mm , 3 Pins</description>
</package>
<package name="691254510003">
<description>&lt;b&gt;WR-TBL Serie 2545 - 5.08 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 5.08mm , 3 Pins</description>
</package>
<package name="691243110006">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 3.5mm , 6 Pins</description>
</package>
<package name="691253900002">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691216900002">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691254410003">
<description>&lt;b&gt;WR-TBL Serie 2544 - 7.62 mm Horizontal Entry Dual Pin w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691254410002">
<description>&lt;b&gt;WR-TBL Serie 2544 - 7.62 mm Horizontal Entry Dual Pin w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691218410002">
<description>&lt;b&gt;WR-TBL Serie 2184 - 7.62 mm Horiz. Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691216410003">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Horizon. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691253410003">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691253410002">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691253400002">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691243410005">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 5 Pins</description>
</package>
<package name="691243410003">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691243410008">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 8 Pins</description>
</package>
<package name="691218410003">
<description>&lt;b&gt;WR-TBL Serie 2184 - 7.62 mm Horiz. Entry Modular 
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691253400003">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691216400002">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Vertical Entry Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691243400008">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 8 Pins</description>
</package>
<package name="691242910010">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 7.5mm , 10 Pins</description>
</package>
<package name="691243400005">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 5 Pins</description>
</package>
<package name="691243410010">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 10 Pins</description>
</package>
<package name="691243400009">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 9 Pins</description>
</package>
<package name="691243410006">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 6 Pins</description>
</package>
<package name="691214400101">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 1 Pins</description>
</package>
<package name="691243400010">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 10 Pins</description>
</package>
<package name="691250910003">
<description>&lt;b&gt;WR-TBL Serie 2509 - 9.52 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 9.52mm , 3 Pins</description>
</package>
<package name="691243400006">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 6 Pins</description>
</package>
<package name="691241810006">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 6 Pins</description>
</package>
<package name="691243410009">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 9 Pins</description>
</package>
<package name="691214410101">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 1 Pins</description>
</package>
<package name="691243410007">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 7 Pins</description>
</package>
<package name="691241810007">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 7 Pins</description>
</package>
<package name="691214400002">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691241810005">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 5 Pins</description>
</package>
<package name="691214410002">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 2 Pins</description>
</package>
<package name="691243400007">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 7 Pins</description>
</package>
<package name="691241810003">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691214400001">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 1 Pins</description>
</package>
<package name="691243400003">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 3 Pins</description>
</package>
<package name="691241810004">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691213800001">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691241810010">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 10 Pins</description>
</package>
<package name="691216810002">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691213800002">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691243400004">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =7.3mm , Pitch 7.62mm , 4 Pins</description>
</package>
<package name="691214410001">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =9.1mm , Pitch 7.62mm , 1 Pins</description>
</package>
<package name="691216800001">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691241810009">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 9 Pins</description>
</package>
<package name="691253800002">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691250910002">
<description>&lt;b&gt;WR-TBL Serie 2509 - 9.52 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =21.5mm , Pitch 9.52mm , 2 Pins</description>
</package>
<package name="691213810002">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691213800101">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691213810101">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691216800101">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691216800002">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691253800001">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691252800002">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =16mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691242810003">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Horizontal Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691241810008">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 8 Pins</description>
</package>
<package name="691213810001">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691244810004">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691244810003">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691244800004">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Vertical Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691242810004">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Horizontal Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691252810001">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =17.5mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691252810101">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =17.5mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691252800001">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =16mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691254810101">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691252810002">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =17.5mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691244800003">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Vertical Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691245810003">
<description>&lt;b&gt;WR-TBL Serie 2458 - 10.00 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691233810004">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691245810004">
<description>&lt;b&gt;WR-TBL Serie 2458 - 10.00 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691253800101">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691242800004">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691254810002">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691241800009">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 9 Pins</description>
</package>
<package name="691201820101">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691233810102">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691233810002">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691241800006">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 6 Pins</description>
</package>
<package name="691241800008">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 8 Pins</description>
</package>
<package name="691241800003">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691241800004">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691241800007">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 7 Pins</description>
</package>
<package name="691254610002">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691254810001">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691201820002">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691235610001">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691249610101">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691241800005">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 5 Pins</description>
</package>
<package name="691247610003">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691213610002">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691249610001">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691241800010">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10mm , 10 Pins</description>
</package>
<package name="691247610006">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 6 Pins</description>
</package>
<package name="691242610003">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691201620002">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691234610004">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691234610102">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691235610002">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691242800003">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Vertical Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691216600001">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691201620001">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691249610002">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691235610101">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691213610101">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691234610002">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691253600101">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691219610002">
<description>&lt;b&gt;WR-TBL Serie 2196 - 10.16 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =28.5mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691247610103">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =45mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691219610003">
<description>&lt;b&gt;WR-TBL Serie 2196 - 10.16 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =28.5mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691201820001">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691252800101">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =16mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691242610004">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp 
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691254610101">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691213610001">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691254610001">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage 
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691216600101">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691242600003">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691245610003">
<description>&lt;b&gt;WR-TBL Serie 2456 - 10.16 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691244610004">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691253600002">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691213600001">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691216600002">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691241610003">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691253600001">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691245610004">
<description>&lt;b&gt;WR-TBL Serie 2456 - 10.16 mm Horizontal Cable Entry Rising Cage
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691244600003">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Vertical Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691236610002">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691244600004">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Vertical Entry Modular w. Rising Clamp
&lt;br&gt;&lt;/b&gt;Max Height =11.2mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691201620101">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =12mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691236610101">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691253610001">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691244610003">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691236610001">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp  
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691233610102">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691241600007">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 7 Pins</description>
</package>
<package name="691241600003">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691241610004">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691253610101">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691233610004">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691241600009">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 9 Pins</description>
</package>
<package name="691241610006">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 6 Pins</description>
</package>
<package name="691256610012">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 12 Pins</description>
</package>
<package name="691241610009">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 9 Pins</description>
</package>
<package name="691256610006">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 6 Pins</description>
</package>
<package name="691213600101">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691241600008">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 8 Pins</description>
</package>
<package name="691241610008">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 8 Pins</description>
</package>
<package name="691241610010">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 10 Pins</description>
</package>
<package name="691213600002">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691241610005">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 5 Pins</description>
</package>
<package name="691256610010">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 10 Pins</description>
</package>
<package name="691242600004">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =9.8mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691216610002">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691256610011">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 11 Pins</description>
</package>
<package name="691256610004">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691241600006">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 6 Pins</description>
</package>
<package name="691241610007">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 10.16mm , 7 Pins</description>
</package>
<package name="691241600005">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 5 Pins</description>
</package>
<package name="691241600004">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 4 Pins</description>
</package>
<package name="691256610003">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 3 Pins</description>
</package>
<package name="691256610009">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 9 Pins</description>
</package>
<package name="691216610101">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691216610001">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =13.8mm , Pitch 10.16mm , 1 Pin</description>
</package>
<package name="691233610002">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =31.5mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691241600010">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =8.1mm , Pitch 10.16mm , 10 Pins</description>
</package>
<package name="691256610002">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691256610008">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 8 Pins</description>
</package>
<package name="691256610005">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 5 Pins</description>
</package>
<package name="691253610002">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp
&lt;br&gt;&lt;/b&gt;Max Height =18mm , Pitch 10.16mm , 2 Pins</description>
</package>
<package name="691256610007">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire 
&lt;br&gt;&lt;/b&gt;Max Height =29.3mm , Pitch 10.16mm , 7 Pins</description>
</package>
</packages>
<symbols>
<symbol name="6PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="10PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2X2PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2X3PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="9PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="8PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3X3PINS_ENTRY">
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3X2PINS_ENTRY">
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2X1PIN_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3X1PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="12PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="11PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="691253710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32944v209%20Family_Con_TBL_Screw_RisingClamp_5_6912537100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32944v209%20Family_Con_TBL_Screw_RisingClamp_5_6912537100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2537_HORIZONTAL_ENTRY_W_RISING_CAGE_69125371000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2537_HORIZONTAL_ENTRY_W_RISING_CAGE_69125371000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691253710002?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691253710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2335 – 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=31.5mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33247v209%20Family_WR-TBL_69123351000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33247v209%20Family_WR-TBL_69123351000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2335_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123351000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2335_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123351000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="PART-NUMBER" value=" 691233510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58442v209%20Family_WR-TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58442v209%20Family_WR-TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691216700003?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691216700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214310003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33236v209%20Family_WR-TBL_69121431000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33236v209%20Family_WR-TBL_69121431000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2143_HORIZONTAL_ENTRY_MODULAR_69121431000X"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2143_HORIZONTAL_ENTRY_MODULAR_69121431000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-13&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214310003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214310003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214310003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691211720002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 211 - 5.00 mm 45° Entry Modular H=15.5mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33232v209%20Family_WR-TBL_69121172000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33232v209%20Family_WR-TBL_69121172000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_211_45-DEGREE_ENTRY_MODULAR_69121172000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_211_45-DEGREE_ENTRY_MODULAR_69121172000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691211720002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691211720002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691211720002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.205 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216510003S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2165S - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55598v209%20Family_Con_TBL_Screw_RisingClamp_5.08_6912165100xxS.psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55598v209%20Family_Con_TBL_Screw_RisingClamp_5.08_6912165100xxS.psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2165S_HORIZONTAL_ENTRY_W_RISING_CAGE_69121351000xS/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2165S_HORIZONTAL_ENTRY_W_RISING_CAGE_69121351000xS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216510003S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value="691216510003S"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2337 - 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33249v209%20Family_WR-TBL_69123371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33249v209%20Family_WR-TBL_69123371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2337_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912337100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2337_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912337100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-5&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691233710006?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691233710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="30V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710005?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32925v209%20Family_WR-TBL2_Series2527.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32925v209%20Family_WR-TBL2_Series2527.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2527_VERTICAL_ENTRYW_RISING_CAGE_69125270000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2527_VERTICAL_ENTRYW_RISING_CAGE_69125270000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691252700002?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691252700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 213 - 5.00 mm Horiz.l Entry Modular  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40024437 
&lt;br&gt;VDE Approval 40024437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33234v209%20Family_WR-TBL_69121371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33234v209%20Family_WR-TBL_69121371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_213_HORIZONTAL_ENTRY_MODULAR_69121371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_213_HORIZONTAL_ENTRY_MODULAR_69121371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691213710002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691213710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.129 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710303" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710303?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710303 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="31 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710005?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110304" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110304?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110304 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710010?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700007?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691230110004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2301 – 3.50 mm Double Level Horiz. Entry Modular w. Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33241v209%20Family_WR-TBL_69123011000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33241v209%20Family_WR-TBL_69123011000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2301_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123011000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2301_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123011000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691230110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691230110004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691230110004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700004?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691215700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2157 - 5.00 mm Vertical Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33237v209%20Family_WR-TBL_69121570000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33237v209%20Family_WR-TBL_69121570000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2157_VERTICAL_ENTRY_MODULAR_69121570000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2157_VERTICAL_ENTRY_MODULAR_69121570000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691215700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691215700002?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691215700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201520002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2015 - 5.08 mm 45° Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32804v209%20Family_WR-TBL2_Series2015.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32804v209%20Family_WR-TBL2_Series2015.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2015_45-DEGREE_ENTRY_W_RISING_CAGE_69120152000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2015_45-DEGREE_ENTRY_W_RISING_CAGE_69120152000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201520002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201520002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214100002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N: CPP (3) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o80663v209%20Family_WR-TBL2_6912141000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o80663v209%20Family_WR-TBL2_6912141000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912141000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912141000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214100002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214100002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214100002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710010?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32805v209%20Family_WR-TBL2_Series2135.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32805v209%20Family_WR-TBL2_Series2135.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2135_HORIZONTAL_ENTRY_MODULAR_69121351000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2135_HORIZONTAL_ENTRY_MODULAR_69121351000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201720002S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 201S - 5.00 mm 45° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: COB (2) 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;VDE Approval 40022115 TYPE: COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58397v209%20Family_Con_TBL_Screw_RisingClamp_5_6912017200xxS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58397v209%20Family_Con_TBL_Screw_RisingClamp_5_6912017200xxS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_201S_45-DEGREE_ENTRY_MODULAR_69120172000xS/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_201S_45-DEGREE_ENTRY_MODULAR_69120172000xS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201720002S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691201720002S ?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691201720002S "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32925v209%20Family_WR-TBL2_Series2527.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32925v209%20Family_WR-TBL2_Series2527.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2527_VERTICAL_ENTRYW_RISING_CAGE_69125270000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2527_VERTICAL_ENTRYW_RISING_CAGE_69125270000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691252700003?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691252700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710008?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710006?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214100003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N: CPP (3) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o80663v209%20Family_WR-TBL2_6912141000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o80663v209%20Family_WR-TBL2_6912141000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912141000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912141000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214100003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214100003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214100003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710007?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310006 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910002?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691231710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2317 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33244v209%20Family_WR-TBL_69123171000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33244v209%20Family_WR-TBL_69123171000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2317_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123171000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2317_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123171000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691231710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691231710004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691231710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="WIRE" value="16 to 26 (AWG) 1.31 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691232510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2325 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=25.3 mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33245v209%20Family_WR-TBL_69123251000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33245v209%20Family_WR-TBL_69123251000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2325_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2325_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691232510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="PART-NUMBER" value=" 691232510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214110002S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141S - 3.50 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPP (3) 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o55594v209%20Family_WR-TBL2_Series2141S.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o55594v209%20Family_WR-TBL2_Series2141S.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141S_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69121411000xS"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141S_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69121411000xS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214110002S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214110002S?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="691214110002S"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214110003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32858v209%20Family_WR-TBL2_Series2141S.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32858v209%20Family_WR-TBL2_Series2141S.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141_HORIZONTAL_ENTRY_MODULAR_69121411000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141_HORIZONTAL_ENTRY_MODULAR_69121411000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214110003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214110003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214110003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32805v209%20Family_WR-TBL2_Series2135.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32805v209%20Family_WR-TBL2_Series2135.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2135_HORIZONTAL_ENTRY_MODULAR_69121351000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2135_HORIZONTAL_ENTRY_MODULAR_69121351000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691231710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2317 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33244v209%20Family_WR-TBL_69123171000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33244v209%20Family_WR-TBL_69123171000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2317_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123171000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2317_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123171000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691231710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691231710006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691231710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Vertical"/>
<attribute name="WIRE" value="16 to 26 (AWG) 1.31 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691236510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2365 - 5.08 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84239v209%20Family_WR-TBL2_6912365100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84239v209%20Family_WR-TBL2_6912365100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2365_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912365100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2365_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912365100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691236510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691236510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal Entry"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243110009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201520003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2015 - 5.08 mm 45° Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32804v209%20Family_WR-TBL2_Series2015.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32804v209%20Family_WR-TBL2_Series2015.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2015_45-DEGREE_ENTRY_W_RISING_CAGE_69120152000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2015_45-DEGREE_ENTRY_W_RISING_CAGE_69120152000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201520003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201520003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691230110006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2301 – 3.50 mm Double Level Horiz. Entry Modular w. Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33241v209%20Family_WR-TBL_69123011000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33241v209%20Family_WR-TBL_69123011000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2301_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123011000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2301_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123011000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691230110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691230110006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691230110006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710308" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710308?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710308 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="35 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710006?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214300002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°:CPP (3);​ E150931 CAT.N°: CPP (3) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84902v209%20WR-TBL_6912143000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84902v209%20WR-TBL_6912143000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2143_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912143000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2143_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912143000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-13&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214300002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214300002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214300002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 
&lt;br&gt;Withstanding Voltage [VDE] 2000 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58403v209%20Family_WR-TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58403v209%20Family_WR-TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213500002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213500002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243110008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710009?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2547 - 5.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel; Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Nickel; Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79272v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79272v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2547_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912547100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2547_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912547100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254710003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691249510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2495 - 5.08 mm Horiz.Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40022114 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84251v209%20Family_WR-TBL2_6912495100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84251v209%20Family_WR-TBL2_6912495100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2495_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912495100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2495_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912495100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691249510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691249510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691232710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2327 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33246v209%20Family_WR-TBL_69123271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33246v209%20Family_WR-TBL_69123271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2327_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2327_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691232710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691232710006?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691232710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216510002S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2165S - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55598v209%20Family_Con_TBL_Screw_RisingClamp_5.08_6912165100xxS.psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55598v209%20Family_Con_TBL_Screw_RisingClamp_5.08_6912165100xxS.psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2165S_HORIZONTAL_ENTRY_W_RISING_CAGE_69121351000xS/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2165S_HORIZONTAL_ENTRY_W_RISING_CAGE_69121351000xS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216510002S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value="691216510002S"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2335 – 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=31.5mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33247v209%20Family_WR-TBL_69123351000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33247v209%20Family_WR-TBL_69123351000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2335_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123351000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2335_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123351000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="PART-NUMBER" value=" 691233510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32862v209%20Family_Con_TBL_Screw_RisingClamp_5_6912167100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32862v209%20Family_Con_TBL_Screw_RisingClamp_5_6912167100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2167_HORIZONTAL_ENTRY_W_RISING_CAGE_69121671000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2167_HORIZONTAL_ENTRY_W_RISING_CAGE_69121671000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691216710002?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691216710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55596v209%20Family_WR-TBL2_Series2537.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55596v209%20Family_WR-TBL2_Series2537.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2537_VERTICAL_ENTRY_W_RISING_CAGE_69125370000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2537_VERTICAL_ENTRY_W_RISING_CAGE_69125370000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691253700003?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691253700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2337 - 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33249v209%20Family_WR-TBL_69123371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33249v209%20Family_WR-TBL_69123371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2337_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912337100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2337_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912337100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-5&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691233710004?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691233710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="30V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710005?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700008?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691232510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2325 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=25.3 mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33245v209%20Family_WR-TBL_69123251000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33245v209%20Family_WR-TBL_69123251000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2325_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912325100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2325_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912325100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691232510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="PART-NUMBER" value=" 691232510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691231510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2315 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=19.1 mm  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33243v209%20Family_WR-TBL_69123151000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33243v209%20Family_WR-TBL_69123151000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2315_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123151000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2315_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123151000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691231510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="PART-NUMBER" value=" 691231510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="16 to 26 (AWG) 1.31 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710009?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691236510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2365 - 5.08 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84239v209%20Family_WR-TBL2_6912365100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84239v209%20Family_WR-TBL2_6912365100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2365_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912365100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2365_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912365100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691236510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691236510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910005?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110308" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110308?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110308 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910008?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691231510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2315 - 5.08 mm Double Level Horiz. Entry Modular w. Rising Cage, H=19.1 mm  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33243v209%20Family_WR-TBL_69123151000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33243v209%20Family_WR-TBL_69123151000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2315_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123151000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2315_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123151000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691231510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="PART-NUMBER" value=" 691231510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="16 to 26 (AWG) 1.31 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710009?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710010?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710006?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710004?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700005?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2547 - 5.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel; Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Nickel; Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79272v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79272v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2547_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912547100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2547_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912547100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254710002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691232710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2327 – 5.00 mm Double Level Horiz. Entry Modular w. Rising Cage  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33246v209%20Family_WR-TBL_69123271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33246v209%20Family_WR-TBL_69123271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2327_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123271000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2327_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123271000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691232710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691232710004?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691232710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 22 (AWG) 3.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 213 - 5.00 mm Horiz.l Entry Modular  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40024437 
&lt;br&gt;VDE Approval 40024437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33234v209%20Family_WR-TBL_69121371000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33234v209%20Family_WR-TBL_69121371000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_213_HORIZONTAL_ENTRY_MODULAR_69121371000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_213_HORIZONTAL_ENTRY_MODULAR_69121371000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektron</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691213710003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691213710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.129 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_HORIZONTAL_ENTRY_W_RISING_CAGE_6912415100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241510010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241510010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58401v209%20Family_WR-TBL_Screw_RisingClamp_5.00_6912527100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58401v209%20Family_WR-TBL_Screw_RisingClamp_5.00_6912527100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2527_HORIZONTAL_ENTRY_W_RISING_CAGE_69125271000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2527_HORIZONTAL_ENTRY_W_RISING_CAGE_69125271000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691252710003?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691252710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710007?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT.N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93004v209%20WR-TBL2_Series2535_6912535100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93004v209%20WR-TBL2_Series2535_6912535100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2535_HORIZONTAL_ENTRY_W_RISING_CAGE_69125351000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2535_HORIZONTAL_ENTRY_W_RISING_CAGE_69125351000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT.N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93004v209%20WR-TBL2_Series2535_6912535100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93004v209%20WR-TBL2_Series2535_6912535100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2535_HORIZONTAL_ENTRY_W_RISING_CAGE_69125351000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2535_HORIZONTAL_ENTRY_W_RISING_CAGE_69125351000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691234510006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 2345 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84231v209%20Family_WR-TBL2_6912345100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84231v209%20Family_WR-TBL2_6912345100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2345_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912345100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2345_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912345100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691234510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691234510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110303" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110303?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110303 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691234510004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 2345 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84231v209%20Family_WR-TBL2_6912345100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84231v209%20Family_WR-TBL2_6912345100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2345_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912345100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2345_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912345100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691234510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691234510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2545 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
tch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79302v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79302v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2545_HORIZONTAL_ENTRY_W_RISING_CAGE_6912545100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2545_HORIZONTAL_ENTRY_W_RISING_CAGE_6912545100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254510002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55596v209%20Family_WR-TBL2_Series2537.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55596v209%20Family_WR-TBL2_Series2537.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2537_VERTICAL_ENTRY_W_RISING_CAGE_69125370000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2537_VERTICAL_ENTRY_W_RISING_CAGE_69125370000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691253700002?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691253700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691235510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2355 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84235v209%20Family_WR-TBL_6912355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84235v209%20Family_WR-TBL_6912355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2355_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912355100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2355_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912355100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691235510002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691235510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912425000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242500005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710306" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710306">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710306?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710306 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="34 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2425 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2425_HORIZONTAL_ENTRY_W_RISING_CAGE_6912425100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2537 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT5 (2) 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;VDE Approval 40021392 TYPE: MRT5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32944v209%20Family_Con_TBL_Screw_RisingClamp_5_6912537100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32944v209%20Family_Con_TBL_Screw_RisingClamp_5_6912537100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2537_HORIZONTAL_ENTRY_W_RISING_CAGE_69125371000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2537_HORIZONTAL_ENTRY_W_RISING_CAGE_69125371000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691253710003?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691253710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243110010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700006?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58442v209%20Family_WR-TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58442v209%20Family_WR-TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2167_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912167000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691216700002?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691216700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4); E150931 CAT. N°: CLA (4)4; E150931 CAT.N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79416v209%20Family_WR-TBL_6912427000xx_6912425000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912427000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2527 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58401v209%20Family_WR-TBL_Screw_RisingClamp_5.00_6912527100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58401v209%20Family_WR-TBL_Screw_RisingClamp_5.00_6912527100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2527_HORIZONTAL_ENTRY_W_RISING_CAGE_69125271000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2527_HORIZONTAL_ENTRY_W_RISING_CAGE_69125271000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691252710002?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691252710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2135 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 
&lt;br&gt;Withstanding Voltage [VDE] 2000 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58403v209%20Family_WR-TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58403v209%20Family_WR-TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2135_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912135000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213500003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213500003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60835v209%20Family_TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_HORIZONTAL_CABLE_ENTRY_W_RISING_CAGE_6912445100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244510004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910004?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58415v209%20Family_WR-TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_6912417100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912417100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691241710008?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691241710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691249510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2495 - 5.08 mm Horiz.Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40022114 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84251v209%20Family_WR-TBL2_6912495100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84251v209%20Family_WR-TBL2_6912495100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2495_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912495100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2495_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912495100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691249510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691249510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110302" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110302?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110302 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214310002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33236v209%20Family_WR-TBL_69121431000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33236v209%20Family_WR-TBL_69121431000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2143_HORIZONTAL_ENTRY_MODULAR_69121431000X"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2143_HORIZONTAL_ENTRY_MODULAR_69121431000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-13&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214310002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214310002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214310002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60812v209%20Family_TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60812v209%20Family_TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253500002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253500002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2417 - 5.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CIA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021365 TYPE: CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2417_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912417000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.0509 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910006?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110306" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110306">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110306?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110306 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691230310006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2303 - 3.81 mm Double Level Horiz. Entry Modular w. Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33242v209%20Family_WR-TBL_69123031000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33242v209%20Family_WR-TBL_69123031000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2303_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123031000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2303_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123031000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691230310006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691230310006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691230310006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2535 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60812v209%20Family_TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60812v209%20Family_TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2535_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125350000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253500003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253500003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2167 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32862v209%20Family_Con_TBL_Screw_RisingClamp_5_6912167100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32862v209%20Family_Con_TBL_Screw_RisingClamp_5_6912167100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2167_HORIZONTAL_ENTRY_W_RISING_CAGE_69121671000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2167_HORIZONTAL_ENTRY_W_RISING_CAGE_69121671000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691216710003?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691216710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691243110004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510009">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691235510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2355 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84235v209%20Family_WR-TBL_6912355100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84235v209%20Family_WR-TBL_6912355100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2355_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912355100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2355_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912355100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691235510003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691235510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691230310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2303 - 3.81 mm Double Level Horiz. Entry Modular w. Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33242v209%20Family_WR-TBL_69123031000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33242v209%20Family_WR-TBL_69123031000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2303_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123031000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2303_DOUBLE_LEVEL_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69123031000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691230310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691230310004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691230310004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691243110005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700009?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710304" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710304?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710304 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="32 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691211720003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 211 - 5.00 mm 45° Entry Modular H=15.5mm &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33232v209%20Family_WR-TBL_69121172000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33232v209%20Family_WR-TBL_69121172000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_211_45-DEGREE_ENTRY_MODULAR_69121172000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_211_45-DEGREE_ENTRY_MODULAR_69121172000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691211720003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691211720003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691211720003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.205 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691250610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2506 - 6.35 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 6.35 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 24 A 
&lt;br&gt;IR VDE 32 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2400 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 8 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013439 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32916v209%20Family_WR-TBL2_series2506.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32916v209%20Family_WR-TBL2_series2506.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_6_35_2506_HORIZONTAL_ENTRY_W_RISING_CAGE_69125061000x/"&gt;https://www.we-online.com/catalog/en/TBL_6_35_2506_HORIZONTAL_ENTRY_W_RISING_CAGE_69125061000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691250610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="24A"/>
<attribute name="IR-VDE" value="32A"/>
<attribute name="PART-NUMBER" value=" 691250610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="6.35mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 30 (AWG) 5.26 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201720003S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 201S - 5.00 mm 45° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: COB (2) 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;VDE Approval 40022115 TYPE: COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58397v209%20Family_Con_TBL_Screw_RisingClamp_5_6912017200xxS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58397v209%20Family_Con_TBL_Screw_RisingClamp_5_6912017200xxS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_201S_45-DEGREE_ENTRY_MODULAR_69120172000xS/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_201S_45-DEGREE_ENTRY_MODULAR_69120172000xS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201720003S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691201720003S?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691201720003S"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710008?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691508110305" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5081 - 3.50 mm Horizontal entry SMT Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58319v209%20Family_WR-TBL_Serie_5081_6915081103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_5081_6915081103XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691508110305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691508110305?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691508110305 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2445 - 5.08 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60847v209%20Family_TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX.jpg.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2445_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912445000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244500010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691247510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2475 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84247v209%20Family_WR-TBL2_6912475100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84247v209%20Family_WR-TBL2_6912475100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2475_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912475100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2475_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912475100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691247510009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691247510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Tripel Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691247510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2475 - 5.08 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84247v209%20Family_WR-TBL2_6912475100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84247v209%20Family_WR-TBL2_6912475100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2475_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912475100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2475_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912475100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691247510006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691247510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Tripel Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691212200101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691212200101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691212200101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691250610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2506 - 6.35 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 6.35 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 24 A 
&lt;br&gt;IR VDE 32 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2400 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 8 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013439 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32916v209%20Family_WR-TBL2_series2506.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32916v209%20Family_WR-TBL2_series2506.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_6_35_2506_HORIZONTAL_ENTRY_W_RISING_CAGE_69125061000x/"&gt;https://www.we-online.com/catalog/en/TBL_6_35_2506_HORIZONTAL_ENTRY_W_RISING_CAGE_69125061000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691250610003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="24A"/>
<attribute name="IR-VDE" value="32A"/>
<attribute name="PART-NUMBER" value=" 691250610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="6.35mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 30 (AWG) 5.26 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691212200001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691212200001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691212200001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253900003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60814v209%20Family_TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60814v209%20Family_TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253900003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253900003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214210002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214210002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214210002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2455 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79304v209%20WR-TBL_6912455100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2455_HORIZONTAL_ENTRY_W_RISING_CAGE_6912455100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245510005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245510005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243300007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm)
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CAP (3); E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60859v209%20Family_TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2433_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912433000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243300007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243300007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243300007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32871v209%20Family_WR-TBL2_Series2169.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32871v209%20Family_WR-TBL2_Series2169.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2169_HORIZONTAL_ENTRY_MODULAR_69121691000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2169_HORIZONTAL_ENTRY_MODULAR_69121691000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216910003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710004?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243200004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60865v209%20Family_TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912432000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243200004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243200004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4); E150931 CAT: N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60845v209%20Family_TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912447000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244700010?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244700010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691212200002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2122 - 7.00 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79469v209%20WR-TBL_6912142000xx_6912144000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2122_VERTICAL_ENTRY_W_RISING_CAGE_6912122000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691212200002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691212200002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214210101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214210101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214210101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2415 - 5.08 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E130931; E150931 
&lt;br&gt;VDE Approval 40021365 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79414v209%20WR-TBL_6912427000xx_6912425000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2415_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912415000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241500008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214210001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2142 - 7.00 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2142_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912142100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214210001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214210001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32871v209%20Family_WR-TBL2_Series2169.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32871v209%20Family_WR-TBL2_Series2169.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2169_HORIZONTAL_ENTRY_MODULAR_69121691000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2169_HORIZONTAL_ENTRY_MODULAR_69121691000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216910002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214110002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141 - 3.50 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32858v209%20Family_WR-TBL2_Series2141S.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32858v209%20Family_WR-TBL2_Series2141S.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141_HORIZONTAL_ENTRY_MODULAR_69121411000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141_HORIZONTAL_ENTRY_MODULAR_69121411000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214110002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214110002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214110002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243310004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66;​ PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin;​ Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm);​ 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3);​ E150931 CAT.N°: CPA (3);​ E150931 CAT. N°: CPA(3);​ E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32902v209%20Family_WR-TBL2_series2433.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2433_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912433100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243310004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243310004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243310004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32947v209%20Family_WR-TBL2_Series2539.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32947v209%20Family_WR-TBL2_Series2539.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2539_HORIZONTAL_ENTRY_W_RISING_CAGE_69125391000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2539_HORIZONTAL_ENTRY_W_RISING_CAGE_69125391000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253910002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2427 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp   &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CLA (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 TYPE: CLA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93979v209%20WR-TBL2_Series2427_6912427100xx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2427_HORIZONTAL_ENTRYW_RISING_CAGE_6912427100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691242710004?ae"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691242710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710305" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710305?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710305 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="33 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214110003S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2141S - 3.50 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPP (3) 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o55594v209%20Family_WR-TBL2_Series2141S.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o55594v209%20Family_WR-TBL2_Series2141S.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2141S_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69121411000xS"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2141S_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_69121411000xS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214110003S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214110003S?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="691214110003S"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691709710302" prefix="J">
<description>&lt;b&gt;WR-TBL Series 7097 - Rising Cage Clamp 5.0mm pitch - Horizontal cable entry - SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
Kind Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Pitch 5 mm

&lt;br&gt;
&lt;br&gt;&lt;b&gt;
General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt; 

&lt;b&gt;Electrical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA46 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;Cage Material Brass 
&lt;br&gt;Cage Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Screw M3 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Certification
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel with Cap 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 up to 8 (mm) 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58289v209%20Family_WR-TBL_Serie_7097_6917097103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/TBL_5_00_SMT_7097_HORIZONTAL_ENTRY_SMT_RISING_CAGE_CLAMP_69170971030X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-08-23&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691709710302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691709710302?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691709710302 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243210004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2432 - 7.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60862v209%20Family_TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_2432_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912432100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243210004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243210004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243100009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o60855v209%20Family_TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912431000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243100009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243100009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691243100009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221120004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2211 - 3.50 mm 55° Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33239v209%20Family_WR-TBL_69122112000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2211_55-DEGREE_ENTRY_MODULAR_69122112000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221120004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221120004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221120004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="55°"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691210910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2109 - 2.54 mm Horiz. Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 4 up to 5 (mm) 
&lt;br&gt;Screw M1.6 
&lt;br&gt;Solid Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 18 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.0509 to 0.823 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33231v209%20Family_WR-TBL_69121091000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X"&gt;https://katalog.we-online.com/en/em/TBL_2_54_2109_HORIZONTAL_ENTRY_69121091000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691210910003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691210910003?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691210910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 18 (AWG) 0.0509 to 0.823 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691215700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2157 - 5.00 mm Vertical Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33237v209%20Family_WR-TBL_69121570000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33237v209%20Family_WR-TBL_69121570000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2157_VERTICAL_ENTRY_MODULAR_69121570000X/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2157_VERTICAL_ENTRY_MODULAR_69121570000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691215700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691215700003?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691215700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691221320006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2213 - 3.81 mm 55° Entry Modular &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Brass 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33240v209%20Family_WR-TBL_69122132000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_2213_55-DEGREE_ENTRY_MODULAR_69122132000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-21&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691221320006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691221320006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691221320006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="55° "/>
<attribute name="WIRE" value="28 to 16 (AWG) 0.081 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691243110007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2447 - 5.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin; Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS;​ ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC); 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6; 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: MRT15 (4) 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;VDE Approval 40015450 TYPE: MRT15 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32911v209%20Family_Con_TBL_Screw_RisingClamp_5_6912447100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_2447_HORIZONTAL_ENTRYW_RISING_CAGE_6912447100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-22&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691244710007?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691244710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.0509 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2549 - 7.50 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79306v209%20WR-TBL_6912549100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79306v209%20WR-TBL_6912549100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2549_HORIZONTAL_ENTRY_W_RISING_CAGE_6912549100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2549_HORIZONTAL_ENTRY_W_RISING_CAGE_6912549100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254910002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214300003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT. N°:CPP (3);​ E150931 CAT.N°: CPP (3) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40015437 TYPE: CPP 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84902v209%20WR-TBL_6912143000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84902v209%20WR-TBL_6912143000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_81_2143_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912143000XX"&gt;https://katalog.we-online.com/en/em/TBL_3_81_2143_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912143000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-13&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214300003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214300003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691214300003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Vertical Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84902v209%20WR-TBL_6912143000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84902v209%20WR-TBL_6912143000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2164_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912164000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2164_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912164000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216400003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216400003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84126v209%20Family_WR-TBL2_6912164100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84126v209%20Family_WR-TBL2_6912164100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2164_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912164100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2164_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912164100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216900003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84131v209%20Family_WR-TBL2_691216900xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84131v209%20Family_WR-TBL2_691216900xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2169_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912169000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2169_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912169000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216900003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216900003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2545 - 5.08 mm Horizontal Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
tch 5.08 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79302v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79302v209%20WR-TBL_6912547100xx_6912545100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_2545_HORIZONTAL_ENTRY_W_RISING_CAGE_6912545100XX/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_2545_HORIZONTAL_ENTRY_W_RISING_CAGE_6912545100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-26&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254510003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2549 - 7.50 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79306v209%20WR-TBL_6912549100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79306v209%20WR-TBL_6912549100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2549_HORIZONTAL_ENTRY_W_RISING_CAGE_6912549100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2549_HORIZONTAL_ENTRY_W_RISING_CAGE_6912549100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254910003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32947v209%20Family_WR-TBL2_Series2539.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32947v209%20Family_WR-TBL2_Series2539.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2539_HORIZONTAL_ENTRY_W_RISING_CAGE_69125391000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2539_HORIZONTAL_ENTRY_W_RISING_CAGE_69125391000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253910003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253900002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2539 - 7.50 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60814v209%20Family_TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60814v209%20Family_TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2539_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125390000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253900002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253900002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243110006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2431 - 3.50 mm Horizontal cable entry with rising clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 130 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 1.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT. N°: CPA (3) 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;VDE Approval 40015434 TYPE: CPA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32893v209%20Family_WR-TBL2_Series2431.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx"&gt;https://katalog.we-online.com/en/em/TBL_3_50_2431_HORIZONTAL_ENTRY_MODULAR_W_RISING_CAGE_6912431100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-12&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243110006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691243110006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691243110006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="30 to 16 (AWG) 0.05 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216900002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2169 - 7.50 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84131v209%20Family_WR-TBL2_691216900xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84131v209%20Family_WR-TBL2_691216900xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2169_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912169000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2169_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912169000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216900002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216900002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2544 - 7.62 mm Horizontal Entry Dual Pin w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32951v209%20Family_Con_TBL_Screw_RisingClamp_762_6912544100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32951v209%20Family_Con_TBL_Screw_RisingClamp_762_6912544100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2544_HORIZONTAL_ENTRY_DUAL_PIN_W_RISING_CAGE_69125341000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2544_HORIZONTAL_ENTRY_DUAL_PIN_W_RISING_CAGE_69125341000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254410002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2544 - 7.62 mm Horizontal Entry Dual Pin w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32951v209%20Family_Con_TBL_Screw_RisingClamp_762_6912544100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32951v209%20Family_Con_TBL_Screw_RisingClamp_762_6912544100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2544_HORIZONTAL_ENTRY_DUAL_PIN_W_RISING_CAGE_69125341000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2544_HORIZONTAL_ENTRY_DUAL_PIN_W_RISING_CAGE_69125341000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254410003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691218410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2184 - 7.62 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 30 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55592v209%20WR-TBL_Serie_2184_69121841000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55592v209%20WR-TBL_Serie_2184_69121841000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2184_HORIZONTAL_ENTRY_MODULAR_69121841000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2184_HORIZONTAL_ENTRY_MODULAR_69121841000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691218410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="30A"/>
<attribute name="PART-NUMBER" value=" 691218410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84126v209%20Family_WR-TBL2_6912164100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84126v209%20Family_WR-TBL2_6912164100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2164_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912164100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2164_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912164100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32930v209%20Family_WR-TBL2_Series2534.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32930v209%20Family_WR-TBL2_Series2534.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2534_HORIZONTAL_ENTRY_W_RISING_CAGE_69125341000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2534_HORIZONTAL_ENTRY_W_RISING_CAGE_69125341000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32930v209%20Family_WR-TBL2_Series2534.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32930v209%20Family_WR-TBL2_Series2534.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2534_HORIZONTAL_ENTRY_W_RISING_CAGE_69125341000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2534_HORIZONTAL_ENTRY_W_RISING_CAGE_69125341000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60822v209%20Family_TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60822v209%20Family_TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253400002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253400002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691218410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2184 - 7.62 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 30 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55592v209%20WR-TBL_Serie_2184_69121841000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55592v209%20WR-TBL_Serie_2184_69121841000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2184_HORIZONTAL_ENTRY_MODULAR_69121841000X/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2184_HORIZONTAL_ENTRY_MODULAR_69121841000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691218410003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="30A"/>
<attribute name="PART-NUMBER" value=" 691218410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2534 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60822v209%20Family_TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60822v209%20Family_TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2534_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125340000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253400003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253400003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2164 - 7.62 mm Vertical Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84902v209%20WR-TBL_6912143000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84902v209%20WR-TBL_6912143000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2164_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912164000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2164_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912164000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216400002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216400002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242910010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2429 - 7.50 mm Horizontal Entry Modular w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32889v209%20Family_WR-TBL2_Series2429.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_2429_HORIZONTAL_ENTRY_W_RISING_CAGE_6912429100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242910010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242910010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214400101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214400101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214400101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691250910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2509 - 9.52 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 9.52 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 24 A 
&lt;br&gt;IR VDE 32 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 8 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013439 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32920v209%20Family_WR-TBL2_Series2509.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32920v209%20Family_WR-TBL2_Series2509.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_9_52_2509_HORIZONTAL_ENTRY_W_RISING_CAGE_69125091000x/"&gt;https://www.we-online.com/catalog/en/TBL_9_52_2509_HORIZONTAL_ENTRY_W_RISING_CAGE_69125091000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691250910003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="24A"/>
<attribute name="IR-VDE" value="32A"/>
<attribute name="PART-NUMBER" value=" 691250910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="9.52mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 30 (AWG) 5.26 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214410101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214410101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214410101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243410007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60871v209%20Family_TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912434100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243410007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243410007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214400002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214400002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214400002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691214410002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214400001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Vertical Cable Entry Rising Cage &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_VERTICAL_ENTRY_W_RISING_CAGE_6912144000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214400001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214400001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213800001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213800001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32867v209%20Family_Con_TBL_Sxrew_RisingClamp_10_6912168100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32867v209%20Family_Con_TBL_Sxrew_RisingClamp_10_6912168100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2168_HORIZONTAL_ENTRY_W_RISING_CAGE_69121681000x/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2168_HORIZONTAL_ENTRY_W_RISING_CAGE_69121681000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213800002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213800002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691214410001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2144 - 7.62 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015437 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79418v209%20WR-TBL_6912142100xx_6912144100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2144_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912144100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691214410001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691214410001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691243400004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2434 - 7.62 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M2 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015434 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60875v209%20Family_TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_2434_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912434000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-27&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691243400004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 691243400004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216800001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216800001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253800002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253800002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691250910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2509 - 9.52 mm Horizontal Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 9.52 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 24 A 
&lt;br&gt;IR VDE 32 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 8 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013439 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32920v209%20Family_WR-TBL2_Series2509.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32920v209%20Family_WR-TBL2_Series2509.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_9_52_2509_HORIZONTAL_ENTRY_W_RISING_CAGE_69125091000x/"&gt;https://www.we-online.com/catalog/en/TBL_9_52_2509_HORIZONTAL_ENTRY_W_RISING_CAGE_69125091000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691250910002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="24A"/>
<attribute name="IR-VDE" value="32A"/>
<attribute name="PART-NUMBER" value=" 691250910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="9.52mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="10 to 30 (AWG) 5.26 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216800101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216800101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213810101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213810101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213800101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84466v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912138000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213800101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253800001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253800001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216800002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2168 - 10.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84129v209%20Family_WR-TBL2_6912168000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2168_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912168000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216800002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252800002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252800002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241810008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Horizontal Entry w. Rising Cage Clamp  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84245v209%20Family_WR-TBL2_6912418100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912418100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241810008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241810008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Horizontal Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58648v209%20Family_WR-TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_69124281000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58648v209%20Family_WR-TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_69124281000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124281000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124281000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60842v209%20Family_TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60842v209%20Family_TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244800004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Vertical Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60851v209%20Family_TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60851v209%20Family_TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244800004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60842v209%20Family_TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60842v209%20Family_TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2448_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124481000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213810001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2138 - 10.00 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84827v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2138_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912138100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213810001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Horizontal Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58648v209%20Family_WR-TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_69124281000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58648v209%20Family_WR-TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_69124281000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124281000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2428_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124281000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252810001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691252810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252810001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252810101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691252810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252810101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252800001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691252800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252800001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254810101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691254810101">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254810101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Horizontal Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60804v209%20Family_TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69125281000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691252810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2458 - 10.00 mm Horizontal Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79422v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79422v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2458_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912458100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2458_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912458100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245810003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Matte Tin over Nickel; Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021395; 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691233810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2458 - 10.00 mm Horizontal Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79422v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79422v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2458_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912458100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2458_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912458100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245810004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253800101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2538 - 10.00 mm Vertical Entry Modular w. Rising Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60806v209%20Family_TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2538_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125380000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253800101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244800003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2448 - 10.00 mm Vertical Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60851v209%20Family_TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60851v209%20Family_TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2448_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124480000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244800003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242800004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79424v209%20WR-TBL_6912428000xx_6912426000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79424v209%20WR-TBL_6912428000xx_6912426000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2428_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912428000XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2428_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912428000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242800004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254810002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201820101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691201820101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201820101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233810102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Matte Tin over Nickel; Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021395; 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691233810102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691233810102 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2338 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Matte Tin over Nickel; Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021395; 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79312v209%20WR-TBL_6912338100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2338_HORIZONTAL_ENTRY_W_RISING_CAGE_6912338100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691233810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691233810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Double Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691254610002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201820002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201820002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201820002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254810001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2548 - 10.00 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2548_HORIZONTAL_ENTRY_W_RISING_CAGE_6912548100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691254810001">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254810001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691249610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691249610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691249610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691235610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691235610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value="691235610001"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691247610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X1PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691247610003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691247610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Tripel Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691249610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691249610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691249610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241800010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2418 - 10.00 mm Vertical Entry w. Rsing Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84243v209%20Family_WR-TBL2_6912418000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2418_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912418000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241800010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241800010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201620002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691201620002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201620002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58476v209%20Family_WR-TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_6912426100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58476v209%20Family_WR-TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_6912426100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912426100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912426100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242610003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691247610006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691247610006">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691247610006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Tripel Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691234610102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691234610102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value="691234610102"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691234610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691234610004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value="691234610004"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691235610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691235610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value="691235610002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242800003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2428 - 10.00 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79424v209%20WR-TBL_6912428000xx_6912426000xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79424v209%20WR-TBL_6912428000xx_6912426000xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2428_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912428000XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2428_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912428000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242800003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216600001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216600001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216600001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201620001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691201620001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201620001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691249610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2496 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84253v209%20Family_WR-TBL2_6912496100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2496_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912496100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691249610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691249610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691235610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2356 - 10.16 mm Horiz. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84237v209%20Family_WR-TBL_6912356100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2356_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912356100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691235610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value="691235610101"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691234610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2346 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84233v209%20Family_WR-TBL2_6912346100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2346_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912346100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691234610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691234610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253600101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253600101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253600101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691247610103" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2476 - 10.16 mm Horizontal Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o86593v209%20Family_WR-TBL2_6912476100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2476_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912476100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X1PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691247610103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691247610103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Tripel Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201820001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2018 - 10.00 mm 45° Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84027v209%20Family_WR-TBL_6912018200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2018_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912018200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-02&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691201820001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201820001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691219610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2196 - 10.16 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 57 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 10 up to 11 (mm) 
&lt;br&gt;Screw M4.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33238v209%20Family_WR-TBL_69121961000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33238v209%20Family_WR-TBL_69121961000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2196_HORIZONTAL_ENTRY_MODULAR_69121961000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2196_HORIZONTAL_ENTRY_MODULAR_69121961000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691219610002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="57A"/>
<attribute name="PART-NUMBER" value=" 691219610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="8 to 22 (AWG) 8.37 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691219610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2196 - 10.16 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 57 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 10 up to 11 (mm) 
&lt;br&gt;Screw M4.5 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33238v209%20Family_WR-TBL_69121961000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33238v209%20Family_WR-TBL_69121961000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2196_HORIZONTAL_ENTRY_MODULAR_69121961000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2196_HORIZONTAL_ENTRY_MODULAR_69121961000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691219610003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="57A"/>
<attribute name="PART-NUMBER" value=" 691219610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="8 to 22 (AWG) 8.37 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691252800101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2528 - 10.00 mm Vertical Entry Modular w. Rising Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC); 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021393 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o127576v209%20Family_TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_2528_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125280000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-29&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691252800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691252800101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Horizon. Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84464v209%20Family_WR-TBL2_6912138100xx_6912136100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_HRIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912136100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58476v209%20Family_WR-TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_6912426100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58476v209%20Family_WR-TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_6912426100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912426100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2426_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_6912426100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242610004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691254610101">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691254610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2546 - 10.16 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79327v209%20WR-TBL_6912548100xx_6912546100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2546_HORIZONTAL_ENTRY_W_RISING_CAGE_6912546100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691254610001">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691254610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216600101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216600101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216600101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242600003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o127573v209%20Family_TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o127573v209%20Family_TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242600003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242600003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244610004">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60843v209%20Family_TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60843v209%20Family_TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244610004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213600001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213600001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213600001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2456 - 10.16 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79333v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79333v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2456_HORIZONTAL_ENTRY_W_RISING_CAGE_6912456100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2456_HORIZONTAL_ENTRY_W_RISING_CAGE_6912456100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245610003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1" route="any"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253600002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253600002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253600002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253600001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60827v209%20Family_TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69125360000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253600001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253600001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691245610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2456 - 10.16 mm Horizontal Cable Entry Rising Cage&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40015450  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79333v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79333v209%20WR-TBL_6912458100xx_6912456100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2456_HORIZONTAL_ENTRY_W_RISING_CAGE_6912456100XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2456_HORIZONTAL_ENTRY_W_RISING_CAGE_6912456100XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691245610004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691245610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216600002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Vertical Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84831v209%20Family_WR-TBL2_6912136000xx_6912138000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912166000xx_2/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216600002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216600002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244600003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Vertical Entry Modular w. Rising Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60853v209%20Family_TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60853v209%20Family_TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244600003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244600003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691236610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691236610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691236610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691201620101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2016 - 10.16 mm 45° Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. COB (2) 
&lt;br&gt;VDE Approval 40022115 Type COB 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84017v209%20Family_WR-TBL_6912016200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2016_45-DEGREE_ENTRY_W_RISING_CAGE_CLAMP_6912016200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691201620101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691201620101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244600004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Vertical Entry Modular w. Rising Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60853v209%20Family_TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60853v209%20Family_TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2446_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_69124460000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244600004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244600004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691236610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691236610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691236610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691244610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2446 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40015450 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60843v209%20Family_TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60843v209%20Family_TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;https://www.we-online.com/catalog/en/TBL_10_16_2446_HORIZONTAL_CABLE_ENTRY_W_RISING_CLAMP_69124461000X/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691244610003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691244610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691236610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2366 - 10.16 mm Horiz. Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84241v209%20Family_WR-TBL2_6912366100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2366_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912366100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691236610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691236610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233610102" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691233610102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691233610102 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691233610004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691233610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691253610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213600101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691213600101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213600101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691213600002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2136 - 10.16 mm Vertical Entry w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CII (4) 
&lt;br&gt;VDE Approval 40021366 Type CII 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84062v209%20Family_WR-TBL2_6912136000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2136_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912136000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691213600002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691213600002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691216610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691242600004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2426 - 10.16 mm Vertical Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021356 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o127573v209%20Family_TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o127573v209%20Family_TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2426_VERTICAL_CABLE_ENTRY_W_RISING_CLAMP_6912426000XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-03&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691242600004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691242600004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610011">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241610007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Horiz Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84543v209%20Family_WR-TBL2_6912416100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912416100xx//a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241610007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241610007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610009">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691233610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2336 - 10.16 mm Horiz. Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 20 A 
&lt;br&gt;IR VDE 20 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT18 (5) 
&lt;br&gt;VDE Approval 40022114 Type MRT18 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84229v209%20Family_WR-TBL2_6912336100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2336_HOROZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912336100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691233610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="PART-NUMBER" value=" 691233610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Dual Level Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216610101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216610101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216610101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691241600010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2416 - 10.16 mm Vertical Entry w. Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 14 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CIA (4) 
&lt;br&gt;VDE Approval 40021365 Type CIA 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84468v209%20Family_WR-TBL2_6912418000xx_6912416000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2416_VERTICAL_ENTRY_W_RISING_CAGE_CLAMP_6912416000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691241600010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="14A"/>
<attribute name="PART-NUMBER" value=" 691241600010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691216610001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2166 - 10.16 mm Horizontal Entry Rising Cage Clamp &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CLL (4) 
&lt;br&gt;VDE Approval 40021356 Type CLL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84314v209%20Family_WR-TBL2_6912166100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2166_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_6912166100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691216610001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691216610001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1" route="any"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691253610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2536 - 10.16 mm Horizontal Entry Modular w. Rising Cage Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;VDE Approval 40021392 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32939v209%20Family_WR-TBL2_Series2536.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2536_HORIZONTAL_ENTRY_W_RISING_CAGE_691253610002/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-04&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691253610002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="PART-NUMBER" value=" 691253610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691256610007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 2566 - 10.16 mm Horizontal Entry w. Rising Cage Clamp Glow Wire &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66G25 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 40 A 
&lt;br&gt;IR VDE 57 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT26 (1) 
&lt;br&gt;VDE Approval 40022112 
&lt;br&gt;VDE Approval 40022112 Type MRT26 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84255v209%20Family_WR-TBL2_6912566100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_2566_HORIZONTAL_ENTRY_W_RISING_CAGE_CLAMP_GLOW_WIRE_6912566100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691256610007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1" route="any"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="IR-UL" value="40A"/>
<attribute name="IR-VDE" value="57A"/>
<attribute name="PART-NUMBER" value=" 691256610007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WIRE" value="6 to 20 (AWG) 13.30 to 0.52 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
