<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Terminal Blocks - WR-TBL Spring Clamp &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023b, 2023-06-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691411510006">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691413720012B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 12pins</description>
</package>
<package name="691412120007MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691412220009M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 9pins</description>
</package>
<package name="691413720003B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 3pins</description>
</package>
<package name="691401700002B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 2pins</description>
</package>
<package name="691411710012B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 12pins</description>
</package>
<package name="691412120011MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 11pins</description>
</package>
<package name="691413720007B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 7pins</description>
</package>
<package name="691412320008">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691401710012B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 12pins</description>
</package>
<package name="691415520002">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691412120003MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691412320010">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691412220011">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 11pins</description>
</package>
<package name="691412120009B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 9pins</description>
</package>
<package name="691411710006B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 6pins</description>
</package>
<package name="691416500004">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691401710010B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 10pins</description>
</package>
<package name="691412320002M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691412220011M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 11pins</description>
</package>
<package name="691401710003B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 3pins</description>
</package>
<package name="691416500010">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691412220008">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 8pins</description>
</package>
<package name="691401710008B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 8pins</description>
</package>
<package name="691401700005B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 5pins</description>
</package>
<package name="691411510007">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691412220008M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 8pins</description>
</package>
<package name="691412320011M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 11pins</description>
</package>
<package name="691411910006">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 6pins</description>
</package>
<package name="691416500003">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691401700007B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 7pins</description>
</package>
<package name="691401700006B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 6pins</description>
</package>
<package name="691411510008">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691411710009B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 9pins</description>
</package>
<package name="691411710019B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 19pins</description>
</package>
<package name="691412320003">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691411710023B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 23pins</description>
</package>
<package name="691411710003B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 3pins</description>
</package>
<package name="691412220005">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 5pins</description>
</package>
<package name="691412220003M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm ,3pins</description>
</package>
<package name="691412220010">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 10pins</description>
</package>
<package name="691412120004B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691412120006B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691412320004M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691412120005B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691411510003">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691412120007B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 7pins</description>
</package>
<package name="691413720002B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 2pins</description>
</package>
<package name="691418320006">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691412220010M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 10pins</description>
</package>
<package name="691411710011B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 11pins</description>
</package>
<package name="691412320005">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691412320012">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691411710020B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 20pins</description>
</package>
<package name="691412120010B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 10pins</description>
</package>
<package name="691417220006">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 6pins</description>
</package>
<package name="691411710008B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 8pins</description>
</package>
<package name="691417320006S">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691411710010B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 10pins</description>
</package>
<package name="691413720011B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 11pins</description>
</package>
<package name="691402910003B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 3pins</description>
</package>
<package name="691411710021B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 21pins</description>
</package>
<package name="691418220005">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 5pins</description>
</package>
<package name="691412320007M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691403900006B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 6pins</description>
</package>
<package name="691417320004S">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691413720009B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 9pins</description>
</package>
<package name="691412220002M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 2pins</description>
</package>
<package name="691412220003">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 3pins</description>
</package>
<package name="691414720002B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 2pins</description>
</package>
<package name="691418320004">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691412320012M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 12pins</description>
</package>
<package name="691417220003">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 3pins</description>
</package>
<package name="691416500007">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 7pins</description>
</package>
<package name="691411710022B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 22pins</description>
</package>
<package name="691417320005S">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691413720004B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 4pins</description>
</package>
<package name="691404910002MB">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 2pins</description>
</package>
<package name="691413720010B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 10pins</description>
</package>
<package name="691418320002">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691417420003">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691411910010">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 10pins</description>
</package>
<package name="691412120010MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 10pins</description>
</package>
<package name="691401710009B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 9pins</description>
</package>
<package name="691412320005M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691403900003B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 3pins</description>
</package>
<package name="691402910002B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 2pins</description>
</package>
<package name="691412320004">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 4pins</description>
</package>
<package name="691411510011">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 11pins</description>
</package>
<package name="691416500006">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691416500008">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 8pins</description>
</package>
<package name="691412120003B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 3pins</description>
</package>
<package name="691411910012">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 12pins</description>
</package>
<package name="691404910003B">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 3pins</description>
</package>
<package name="691411510002">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691404910005MB">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 5pins</description>
</package>
<package name="691404910005B">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 5pins</description>
</package>
<package name="691417420002">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691412220012">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 12pins</description>
</package>
<package name="691404910002B">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 2pins</description>
</package>
<package name="691411410002">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691411910011">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 11pins</description>
</package>
<package name="691411910009">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 9pins</description>
</package>
<package name="691411710007B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 7pins</description>
</package>
<package name="691418420006">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless  
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691414720006B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 6pins</description>
</package>
<package name="691417420005">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691412320006M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691401700008B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 8pins</description>
</package>
<package name="691411910002">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 2pins</description>
</package>
<package name="691414720003B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 3pins</description>
</package>
<package name="691418420003">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless  
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691411710004B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 4pins</description>
</package>
<package name="691411910008">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 8pins</description>
</package>
<package name="691411910007">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 7pins</description>
</package>
<package name="691412320007">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 7pins</description>
</package>
<package name="691417420006">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691418220003">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 3pins</description>
</package>
<package name="691414720004B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 4pins</description>
</package>
<package name="691414720008B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 8pins</description>
</package>
<package name="691412420002M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691412220007">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 7pins</description>
</package>
<package name="691805010303">
<description>&lt;b&gt;WR-TBL Serie 8050 - 2.50 mm Screwless SMT  
&lt;br&gt;&lt;/b&gt;Max Height = 5mm , Pitch 2.5mm , 3pins</description>
</package>
<package name="691415520005">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691412120013B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 13pins</description>
</package>
<package name="691411510004">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691411510012">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 12pins</description>
</package>
<package name="691411910004">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 4pins</description>
</package>
<package name="691401700003B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 3pins</description>
</package>
<package name="691413720008B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 8pins</description>
</package>
<package name="691412220005M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 5pins</description>
</package>
<package name="691411910003">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 3pins</description>
</package>
<package name="691416500009">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691412120009MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 9pins</description>
</package>
<package name="691403900002B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 2pins</description>
</package>
<package name="691401700012B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 12pins</description>
</package>
<package name="691411410004">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691411510010">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 10pins</description>
</package>
<package name="691411410003">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691418420002">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless  
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691412220009">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 9pins</description>
</package>
<package name="691418220004">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 4pins</description>
</package>
<package name="691416500002">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691411710005B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 5pins</description>
</package>
<package name="691416500005">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691412320006">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 6pins</description>
</package>
<package name="691418420004">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless  
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691412320009">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 9pins</description>
</package>
<package name="691401710006B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 6pins</description>
</package>
<package name="691411910005">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.5mm , 5pins</description>
</package>
<package name="691412320003M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691415520003">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691412120005MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 5pins</description>
</package>
<package name="691411510009">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 9pins</description>
</package>
<package name="691412420003M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691412320009M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 9pins</description>
</package>
<package name="691412420006M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691417320002S">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691412420008M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691411410008">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691412120004MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 4pins</description>
</package>
<package name="691418420005">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless  
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691412420007M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691411710024B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 24pins</description>
</package>
<package name="691411410011">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 11pins</description>
</package>
<package name="691411410006">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691411410007">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691411410012">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691412420004M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691404910003MB">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector 
&lt;br&gt;&lt;/b&gt;Max Height = 24.1mm , Pitch 7.5mm , 3pins</description>
</package>
<package name="691412420011M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 11pins</description>
</package>
<package name="691417420004">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691412420012M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691412420007">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 7pins</description>
</package>
<package name="691411410009">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 9pins</description>
</package>
<package name="691412420004">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 4pins</description>
</package>
<package name="691412420009M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 9pins</description>
</package>
<package name="691411810003">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10mm , 3pins</description>
</package>
<package name="691412420005M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691412420002">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 2pins</description>
</package>
<package name="691411810004">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10mm , 4pins</description>
</package>
<package name="691412420010M">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 10pins</description>
</package>
<package name="691412420011">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 11pins</description>
</package>
<package name="691412420006">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 6pins</description>
</package>
<package name="691412420010">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 10pins</description>
</package>
<package name="691805010302">
<description>&lt;b&gt;WR-TBL Serie 8050 - 2.50 mm Screwless SMT  
&lt;br&gt;&lt;/b&gt;Max Height = 5mm , Pitch 2.5mm , 2pins</description>
</package>
<package name="691412420005">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691411410005">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 5pins</description>
</package>
<package name="691411410010">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 7.62mm , 10pins</description>
</package>
<package name="691418320005">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 5pins</description>
</package>
<package name="691416600005">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 10.16mm , 5pins</description>
</package>
<package name="691411610005">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10.16mm , 5pins</description>
</package>
<package name="691416600003">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 10.16mm , 3pins</description>
</package>
<package name="691416600004">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 10.16mm , 4pins</description>
</package>
<package name="691412220012M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 12pins</description>
</package>
<package name="691412420008">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 8pins</description>
</package>
<package name="691413720005B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 5pins</description>
</package>
<package name="691412120002MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691415620003">
<description>&lt;b&gt;WR-TBL Serie 4156 - 10.16 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10.16mm , 3pins</description>
</package>
<package name="691402910005B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 5pins</description>
</package>
<package name="691412320008M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 8pins</description>
</package>
<package name="691412220004M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 4pins</description>
</package>
<package name="691418220002">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 2pins</description>
</package>
<package name="691403900008B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 8pins</description>
</package>
<package name="691401700004B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 4pins</description>
</package>
<package name="691417220002">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 2pins</description>
</package>
<package name="691415620002">
<description>&lt;b&gt;WR-TBL Serie 4156 - 10.16 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10.16mm , 2pins</description>
</package>
<package name="691412220004">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 4pins</description>
</package>
<package name="691401710011B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 11pins</description>
</package>
<package name="691401700009B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 9pins</description>
</package>
<package name="691412220006">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 6pins</description>
</package>
<package name="691401700010B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 10pins</description>
</package>
<package name="691412220006M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 6pins</description>
</package>
<package name="691401700011B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 14mm , Pitch 5mm , 11pins</description>
</package>
<package name="691412420012">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 12pins</description>
</package>
<package name="691403900004B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 4pins</description>
</package>
<package name="691417320003S">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691418320003">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 3pins</description>
</package>
<package name="691411710002B">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 15.25mm , Pitch 5mm , 2pins</description>
</package>
<package name="691412420003">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 3pins</description>
</package>
<package name="691412120006MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 6pins</description>
</package>
<package name="691402910004B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 4pins</description>
</package>
<package name="691411610004">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10.16mm , 4pins</description>
</package>
<package name="691416600006">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 10.16mm , 6pins</description>
</package>
<package name="691414720005B">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 18.98mm , Pitch 5mm , 5pins</description>
</package>
<package name="691411510005">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 5.08mm , 5pins</description>
</package>
<package name="691402910008B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 8pins</description>
</package>
<package name="691406510004B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 4pins</description>
</package>
<package name="691411610002">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10.16mm , 2pins</description>
</package>
<package name="691412320010M">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 10pins</description>
</package>
<package name="691411810002">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10mm , 2pins</description>
</package>
<package name="691411810005">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10mm , 5pins</description>
</package>
<package name="691412420009">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7.62mm , 9pins</description>
</package>
<package name="691406510010B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 10pins</description>
</package>
<package name="691406510003B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 3pins</description>
</package>
<package name="691406510005B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 5pins</description>
</package>
<package name="691406510006B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 6pins</description>
</package>
<package name="691406510007B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 7pins</description>
</package>
<package name="691406510002B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 2pins</description>
</package>
<package name="691411610003">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.9mm , Pitch 10.16mm , 3pins</description>
</package>
<package name="691406510012B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 12pins</description>
</package>
<package name="691406510009B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 9pins</description>
</package>
<package name="691408520002B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 2pins</description>
</package>
<package name="691406510008B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 8pins</description>
</package>
<package name="691406710005B">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4067B, Pitch 5mm,THT, 5pins</description>
</package>
<package name="691416600002">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 12.5mm , Pitch 10.16mm , 2pins</description>
</package>
<package name="691406510011B">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4065B, Pitch 5.08mm,THT, 11pins</description>
</package>
<package name="691408520006B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 6pins</description>
</package>
<package name="691408520004B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 4pins</description>
</package>
<package name="691406710002B">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4067B, Pitch 5mm,THT, 2pins</description>
</package>
<package name="691406710003B">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4067B, Pitch 5mm,THT, 3pins</description>
</package>
<package name="691408520005B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 5pins</description>
</package>
<package name="691406710004B">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4067B, Pitch 5mm,THT, 4pins</description>
</package>
<package name="691408520008B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 8pins</description>
</package>
<package name="691408520010B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 10pins</description>
</package>
<package name="691408720006B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 6pins</description>
</package>
<package name="691408520009B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 9pins</description>
</package>
<package name="691406710006B">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4067B, Pitch 5mm,THT, 6pins</description>
</package>
<package name="691408520007B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 7pins</description>
</package>
<package name="691408720005B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 5pins</description>
</package>
<package name="691408720002B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 2pins</description>
</package>
<package name="691408520003B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 3pins</description>
</package>
<package name="691408720008B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 8pins</description>
</package>
<package name="691408720010B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 10pins</description>
</package>
<package name="691408520011B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 11pins</description>
</package>
<package name="691408720012B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 12pins</description>
</package>
<package name="691408520012B">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4085B, Pitch 5.08mm,THT, 7pins</description>
</package>
<package name="691408720007B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 7pins</description>
</package>
<package name="691408720003B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 3pins</description>
</package>
<package name="691408720009B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 9pins</description>
</package>
<package name="691408720011B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 11pins</description>
</package>
<package name="691401710002B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 2pins</description>
</package>
<package name="691418220006">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 6pins</description>
</package>
<package name="691412120008MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691417220005">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 5pins</description>
</package>
<package name="691408720004B">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Series 4087B, Pitch 5mm,THT, 4pins</description>
</package>
<package name="691402910006B">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 2.54mm , 6pins</description>
</package>
<package name="691412320011">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 11pins</description>
</package>
<package name="691401710005B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 5pins</description>
</package>
<package name="691403900005B">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.6mm , Pitch 2.54mm , 5pins</description>
</package>
<package name="691412120012B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691413720006B">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 6pins</description>
</package>
<package name="691409320002">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 2pins</description>
</package>
<package name="691412120008B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 8pins</description>
</package>
<package name="691409320003">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 3pins</description>
</package>
<package name="691409320007">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 7pins</description>
</package>
<package name="691401710004B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 4pins</description>
</package>
<package name="691412120002B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 2pins</description>
</package>
<package name="691409320005">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 5pins</description>
</package>
<package name="691409320004">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 4pins</description>
</package>
<package name="691415520004">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5.08mm , 4pins</description>
</package>
<package name="691412220007M">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 7pins</description>
</package>
<package name="691409320006">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 6pins</description>
</package>
<package name="691412320002">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 2pins</description>
</package>
<package name="691415520006">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5.08mm , 6pins</description>
</package>
<package name="691409320008">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 8pins</description>
</package>
<package name="691412120012MB">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 12pins</description>
</package>
<package name="691412220002">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 2pins</description>
</package>
<package name="691409320010">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 10pins</description>
</package>
<package name="691410100002">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 2pins</description>
</package>
<package name="691409320012">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THT, 12pins</description>
</package>
<package name="691410100003">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 3pins</description>
</package>
<package name="691401710007B">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 7pins</description>
</package>
<package name="691410100006">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 6pins</description>
</package>
<package name="691412120011B">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires 
&lt;br&gt;&lt;/b&gt;Max Height = 12.8mm , Pitch 3.5mm , 11pins</description>
</package>
<package name="691410100008">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 8pins</description>
</package>
<package name="691410100004">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 4pins</description>
</package>
<package name="691410100005">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 5pins</description>
</package>
<package name="691417220004">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 7mm , 4pins</description>
</package>
<package name="691410100007">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 7pins</description>
</package>
<package name="691410110003">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 3pins</description>
</package>
<package name="691410100012">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 12pins</description>
</package>
<package name="691410100010">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 10pins</description>
</package>
<package name="691410110002">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 2pins</description>
</package>
<package name="691410110006">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 6pins</description>
</package>
<package name="691410110004">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 4pins</description>
</package>
<package name="691410110010">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 10pins</description>
</package>
<package name="691410110007">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 7pins</description>
</package>
<package name="691410110008">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 8pins</description>
</package>
<package name="691410110005">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 5pins</description>
</package>
<package name="691410110012">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 12pins</description>
</package>
<package name="691410120003">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 3pins</description>
</package>
<package name="691410120004">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 4pins</description>
</package>
<package name="691410120002">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 2pins</description>
</package>
<package name="691410120005">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 5pins</description>
</package>
<package name="691410120006">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 6pins</description>
</package>
<package name="691410120007">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 7pins</description>
</package>
<package name="691410120008">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 8pins</description>
</package>
<package name="691410120012">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 12pins</description>
</package>
<package name="691410120010">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THT, 10pins</description>
</package>
<package name="691809320302">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 2pins</description>
</package>
<package name="691809320303">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 3pins</description>
</package>
<package name="691809320308">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 8pins</description>
</package>
<package name="691809320305">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 5pins</description>
</package>
<package name="691809320306">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 6pins</description>
</package>
<package name="691809320304">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 4pins</description>
</package>
<package name="691810100302">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 2pins</description>
</package>
<package name="691809320312">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 12pins</description>
</package>
<package name="691809320307">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 7pins</description>
</package>
<package name="691809320310">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.81mm, THR, 10pins</description>
</package>
<package name="691810100305">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 5pins</description>
</package>
<package name="691810100303">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 3pins</description>
</package>
<package name="691810100306">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 6pins</description>
</package>
<package name="691810100308">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 8pins</description>
</package>
<package name="691810100304">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 4pins</description>
</package>
<package name="691810100307">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 7pins</description>
</package>
<package name="691810100312">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 12pins</description>
</package>
<package name="691810100310">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR 
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 10pins</description>
</package>
<package name="691810110304">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 4pins</description>
</package>
<package name="691810110302">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 2pins</description>
</package>
<package name="691810110305">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 5pins</description>
</package>
<package name="691810110306">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 6pins</description>
</package>
<package name="691810110303">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 3pins</description>
</package>
<package name="691810110310">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 10pins</description>
</package>
<package name="691810110307">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 7pins</description>
</package>
<package name="691810110308">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 8pins</description>
</package>
<package name="691810120303">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 3pins</description>
</package>
<package name="691810120302">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 2pins</description>
</package>
<package name="691810120304">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 4pins</description>
</package>
<package name="691810110312">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 12pins</description>
</package>
<package name="691810120305">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 5pins</description>
</package>
<package name="691810120308">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 8pins</description>
</package>
<package name="691810120306">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 6pins</description>
</package>
<package name="691810120307">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 7pins</description>
</package>
<package name="691810120310">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 10pins</description>
</package>
<package name="691810120312">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR
&lt;br&gt;&lt;/b&gt;Pitch 3.5mm, THR, 12pins</description>
</package>
</packages>
<symbols>
<symbol name="6X2+1FT_BOTTOM_RIGHT">
<description>6X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="13ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="18ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="16ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="14ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="6X2+1FT_TOP_RIGHT">
<description>6X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="15ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="17ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
</symbol>
<symbol name="12ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4X2FT_BOTTOM_RIGHT">
<description>4X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4X2+1FT_TOP_RIGHT">
<description>4X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3X2+1FT_TOP_LEFT">
<description>3X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="7ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1X2+1FT_TOP_LEFT">
<description>1X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="1X2FT_TOP_RIGHT">
<description>1X2Rows Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4X2+1FT_BOTTOM_LEFT">
<description>4X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="10ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5X2+1FT_BOTTOM_RIGHT">
<description>5X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="5X2+1FT_TOP_LEFT">
<description>5X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="4ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5X2FT_BOTTOM_RIGHT">
<description>5X2Rows  Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5X2+1FT_TOP_RIGHT">
<description>5X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="8ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4X2FT_TOP_RIGHT">
<description>4X2Rows  Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2+1FT_BOTTOM_RIGHT">
<description>2X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="19ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
</symbol>
<symbol name="9ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="1X2+1FT_BOTTOM_RIGHT">
<description>1X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2X2FT_BOTTOM_LEFT">
<description>2X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2FT_BOTTOM_LEFT">
<description>3X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="1X2+1FT_TOP_RIGHT">
<description>1X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2X2FT_TOP_RIGHT">
<description>2X2Rows  Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="23ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
</symbol>
<symbol name="3X2+1FT_BOTTOM_LEFT">
<description>3X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="5X2FT_TOP_RIGHT">
<description>5X2Rows  Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="20ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="6X2FT_BOTTOM_RIGHT">
<description>6X2Rows  Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2X2+1FT_BOTTOM_LEFT">
<description>2X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="11ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="21ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
</symbol>
<symbol name="5X2FT_BOTTOM_LEFT">
<description>5X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="3X2+1FT_TOP_RIGHT">
<description>3X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="22ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="6X2FT_TOP_RIGHT">
<description>6X2Rows  Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="1X2FT_TOP_LEFT">
<description>1X2Rows Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2X2FT_BOTTOM_RIGHT">
<description>2X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2X2+1FT_TOP_RIGHT">
<description>2X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5X2FT_TOP_LEFT">
<description>5X2Rows Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="1X2+1FT_BOTTOM_LEFT">
<description>1X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2X2+1FT_TOP_LEFT">
<description>2X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="1X2FT_BOTTOM_LEFT">
<description>1X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3X2FT_TOP_RIGHT">
<description>2X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3X2+1FT_BOTTOM_RIGHT">
<description>3X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="3FS">
<description>3 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6X2+1FT_BOTTOM_LEFT">
<description>6X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="4X2+1FT_TOP_LEFT">
<description>4X2Rows +1 Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="4X2+1FT_BOTTOM_RIGHT">
<description>4X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3X2FT_BOTTOM_RIGHT">
<description>3X2Rows  Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2FT_TOP_LEFT">
<description>2X2Rows Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="24ST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="1X2FT_BOTTOM_RIGHT">
<description>1X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM RIGHT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2FS">
<description>2 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3X2FT_TOP_LEFT">
<description>3X2Rows  Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="9ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="5ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="11ST-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="3ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="9ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="10ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6ST-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="4ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5ST-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2ST-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="3ST-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="11ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="10ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="11ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="7ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="9ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="12ST-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="12ST-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4ST-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2FT_TOP_LEFT">
<description>4X2Rows  Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6X2FT_BOTTOM_LEFT">
<description>6X2Rows  Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4X2FT_BOTTOM_LEFT">
<description>4X2Rows Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6X2FT_TOP_LEFT">
<description>6X2Rows  Female THT
&lt;br&gt;START ON THE TOP LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5X2+1FT_BOTTOM_LEFT">
<description>5X2Rows +1 Female THT
&lt;br&gt;START ON THE BOTTOM LEFT CORNER</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="3PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="12PT">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12PT-1">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="12PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PT-2">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6PT-7">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6PT-6">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="12PT-3">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6PT-8">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12PT-4">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6PT-9">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PT-11">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6PT-10">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12PT-5">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT-12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6PT-13">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12PT-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6PT-15">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PT-14">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="12PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10PT-7">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="691411510006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691411510006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691413720012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720012B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720012B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220009M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220009M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220009M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220009M"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220009M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120007MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120007MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120007MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120007MB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120007MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691413720003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720003B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720003B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691411710012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710012B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710012B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120011MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120011MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120011MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120011MB"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120011MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691401700002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700002B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700002B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691413720007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720007B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720007B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320008?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320010?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415520002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021374 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691415520002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415520002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415520002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415520002 "/>
<attribute name="WIRE" value="18 to 22 (AWG) 0.823 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691401710012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710012B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710012B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120003MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120003MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120003MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120003MB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120003MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220011?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120009B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120009B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120009B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120009B"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120009B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB"&gt;www.we-online.com/en/components/products/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-02-17&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691411710006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710006B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710006B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691401710010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710010B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710010B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691416500004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320002M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320002M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320002M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320002M"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320002M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691401710003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710003B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710003B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220011M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220011M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220011M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220011M"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220011M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691401710008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710008B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710008B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220008?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691416500010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691401700005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700005B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700005B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691411510007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220008M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220008M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220008M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220008M"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220008M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320011M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320011M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320011M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320011M"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320011M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691411910006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691416500003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691401700007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700007B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700007B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691401700006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700006B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700006B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691411510008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710019B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="19ST"/>
</gates>
<devices>
<device name="" package="691411710019B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710019B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710019B"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710019B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710009B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691411710009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710009B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710009B"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710009B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710023B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="23ST"/>
</gates>
<devices>
<device name="" package="691411710023B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="20" pad="20 A20"/>
<connect gate="G$1" pin="21" pad="21 A21"/>
<connect gate="G$1" pin="22" pad="22 A22"/>
<connect gate="G$1" pin="23" pad="23 A23"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710023B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710023B"/>
<attribute name="PINS" value=" 23 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710023B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411710003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710003B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710003B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220010?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120004B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120004B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120004B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220003M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220003M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220003M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220003M"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220003M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120006B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120006B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120006B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320004M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320004M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320004M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320004M"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320004M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120007B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120007B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120007B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411510003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120005B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120005B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418320006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691418320006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418320006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418320006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418320006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691413720002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720002B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720002B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710011B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691411710011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710011B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710011B"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710011B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320012?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220010M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220010M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220010M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220010M"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220010M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710020B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="20ST"/>
</gates>
<devices>
<device name="" package="691411710020B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="20" pad="20 A20"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710020B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710020B"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710020B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120010B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120010B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120010B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691411710008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710008B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710008B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720011B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691413720011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720011B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720011B"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720011B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417220006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691417220006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417220006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417220006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417220006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691411710010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710010B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710010B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417320006S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691417320006S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417320006S?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691417320006S"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691417320006S"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691402910003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910003B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910003B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710021B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="21ST"/>
</gates>
<devices>
<device name="" package="691411710021B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="20" pad="20 A20"/>
<connect gate="G$1" pin="21" pad="21 A21"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710021B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710021B"/>
<attribute name="PINS" value=" 21 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710021B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418220005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691418220005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418220005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418220005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418220005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320007M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320007M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320007M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320007M"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320007M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417320004S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691417320004S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417320004S?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691417320004S"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691417320004S"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691403900006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900006B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900006B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720009B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691413720009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720009B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720009B"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720009B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220002M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220002M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220002M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220002M"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220002M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691414720002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720002B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720002B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418320004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691418320004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418320004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418320004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418320004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417220003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691417220003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417220003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417220003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417220003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691416500007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320012M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320012M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320012M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320012M"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320012M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691413720004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720004B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720004B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910002MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049MB - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691404910002MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910002MB?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910002MB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910002MB"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418320002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691418320002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418320002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418320002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418320002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710022B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="22ST"/>
</gates>
<devices>
<device name="" package="691411710022B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="20" pad="20 A20"/>
<connect gate="G$1" pin="21" pad="21 A21"/>
<connect gate="G$1" pin="22" pad="22 A22"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710022B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710022B"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710022B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691413720010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720010B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720010B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417320005S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691417320005S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417320005S?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691417320005S"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691417320005S"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120010MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120010MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120010MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120010MB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120010MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417420003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691417420003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417420003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417420003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417420003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691411910010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710009B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691401710009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710009B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710009B"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710009B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320005M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320005M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320005M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320005M"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320005M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691403900003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900003B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900003B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691402910002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910002B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910002B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691411510011">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510011?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691416500006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691416500008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120003B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120003B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691411910012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910012?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691404910003B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910003B?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910003B"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411510002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910005MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049MB - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691404910005MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910005MB?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910005MB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910005MB"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm��) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691404910005B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910005B?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910005B"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220012?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411410002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049B - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78640v209%20WR-TBL_6914049100xxB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049B_SCREWLESS_POWER_6914049100xxB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691404910002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910002B?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910002B"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691411910011">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910011?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691411710007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710007B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710007B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418420006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691418420006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418420006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418420006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418420006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691411910009">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417420005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691417420005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417420005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417420005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417420005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691414720006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720006B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720006B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320006M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320006M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320006M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320006M"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320006M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417420002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691417420002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417420002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417420002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417420002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691401700008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700008B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700008B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411910002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691414720003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720003B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720003B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418420003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691418420003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418420003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418420003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418420003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691411910007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411710004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710004B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710004B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417420006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691417420006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417420006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417420006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417420006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320007?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418220003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691418220003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418220003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418220003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418220003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691411910008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691414720004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720004B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720004B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691414720008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720008B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720008B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420002M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420002M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420002M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420002M"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420002M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691805010303" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 8050 - 2.50 mm Screwless SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -45 up to +130 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 6 A 
&lt;br&gt;IR cULus 3 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Gauge Tin Dipped (AWG) 26 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section Tin Dipped (Metric) 0.129 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E323964 
&lt;br&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97266v209%20Family_WR-TBL_6918050103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97266v209%20Family_WR-TBL_6918050103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_8050_SCREWLESS_SMT_HORIZONTAL_ENTRY_6918050103XX/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_8050_SCREWLESS_SMT_HORIZONTAL_ENTRY_6918050103XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3FS"/>
</gates>
<devices>
<device name="" package="691805010303">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691805010303?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691805010303 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691805010303 "/>
<attribute name="WIRE" value="26 to 20 (AWG) 0.129 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220007?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120013B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120013B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120013B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120013B"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120013B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411510004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691411510012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510012?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415520005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021374 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691415520005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415520005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415520005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415520005 "/>
<attribute name="WIRE" value="18 to 22 (AWG) 0.823 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411910004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691401700003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700003B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700003B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220005M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220005M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220005M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220005M"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220005M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411910003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691413720008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720008B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720008B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120009MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120009MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120009MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120009MB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120009MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691403900002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900002B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900002B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691416500009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691401700012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700012B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700012B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411410004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411410003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691411510010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220009?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418420002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691418420002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418420002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418420002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418420002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418220004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691418220004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418220004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418220004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418220004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691416500002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm��) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB"&gt;www.we-online.com/en/components/products/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2023-02-17&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411710005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710005B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710005B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416500005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4165 - 5.08 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66; PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS; RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7; 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150391; E150931 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60619v209%20Family_TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4165_SCREWLESS_VERTICAL_ENTRY_6914165000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691416500005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416500005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416500005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416500005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418420004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691418420004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418420004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418420004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418420004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691401710006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710006B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710006B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320009?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411910005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4119 - 7.50 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32959v209%20Family_Con_TBL_Screwless_70_6914119100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4119_SCREWLESS_HORIZONTAL_ENTRY_6914119100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411910005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411910005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411910005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411910005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320003M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320003M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320003M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320003M"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320003M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120005MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120005MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120005MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120005MB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120005MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415520003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021374 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691415520003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415520003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415520003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415520003 "/>
<attribute name="WIRE" value="18 to 22 (AWG) 0.823 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691411510009">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417320002S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691417320002S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417320002S?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691417320002S"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691417320002S"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420003M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420003M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420003M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420003M"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420003M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420006M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420006M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420006M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420006M"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420006M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420008M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420008M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420008M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420008M"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420008M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320009M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320009M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320009M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320009M"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320009M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691411410008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120004MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120004MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120004MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120004MB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120004MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710024B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="24ST"/>
</gates>
<devices>
<device name="" package="691411710024B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="13" pad="13 A13"/>
<connect gate="G$1" pin="14" pad="14 A14"/>
<connect gate="G$1" pin="15" pad="15 A15"/>
<connect gate="G$1" pin="16" pad="16 A16"/>
<connect gate="G$1" pin="17" pad="17 A17"/>
<connect gate="G$1" pin="18" pad="18 A18"/>
<connect gate="G$1" pin="19" pad="19 A19"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="20" pad="20 A20"/>
<connect gate="G$1" pin="21" pad="21 A21"/>
<connect gate="G$1" pin="22" pad="22 A22"/>
<connect gate="G$1" pin="23" pad="23 A23"/>
<connect gate="G$1" pin="24" pad="24 A24"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710024B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710024B"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710024B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691411410011">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410011?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420007M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420007M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420007M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420007M"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420007M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418420005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4184 - 7.62 mm 45° Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79427v209%20WR-TBL_6914183200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4184_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914184200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691418420005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418420005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418420005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418420005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691411410006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="691411410012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410012?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691411410007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420004M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420004M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420004M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420004M"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420004M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691404910003MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4049MB - 7.50 mm Screwless Spring Clamp Power Connector &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 30 A 
&lt;br&gt;Working Voltage [UL] 600 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 2200 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 12 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 10 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 5.26 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78644v209%20WR-TBL_6914049100xxMB_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/"&gt;https://www.we-online.com/catalog/en/TBL_7_50_4049MB_SCREWLESS_POWER_6914049100xxMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691404910003MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691404910003MB?ae"/>
<attribute name="IR-UL" value="30A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691404910003MB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal Power Connector"/>
<attribute name="VALUE" value="691404910003MB"/>
<attribute name="WIRE" value="10 to 24 (AWG) 5.26 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417420004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4174 - 7.62 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79426v209%20WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4174_45-DEGREE_CABLE_ENTRY_SCREWLESS_6914174200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691417420004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417420004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417420004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417420004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691411410009">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410009?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420011M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420011M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420011M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420011M"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420011M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420012M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420012M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420012M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420012M"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420012M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420009M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420009M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420009M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420009M"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420009M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420007?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420007 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411810003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411810003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411810003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420005M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420005M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420005M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420005M"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420005M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420010M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124M - 7.62 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84307v209%20Family_WR-TBL_6914124200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124M_SCREWLESS_45-DEGREE_ENTRY_6914124200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420010M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420010M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412420010M"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412420010M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411810004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411810004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411810004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420011?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420010?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411410005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691805010302" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 8050 - 2.50 mm Screwless SMT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -45 up to +130 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 6 A 
&lt;br&gt;IR cULus 3 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Gauge Tin Dipped (AWG) 26 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section Tin Dipped (Metric) 0.129 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E323964 
&lt;br&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97266v209%20Family_WR-TBL_6918050103xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97266v209%20Family_WR-TBL_6918050103xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_50_8050_SCREWLESS_SMT_HORIZONTAL_ENTRY_6918050103XX/"&gt;https://www.we-online.com/catalog/en/TBL_2_50_8050_SCREWLESS_SMT_HORIZONTAL_ENTRY_6918050103XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2FS"/>
</gates>
<devices>
<device name="" package="691805010302">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691805010302?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 691805010302 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691805010302 "/>
<attribute name="WIRE" value="26 to 20 (AWG) 0.129 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411410010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4114 - 7.62 mm Screwless Horizontal Cable Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm      
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4114_SCREWLESS_HORIZONTAL_ENTRY_6914114100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691411410010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411410010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411410010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411410010 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416600005">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 7  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691416600005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416600005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416600005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416600005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418320005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691418320005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418320005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418320005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418320005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411610005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411610005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411610005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411610005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411610005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220012M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220012M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220012M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220012M"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220012M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416600003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 7  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691416600003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416600003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416600003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416600003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416600004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 7  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691416600004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416600004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416600004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416600004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420008?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420008 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120002MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120002MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120002MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120002MB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120002MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691413720005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720005B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720005B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415620003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4156 - 10.16 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 10 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60615v209%20Family_TBL_10_16_4156_SCREWLESS_45_ENTRY_6914156200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60615v209%20Family_TBL_10_16_4156_SCREWLESS_45_ENTRY_6914156200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4156_SCREWLESS_45-DEGREE_ENTRY_6914156200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4156_SCREWLESS_45-DEGREE_ENTRY_6914156200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691415620003">
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415620003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415620003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415620003 "/>
<attribute name="WIRE" value="16 to 22 (AWG) 1.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691402910005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910005B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910005B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320008M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320008M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320008M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320008M"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320008M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220004M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220004M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220004M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220004M"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220004M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418220002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691418220002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418220002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418220002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418220002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691401700004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700004B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700004B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691403900008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900008B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900008B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415620002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4156 - 10.16 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 10 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60615v209%20Family_TBL_10_16_4156_SCREWLESS_45_ENTRY_6914156200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60615v209%20Family_TBL_10_16_4156_SCREWLESS_45_ENTRY_6914156200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4156_SCREWLESS_45-DEGREE_ENTRY_6914156200xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4156_SCREWLESS_45-DEGREE_ENTRY_6914156200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691415620002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415620002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415620002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415620002 "/>
<attribute name="WIRE" value="16 to 22 (AWG) 1.31 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417220002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691417220002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417220002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417220002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417220002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710011B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691401710011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710011B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710011B"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710011B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700009B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="691401700009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700009B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700009B"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700009B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220006M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220006M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220006M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220006M"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220006M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700010B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="691401700010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700010B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700010B"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700010B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401700011B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Vertical Entry - 2.0 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33321v209%20Family_WR-TBL_6914017000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_VERTICAL_ENTRY_2_0MM2_WIRES_6914017000XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="691401700011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401700011B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401700011B"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691401700011B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420012" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420012?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420012 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420012 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691403900004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900004B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900004B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417320003S" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4173S - 3.81 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79334v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4173S_SCREWLESS_ANGLED_ENTRY_6914173200XXS/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691417320003S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417320003S?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691417320003S"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691417320003S"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 411B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;R cULus 10 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33341v209%20Family_WR-TLB_6914117100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_411B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914117100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411710002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411710002B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691411710002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691411710002B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418320003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4183 - 3.81 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79471v209%20Family_WR-TBL_6914173200xxS_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4183_SCREWLESS_ANGLED_ENTRY_6914183200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691418320003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418320003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418320003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418320003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420003?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120006MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120006MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120006MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120006MB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120006MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691402910004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910004B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910004B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416600006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 7  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691416600006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416600006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416600006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416600006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691414720005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4147B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1300 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33327v209%20Family_WR-TBL_69141472000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_4147B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_69141472000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691414720005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691414720005B?ae"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691414720005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691414720005B"/>
<attribute name="WIRE" value="14 to 28 (AWG) 2.08 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411610004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691411610004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411610004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411610004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411610004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411510005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4115 - 5.08 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32955v209%20Family_Con_TBL_Screwless_508_6914115100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4115_SCREWLESS_HORIZONTAL_ENTRY_6914115100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411510005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411510005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411510005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411510005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="691402910008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910008B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910008B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST-1"/>
</gates>
<devices>
<device name="" package="691406510004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510004B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510004B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411610002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411610002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411610002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411610002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411610002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411810005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691411810005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411810005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411810005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411810005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4118 - 10.00 mm Screwless Horizontal Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84296v209%20Family_WR-TBL4_6914114100xx" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_00_4118_SCREWLESS_HORIZONTAL_ENTRY_6914118100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691411810002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411810002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411810002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320010M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123M - 3.81 mm Screwless 45° Entry  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84319v209%20Family_WR-TBL_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123M_SCREWLESS_45-DEGREE_ENTRY_6914123200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320010M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320010M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412320010M"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412320010M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST-1"/>
</gates>
<devices>
<device name="" package="691406510003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510003B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510003B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST-1"/>
</gates>
<devices>
<device name="" package="691406510010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7" route="any"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510010B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510010B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412420009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4124 - 7.62 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.62 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84305v209%20Family_WR-TBL4_6914124200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_62_4124_SCREWLESS_45-DEGREE_ENTRY_6914124200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412420009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412420009?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412420009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412420009 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST-1"/>
</gates>
<devices>
<device name="" package="691406510005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510005B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510005B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST-1"/>
</gates>
<devices>
<device name="" package="691406510002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510002B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510002B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST-1"/>
</gates>
<devices>
<device name="" package="691406510006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510006B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510006B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510007B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST-1"/>
</gates>
<devices>
<device name="" package="691406510007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510007B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510007B"/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510007B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691411610003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4116 - 10.16 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931; E150931 Cat No. MRT1 (1) 
&lt;br&gt;VDE Approval 40021396 
&lt;br&gt;VDE Approval 40021396 Type MRT1 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84491v209%20Family_WR-TBL_6914118100xx_6914116100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4116_SCREWLESS_HORIZONTAL_ENTRY_6914116100xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="691411610003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691411610003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691411610003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691411610003 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST-1"/>
</gates>
<devices>
<device name="" package="691406510012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510012B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510012B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510009B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST-1"/>
</gates>
<devices>
<device name="" package="691406510009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510009B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510009B"/>
<attribute name="PINS" value="9"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510009B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST-3"/>
</gates>
<devices>
<device name="" package="691408520002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520002B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520002B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST-1"/>
</gates>
<devices>
<device name="" package="691406510008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510008B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510008B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST-2"/>
</gates>
<devices>
<device name="" package="691406710005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406710005B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406710005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406710005B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406510011B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4065B - Screwless Push In 5.08 mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257335v209%206914065100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4065B_SCREWLESSPUSHIN_5_08MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-23&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST-1"/>
</gates>
<devices>
<device name="" package="691406510011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406510011B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406510011B"/>
<attribute name="PINS" value="11"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406510011B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691416600002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4166 - 10.16 mm Screwless Vertical Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10.16 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/B&gt;Wire Strip Length 7  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60621v209%20Family_TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/"&gt;https://www.we-online.com/catalog/en/TBL_10_16_4166_SCREWLESS_VERTICAL_ENTRY_6914166000xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691416600002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691416600002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691416600002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10.16mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691416600002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST-3"/>
</gates>
<devices>
<device name="" package="691408520004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520004B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520004B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST-3"/>
</gates>
<devices>
<device name="" package="691408520006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520006B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520006B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST-2"/>
</gates>
<devices>
<device name="" package="691406710002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406710002B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406710002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406710002B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST-3"/>
</gates>
<devices>
<device name="" package="691408520005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520005B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520005B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST-2"/>
</gates>
<devices>
<device name="" package="691406710003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406710003B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406710003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406710003B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST-2"/>
</gates>
<devices>
<device name="" package="691406710004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406710004B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406710004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406710004B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST-2"/>
</gates>
<devices>
<device name="" package="691408520008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6" route="any"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520008B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520008B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST-2"/>
</gates>
<devices>
<device name="" package="691408520010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520010B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520010B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520009B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST-2"/>
</gates>
<devices>
<device name="" package="691408520009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520009B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520009B"/>
<attribute name="PINS" value="9"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520009B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST-4"/>
</gates>
<devices>
<device name="" package="691408720006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720006B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720006B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691406710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4067B - Screwless Push In 5.0mm pitch - Horizontal cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257327v209%206914067100xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES_4067B_SCREWLESS-PUSH-IN-5_0MM-PITCH_HORIZONTAL-CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST-2"/>
</gates>
<devices>
<device name="" package="691406710006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691406710006B?ae"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691406710006B"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value="691406710006B"/>
<attribute name="WIRE" value="24 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST-3"/>
</gates>
<devices>
<device name="" package="691408520003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520003B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520003B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520007B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST-2"/>
</gates>
<devices>
<device name="" package="691408520007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520007B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520007B"/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520007B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720002B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST-4"/>
</gates>
<devices>
<device name="" package="691408720002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720002B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720002B"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720002B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720005B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST-4"/>
</gates>
<devices>
<device name="" package="691408720005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720005B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720005B"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720005B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720010B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST-3"/>
</gates>
<devices>
<device name="" package="691408720010B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720010B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720010B"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720010B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720008B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST-3"/>
</gates>
<devices>
<device name="" package="691408720008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720008B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720008B"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720008B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST-3"/>
</gates>
<devices>
<device name="" package="691408720012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720012B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720012B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520012B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST-2"/>
</gates>
<devices>
<device name="" package="691408520012B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5" route="any"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520012B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520012B"/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520012B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408520011B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4085B - Screwless Push In 5.08mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o257340v209%206914085200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT"&gt;https://www.we-online.com/catalog/en/SERIES4085B_SCREWLESS-PUSH-IN_5_08MM_PITCH_45__CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST-2"/>
</gates>
<devices>
<device name="" package="691408520011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408520011B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408520011B"/>
<attribute name="PINS" value="11"/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408520011B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720007B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST-3"/>
</gates>
<devices>
<device name="" package="691408720007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720007B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720007B"/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720007B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720009B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST-3"/>
</gates>
<devices>
<device name="" package="691408720009B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720009B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720009B"/>
<attribute name="PINS" value="9"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720009B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720011B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST-3"/>
</gates>
<devices>
<device name="" package="691408720011B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720011B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720011B"/>
<attribute name="PINS" value="11"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720011B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720003B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST-4"/>
</gates>
<devices>
<device name="" package="691408720003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720003B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720003B"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720003B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691408720004B" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4087B - Screwless Push In 5.0mm pitch - 45° cable entry - THT  &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 up to 10 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 28 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 2.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt; cULus 15 A 
&lt;br&gt;Working Voltage 300 V 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o257338v209%206914087200xxB_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT"&gt;https://www.we-online.com/catalog/en/WR-TBL_SERIES4087B_SCREWLESS-PUSH-IN-5_0MM-PITCH_45__CABLE-ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2021-02-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST-4"/>
</gates>
<devices>
<device name="" package="691408720004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691408720004B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691408720004B"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value="691408720004B"/>
<attribute name="WIRE" value="28 to 12 (AWG) 0.2 to 2.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="691401710002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710002B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710002B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691418220006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4182 - 7.00 mm 45° Cable Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79353v209%20WR-TBL_6914182200xx_6914184200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4182_SCREWLESS_ANGLED_ENTRY_6914182200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691418220006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691418220006?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691418220006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691418220006 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120008MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120008MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120008MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120008MB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120008MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320011" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320011?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320011 "/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320011 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691402910006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4029 - 2.54 mm Screwless Horizontal Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64650v209%20Family_WR-TBL_691402910008B.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4029_SCREWLESS_HORIZONTAL_ENTRY_69140291000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691402910006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691402910006B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691402910006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691402910006B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417220005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691417220005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417220005?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417220005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417220005 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="691409320002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320002?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320002 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691413720006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 413B - 5.00 mm Screwless 45° Entry - 3.00 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 28 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.0810 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33326v209%20Family_WR-TBL_6914137200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_413B_SCREWLESS_45-DEGREE_ENTRY_3_0MM2_WIRES_6914137200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691413720006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691413720006B?ae"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691413720006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691413720006B"/>
<attribute name="WIRE" value="12 to 28 (AWG) 3.31 to 0.0810 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120012B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120012B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120012B"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120012B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691401710005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710005B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710005B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691403900005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4039 - 2.54 mm Screwless Vertical Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 2.54 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;Working Voltage [cULus] 150 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 20 to 26 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.518 to 0.129 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33323v209%20Family_WR-TBL_69140390000xB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/"&gt;https://www.we-online.com/catalog/en/TBL_2_54_4039B_SCREWLESS_VERTICAL_ENTRY_69140390000XB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="691403900005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691403900005B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691403900005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="691403900005B"/>
<attribute name="WIRE" value="20 to 26 (AWG) 0.518 to 0.129 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="150V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="691409320003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320003 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120008B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120008B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120008B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320007" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-1"/>
</gates>
<devices>
<device name="" package="691409320007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320007?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320007 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320007 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120002B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120002B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120002B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691401710004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710004B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710004B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="691409320005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320005?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320005 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320005 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="691409320004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320004 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415520004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021374 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691415520004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415520004?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415520004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415520004 "/>
<attribute name="WIRE" value="18 to 22 (AWG) 0.823 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="691409320006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320006 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320006 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412320002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²)
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84303v209%20Family_WR-TBL4_6914123200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/"&gt;https://www.we-online.com/catalog/en/TBL_3_81_4123_SCREWLESS_45-DEGREE_ENTRY_6914123200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412320002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412320002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412320002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220007M" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122M - 7.00 mm 45° Entry Screwless&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84317v209%20Family_WR-TBL_6914122200xxM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122M_SCREWLESS_45-DEGREE_ENTRY_6914122200xxM/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2+1FT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220007M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220007M?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412220007M"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412220007M"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691415520006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4155 - 5.08 mm Screwless 45° Entry&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5.08 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material INOX Steel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance ROHS &amp; Reach 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 22 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.326 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 22 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.326 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021374 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32963v209%20Family_WR-TBL4_Series4155.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/"&gt;https://www.we-online.com/catalog/en/TBL_5_08_4155_SCREWLESS_45-DEGREE_ENTRY_69141552000x/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="691415520006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691415520006?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691415520006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691415520006 "/>
<attribute name="WIRE" value="18 to 22 (AWG) 0.823 to 0.326 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120012MB" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412MB - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33325v209%20S534_WR-TBL_6914121200xxMB_a_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412MB_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXMB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2FT_TOP_LEFT"/>
</gates>
<devices>
<device name="" package="691412120012MB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120012MB?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120012MB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120012MB"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320008" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="691409320008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320008?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320008 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320008 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412220002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4122 - 7.00 mm Screwless 45° Entry &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. MRT24 (3) 
&lt;br&gt;VDE Approval 40013441 Type MRT24 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o84301v209%20Family_WR-TBL4_6914122200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4122_SCREWLESS_45-DEGREE_ENTRY_6914122200xx/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2FT_BOTTOM_RIGHT"/>
</gates>
<devices>
<device name="" package="691412220002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412220002?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412220002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691412220002 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320010" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="691409320010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320010?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320010 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320010 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-1"/>
</gates>
<devices>
<device name="" package="691410100002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100002?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100002 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-1"/>
</gates>
<devices>
<device name="" package="691410100003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100003?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100003 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691412120011B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 412B - 3.50 mm Screwless 45° Entry - 2.1 mm 2 Wires&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 6 A 
&lt;br&gt;IR VDE 2 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7.5 up to 8.5 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 20 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.518 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036145 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33324v209%20Family_WR-TBL_6914121200xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/"&gt;https://www.we-online.com/catalog/en/TBL_3_50_412B_SCREWLESS_45-DEGREE_ENTRY_2_1MM2_WIRES_6914121200XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2+1FT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="691412120011B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691412120011B?ae"/>
<attribute name="IR-UL" value="6A"/>
<attribute name="IR-VDE" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691412120011B"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value="691412120011B"/>
<attribute name="WIRE" value="14 to 20 (AWG) 2.08 to 0.518 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-2"/>
</gates>
<devices>
<device name="" package="691410100006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100006?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100006 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100006 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691409320012" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4093 - Screwless Push In 3.81mm pitch - 45° cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055091 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722431v209%20family-wr-tbl-6914093200xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4093_SCREWLESS_PUSH_45_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="691409320012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691409320012?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691409320012 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691409320012 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691401710007B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 401B - 5.00 mm Screwless Horizontal Entry - 2.0 mm 2 Wires &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm     
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 9 up to 10 (mm)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.205 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40036896 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33322v209%20Family_WR-TBL_6914017100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/"&gt;https://www.we-online.com/catalog/en/TBL_5_00_401B_SCREWLESS_HORIZONTAL_ENTRY_2_0MM2_WIRES_6914017100XXB/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="691401710007B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691401710007B?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691401710007B"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691401710007B"/>
<attribute name="WIRE" value="14 to 24 (AWG) 2.08 to 0.205 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-1"/>
</gates>
<devices>
<device name="" package="691410100005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100005?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100005 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100005 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-1"/>
</gates>
<devices>
<device name="" package="691410100004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100004?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100004 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100008" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-1"/>
</gates>
<devices>
<device name="" package="691410100008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100008?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100008 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100008 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100007" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-3"/>
</gates>
<devices>
<device name="" package="691410100007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100007?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100007 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100007 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691417220004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 4172 - 7.00 mm 45° Cable Entry Screwless &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin 
&lt;br&gt;Wire Guard Material Phosphor Bronze 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 4 A 
&lt;br&gt;IR VDE 4 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 16 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 1.31 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40013441 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79347v209%20WR-TBL_6914172200xx_6914174200xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/"&gt;https://www.we-online.com/catalog/en/TBL_7_00_4172_SCREWLESS_ANGLED_ENTRY_6914172200XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-12-31&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="691417220004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691417220004?ae"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691417220004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="VALUE" value=" 691417220004 "/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100010" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-1"/>
</gates>
<devices>
<device name="" package="691410100010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100010?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100010 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100010 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-2"/>
</gates>
<devices>
<device name="" package="691410110002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110002?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110002 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410100012" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722745v209%206914101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH__VERTICAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-1"/>
</gates>
<devices>
<device name="" package="691410100012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410100012?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410100012 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691410100012 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-2"/>
</gates>
<devices>
<device name="" package="691410110003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110003?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110003 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-4"/>
</gates>
<devices>
<device name="" package="691410110006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110006?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110006 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110006 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110010" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-2"/>
</gates>
<devices>
<device name="" package="691410110010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110010?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110010 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110010 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-2"/>
</gates>
<devices>
<device name="" package="691410110004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110004?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110004 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110007" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-5"/>
</gates>
<devices>
<device name="" package="691410110007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110007?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110007 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110007 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-2"/>
</gates>
<devices>
<device name="" package="691410110005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110005?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110005 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110005 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110012" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-2"/>
</gates>
<devices>
<device name="" package="691410110012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110012?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110012 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110012 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410110008" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5 mm pitch - Horizontal cable entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C   
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722750v209%20Multi-WR-TBL-6914101100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-2"/>
</gates>
<devices>
<device name="" package="691410110008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410110008?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410110008 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691410110008 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-3"/>
</gates>
<devices>
<device name="" package="691410120003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120003?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120003 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-3"/>
</gates>
<devices>
<device name="" package="691410120002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120002?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120002 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-3"/>
</gates>
<devices>
<device name="" package="691410120004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120004?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120004 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-6"/>
</gates>
<devices>
<device name="" package="691410120006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120006?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120006 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120006 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120007" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-7"/>
</gates>
<devices>
<device name="" package="691410120007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120007?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120007 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120007 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-3"/>
</gates>
<devices>
<device name="" package="691410120005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120005?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120005 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120005 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120008" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-3"/>
</gates>
<devices>
<device name="" package="691410120008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120008?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120008 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120008 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120012" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-3"/>
</gates>
<devices>
<device name="" package="691410120012">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120012?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120012 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120012 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691410120010" prefix="J">
<description>&lt;b&gt;WR-TBL Series 4101 - Screwless Push In 3.5mm pitch - 45° cable entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +110 °C  
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722754v209%206914101200xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;https://www.we-online.com/en/components/products/WR-TBL_SERIES_4101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-3"/>
</gates>
<devices>
<device name="" package="691410120010">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691410120010?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691410120010 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691410120010 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320302" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-4"/>
</gates>
<devices>
<device name="" package="691809320302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320302?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320302 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320302 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320303" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-4"/>
</gates>
<devices>
<device name="" package="691809320303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320303?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320303 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320303 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320305" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-4"/>
</gates>
<devices>
<device name="" package="691809320305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320305?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320305 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320305 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320308" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-4"/>
</gates>
<devices>
<device name="" package="691809320308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320308?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320308 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320308 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320304" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-4"/>
</gates>
<devices>
<device name="" package="691809320304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320304?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320304 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320304 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100302" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-5"/>
</gates>
<devices>
<device name="" package="691810100302">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100302?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100302 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100302 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320312" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-4"/>
</gates>
<devices>
<device name="" package="691809320312">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320312?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320312 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320312 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320307" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-9"/>
</gates>
<devices>
<device name="" package="691809320307">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320307?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320307 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320307 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320306" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-8"/>
</gates>
<devices>
<device name="" package="691809320306">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320306?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320306 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320306 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691809320310" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8093 - Screwless Push In 3.81mm pitch - 45° cable entry - THR &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.81 mm    
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +115 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 10 A 
&lt;br&gt;IR VDE 9 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 130 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1250 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055182 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel x 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722757v209%206918093203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8093_SCREWLESS_PUSH_IN_3_81MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-4"/>
</gates>
<devices>
<device name="" package="691809320310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691809320310?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="IR-VDE" value="9A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691809320310 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691809320310 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="130V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100303" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-5"/>
</gates>
<devices>
<device name="" package="691810100303">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100303?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100303 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100303 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100305" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-5"/>
</gates>
<devices>
<device name="" package="691810100305">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100305?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100305 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100305 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100308" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-5"/>
</gates>
<devices>
<device name="" package="691810100308">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100308?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100308 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100308 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100306" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-10"/>
</gates>
<devices>
<device name="" package="691810100306">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100306?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100306 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100306 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100304" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-5"/>
</gates>
<devices>
<device name="" package="691810100304">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100304?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100304 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100304 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100307" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-11"/>
</gates>
<devices>
<device name="" package="691810100307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100307?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100307 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100307 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100310" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-5"/>
</gates>
<devices>
<device name="" package="691810100310">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100310?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100310 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100310 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810100312" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Vertical cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722794v209%206918101000xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_VERTICAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-5"/>
</gates>
<devices>
<device name="" package="691810100312">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810100312?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810100312 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691810100312 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110304" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-6"/>
</gates>
<devices>
<device name="" package="691810110304">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110304?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110304 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110304 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110302" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-6"/>
</gates>
<devices>
<device name="" package="691810110302">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110302?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110302 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110302 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110303" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-6"/>
</gates>
<devices>
<device name="" package="691810110303">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110303?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110303 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110303 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110306" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-12"/>
</gates>
<devices>
<device name="" package="691810110306">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110306?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110306 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110306 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110305" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-6"/>
</gates>
<devices>
<device name="" package="691810110305">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110305?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110305 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110305 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110310" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-6"/>
</gates>
<devices>
<device name="" package="691810110310">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110310?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110310 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110310 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120303" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT-7"/>
</gates>
<devices>
<device name="" package="691810120303">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120303?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120303 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120303 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110308" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-6"/>
</gates>
<devices>
<device name="" package="691810110308">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110308?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110308 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110308 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110307" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-13"/>
</gates>
<devices>
<device name="" package="691810110307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110307?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110307 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110307 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120302" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT-7"/>
</gates>
<devices>
<device name="" package="691810120302">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120302?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120302 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120302 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120304" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT-7"/>
</gates>
<devices>
<device name="" package="691810120304">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120304?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120304 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120304 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810110312" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - Horizontal cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722796v209%206918101103xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_HORIZONTAL_CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-6"/>
</gates>
<devices>
<device name="" package="691810110312">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810110312?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810110312 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691810110312 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120308" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT-7"/>
</gates>
<devices>
<device name="" package="691810120308">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120308?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120308 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120308 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120305" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT-7"/>
</gates>
<devices>
<device name="" package="691810120305">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120305?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120305 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120305 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120307" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-15"/>
</gates>
<devices>
<device name="" package="691810120307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120307?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120307 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120307 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120306" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT-14"/>
</gates>
<devices>
<device name="" package="691810120306">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120306?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120306 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120306 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120312" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT-7"/>
</gates>
<devices>
<device name="" package="691810120312">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="11" pad="11 A11"/>
<connect gate="G$1" pin="12" pad="12 A12"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120312?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120312 "/>
<attribute name="PINS" value="12"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120312 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691810120310" prefix="J">
<description>&lt;b&gt;WR-TBL Series 8101 - Screwless Push In 3.5mm pitch - 45° cable entry - THR&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm   
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA4T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Spring Material Stainless Steel 
&lt;br&gt;Pin Material Brass 
&lt;br&gt;Pin Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +125 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 7 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 160 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1400 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Wire Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Solid Wire Section (AWG) 24 to 18 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.2 to 1 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.2 to 1.5 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40055316 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722798v209%206918101203xx_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/WR-TBL_SERIES_8101_SCREWLESS_PUSH_IN_3_5MM_PITCH_45___CABLE_ENTRY_THR&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2023-06-13&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT-7"/>
</gates>
<devices>
<device name="" package="691810120310">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691810120310?ae"/>
<attribute name="IR-UL" value="7A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value=" 691810120310 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="45° Cable Entry"/>
<attribute name="VALUE" value=" 691810120310 "/>
<attribute name="WIRE" value="22 to 16 (AWG) 0.2 to 1.5 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V"/>
<attribute name="WORKING-VOLTAGE-VDE" value="160V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
