<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Terminal Blocks - WR-TBL  Wire Protector &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-04-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691136800008">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 8 Pins</description>
</package>
<package name="691103810101">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 10mm ,  1 Pins</description>
</package>
<package name="691101810008">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 8 Pins</description>
</package>
<package name="691134710003">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691104700002">
<description>&lt;b&gt;WR-TBL Serie 1047 - 5.00 mm Vertical Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136810007">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 7 Pins</description>
</package>
<package name="691137810002">
<description>&lt;b&gt;WR-TBL Serie 1378 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691137710008">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691136810008">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 8 Pins</description>
</package>
<package name="691135700007">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691126710004B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691134710002">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691104800101">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691136710008">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691134810001">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691135710006">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691134810002">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691101810007">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 7 Pins</description>
</package>
<package name="691131810002">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136810009">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 9 Pins</description>
</package>
<package name="691136810004">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691136800006">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 6 Pins</description>
</package>
<package name="691132700004">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691135710008">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691133710005">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691137710006">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691137810003">
<description>&lt;b&gt;WR-TBL Serie 1378 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691135710004">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691131710006">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691101810009">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 9 Pins</description>
</package>
<package name="691103810001">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 10mm ,  1 Pins</description>
</package>
<package name="691103110002">
<description>&lt;b&gt;WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 8.4mm , Pitch 3.5mm , 2 Pins</description>
</package>
<package name="691104700003">
<description>&lt;b&gt;WR-TBL Serie 1047 - 5.00 mm Vertical Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691131810003">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691102810001">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691101810010">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 10 Pins</description>
</package>
<package name="691137910005">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 5 Pins</description>
</package>
<package name="691136800004">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691101810101">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691126710006B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691106800003">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT
&lt;br&gt;&lt;/b&gt;Max Height =7.8mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691131710002">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691131710004">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691136810006">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 6 Pins</description>
</package>
<package name="691136710005">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691135700004">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691102810002">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691136700004">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691137710003">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691106800004">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT
&lt;br&gt;&lt;/b&gt;Max Height =7.8mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691136710010">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691135800003">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691127700004B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691126710003B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691106800001">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT
&lt;br&gt;&lt;/b&gt;Max Height =7.8mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691136710009">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691102810003">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691136700009">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691135700009">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691132700006">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691103810002">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 10mm ,  2 Pins</description>
</package>
<package name="691137910003">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 3 Pins</description>
</package>
<package name="691106800002">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT
&lt;br&gt;&lt;/b&gt;Max Height =7.8mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691136710004">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691127700003B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691106800101">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT
&lt;br&gt;&lt;/b&gt;Max Height =7.8mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691132700005">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691136700005">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691137910004">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 4 Pins</description>
</package>
<package name="691136800010">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 10 Pins</description>
</package>
<package name="691135710009">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691102810101">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691111710003">
<description>&lt;b&gt;WR-TBL Serie 111 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 11mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691102810004">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 10.3mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691132700008">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691101710003">
<description>&lt;b&gt;WR-TBL Serie 101 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691136800003">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691133710007">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691101710002">
<description>&lt;b&gt;WR-TBL Serie 101 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691126710008B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691136800007">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 7 Pins</description>
</package>
<package name="691137910008">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 8 Pins</description>
</package>
<package name="691135710005">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691131710005">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691135710007">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691137910002">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 2 Pins</description>
</package>
<package name="691136700008">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691502710003">
<description>&lt;b&gt;WR-TBL Serie 5027 - 5.00 mm Horizontal Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691135810004">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Horiz. Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691502710002">
<description>&lt;b&gt;WR-TBL Serie 5027 - 5.00 mm Horizontal Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =10mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136700010">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691127700005B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691135700010">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691133710008">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691127700008B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691136800009">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 9 Pins</description>
</package>
<package name="691102710003">
<description>&lt;b&gt;WR-TBL Serie 102 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 9.9mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691136810003">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691135700006">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691132700002">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691135810003">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Horiz. Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 10mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691102710002">
<description>&lt;b&gt;WR-TBL Serie 102 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 9.9mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691127700002B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136810005">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 5 Pins</description>
</package>
<package name="691104800002">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691136700007">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691132700003">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible
&lt;br&gt;&lt;/b&gt;Max Height = 10.5mm , Pitch 5mm , 3 Pins</description>
</package>
<package name="691101810001">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 1 Pin</description>
</package>
<package name="691134810101">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691126710005B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691136710006">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691137710005">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691133710006">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691101810006">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 6 Pins</description>
</package>
<package name="691131710008">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691135700005">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 5 Pins</description>
</package>
<package name="691131810004">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691101810004">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691137710004">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691133710010">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 10 Pins</description>
</package>
<package name="691136800005">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 10mm , 5 Pins</description>
</package>
<package name="691111710002">
<description>&lt;b&gt;WR-TBL Serie 111 - 5.00 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 11mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136700006">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 9mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691133710009">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 9 Pins</description>
</package>
<package name="691101810005">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 5 Pins</description>
</package>
<package name="691135700008">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 5mm , 8 Pins</description>
</package>
<package name="691133810002">
<description>&lt;b&gt;WR-TBL Serie 1338 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691126710002B">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 18.6mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691136710007">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 7 Pins</description>
</package>
<package name="691101810002">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 2 Pins</description>
</package>
<package name="691135800004">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 10mm , 4 Pins</description>
</package>
<package name="691133710004">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 5mm , 4 Pins</description>
</package>
<package name="691133810003">
<description>&lt;b&gt;WR-TBL Serie 1338 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691103110003">
<description>&lt;b&gt;WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height = 8.4mm , Pitch 3.5mm ,  3 Pins</description>
</package>
<package name="691137710002">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 5mm , 2 Pins</description>
</package>
<package name="691101810003">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT 
&lt;br&gt;&lt;/b&gt;Max Height = 12.6mm , Pitch 10mm , 3 Pins</description>
</package>
<package name="691137910006">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 11.5mm , Pitch 7.5mm , 6 Pins</description>
</package>
<package name="691104800001">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire
&lt;br&gt;&lt;/b&gt;Max Height = 7.5mm , Pitch 10mm , 1 Pins</description>
</package>
<package name="691136810010">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp
&lt;br&gt;&lt;/b&gt;Max Height = 13mm , Pitch 10mm , 10 Pins</description>
</package>
<package name="691127700006B">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp
&lt;br&gt;&lt;/b&gt;Max Height = 19.5mm , Pitch 5mm , 6 Pins</description>
</package>
<package name="691131710003">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible
&lt;br&gt;&lt;/b&gt;Max Height = 15.5mm , Pitch 5mm , 3 Pins</description>
</package>
</packages>
<symbols>
<symbol name="8PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="7PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="8PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="9PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="5PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="9PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="10PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-3">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-2">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="3PINS_ENTRY-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-5">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2PINS_ENTRY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PINS_ENTRY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="10PINS_ENTRY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-6">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="4PINS_ENTRY-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2PINS_ENTRY-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-4">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="4PINS_ENTRY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="1PIN_ENTRY-1">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="6PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3PINS_ENTRY-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="691136800008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691103810101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691103810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691103810101.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691103810101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691103810101 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691134710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CMM (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021375 TYPE: CMM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32799v209%20Family_WR-TBL1_Series1347.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32799v209%20Family_WR-TBL1_Series1347.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1347_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113471000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1347_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113471000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691134710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691134710003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691134710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691134710003 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810008" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810008 "/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810008 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810007.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691104700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1047 - 5.00 mm Vertical Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33227v209%20Family_WR-TBL_69110470000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33227v209%20Family_WR-TBL_69110470000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1047_6911047000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1047_6911047000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691104700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691104700002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691104700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691104700002 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1378 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58985v209%20Family_Con-TBL_Screw_PressureClamp_6911378100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58985v209%20Family_Con-TBL_Screw_PressureClamp_6911378100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1378_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113781000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1378_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113781000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137810002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137810002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710008 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700007.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710004B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710004B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691134710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1347- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CMM (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021375 TYPE: CMM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32799v209%20Family_WR-TBL1_Series1347.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32799v209%20Family_WR-TBL1_Series1347.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1347_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113471000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1347_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113471000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691134710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691134710002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691134710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691134710002 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691104800101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931;​ E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691104800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691104800101.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691104800101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691104800101 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691134810001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1348 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CMM (1) 
&lt;br&gt;VDE Approval 40021375 
&lt;br&gt;VDE Approval 40021375 TYPE: CMM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691134810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691134810001.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691134810001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691134810001 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810007" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810007.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810007 "/>
<attribute name="PINS" value="7"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810007 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710006.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm��) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810009.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691134810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1348 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CMM (1) 
&lt;br&gt;VDE Approval 40021375 
&lt;br&gt;VDE Approval 40021375 TYPE: CMM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691134810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691134810002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691134810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691134810002 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU (2) 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131810002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131810002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710008.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700004 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710005.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710005 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710006 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1378 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58985v209%20Family_Con-TBL_Screw_PressureClamp_6911378100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58985v209%20Family_Con-TBL_Screw_PressureClamp_6911378100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1378_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113781000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1378_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113781000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137810003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137810003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710004.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810009" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810009.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810009 "/>
<attribute name="PINS" value="9"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810009 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710006 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691103810001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691103810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691103810001.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691103810001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691103810001 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691103110002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 125 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 1.31 (mm²)  
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.129 to 1.31 (mm²)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33226v209%20Family_WR-TBL_69110311000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33226v209%20Family_WR-TBL_69110311000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_1031_6911031100XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_1031_6911031100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691103110002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691103110002.pdf"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691103110002"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691103110002"/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.129 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691104700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1047 - 5.00 mm Vertical Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33227v209%20Family_WR-TBL_69110470000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33227v209%20Family_WR-TBL_69110470000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1047_6911047000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1047_6911047000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691104700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691104700003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691104700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691104700003 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU (2) 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131810003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131810003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810010" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810010.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810010 "/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810010 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102810001" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-3"/>
</gates>
<devices>
<device name="" package="691102810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102810001.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102810001 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691102810001 "/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910005 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810101" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-2"/>
</gates>
<devices>
<device name="" package="691101810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810101.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810101 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810101 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710006B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710006B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691106800003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V 
&lt;br&gt;Withstanding Voltage 1500 V 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY-3"/>
</gates>
<devices>
<device name="" package="691106800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691106800003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691106800003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691106800003 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710004 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm��) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700004.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102810002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY-2"/>
</gates>
<devices>
<device name="" package="691102810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102810002.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102810002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691102810002 "/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710003 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691106800004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V 
&lt;br&gt;Withstanding Voltage 1500 V 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY-3"/>
</gates>
<devices>
<device name="" package="691106800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691106800004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691106800004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691106800004 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135800003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZI (2) 
&lt;br&gt;VDE Approval 40021362 Type CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84010v209%20Family_WR-TBL1_6911358000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84010v209%20Family_WR-TBL1_6911358000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1358_VERTICAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358000xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1358_VERTICAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135800003.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135800003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135800003 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710010.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710010 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691106800001" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V 
&lt;br&gt;Withstanding Voltage 1500 V 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-5"/>
</gates>
<devices>
<device name="" package="691106800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691106800001.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691106800001 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691106800001 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710003B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710003B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700004B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700004B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700004B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700004B"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700004B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710009.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700009.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102810003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY-2"/>
</gates>
<devices>
<device name="" package="691102810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102810003.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102810003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691102810003 "/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700009.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691103810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1038 - 10.00 mm Horiz. Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o83521v209%20WR-TBL1_6911038100xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1038_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911038100x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691103810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691103810002.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691103810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691103810002 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700006 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691106800002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V 
&lt;br&gt;Withstanding Voltage 1500 V 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY-3"/>
</gates>
<devices>
<device name="" package="691106800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691106800002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691106800002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691106800002 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710004 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691106800101" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1068 - 10.00 mm Modular Vertical Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V 
&lt;br&gt;Withstanding Voltage 1500 V 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678620v209%20family-wr-tbl-6911068000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1068_10_00_MM_VERTICAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-6"/>
</gates>
<devices>
<device name="" package="691106800101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691106800101.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691106800101 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical Cable Entry"/>
<attribute name="VALUE" value=" 691106800101 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700003B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700003B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700003B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700003B"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700003B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700005 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910004 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800010.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800010 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102810101" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-4"/>
</gates>
<devices>
<device name="" package="691102810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102810101.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102810101 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691102810101 "/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710009.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691111710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 111 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 24 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33228v209%20WR-TBL_6911117100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33228v209%20WR-TBL_6911117100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_111_6911117100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_111_6911117100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691111710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691111710003.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691111710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691111710003 "/>
<attribute name="WIRE" value="24 to 14 (AWG) 0.205 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700008 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102810004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1028 - 10.00 mm Modular Horizontal Cable Entry - THT &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678615v209%20family-wr-tbl-6911028100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_WIRE_PROTECTOR_10_00_MM_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY-2"/>
</gates>
<devices>
<device name="" package="691102810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102810004.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102810004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691102810004 "/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 101 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 26 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.129 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33380v209%20Family_WR_TBL_691101710002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33380v209%20Family_WR_TBL_691101710002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_101_6911017100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_101_6911017100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691101710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101710003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691101710003 "/>
<attribute name="WIRE" value="26 to 14 (AWG) 0.129 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800003 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 101 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 26 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 26 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.129 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33380v209%20Family_WR_TBL_691101710002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33380v209%20Family_WR_TBL_691101710002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_101_6911017100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_101_6911017100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691101710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101710002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691101710002 "/>
<attribute name="WIRE" value="26 to 14 (AWG) 0.129 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710007.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710007 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800007.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710008B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710008B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910008 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710005.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710005 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32801v209%20Family_WR-TBL1_Series1357.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113571000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135710007.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135710007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691502710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5027 - 5.00 mm Horizontal Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA 9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58965v209%20691502710002_.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58965v209%20691502710002_.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_THT_5027_69150271000X"&gt;https://katalog.we-online.com/en/em/TBL_5_00_THT_5027_69150271000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691502710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691502710003.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691502710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691502710003 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691502710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 5027 - 5.00 mm Horizontal Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA 9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +130 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 15 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58965v209%20691502710002_.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58965v209%20691502710002_.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_THT_5027_69150271000X"&gt;https://katalog.we-online.com/en/em/TBL_5_00_THT_5027_69150271000X&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691502710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691502710002.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691502710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691502710002 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Horiz. Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZI (2) 
&lt;br&gt;VDE Approval 40021362 Type CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84012v209%20Family_WR-TBL1_6911358100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84012v209%20Family_WR-TBL1_6911358100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1358_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358100xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1358_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135810004.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135810004 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700010.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700010 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700010.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700010 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700005B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700005B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710008.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710008 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700008B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700008B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700008B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700008B"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700008B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 102 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;VDE Approval 40022612 Model number 102 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33225v209%20Family_WR-TBL_69110271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33225v209%20Family_WR-TBL_69110271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_102_6911027100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_102_6911027100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691102710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102710003.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691102710003 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800009.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800009 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm��) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810003 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Horiz. Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZI (2) 
&lt;br&gt;VDE Approval 40021362 Type CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84012v209%20Family_WR-TBL1_6911358100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84012v209%20Family_WR-TBL1_6911358100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1358_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358100xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1358_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135810003.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691135810003 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700006.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691102710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 102 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 15 A 
&lt;br&gt;IR VDE 17.5 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.6 
&lt;br&gt;Solid Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 22 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.326 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022612 
&lt;br&gt;VDE Approval 40022612 Model number 102 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33225v209%20Family_WR-TBL_69110271000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33225v209%20Family_WR-TBL_69110271000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_102_6911027100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_102_6911027100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691102710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691102710002.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="IR-VDE" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691102710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691102710002 "/>
<attribute name="WIRE" value="22 to 14 (AWG) 0.326 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700002B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700002B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691104800002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931;​ E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691104800002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691104800002.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691104800002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691104800002 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700007.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691132700003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1327 - 5.00 mm - Vertical Entry with Pressure Clamp divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58317v209%20Family_WR-TBL_Screw_PClamp_6911327000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1327_6911327000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691132700003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691132700003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691132700003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691132700003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810001" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810001.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810001 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810001 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710005B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710005B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710005B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710005B"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710005B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691134810101" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1348 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CMM (1) 
&lt;br&gt;VDE Approval 40021375 
&lt;br&gt;VDE Approval 40021375 TYPE: CMM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32800v209%20Family_WR-TBL1_Series1348.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1348_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113481000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691134810101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691134810101.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691134810101 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691134810101 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710005 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810006" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810006 "/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810006 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710006.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710006 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131810004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1318 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU (2) 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58322v209%20Family_WR-TBL_Screw_PressureClamp_6911318100xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1318_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113181000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131810004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131810004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131810004 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700005.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810004" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810004 "/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810004 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710010.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710010 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136800005" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58335v209%20Family_WR-TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911368000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136800005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136800005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136800005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136800005 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710004.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710004 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136700006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E315414 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40023402 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58330v209%20Family_WR-TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911367000XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136700006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136700006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136700006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691136700006 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691111710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 111 - 5.00 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 16 A 
&lt;br&gt;Working Voltage [cULus] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 24 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.205 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 24 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.205 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33228v209%20WR-TBL_6911117100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33228v209%20WR-TBL_6911117100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_111_6911117100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_111_6911117100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691111710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691111710002.pdf"/>
<attribute name="IR-UL" value="15A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691111710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691111710002 "/>
<attribute name="WIRE" value="24 to 14 (AWG) 0.205 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710009" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710009">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710009.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710009 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710009 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810005" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810005.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810005 "/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810005 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691126710002B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 126 B - 5.00 mm Horiz. Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33229v209%20Family_WR-TBL_6911267100xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_126B_6911267100XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691126710002B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691126710002B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691126710002B"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691126710002B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135700008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1357- 5.00 mm Vertical Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZI (2) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021362 TYPE: CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58326v209%20Family_WR-TBL_Screw_PressureClamp_6911357100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1357_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911357000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135700008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135700008.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135700008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135700008 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710008" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710008.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710008 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136710007" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1367- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021362 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58328v209%20Family_WR-TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1367_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911367100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136710007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136710007.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136710007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136710007 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133810002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1338 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58324v209%20Family_WR-TBL_Screw_PressureClamp_6911338100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58324v209%20Family_WR-TBL_Screw_PressureClamp_6911338100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1338_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113381000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1338_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113381000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133810002.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133810002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133810002 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133710004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1337- 5.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32968v209%20Family_WR-TBL_Series1337.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1337_6911337100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133710004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133710004.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133710004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133710004 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691135800004" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1358 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 Cat No. CZI (2) 
&lt;br&gt;VDE Approval 40021362 Type CZI 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84010v209%20Family_WR-TBL1_6911358000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84010v209%20Family_WR-TBL1_6911358000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1358_VERTICAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358000xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1358_VERTICAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911358000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691135800004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691135800004.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691135800004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691135800004 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691133810003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1338 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 18 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CBL (6) 
&lt;br&gt;VDE Approval 40021373 
&lt;br&gt;VDE Approval 40021373 TYPE: CBL 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58324v209%20Family_WR-TBL_Screw_PressureClamp_6911338100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58324v209%20Family_WR-TBL_Screw_PressureClamp_6911338100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1338_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113381000x"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1338_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113381000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691133810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691133810003.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691133810003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691133810003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691103110003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 3.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Copper over Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 10 A 
&lt;br&gt;Working Voltage [UL] 125 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1250 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 5 up to 6 (mm) 
&lt;br&gt;Screw M2 
&lt;br&gt;Solid Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.129 to 1.31 (mm²)  
&lt;br&gt;Stranded Wire Section (AWG) 26 to 16 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.129 to 1.31 (mm²)  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33226v209%20Family_WR-TBL_69110311000x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33226v209%20Family_WR-TBL_69110311000x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_3_50_1031_6911031100XX"&gt;https://katalog.we-online.com/en/em/TBL_3_50_1031_6911031100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-07&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691103110003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691103110003.pdf"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691103110003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691103110003 "/>
<attribute name="WIRE" value="26 to 16 (AWG) 0.129 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810002" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810002 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810002 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691101810003" prefix="J">
<description>&lt;b&gt;WR-TBL Series 1018 - 10.00 mm Modular Horizontal Cable Entry - THT&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Blue 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 16 A 
&lt;br&gt;Working Voltage [UL] 250 V 
&lt;br&gt;Working Voltage [VDE] 250 V 
&lt;br&gt;Withstanding Voltage [UL] 1500 V 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;VDE Approval 40022614 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o678601v209%20family-wr-tbl-6911018100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT"&gt;https://www.we-online.com/catalog/en/WR_TBL_SERIES_1018_10_MM_MODULAR_HORIZONTAL_THT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-04-07&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY-1"/>
</gates>
<devices>
<device name="" package="691101810003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691101810003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691101810003 "/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal Cable Entry"/>
<attribute name="VALUE" value=" 691101810003 "/>
<attribute name="WORKING-VOLTAGE-UL" value="250V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137710002" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 12 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 3.31 to 0.05 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84014v209%20Family_WR-TBL1_6911377100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1377_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_GLOW_WIRE_6911377100xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137710002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137710002.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137710002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137710002 "/>
<attribute name="WIRE" value="12 to 30 (AWG) 3.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691104800001" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1048 - 10.00 mm Vertical Entry w. Pressure Clamp Glow Wire&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel tin-plated surface 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy with Tin 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 14 A 
&lt;br&gt;IR VDE 13.5 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 14 to 30 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 2.08 to 0.0509 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931;​ E150931 Cat No. CZM (2) 
&lt;br&gt;VDE Approval 40021394 
&lt;br&gt;VDE Approval 40021394 Type CZM 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o84311v209%20Family_WR-TBL1_6911048000xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1048_VERTICAL_ENTRY_W_PRESSURE_CLAMP_6911048000xx&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PIN_ENTRY"/>
</gates>
<devices>
<device name="" package="691104800001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691104800001.pdf"/>
<attribute name="IR-UL" value="14A"/>
<attribute name="IR-VDE" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691104800001 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 691104800001 "/>
<attribute name="WIRE" value="14 to 30 (AWG) 2.08 to 0.0509 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691127700006B" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 127 B - 5.00 mm Vertical Entry w. stamping clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Steel over Zinc 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR cULus 20 A 
&lt;br&gt;Working Voltage [cULus] 300 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 2000 V (AC) 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 9 (mm) 
&lt;br&gt;Screw M4 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E315414 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58312v209%20Family_WR-TBL_Screw_PressureClamp_6911277000xxB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB"&gt;https://katalog.we-online.com/en/em/TBL_5_00_127B_6911277000XXB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691127700006B">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691127700006B.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="691127700006B"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="691127700006B"/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691137910006" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1379 - 7.50 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 7.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA6/66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3000 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: MRT12 (7) 
&lt;br&gt;VDE Approval 40021397 
&lt;br&gt;VDE Approval 40021397 TYPE: MRT12 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o32803v209%20Family_WR-TBL1_Series1379.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x"&gt;https://katalog.we-online.com/en/em/TBL_7_50_1379_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_69113791000x&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691137910006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691137910006.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691137910006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691137910006 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691131710003" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1317 - 5.00 mm Horizontal Entry with Pressure Clamp Divisible&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Zinc 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 22 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 450 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 2500 V (AC);​ 2000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 6 (mm) 
&lt;br&gt;Screw M2.5 
&lt;br&gt;Solid Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 12 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 3.31 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E150931 CAT N: CUU 
&lt;br&gt;VDE Approval 40021359 
&lt;br&gt;VDE Approval 40021359 TYPE: CUU 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58315v209%20Family_WR-TBL_Screw_PClamp_6911317100xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX"&gt;https://katalog.we-online.com/en/em/TBL_5_00_1317_6911317100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-08&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691131710003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691131710003.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="22A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691131710003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691131710003 "/>
<attribute name="WIRE" value="30 to 12 (AWG) 0.05 to 3.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="691136810010" prefix="J">
<description>&lt;b&gt;WR-TBL Serie 1368 - 10.00 mm Horizontal Cable Entry w. Pressure Clamp&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;
KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Pitch 10 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Nickel over Tin 
&lt;br&gt;Terminal Screw Material Steel 
&lt;br&gt;Terminal Screw Plating Zinc 
&lt;br&gt;Wire Guard Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;IR UL 16 A 
&lt;br&gt;IR VDE 24 A 
&lt;br&gt;Working Voltage [UL] 300 V (AC) 
&lt;br&gt;Working Voltage [VDE] 750 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1600 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;Contact Resistance [cULus] 20 mΩ 
&lt;br&gt;Contact Resistance [VDE] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Wire Strip Length 7 (mm) 
&lt;br&gt;Screw M3 
&lt;br&gt;Solid Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 30 to 14 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.05 to 2.08 (mm²) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;cULus Approval E150931 
&lt;br&gt;UL Approval E150931 CAT N: CZZ (1) 
&lt;br&gt;VDE Approval 40021377 
&lt;br&gt;VDE Approval 40021377 TYPE: CZZ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58333v209%20Family_WR-TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX"&gt;https://katalog.we-online.com/en/em/TBL_10_00_1368_HORIZONTAL_ENTRY_W_PRESSURE_CLAMP_6911368100XX&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PINS_ENTRY"/>
</gates>
<devices>
<device name="" package="691136810010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691136810010.pdf"/>
<attribute name="IR-UL" value="16A"/>
<attribute name="IR-VDE" value="24A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691136810010 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 691136810010 "/>
<attribute name="WIRE" value="30 to 14 (AWG) 0.05 to 2.08 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V(AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="750V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
