<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Coaxial Connectors - WR-UMRF&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-06-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="636101111001">
<description>&lt;B&gt;WR-UMRF PCB Receptacle SMT with 3 Pads
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;SMT, 3pins</description>
</package>
<package name="636101112001">
<description>&lt;B&gt;WR-UMRF PCB Receptacle SMT with 3 Pads</description>
</package>
</packages>
<symbols>
<symbol name="PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="636101111001" prefix="J">
<description>&lt;b&gt; WR-UMRF PCB Receptacle SMT with 3 Pads&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Natural 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +90 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;f DC~6 GHz
&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.we-online.com/components/media/o325314v209%20Single_WR-UMRF_63610111x001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o325314v209%20Single_WR-UMRF_63610111x001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PCB_RECECTACLE_SMT_WITH_3_PADS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/PCB_RECECTACLE_SMT_WITH_3_PADS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-06-16&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="636101111001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/636101111001?ae"/>
<attribute name="GENDER" value="PCB Receptacle"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="636101111001"/>
<attribute name="VALUE" value="636101111001"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="636101112001" prefix="J">
<description>&lt;b&gt; WR-UMRF PCB Receptacle SMT with 3 Pads&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Natural 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +90 °C 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o325314v209%20Single_WR-UMRF_63610111x001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o325314v209%20Single_WR-UMRF_63610111x001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/PCB_RECECTACLE_SMT_WITH_3_PADS"&gt;https://www.we-online.com/katalog/en/PCB_RECECTACLE_SMT_WITH_3_PADS&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-07-20&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="636101112001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/636101112001?ae"/>
<attribute name="GENDER" value="PCB Receptacle"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="636101112001"/>
<attribute name="VALUE" value="636101112001"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
