<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-USB&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-01-15&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="632722200212">
<description>&lt;b&gt;WR-COM USB 3.1 Type C Receptacle Horizontal High-Rise SMT 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; SMT, 24pins</description>
</package>
<package name="629105150921">
<description>&lt;b&gt;WR-COM Micro USB 2.0 Type AB Horizontal
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Micro USB 2.0, SMT, 5pins</description>
</package>
<package name="62900416021">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt;USB 2.0 SMT Type A Horizontal , 4 pins</description>
</package>
<package name="614004185023">
<description>&lt;b&gt;WR-COM &lt;/b&gt;&lt;br&gt;USB 2.0 Type A Vertical Short Type THT</description>
</package>
<package name="61400416121">
<description>WR-COM Horizontal USB Type B</description>
</package>
<package name="629104151021">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type A Horizontal SMT with pegs</description>
</package>
<package name="692122030100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;BR&gt; USB 3.0 Type A Horizontal SMD</description>
</package>
<package name="632723130112">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 3.1 Type C Receptacle Horizontal Mid-Mount THR / SMT 1.6 mm</description>
</package>
<package name="61400826021">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type A Horizontal Dual Stacked</description>
</package>
<package name="629104190121">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 2.0 Type A Horizontal SMT Short Type</description>
</package>
<package name="614105150721">
<description>&lt;B&gt;WR-COM Micro USB 2.0 Type B Vertical 5 Contacts
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;THT, 5 pins</description>
</package>
<package name="692221030100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;br&gt; USB 3.0 Type B Horizontal</description>
</package>
<package name="61410416121R">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type B Horizontal THR ,4Pins</description>
</package>
<package name="614004134726">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 2.0 Type A Up Right , 4 pins</description>
</package>
<package name="692112030100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;BR&gt; USB 3.0 Type A SMT Plug with Clip</description>
</package>
<package name="692121430000">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 3.0 Type A Vertical THT</description>
</package>
<package name="692141030100">
<description>&lt;B&gt;WR-COM &lt;/B&gt; &lt;BR&gt;USB 3.0 STACKED TYPE A</description>
</package>
<package name="692622030100">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;br&gt;Micro USB 3.0 Type B Horizontal SMT</description>
</package>
<package name="632722110112">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;BR&gt;USB 3.1 Type C Receptacle Vertical SMT 1.0 mm</description>
</package>
<package name="614104150121">
<description>&lt;b&gt;WR-COM&lt;/b&gt; &lt;br&gt;USB 2.0 THT Type A Horizontal Slim Type ,4Pins</description>
</package>
<package name="692121030100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;BR&gt; USB 3.0 HORIZONTAL TYPE A</description>
</package>
<package name="61400416021">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type A Horizontal</description>
</package>
<package name="614004190021">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt;USB 2.0 Type A Horizontal THT</description>
</package>
<package name="629004113921">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; 2.0 Plug Type A SMT w. Clip</description>
</package>
<package name="65100516121">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; Mini USB 2.0 Type B SMT Horizontal 5 Contacts</description>
</package>
<package name="614008235023">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type A Vertical Dual</description>
</package>
<package name="692121330100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;br&gt; USB 3.0 Type A Reverse Horizontal w. Offset 1.75 mm</description>
</package>
<package name="651005136421">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt;Mini USB 2.0 Type B Vertical 5 Contacts , 5 pins</description>
</package>
<package name="614104135023R">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 2.0 Type A Vertical THR</description>
</package>
<package name="629722000214">
</package>
<package name="632712000112">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 3.1 Type C Plug Horizontal 0.8 mm</description>
</package>
<package name="651305142821">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; Mini USB 2.0 Type AB SMT Horizontal 5 Contacts</description>
</package>
<package name="614104190121">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt;USB 2.0 Type A Horizontal THT Short Type ,4Pins</description>
</package>
<package name="61400413321">
<description>&lt;B&gt;WR-COM USB 2.0 Type B Vertical
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;THT, 4 pins</description>
</package>
<package name="632723300011">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 3.1 Type C Receptacle Horizontal THT / SMT</description>
</package>
<package name="629105136821">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; Micro USB 2.0 SMT Type B Horizontal 5 Contacts</description>
</package>
<package name="692622420101">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; Micro USB 3.0 Type B Vertical SMT</description>
</package>
<package name="629105150521">
<description>&lt;B&gt;WR-COM&lt;/b&gt;&lt;BR&gt;Type B with Pegs, High Current at Pin 1 &amp; Pin 5 Micro USB 2.0 SMT Type B Horizontal 5 Contacts High Current</description>
</package>
<package name="614108646521">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt;Type A Horizontal THR Dual Mid-Mount,8Pins</description>
</package>
<package name="692121130100">
<description>&lt;B&gt;WR-COM &lt;/B&gt;&lt;br&gt;USB 3.0 Type A Reverse Horizontal w. Offset 0.14 mm</description>
</package>
<package name="61410416021R">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type A Horizontal THR</description>
</package>
<package name="692121230100">
<description>&lt;B&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 3.0 Type A Horizontal w. Offset 1.04 mm</description>
</package>
<package name="62910416121">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 2.0 Type B SMT Horizontal , 4 pins</description>
</package>
<package name="632722100213">
</package>
<package name="614105150621">
<description>&lt;b&gt;WR-COM&lt;/B&gt;&lt;BR&gt; Micro USB 2.0 Type AB Vertical 5 Contacts</description>
</package>
<package name="614004184726">
<description>&lt;b&gt;WR-COM USB 2.0 Type A Up Right THT</description>
</package>
<package name="632712000011">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 3.1 Type C Plug Horizontal SMT 0.8 mm</description>
</package>
<package name="632722200211">
<description>&lt;b&gt;WR-COM USB 3.1 Type C Receptacle Horizontal SMT</description>
</package>
<package name="632121300001">
<description>&lt;b&gt;WR-COM&lt;/b&gt;&lt;br&gt; USB 3.1 Type A Receptacle Horizontal THT Power Delivery</description>
</package>
<package name="614004135023">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt; USB 2.0 Type A Vertical</description>
</package>
<package name="632723100011">
<description>&lt;B&gt;WR-COM&lt;/B&gt;&lt;BR&gt;USB 3.1 Type C Receptacle Horizontal THT / SMT</description>
</package>
<package name="629712010214">
</package>
</packages>
<symbols>
<symbol name="USB2.0_TYPEB">
<description>USB 2.0 TYPE B</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="SSTXP1" direction="pas"/>
<pin name="SSTXN1" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC" direction="pas"/>
<pin name="DP1" direction="pas"/>
<pin name="DN1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="SSRXN2" direction="pas"/>
<pin name="SSRXP2" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="SSRXP1" direction="pas"/>
<pin name="SSRXN1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="VCONN" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="SSTXN2" direction="pas"/>
<pin name="SSTXP2" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="DP2" direction="pas"/>
<pin name="DN2" direction="pas"/>
</symbol>
<symbol name="USB2.0_MICRO_TYPEB">
<description>Micro USB 2.0 Type B</description>
<pin name="GND" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEA">
<description>USB 2.0 Type A</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3_TYPEA">
<description>USB 3.0 Type A</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDA_SSRX-" direction="pas"/>
<pin name="STDA_SSRX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDA_SSTX-" direction="pas"/>
<pin name="STDA_SSTX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632722200212">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="TX1+" direction="pas"/>
<pin name="TX1-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="RX2-" direction="pas"/>
<pin name="RX2+" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="RX1+" direction="pas"/>
<pin name="RX1-" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="TX2-" direction="pas"/>
<pin name="TX2+" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="D+2" direction="pas"/>
<pin name="D-2" direction="pas"/>
</symbol>
<symbol name="USB3_TYPEB">
<description>USB 3.0 Type B</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDB_SSTX-" direction="pas"/>
<pin name="STDB_SSTX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDB_SSRX-" direction="pas"/>
<pin name="STDB_SSRX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3_MICRO_TYPEB">
<description>Micro USB 3.0 Type B</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="MICB_SSTX-" direction="pas"/>
<pin name="MICB_SSTX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="MICB_SSRX-" direction="pas"/>
<pin name="MICB_SSRX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_PLUG_TYPEA">
<description>USB2.0_PLUG_TYPEA</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEC">
<description>USB 2.0 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="D-2" direction="pas"/>
<pin name="D+2" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_6PINS">
<description>USB 3.1 Type C</description>
<pin name="CC1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632722200211">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="TX1+" direction="pas"/>
<pin name="TX1-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="RX2-" direction="pas"/>
<pin name="RX2+" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="RX1+" direction="pas"/>
<pin name="RX1-" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="TX2-" direction="pas"/>
<pin name="TX2+" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="D+2" direction="pas"/>
<pin name="D-2" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632712000011">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="SSTXP1" direction="pas"/>
<pin name="SSTXN1" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC" direction="pas"/>
<pin name="DP1" direction="pas"/>
<pin name="DN1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="SSRXN2" direction="pas"/>
<pin name="SSRXP2" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SSRXP1" direction="pas"/>
<pin name="SSRXN1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="VCONN" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="SSTXN2" direction="pas"/>
<pin name="SSTXP2" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEA">
<description>USB 3.1 Type A</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDA_SSRX-" direction="pas"/>
<pin name="STDA_SSRX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDA_SSTX-" direction="pas"/>
<pin name="STDA_SSTX+" direction="pas"/>
<pin name="PDDETECT" direction="pas"/>
<pin name="INSERTIONDETECT" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="632722200212" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632722200212"/>
</gates>
<devices>
<device name="" package="632722200212">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="RX1+" pad="B11"/>
<connect gate="G$1" pin="RX1-" pad="B10"/>
<connect gate="G$1" pin="RX2+" pad="A11"/>
<connect gate="G$1" pin="RX2-" pad="A10"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2" route="any"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4" route="any"/>
<connect gate="G$1" pin="TX1+" pad="A2"/>
<connect gate="G$1" pin="TX1-" pad="A3"/>
<connect gate="G$1" pin="TX2+" pad="B2"/>
<connect gate="G$1" pin="TX2-" pad="B3"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.2 Gen 1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632722200212?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722200212"/>
<attribute name="PCB-THICKNESS" value="1.2mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632722200212"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105150921" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105150921">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629105150921?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105150921"/>
<attribute name="PCB-THICKNESS" value="1.2mm"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629105150921"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004185023" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella,Wu 2020-03-24&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004185023">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614004185023?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004185023"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Vertical - Short Type"/>
<attribute name="VALUE" value="614004185023"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62900416021" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-15&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="62900416021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62900416021?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="62900416021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62900416021"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400416121" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61400416121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61400416121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400416121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="61400416121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629104151021" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-09-04&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="629104151021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629104151021?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629104151021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629104151021"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692122030100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692122030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692122030100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692122030100"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692122030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723130112" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723130112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632723130112?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723130112"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632723130112"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400826021" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61400826021">
<connects>
<connect gate="USBA" pin="D+" pad="3"/>
<connect gate="USBA" pin="D-" pad="2"/>
<connect gate="USBA" pin="GND" pad="4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBA" pin="VBUS" pad="1"/>
<connect gate="USBB" pin="D+" pad="7"/>
<connect gate="USBB" pin="D-" pad="6"/>
<connect gate="USBB" pin="GND" pad="8"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61400826021?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400826021"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="VALUE" value="61400826021"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629104190121" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-08-05&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="629104190121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629104190121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="629104190121"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="VALUE" value="629104190121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692221030100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Yingchun, Shan 2020-01-17&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEB"/>
</gates>
<devices>
<device name="" package="692221030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDB_SSRX+" pad="9"/>
<connect gate="G$1" pin="STDB_SSRX-" pad="8"/>
<connect gate="G$1" pin="STDB_SSTX+" pad="6"/>
<connect gate="G$1" pin="STDB_SSTX-" pad="5"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692221030100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692221030100"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692221030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614105150721" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="614105150721">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614105150721?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614105150721"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="614105150721"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004134726" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004134726">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614004134726?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004134726"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Up Right"/>
<attribute name="VALUE" value="614004134726"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692112030100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692112030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692112030100?ae"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692112030100"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692112030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61410416121R" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-08-17&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61410416121R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61410416121R?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="61410416121R"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="61410416121R"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121430000" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121430000">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692121430000?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692121430000"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="692121430000"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692622030100" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;
Updated by Yingchun, Shan 2020-01-17&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="692622030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND_DRAIN" pad="8"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="MICB_SSRX+" pad="10"/>
<connect gate="G$1" pin="MICB_SSRX-" pad="9"/>
<connect gate="G$1" pin="MICB_SSTX+" pad="7"/>
<connect gate="G$1" pin="MICB_SSTX-" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692622030100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692622030100"/>
<attribute name="PINS" value="10pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692622030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692141030100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB3_TYPEA"/>
<gate name="USBB" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692141030100">
<connects>
<connect gate="USBA" pin="D+" pad="3"/>
<connect gate="USBA" pin="D-" pad="2"/>
<connect gate="USBA" pin="GND" pad="4"/>
<connect gate="USBA" pin="GND_DRAIN" pad="7"/>
<connect gate="USBA" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBA" pin="STDA_SSRX+" pad="6"/>
<connect gate="USBA" pin="STDA_SSRX-" pad="5"/>
<connect gate="USBA" pin="STDA_SSTX+" pad="9"/>
<connect gate="USBA" pin="STDA_SSTX-" pad="8"/>
<connect gate="USBA" pin="VBUS" pad="1"/>
<connect gate="USBB" pin="D+" pad="12"/>
<connect gate="USBB" pin="D-" pad="11"/>
<connect gate="USBB" pin="GND" pad="13"/>
<connect gate="USBB" pin="GND_DRAIN" pad="16"/>
<connect gate="USBB" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBB" pin="STDA_SSRX+" pad="15"/>
<connect gate="USBB" pin="STDA_SSRX-" pad="14"/>
<connect gate="USBB" pin="STDA_SSTX+" pad="18"/>
<connect gate="USBB" pin="STDA_SSTX-" pad="17"/>
<connect gate="USBB" pin="VBUS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692141030100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692141030100"/>
<attribute name="PINS" value="18pcs"/>
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="VALUE" value="692141030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722110112" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632722110112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632722110112?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722110112"/>
<attribute name="PCB-THICKNESS" value="1.2mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="632722110112"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614104150121" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-15&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104150121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614104150121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="614104150121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="VALUE" value="614104150121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121030100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692121030100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121030100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692121030100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400416021" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61400416021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61400416021?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400416021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="61400416021"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="65100516121" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="65100516121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/65100516121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="65100516121"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="65100516121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004190021" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004190021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614004190021?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004190021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="614004190021"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614008235023" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614008235023">
<connects>
<connect gate="USBA" pin="D+" pad="A3"/>
<connect gate="USBA" pin="D-" pad="A2"/>
<connect gate="USBA" pin="GND" pad="A4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBA" pin="VBUS" pad="A1"/>
<connect gate="USBB" pin="D+" pad="B3"/>
<connect gate="USBB" pin="D-" pad="B2"/>
<connect gate="USBB" pin="GND" pad="B4"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614008235023?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614008235023"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="TYPE" value="Stacked Vertical"/>
<attribute name="VALUE" value="614008235023"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121330100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-01-17&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121330100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692121330100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121330100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Reverse Horizontal"/>
<attribute name="VALUE" value="692121330100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="651005136421" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="651005136421">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/651005136421?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="651005136421"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="651005136421"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629004113921" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_PLUG_TYPEA"/>
</gates>
<devices>
<device name="" package="629004113921">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629004113921?ae"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="629004113921"/>
<attribute name="PCB-THICKNESS" value="1.2mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629004113921"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614104135023R" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104135023R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614104135023R?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614104135023R"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="614104135023R"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632712000112" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632712000112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632712000112?ae"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="632712000112"/>
<attribute name="PCB-THICKNESS" value="0.8mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632712000112"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629722000214" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC"/>
</gates>
<devices>
<device name="" package="629722000214">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="GND3" pad="B1"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
<connect gate="G$1" pin="VBUS3" pad="B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629722000214?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629722000214"/>
<attribute name="PCB-THICKNESS" value="0.8mm"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629722000214"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="651305142821" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="651305142821">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/651305142821?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="651305142821"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="651305142821"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614104190121" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104190121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614104190121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="614104190121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="VALUE" value="614104190121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400413321" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61400413321">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61400413321?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400413321"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61400413321"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105136821" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105136821">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629105136821?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105136821"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629105136821"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723300011" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723300011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="GND GND1"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632723300011?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723300011"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632723300011"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692622420101" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-12-28&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="692622420101">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND_DRAIN" pad="8"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="MICB_SSRX+" pad="10"/>
<connect gate="G$1" pin="MICB_SSRX-" pad="9"/>
<connect gate="G$1" pin="MICB_SSTX+" pad="7"/>
<connect gate="G$1" pin="MICB_SSTX-" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692622420101?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="692622420101"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="10pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="692622420101"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105150521" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105150521">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629105150521?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105150521"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="629105150521"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614108646521" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2020-12-28&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614108646521">
<connects>
<connect gate="USBA" pin="D+" pad="3"/>
<connect gate="USBA" pin="D-" pad="2"/>
<connect gate="USBA" pin="GND" pad="4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBA" pin="VBUS" pad="1"/>
<connect gate="USBB" pin="D+" pad="7"/>
<connect gate="USBB" pin="D-" pad="6"/>
<connect gate="USBB" pin="GND" pad="8"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614108646521?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614108646521"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="VALUE" value="614108646521"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121130100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121130100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692121130100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121130100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Reverse Horizontal"/>
<attribute name="VALUE" value="692121130100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61410416021R" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-01-30&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61410416021R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61410416021R?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="61410416021R"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="61410416021R"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121230100" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121230100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/692121230100?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121230100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="692121230100"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722100213" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_6PINS"/>
</gates>
<devices>
<device name="" package="632722100213">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB Power Delivery"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632722100213?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722100213"/>
<attribute name="PCB-THICKNESS" value="1mm"/>
<attribute name="PINS" value="6pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632722100213"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62910416121" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-08-17&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="62910416121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62910416121?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="62910416121"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62910416121"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614105150621" prefix="J">
<description>&lt;B&gt;WR-USB Mini/Micro Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mini and Micro form factors, ideal for space-constrained designs
&lt;BR&gt;Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
&lt;BR&gt;Designed for high cycle durability
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile and handheld devices
&lt;BR&gt;Wearables and portable accessories
&lt;BR&gt;Embedded systems and IoT modules
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32880v209%20Family%20USB%202%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_MINI_MICRO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_MINI_MICRO&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-16&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="614105150621">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614105150621?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1.8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614105150621"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="614105150621"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004184726" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-20&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004184726">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614004184726?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004184726"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Up Right - Short Type"/>
<attribute name="VALUE" value="614004184726"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632712000011" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632712000011"/>
</gates>
<devices>
<device name="" package="632712000011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632712000011?ae"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="632712000011"/>
<attribute name="PCB-THICKNESS" value="0.8mm"/>
<attribute name="PINS" value="22pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632712000011"/>
<attribute name="WORKING-VOLTAGE" value="20VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722200211" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632722200211"/>
</gates>
<devices>
<device name="" package="632722200211">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="RX1+" pad="B11"/>
<connect gate="G$1" pin="RX1-" pad="B10"/>
<connect gate="G$1" pin="RX2+" pad="A11"/>
<connect gate="G$1" pin="RX2-" pad="A10"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="TX1+" pad="A2"/>
<connect gate="G$1" pin="TX1-" pad="A3"/>
<connect gate="G$1" pin="TX2+" pad="B2"/>
<connect gate="G$1" pin="TX2-" pad="B3"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.2 Gen 1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632722200211?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722200211"/>
<attribute name="PCB-THICKNESS" value="0.6mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632722200211"/>
<attribute name="WORKING-VOLTAGE" value="20VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632121300001" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-09-28&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEA"/>
</gates>
<devices>
<device name="" package="632121300001">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="INSERTIONDETECT" pad="11"/>
<connect gate="G$1" pin="PDDETECT" pad="10"/>
<connect gate="G$1" pin="SHIELD" pad="12 13 S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632121300001?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="632121300001"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632121300001"/>
<attribute name="WORKING-VOLTAGE" value="20VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004135023" prefix="J">
<description>&lt;B&gt;WR-USB Standard Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Widely used Type-A and Type-B connectors, available in different orientation
&lt;BR&gt;Various mount types: SMT, THT, THR
&lt;BR&gt;Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
&lt;BR&gt;Durable and backward compatible with older USB versions
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Office and desktop computing systems
&lt;BR&gt;Industrial control and automation equipment
&lt;BR&gt;Consumer electronics and peripherals
&lt;BR&gt;Audio-visual and broadcast systems
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870535v209%20Family%20USB%201%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_STANDARD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_STANDARD&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-15&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004135023">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/614004135023?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004135023"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="614004135023"/>
<attribute name="WORKING-VOLTAGE" value="30VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629712010214" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC"/>
</gates>
<devices>
<device name="" package="629712010214">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="GND3" pad="B1"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
<connect gate="G$1" pin="VBUS3" pad="B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/629712010214?ae"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629712010214"/>
<attribute name="PCB-THICKNESS" value="0.8mm"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="629712010214"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723100011" prefix="J">
<description>&lt;B&gt;WR-USB Type C Connectors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
&lt;BR&gt;Aligned with Power Delivery up to 240W
&lt;BR&gt;High durability (10 000 cycles)
&lt;BR&gt;UL, TID listing for USB standards
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Mobile computing and smart devices
&lt;BR&gt;High-performance industrial and medical systems
&lt;BR&gt;Consumer electronics and multimedia hubs
&lt;BR&gt;Smart buildings
&lt;BR&gt;&lt;BR&gt;


&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870537v209%20Family%20USB%203%20psd.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/INPUT_OUTPUT_WR_USB_TYPE_C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/INPUT_OUTPUT_WR_USB_TYPE_C&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-01-15&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723100011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="GND GND1"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/632723100011?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723100011"/>
<attribute name="PCB-THICKNESS" value="1mm"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="632723100011"/>
<attribute name="WORKING-VOLTAGE" value="48VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
