<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-USB Connectors

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-03
Copyright: Würth Elektronik</description>
<packages>
<package name="614104150121">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal - Short Type
THT, 4Pins</description>
</package>
<package name="692622030100">
<description>WR-USB Mini/Micro Connectors
Micro USB 3.0, Type B, Horizontal
SMT, 10Pins</description>
</package>
<package name="614008235023">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Stacked Vertical
THT, 8Pins</description>
</package>
<package name="692121430000">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Vertical
THT, 9Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="614104135023R">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Vertical
THR, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="61400826021">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Stacked Horizontal
THT, 8Pins</description>
</package>
<package name="692112030100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Horizontal
SMT, 9Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="61400416021">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
THT, 4Pins</description>
</package>
<package name="651005136421">
<description>WR-USB Mini/Micro Connectors
Mini USB 2.0, Type B, Vertical
THT, 5Pins</description>
</package>
<package name="632722200212">
<description>WR-USB Type C Connectors
USB 3.2 Gen 1, Type C, Horizontal
SMT, 24Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="632712000112">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Horizontal
SMT, 24Pins, PCB Thickness:0.8 mm</description>
</package>
<package name="614004134726">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Up Right
THT, 4Pins</description>
</package>
<package name="614004185023">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Vertical - Short Type
THT, 4Pins</description>
</package>
<package name="629105150921">
<description>WR-USB Mini/Micro Connectors
Micro USB 2.0, Type AB, Horizontal
SMT, 5Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="629004113921">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
SMT, 4Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="62900416021">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
SMT, 4Pins</description>
</package>
<package name="692122030100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Horizontal
SMT, 9Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="629722050114">
<description>WR-USB Type C Connectors
USB 2.0, Type C, Vertical
SMT, 16Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="61410416121R">
<description>WR-USB Standard Connectors
USB 2.0, Type B, Horizontal
THR, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="614104190121">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal - Short Type
THT, 4Pins</description>
</package>
<package name="692141030100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Stacked Horizontal
THT, 18Pins</description>
</package>
<package name="692221030100">
<description>WR-USB Standard Connectors
USB 3.0, Type B, Horizontal
THT, 9Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="692121330100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Reverse Horizontal
THR, 9Pins</description>
</package>
<package name="629104190121">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal - Short Type
SMT, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="692121030100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Horizontal
THT, 9Pins</description>
</package>
<package name="614004190021">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
THT, 4Pins</description>
</package>
<package name="651305142821">
<description>WR-USB Mini/Micro Connectors
Mini USB 2.0, Type AB, Horizontal
SMT, 5Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="614108646521">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Stacked Horizontal
THR, 8Pins</description>
</package>
<package name="632723130112">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Horizontal
THR, 24Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="632723300011">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Horizontal
THR, 24Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="614105150721">
<description>WR-USB Mini/Micro Connectors
Micro USB 2.0, Type B, Vertical
THT, 5Pins</description>
</package>
<package name="692622420101">
<description>WR-USB Mini/Micro Connectors
Micro USB 3.0, Type B, Vertical
SMT, 10Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="632722110112">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Vertical
SMT, 24Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="629104151021">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
SMT, 4Pins</description>
</package>
<package name="61400413321">
<description>WR-USB Standard Connectors
USB 2.0, Type B, Vertical
THT, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="629105150521">
<description>WR-USB Mini/Micro Connectors
Micro USB 2.0, Type B, Horizontal
SMT, 5Pins</description>
</package>
<package name="614105150621">
<description>WR-USB Mini/Micro Connectors
Micro USB 2.0, Type AB, Vertical
THT, 5Pins</description>
</package>
<package name="629722010114">
<description>WR-USB Type C Connectors
USB 2.0, Type C, Vertical
SMT, 16Pins, PCB Thickness:1.2 mm</description>
</package>
<package name="629722000214">
<description>WR-USB Type C Connectors
USB 2.0, Type C, Horizontal
SMT, 16Pins, PCB Thickness:0.8 mm</description>
</package>
<package name="629105136821">
<description>WR-USB Mini/Micro Connectors
Micro USB 2.0, Type B, Horizontal
SMT, 5Pins</description>
</package>
<package name="692121130100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Reverse Horizontal
THR, 9Pins</description>
</package>
<package name="61410416021R">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Horizontal
THR, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="632121300001">
<description>WR-USB Standard Connectors
USB 3.1, Type A, Horizontal
THR, 9Pins</description>
</package>
<package name="62910416121">
<description>WR-USB Standard Connectors
USB 2.0, Type B, Horizontal
SMT, 4Pins, PCB Thickness:1.6 mm</description>
</package>
<package name="629722330214">
<description>WR-USB Type C Connectors
USB 2.0, Type C, Horizontal
SMT, 16Pins, PCB Thickness:0.8 mm</description>
</package>
<package name="65100516121">
<description>WR-USB Mini/Micro Connectors
Mini USB 2.0, Type B, Horizontal
SMT, 5Pins</description>
</package>
<package name="692121230100">
<description>WR-USB Standard Connectors
USB 3.0, Type A, Horizontal
THR, 9Pins</description>
</package>
<package name="629712010214">
<description>WR-USB Type C Connectors
USB 2.0, Type C, Vertical
SMT, 16Pins, PCB Thickness:0.8 mm</description>
</package>
<package name="614004135023">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Vertical
THT, 4Pins</description>
</package>
<package name="632712000011">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Horizontal
SMT, 22Pins, PCB Thickness:0.8 mm</description>
</package>
<package name="632722100213">
<description>WR-USB Type C Connectors
USB Power Delivery, Type C, Horizontal
SMT, 6Pins, PCB Thickness:1 mm</description>
</package>
<package name="61400416121">
<description>WR-USB Standard Connectors
USB 2.0, Type B, Horizontal
THT, 4Pins</description>
</package>
<package name="614004184726">
<description>WR-USB Standard Connectors
USB 2.0, Type A, Up Right - Short Type
THT, 4Pins</description>
</package>
<package name="632722200211">
<description>WR-USB Type C Connectors
USB 3.2 Gen 1, Type C, Horizontal
SMT, 24Pins, PCB Thickness:0.6 mm</description>
</package>
<package name="632723100011">
<description>WR-USB Type C Connectors
USB 3.1, Type C, Horizontal
THR, 24Pins, PCB Thickness:1 mm</description>
</package>
</packages>
<symbols>
<symbol name="USB2.0_TYPEA">
<description>USB 2.0 Type A</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3_MICRO_TYPEB">
<description>Micro USB 3.0 Type B</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="MICB_SSTX-" direction="pas"/>
<pin name="MICB_SSTX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="MICB_SSRX-" direction="pas"/>
<pin name="MICB_SSRX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3_TYPEA">
<description>USB 3.0 Type A</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDA_SSRX-" direction="pas"/>
<pin name="STDA_SSRX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDA_SSTX-" direction="pas"/>
<pin name="STDA_SSTX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_MICRO_TYPEB">
<description>Micro USB 2.0 Type B</description>
<pin name="GND" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632722200212">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="TX1+" direction="pas"/>
<pin name="TX1-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="RX2-" direction="pas"/>
<pin name="RX2+" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="RX1+" direction="pas"/>
<pin name="RX1-" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="TX2-" direction="pas"/>
<pin name="TX2+" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="D+2" direction="pas"/>
<pin name="D-2" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="SSTXP1" direction="pas"/>
<pin name="SSTXN1" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC" direction="pas"/>
<pin name="DP1" direction="pas"/>
<pin name="DN1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="SSRXN2" direction="pas"/>
<pin name="SSRXP2" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="SSRXP1" direction="pas"/>
<pin name="SSRXN1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="VCONN" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="SSTXN2" direction="pas"/>
<pin name="SSTXP2" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="DP2" direction="pas"/>
<pin name="DN2" direction="pas"/>
</symbol>
<symbol name="USB2.0_PLUG_TYPEA">
<description>USB2.0_PLUG_TYPEA</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEC_1-1">
<description>USB 2.0 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="D-2" direction="pas"/>
<pin name="D+2" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEB">
<description>USB 2.0 TYPE B</description>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB3_TYPEB">
<description>USB 3.0 Type B</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDB_SSTX-" direction="pas"/>
<pin name="STDB_SSTX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDB_SSRX-" direction="pas"/>
<pin name="STDB_SSRX+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEC_1">
<description>USB 2.0 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="D-2" direction="pas"/>
<pin name="D+2" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEC">
<description>USB 2.0 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="D-2" direction="pas"/>
<pin name="D+2" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEA">
<description>USB 3.1 Type A</description>
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="STDA_SSRX-" direction="pas"/>
<pin name="STDA_SSRX+" direction="pas"/>
<pin name="GND_DRAIN" direction="pas"/>
<pin name="STDA_SSTX-" direction="pas"/>
<pin name="STDA_SSTX+" direction="pas"/>
<pin name="PDDETECT" direction="pas"/>
<pin name="INSERTIONDETECT" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="USB2.0_TYPEC-1">
<description>USB 2.0 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="D-2" direction="pas"/>
<pin name="D+2" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632712000011">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="SSTXP1" direction="pas"/>
<pin name="SSTXN1" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC" direction="pas"/>
<pin name="DP1" direction="pas"/>
<pin name="DN1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="SSRXN2" direction="pas"/>
<pin name="SSRXP2" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SSRXP1" direction="pas"/>
<pin name="SSRXN1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="VCONN" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="SSTXN2" direction="pas"/>
<pin name="SSTXP2" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_6PINS">
<description>USB 3.1 Type C</description>
<pin name="CC1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
</symbol>
<symbol name="USB3.1_TYPEC_632722200211">
<description>USB 3.1 Type C</description>
<pin name="GND" direction="pas"/>
<pin name="TX1+" direction="pas"/>
<pin name="TX1-" direction="pas"/>
<pin name="VBUS" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D+1" direction="pas"/>
<pin name="D-1" direction="pas"/>
<pin name="SBU1" direction="pas"/>
<pin name="VBUS1" direction="pas"/>
<pin name="RX2-" direction="pas"/>
<pin name="RX2+" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="RX1+" direction="pas"/>
<pin name="RX1-" direction="pas"/>
<pin name="VBUS2" direction="pas"/>
<pin name="SBU2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="VBUS3" direction="pas"/>
<pin name="TX2-" direction="pas"/>
<pin name="TX2+" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="D+2" direction="pas"/>
<pin name="D-2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="614104150121" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104150121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="614104150121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614104150121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614104150121?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692622030100" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="692622030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND_DRAIN" pad="8"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="MICB_SSRX+" pad="10"/>
<connect gate="G$1" pin="MICB_SSRX-" pad="9"/>
<connect gate="G$1" pin="MICB_SSTX+" pad="7"/>
<connect gate="G$1" pin="MICB_SSTX-" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Micro USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692622030100"/>
<attribute name="PINS" value="10pcs"/>
<attribute name="VALUE" value="692622030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692622030100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614008235023" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614008235023">
<connects>
<connect gate="USBA" pin="D+" pad="A3"/>
<connect gate="USBA" pin="D-" pad="A2"/>
<connect gate="USBA" pin="GND" pad="A4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBA" pin="VBUS" pad="A1"/>
<connect gate="USBB" pin="D+" pad="B3"/>
<connect gate="USBB" pin="D-" pad="B2"/>
<connect gate="USBB" pin="GND" pad="B4"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Stacked Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614008235023"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="VALUE" value="614008235023"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614008235023?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121430000" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121430000">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692121430000"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692121430000"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692121430000?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614104135023R" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104135023R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614104135023R"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614104135023R"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614104135023R?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400826021" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61400826021">
<connects>
<connect gate="USBA" pin="D+" pad="3"/>
<connect gate="USBA" pin="D-" pad="2"/>
<connect gate="USBA" pin="GND" pad="4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBA" pin="VBUS" pad="1"/>
<connect gate="USBB" pin="D+" pad="7"/>
<connect gate="USBB" pin="D-" pad="6"/>
<connect gate="USBB" pin="GND" pad="8"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400826021"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="VALUE" value="61400826021"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61400826021?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692112030100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692112030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692112030100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692112030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692112030100?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400416021" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61400416021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400416021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="61400416021"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61400416021?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="651005136421" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="651005136421">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="651005136421"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="651005136421"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/651005136421?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722200212" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632722200212"/>
</gates>
<devices>
<device name="" package="632722200212">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="RX1+" pad="B11"/>
<connect gate="G$1" pin="RX1-" pad="B10"/>
<connect gate="G$1" pin="RX2+" pad="A11"/>
<connect gate="G$1" pin="RX2-" pad="A10"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2" route="any"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4" route="any"/>
<connect gate="G$1" pin="TX1+" pad="A2"/>
<connect gate="G$1" pin="TX1-" pad="A3"/>
<connect gate="G$1" pin="TX2+" pad="B2"/>
<connect gate="G$1" pin="TX2-" pad="B3"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.2 Gen 1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722200212"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632722200212"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632722200212?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632712000112" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632712000112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="632712000112"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632712000112"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632712000112?ae"/>
<attribute name="PCB-THICKNESS" value="0.8 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004134726" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004134726">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Up Right"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004134726"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614004134726"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614004134726?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004185023" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004185023">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical - Short Type"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004185023"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614004185023"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614004185023?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105150921" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105150921">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105150921"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="629105150921"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629105150921?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629004113921" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_PLUG_TYPEA"/>
</gates>
<devices>
<device name="" package="629004113921">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="629004113921"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="629004113921"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629004113921?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62900416021" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="62900416021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="62900416021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="62900416021"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/62900416021?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692122030100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692122030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692122030100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692122030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692122030100?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629722050114" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC_1-1"/>
</gates>
<devices>
<device name="" package="629722050114">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A12"/>
<connect gate="G$1" pin="GND1" pad="A1"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="A9"/>
<connect gate="G$1" pin="VBUS1" pad="A4"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="629722050114"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="VALUE" value="629722050114"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629722050114?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61410416121R" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61410416121R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="61410416121R"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="61410416121R"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61410416121R?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614104190121" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614104190121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="614104190121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614104190121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614104190121?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692141030100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB3_TYPEA"/>
<gate name="USBB" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692141030100">
<connects>
<connect gate="USBA" pin="D+" pad="3"/>
<connect gate="USBA" pin="D-" pad="2"/>
<connect gate="USBA" pin="GND" pad="4"/>
<connect gate="USBA" pin="GND_DRAIN" pad="7"/>
<connect gate="USBA" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBA" pin="STDA_SSRX+" pad="6"/>
<connect gate="USBA" pin="STDA_SSRX-" pad="5"/>
<connect gate="USBA" pin="STDA_SSTX+" pad="9"/>
<connect gate="USBA" pin="STDA_SSTX-" pad="8"/>
<connect gate="USBA" pin="VBUS" pad="1"/>
<connect gate="USBB" pin="D+" pad="12"/>
<connect gate="USBB" pin="D-" pad="11"/>
<connect gate="USBB" pin="GND" pad="13"/>
<connect gate="USBB" pin="GND_DRAIN" pad="16"/>
<connect gate="USBB" pin="SHIELD" pad="S1 S2"/>
<connect gate="USBB" pin="STDA_SSRX+" pad="15"/>
<connect gate="USBB" pin="STDA_SSRX-" pad="14"/>
<connect gate="USBB" pin="STDA_SSTX+" pad="18"/>
<connect gate="USBB" pin="STDA_SSTX-" pad="17"/>
<connect gate="USBB" pin="VBUS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692141030100"/>
<attribute name="PINS" value="18pcs"/>
<attribute name="VALUE" value="692141030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692141030100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692221030100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEB"/>
</gates>
<devices>
<device name="" package="692221030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDB_SSRX+" pad="9"/>
<connect gate="G$1" pin="STDB_SSRX-" pad="8"/>
<connect gate="G$1" pin="STDB_SSTX+" pad="6"/>
<connect gate="G$1" pin="STDB_SSTX-" pad="5"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="692221030100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692221030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692221030100?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121330100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121330100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Reverse Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121330100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692121330100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692121330100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629104190121" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="629104190121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal - Short Type"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="629104190121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="629104190121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629104190121?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121030100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121030100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121030100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692121030100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692121030100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004190021" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004190021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="3 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004190021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614004190021"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614004190021?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="651305142821" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="651305142821">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="651305142821"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="651305142821"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/651305142821?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614108646521" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="USBA" symbol="USB2.0_TYPEA"/>
<gate name="USBB" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614108646521">
<connects>
<connect gate="USBA" pin="D+" pad="3 B3 T3"/>
<connect gate="USBA" pin="D-" pad="2 B2 T2"/>
<connect gate="USBA" pin="GND" pad="4 B4 T4"/>
<connect gate="USBA" pin="SHIELD" pad="S1 S2 SB1 SB2 ST1 ST2" route="any"/>
<connect gate="USBA" pin="VBUS" pad="1 B1 T1"/>
<connect gate="USBB" pin="D+" pad="7 B7 T7"/>
<connect gate="USBB" pin="D-" pad="6 B6 T6"/>
<connect gate="USBB" pin="GND" pad="8 B8 T8"/>
<connect gate="USBB" pin="SHIELD" pad="S3 S4"/>
<connect gate="USBB" pin="VBUS" pad="5 B5 T5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Stacked Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="2.5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614108646521"/>
<attribute name="PINS" value="8pcs"/>
<attribute name="VALUE" value="614108646521"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614108646521?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723130112" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723130112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723130112"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632723130112"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632723130112?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723300011" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723300011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="GND GND1"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723300011"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632723300011"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632723300011?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614105150721" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="614105150721">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614105150721"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="614105150721"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614105150721?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692622420101" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="692622420101">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND_DRAIN" pad="8"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="MICB_SSRX+" pad="10"/>
<connect gate="G$1" pin="MICB_SSRX-" pad="9"/>
<connect gate="G$1" pin="MICB_SSTX+" pad="7"/>
<connect gate="G$1" pin="MICB_SSTX-" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="Micro USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="692622420101"/>
<attribute name="PINS" value="10pcs"/>
<attribute name="VALUE" value="692622420101"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692622420101?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722110112" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632722110112">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722110112"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632722110112"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632722110112?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629104151021" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="629104151021">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629104151021"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="629104151021"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629104151021?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400413321" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61400413321">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400413321"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="61400413321"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61400413321?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105150521" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105150521">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="3 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105150521"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="629105150521"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629105150521?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614105150621" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="614105150621">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type AB"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="614105150621"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="614105150621"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614105150621?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629722010114" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC_1"/>
</gates>
<devices>
<device name="" package="629722010114">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A12"/>
<connect gate="G$1" pin="GND1" pad="A1"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="A9"/>
<connect gate="G$1" pin="VBUS1" pad="A4"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="629722010114"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="VALUE" value="629722010114"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629722010114?ae"/>
<attribute name="PCB-THICKNESS" value="1.2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629722000214" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC"/>
</gates>
<devices>
<device name="" package="629722000214">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="GND3" pad="B1"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
<connect gate="G$1" pin="VBUS3" pad="B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629722000214"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="VALUE" value="629722000214"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629722000214?ae"/>
<attribute name="PCB-THICKNESS" value="0.8 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629105136821" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="629105136821">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Micro USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629105136821"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="629105136821"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629105136821?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121130100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121130100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Reverse Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121130100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692121130100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692121130100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61410416021R" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="61410416021R">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="61410416021R"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="61410416021R"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61410416021R?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632121300001" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEA"/>
</gates>
<devices>
<device name="" package="632121300001">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="INSERTIONDETECT" pad="11"/>
<connect gate="G$1" pin="PDDETECT" pad="10"/>
<connect gate="G$1" pin="SHIELD" pad="12 13 S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="632121300001"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="632121300001"/>
<attribute name="WORKING-VOLTAGE" value="20 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632121300001?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62910416121" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="62910416121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="62910416121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="62910416121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/62910416121?ae"/>
<attribute name="PCB-THICKNESS" value="1.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629722330214" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC-1"/>
</gates>
<devices>
<device name="" package="629722330214">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="GND3" pad="B1"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
<connect gate="G$1" pin="VBUS3" pad="B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="629722330214"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="VALUE" value="629722330214"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629722330214?ae"/>
<attribute name="PCB-THICKNESS" value="0.8 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="65100516121" prefix="J">
<description>WR-USB Mini/Micro Connectors

Characteristics
Mini and Micro form factors, ideal for space-constrained designs
Pin configuration: 5 pins for USB 2.0 / 10 pins for USB 3.x
Designed for high cycle durability
UL, TID listing for USB standards

Applications
Mobile and handheld devices
Wearables and portable accessories
Embedded systems and IoT modules

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_MICRO_TYPEB"/>
</gates>
<devices>
<device name="" package="65100516121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="Mini USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="PART-NUMBER" value="65100516121"/>
<attribute name="PINS" value="5pcs"/>
<attribute name="VALUE" value="65100516121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/65100516121?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="692121230100" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3_TYPEA"/>
</gates>
<devices>
<device name="" package="692121230100">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND_DRAIN" pad="7"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="STDA_SSRX+" pad="6"/>
<connect gate="G$1" pin="STDA_SSRX-" pad="5"/>
<connect gate="G$1" pin="STDA_SSTX+" pad="9"/>
<connect gate="G$1" pin="STDA_SSTX-" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.8 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="692121230100"/>
<attribute name="PINS" value="9pcs"/>
<attribute name="VALUE" value="692121230100"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/692121230100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="629712010214" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEC"/>
</gates>
<devices>
<device name="" package="629712010214">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="GND3" pad="B1"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
<connect gate="G$1" pin="VBUS3" pad="B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="629712010214"/>
<attribute name="PINS" value="16pcs"/>
<attribute name="VALUE" value="629712010214"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/629712010214?ae"/>
<attribute name="PCB-THICKNESS" value="0.8 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004135023" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004135023">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Vertical"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004135023"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614004135023"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614004135023?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632712000011" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632712000011"/>
</gates>
<devices>
<device name="" package="632712000011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Plug"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="632712000011"/>
<attribute name="PINS" value="22pcs"/>
<attribute name="VALUE" value="632712000011"/>
<attribute name="WORKING-VOLTAGE" value="20 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632712000011?ae"/>
<attribute name="PCB-THICKNESS" value="0.8 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722100213" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_6PINS"/>
</gates>
<devices>
<device name="" package="632722100213">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B12"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB Power Delivery"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722100213"/>
<attribute name="PINS" value="6pcs"/>
<attribute name="VALUE" value="632722100213"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632722100213?ae"/>
<attribute name="PCB-THICKNESS" value="1 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61400416121" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEB"/>
</gates>
<devices>
<device name="" package="61400416121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type B"/>
<attribute name="IR" value="1.5 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61400416121"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="61400416121"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61400416121?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="614004184726" prefix="J">
<description>WR-USB Standard Connectors

Characteristics
Widely used Type-A and Type-B connectors, available in different orientation
Various mount types: SMT, THT, THR
Pin configuration: 4 pins for USB 2.0 / 9 pins for USB 3.x
Durable and backward compatible with older USB versions
UL, TID listing for USB standards

Applications
Office and desktop computing systems
Industrial control and automation equipment
Consumer electronics and peripherals
Audio-visual and broadcast systems

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2024-05-21
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB2.0_TYPEA"/>
</gates>
<devices>
<device name="" package="614004184726">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Up Right - Short Type"/>
<attribute name="APPLICATION" value="USB 2.0"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type A"/>
<attribute name="IR" value="2 A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="614004184726"/>
<attribute name="PINS" value="4pcs"/>
<attribute name="VALUE" value="614004184726"/>
<attribute name="WORKING-VOLTAGE" value="30 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/614004184726?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632722200211" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC_632722200211"/>
</gates>
<devices>
<device name="" package="632722200211">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+1" pad="A6"/>
<connect gate="G$1" pin="D+2" pad="B6"/>
<connect gate="G$1" pin="D-1" pad="A7"/>
<connect gate="G$1" pin="D-2" pad="B7"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="RX1+" pad="B11"/>
<connect gate="G$1" pin="RX1-" pad="B10"/>
<connect gate="G$1" pin="RX2+" pad="A11"/>
<connect gate="G$1" pin="RX2-" pad="A10"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S5 S6"/>
<connect gate="G$1" pin="SHIELD1" pad="S3 S4"/>
<connect gate="G$1" pin="TX1+" pad="A2"/>
<connect gate="G$1" pin="TX1-" pad="A3"/>
<connect gate="G$1" pin="TX2+" pad="B2"/>
<connect gate="G$1" pin="TX2-" pad="B3"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.2 Gen 1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632722200211"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632722200211"/>
<attribute name="WORKING-VOLTAGE" value="20 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632722200211?ae"/>
<attribute name="PCB-THICKNESS" value="0.6 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="632723100011" prefix="J">
<description>WR-USB Type C Connectors

Characteristics
Available in 24p (3.x), 16p (2.0) and 6p (Power Delivery only)
Aligned with Power Delivery up to 240W
High durability (10 000 cycles)
UL, TID listing for USB standards

Applications
Mobile computing and smart devices
High-performance industrial and medical systems
Consumer electronics and multimedia hubs
Smart buildings

Details see: www.we-online.com/en/components/products/INPUT_OUTPUT_WR_USB_STANDARD

Updated by Ella 2026-07-03
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="USB3.1_TYPEC"/>
</gates>
<devices>
<device name="" package="632723100011">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="DN1" pad="A7"/>
<connect gate="G$1" pin="DN2" pad="B7"/>
<connect gate="G$1" pin="DP1" pad="A6"/>
<connect gate="G$1" pin="DP2" pad="B6"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND1" pad="A12"/>
<connect gate="G$1" pin="GND2" pad="B1"/>
<connect gate="G$1" pin="GND3" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SHIELD" pad="GND GND1"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="SSRXN1" pad="B10"/>
<connect gate="G$1" pin="SSRXN2" pad="A10"/>
<connect gate="G$1" pin="SSRXP1" pad="B11"/>
<connect gate="G$1" pin="SSRXP2" pad="A11"/>
<connect gate="G$1" pin="SSTXN1" pad="A3"/>
<connect gate="G$1" pin="SSTXN2" pad="B3"/>
<connect gate="G$1" pin="SSTXP1" pad="A2"/>
<connect gate="G$1" pin="SSTXP2" pad="B2"/>
<connect gate="G$1" pin="VBUS" pad="A4"/>
<connect gate="G$1" pin="VBUS1" pad="A9"/>
<connect gate="G$1" pin="VBUS2" pad="B4"/>
<connect gate="G$1" pin="VBUS3" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="TYPE" value="Horizontal"/>
<attribute name="APPLICATION" value="USB 3.1"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="INTERFACE-TYPE" value="Type C"/>
<attribute name="IR" value="5 A"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="632723100011"/>
<attribute name="PINS" value="24pcs"/>
<attribute name="VALUE" value="632723100011"/>
<attribute name="WORKING-VOLTAGE" value="48 V (DC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/632723100011?ae"/>
<attribute name="PCB-THICKNESS" value="1 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
