<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Wire-to-Board Connectors - WR-WST &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019b, 2019-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="490107672012">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107672012_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671812_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671612_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671612">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107671212_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671812">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107671412">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107671412_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671212">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107671012_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107670612">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107670812">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107670812_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107670412_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107670612_DEBUGGING">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;/b&gt;&lt;br&gt;Only use for debugging or programming application.&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application.</description>
</package>
<package name="490107671012">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
<package name="490107670412">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
</packages>
<symbols>
<symbol name="9X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="8X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="10X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="6X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="7X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="4X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="3X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="490107672012" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2"/>
</gates>
<devices>
<device name="" package="490107672012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107672012.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="32.99mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107672012"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107672012"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107672012_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2"/>
</gates>
<devices>
<device name="" package="490107672012_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107672012.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="32.99mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107672012"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107672012"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671812_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2"/>
</gates>
<devices>
<device name="" package="490107671812_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671812.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="30.45mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671812"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671812"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671612_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2"/>
</gates>
<devices>
<device name="" package="490107671612_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671612.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="27.91mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671612"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671612"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671612" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2"/>
</gates>
<devices>
<device name="" package="490107671612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671612.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="27.91mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671612"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671612"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671212_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2"/>
</gates>
<devices>
<device name="" package="490107671212_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671212.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="22.83mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671212"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671212"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671812" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2"/>
</gates>
<devices>
<device name="" package="490107671812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671812.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="30.45mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671812"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671812"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671412" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2"/>
</gates>
<devices>
<device name="" package="490107671412">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671412.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="25.37mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671412"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671412"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671212" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2"/>
</gates>
<devices>
<device name="" package="490107671212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671212.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="22.83mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671212"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671212"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671012_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2"/>
</gates>
<devices>
<device name="" package="490107671012_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671012.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="20.29mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671012"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671012"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671412_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2"/>
</gates>
<devices>
<device name="" package="490107671412_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671412.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="25.37mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671412"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671412"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670812_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2"/>
</gates>
<devices>
<device name="" package="490107670812_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670812.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="17.75mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670812"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670812"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670412_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2"/>
</gates>
<devices>
<device name="" package="490107670412_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670412.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12.67mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670412"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670412"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670612" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2"/>
</gates>
<devices>
<device name="" package="490107670612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670612.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="15.21mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670612"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670612"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670612_DEBUGGING" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;Only use for debugging or programming application. &lt;/font&gt;
&lt;br&gt;For mechanical stressed application please use the PCB layout for permanent application
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2"/>
</gates>
<devices>
<device name="" package="490107670612_DEBUGGING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670612.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="15.21mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670612"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670612"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107671012" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2"/>
</gates>
<devices>
<device name="" package="490107671012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671012.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="20.29mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671012"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107671012"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670812" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2"/>
</gates>
<devices>
<device name="" package="490107670812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670812.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="17.75mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670812"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670812"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="490107670412" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;font color="#0000FF"&gt;For permanent application up to 10g vibration stable &lt;/font&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging  Tube 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR1  1 A 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage  500 V (AC) 
&lt;br&gt;Contact Resistance  10 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material   LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color  Black 
&lt;br&gt;Contact Material  CuNiSi 
&lt;br&gt;Contact Plating  Au (SKEDD), Sn (IDC) 
&lt;br&gt;Pitch  2.54 mm 
&lt;br&gt;Cable  AWG 28/1.27 mm ribbon cable 
&lt;br&gt;Operating Temperature  -25 up to +105 °C 
&lt;br&gt;Compliance  Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o104848v209%20Single_WR-WST_REDFIT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD"&gt;https://katalog.we-online.com/en/em/REDFIT_IDC_SKEDD&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-05-21&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2"/>
</gates>
<devices>
<device name="" package="490107670412">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107670412.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12.67mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107670412"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="WE-NUMBER" value="490107670412"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
