<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-WTB &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="62401421622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,14 Pins</description>
</package>
<package name="61901011121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,10 Pins</description>
</package>
<package name="648106131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header,6pins</description>
</package>
<package name="679308124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="645010117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header,10 Pins</description>
</package>
<package name="68800211622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header,2 Pins</description>
</package>
<package name="64600511622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header,5 Pins</description>
</package>
<package name="645008117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header,8 Pins</description>
</package>
<package name="64800611622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header,6 pins;</description>
</package>
<package name="68800711722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,7 Pins</description>
</package>
<package name="62400821722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 8 pins</description>
</package>
<package name="62404021722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking,  40 pins</description>
</package>
<package name="648102131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header,2 Pins</description>
</package>
<package name="62401021622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,10 Pins</description>
</package>
<package name="645002114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header, 2 Pins</description>
</package>
<package name="62403621722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 36 pins</description>
</package>
<package name="653104124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,4 Pins</description>
</package>
<package name="61900211121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,2 Pins</description>
</package>
<package name="653102131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 2 Pins</description>
</package>
<package name="61900511021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 5 Pins</description>
</package>
<package name="62000411722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,4 Pins</description>
</package>
<package name="653006114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,6 Pins</description>
</package>
<package name="62000311622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,3 Pins</description>
</package>
<package name="62001011722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,10 Pins</description>
</package>
<package name="62000311722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,3 Pins</description>
</package>
<package name="62401421722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 14 pins</description>
</package>
<package name="645008114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header,  8 Pins</description>
</package>
<package name="62000211722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,2 Pins</description>
</package>
<package name="62401621622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 16 Pins</description>
</package>
<package name="61900411021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 4 Pins</description>
</package>
<package name="66100411622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,4Pins</description>
</package>
<package name="64800911622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header, 9 Pins</description>
</package>
<package name="653109131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 9 Pins</description>
</package>
<package name="66100211722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,2Pins</description>
</package>
<package name="62403621622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 36 Pins</description>
</package>
<package name="64800411622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header, 4 Pins</description>
</package>
<package name="679307124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,7 Pins</description>
</package>
<package name="62000611722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,6 Pins</description>
</package>
<package name="62401621722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 16 pins</description>
</package>
<package name="620302124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header, 2 Pins</description>
</package>
<package name="66100511722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,5Pins</description>
</package>
<package name="61900519521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking, 5 Pins</description>
</package>
<package name="62403821722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 38 pins</description>
</package>
<package name="679309124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,9 Pins</description>
</package>
<package name="66100511622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,5Pins</description>
</package>
<package name="653007114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,7 Pins</description>
</package>
<package name="61900711121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,7 Pins</description>
</package>
<package name="62000711622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,7 Pins</description>
</package>
<package name="61900219521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking, 2 Pins</description>
</package>
<package name="653005117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,5 Pins</description>
</package>
<package name="61900811121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,8 Pins</description>
</package>
<package name="62401221722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 12 pins</description>
</package>
<package name="645002117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header,2 Pins</description>
</package>
<package name="61900619521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking,6 pins;</description>
</package>
<package name="62401021722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 10 pins</description>
</package>
<package name="620307124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,7 Pins</description>
</package>
<package name="64801011622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header,10 Pins</description>
</package>
<package name="62000411622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,4 Pins</description>
</package>
<package name="66100311622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,3 Pins</description>
</package>
<package name="62000711722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,7 Pins</description>
</package>
<package name="653105131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header,  5 Pins</description>
</package>
<package name="620103131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,3 Pins</description>
</package>
<package name="653114124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,14 Pins</description>
</package>
<package name="653008117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,8 Pins</description>
</package>
<package name="648103131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header, 3 Pins</description>
</package>
<package name="620102131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,2 Pins</description>
</package>
<package name="62402221722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 22 pins</description>
</package>
<package name="68800311722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,3 Pins</description>
</package>
<package name="653104131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 4 Pins</description>
</package>
<package name="61900311021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 3 Pins</description>
</package>
<package name="653003117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,3 Pins</description>
</package>
<package name="64600411622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header,4 Pins</description>
</package>
<package name="620305124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,5 Pins</description>
</package>
<package name="679302124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="645010114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header, 10 Pins</description>
</package>
<package name="62400821622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 8 Pins</description>
</package>
<package name="61900211021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 2 Pins</description>
</package>
<package name="648104131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header,4 Pins</description>
</package>
<package name="68801011722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,10  Pins</description>
</package>
<package name="653005114822">
<description>WR-WTB 1.25mm Male Vertical Shrouded Header, 5 Pins</description>
</package>
<package name="653004114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,4 Pins</description>
</package>
<package name="620303124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,3 Pins</description>
</package>
<package name="653002114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="62404021622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,40 Pins</description>
</package>
<package name="679303124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header, 3 Pins</description>
</package>
<package name="648109131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header, 9 Pins</description>
</package>
<package name="653002117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header, 2 Pins</description>
</package>
<package name="653004117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,4 Pins</description>
</package>
<package name="645003114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header,  3 Pins</description>
</package>
<package name="61900819521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking,8 Pins</description>
</package>
<package name="62000911622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,9 Pins</description>
</package>
<package name="68800211722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,2 Pins</description>
</package>
<package name="61900611121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,6 Pins</description>
</package>
<package name="653003114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,3 Pins</description>
</package>
<package name="620310124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,10 Pins</description>
</package>
<package name="64600711622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header, 7 Pins</description>
</package>
<package name="653006117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,6 Pins</description>
</package>
<package name="679306124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,6Pins</description>
</package>
<package name="66101011722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,10Pins</description>
</package>
<package name="648108131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header, 8 Pins</description>
</package>
<package name="64601011622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header,10 Pins</description>
</package>
<package name="653112124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,12 Pins</description>
</package>
<package name="648107131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header,7 Pins</description>
</package>
<package name="653109124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,9 Pins</description>
</package>
<package name="653107131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 7 Pins</description>
</package>
<package name="653103131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 3 Pins</description>
</package>
<package name="653111124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,11 Pins</description>
</package>
<package name="665303124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header,3 pins</description>
</package>
<package name="653009117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,9 Pins</description>
</package>
<package name="66100411722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,4Pins</description>
</package>
<package name="653111131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 11 Pins</description>
</package>
<package name="653112131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 12 Pins</description>
</package>
<package name="653108131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header,  8 Pins</description>
</package>
<package name="653107124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header, 7 Pins</description>
</package>
<package name="665304124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header,4 pins</description>
</package>
<package name="653106124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,6 Pins</description>
</package>
<package name="653115131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header,15 Pins</description>
</package>
<package name="653113131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 13 Pins</description>
</package>
<package name="653110131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 10 Pins</description>
</package>
<package name="653108124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="665302124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header,2 pins</description>
</package>
<package name="653110124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header, 10 Pins</description>
</package>
<package name="665110131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded, 10 pins</description>
</package>
<package name="665310124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header,10 pins</description>
</package>
<package name="61900411121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,4 Pins</description>
</package>
<package name="665306124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header, 6 pins</description>
</package>
<package name="61900511121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,5 Pins</description>
</package>
<package name="665104131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded,  4 pins</description>
</package>
<package name="665308124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header, 8 pins</description>
</package>
<package name="62402421722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 24 pins</description>
</package>
<package name="61900311121">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Locking Header,3 Pins</description>
</package>
<package name="620304124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,4 Pins</description>
</package>
<package name="648110131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header, 10 Pins</description>
</package>
<package name="64600311622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header,3 Pins</description>
</package>
<package name="620109131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,9 Pins</description>
</package>
<package name="653010114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header,10 Pins</description>
</package>
<package name="68800811722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header, 8 Pins</description>
</package>
<package name="66100311722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,3Pins</description>
</package>
<package name="68800411622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header, 4 Pins</description>
</package>
<package name="62401821722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 18 pins</description>
</package>
<package name="679304124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,4 Pins</description>
</package>
<package name="653010117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,10 Pins</description>
</package>
<package name="653009114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header, 9 Pins</description>
</package>
<package name="653008114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Vertical Shrouded Header, 8 Pins</description>
</package>
<package name="653103124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,3 Pins</description>
</package>
<package name="653105124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,5 Pins</description>
</package>
<package name="620306124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,6 Pins</description>
</package>
<package name="62402621722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 26 pins</description>
</package>
<package name="62403221722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 32 pins</description>
</package>
<package name="620308124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="61900319521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking, 3 Pins</description>
</package>
<package name="68800511722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,5 Pins</description>
</package>
<package name="645005114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header, 5 Pins</description>
</package>
<package name="64800311622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header, 3 Pins</description>
</package>
<package name="620107131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,7 Pins</description>
</package>
<package name="66100811622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="620309124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm SMT Male Vertical Shrouded Header,9 Pins</description>
</package>
<package name="64600211622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm Male Shrouded Header,2 Pins</description>
</package>
<package name="653113124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,13 Pins</description>
</package>
<package name="62000611622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,6 Pins</description>
</package>
<package name="620104131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,4 Pins</description>
</package>
<package name="64800511622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header,5 Pins</description>
</package>
<package name="68800611722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,6 Pins</description>
</package>
<package name="64800711622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header, 7 Pins</description>
</package>
<package name="645004117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header,4 Pins</description>
</package>
<package name="679310124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,10 Pins</description>
</package>
<package name="62402221622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,22 Pins</description>
</package>
<package name="62401221622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,12 Pins</description>
</package>
<package name="68800911622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header, 9 Pins</description>
</package>
<package name="620105131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,5 Pins</description>
</package>
<package name="62000211622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="61901019521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking,10 Pins</description>
</package>
<package name="653007117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.25 mm Male Horizontal Shrouded Header,7 Pins</description>
</package>
<package name="62403821622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,38 Pins</description>
</package>
<package name="62402021722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 20 pins</description>
</package>
<package name="68800311622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header,3 Pins</description>
</package>
<package name="648105131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Horizontal Shrouded Header, 5 Pins</description>
</package>
<package name="64800811622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="653114131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header, 14 Pins</description>
</package>
<package name="66101011622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,10Pins</description>
</package>
<package name="653106131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Horizontal Shrouded Header,  6 Pins</description>
</package>
<package name="61900611021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 6 pins;</description>
</package>
<package name="68801011622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header,10 Pins</description>
</package>
<package name="665105131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded, 5 pins</description>
</package>
<package name="665305124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 1.00 mm SMT Male Vertical Shrouded Header,5 pins</description>
</package>
<package name="66100811722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,8Pins</description>
</package>
<package name="68800911722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,9 Pins</description>
</package>
<package name="653115124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,15 Pins</description>
</package>
<package name="62000511722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,5 Pins</description>
</package>
<package name="620106131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header, 6 Pins</description>
</package>
<package name="66100421622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 4Pins</description>
</package>
<package name="68800811622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header, 8 Pins</description>
</package>
<package name="64800211622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="62000911722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,9 Pins</description>
</package>
<package name="679305124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.50 mm SMT Male Vertical Shrouded Header,5 Pins</description>
</package>
<package name="620108131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,8 Pins</description>
</package>
<package name="62000811622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,8 Pins</description>
</package>
<package name="653102124022">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  1.25 mm SMT Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="665102131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded, 2 pins</description>
</package>
<package name="61900419521">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Locking Header Top Locking,4 Pins</description>
</package>
<package name="62402021622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,20 Pins</description>
</package>
<package name="645004114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header,  4 Pins</description>
</package>
<package name="62403421622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,34 Pins</description>
</package>
<package name="665103131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded,  3 pins</description>
</package>
<package name="62402421622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 24 Pins</description>
</package>
<package name="68800611622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header, 6 Pins</description>
</package>
<package name="665108131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded, 8 pins</description>
</package>
<package name="62402821622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 28 Pins</description>
</package>
<package name="62403221622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 32 Pins</description>
</package>
<package name="62000811722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Horizontal Shrouded Header,8 Pins</description>
</package>
<package name="66100611622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 6Pins</description>
</package>
<package name="62402621622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking, 26 Pins</description>
</package>
<package name="62403421722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 34 pins</description>
</package>
<package name="62001011622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,10 Pins</description>
</package>
<package name="66100821622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 8Pins</description>
</package>
<package name="66100911622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 9Pins</description>
</package>
<package name="66100621622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 6Pins</description>
</package>
<package name="665106131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;1.00 mm SMT Male Horizontal Shrouded, 6 pins</description>
</package>
<package name="68800411722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.50 mm “J” Type Male Horizontal Shrouded Header,4 Pins</description>
</package>
<package name="62402821722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 28 pins</description>
</package>
<package name="62403021622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,30 Pins</description>
</package>
<package name="66100211622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.54 mm Male Vertical Shrouded Header,2 Pins</description>
</package>
<package name="62403021722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;  2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking, 30 pins</description>
</package>
<package name="66100711622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 7Pins</description>
</package>
<package name="645006114822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Vertical Locking Header, 6 Pins</description>
</package>
<package name="68800511622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header, 5 Pins</description>
</package>
<package name="66101211622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 12Pins</description>
</package>
<package name="66101021622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 10Pins</description>
</package>
<package name="61901011021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 10 Pins</description>
</package>
<package name="645003117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header, 3 Pins</description>
</package>
<package name="62000511622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.00 mm Male Vertical Shrouded Header,5 Pins</description>
</package>
<package name="62401821622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking,18 Pins</description>
</package>
<package name="66100611722">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54 mm Male Right Angled Shrouded Header,6Pins</description>
</package>
<package name="689112131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 12Pins</description>
</package>
<package name="66101411622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 14Pins</description>
</package>
<package name="66101621622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 16Pins</description>
</package>
<package name="68800711622">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.50 mm “J” Type Vertical Male Shrouded Header,7 Pins</description>
</package>
<package name="66101421622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 14Pins</description>
</package>
<package name="66101221622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 12Pins</description>
</package>
<package name="689108131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 8Pins</description>
</package>
<package name="689102131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 2Pins</description>
</package>
<package name="645005117322">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 3.96 mm Male Right Angled Locking Header, 5  Pins</description>
</package>
<package name="689106131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 6Pins</description>
</package>
<package name="61900811021">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt;2.54mm Male Left Angled Header Bottom Locking, 8 Pins</description>
</package>
<package name="689103131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 3Pins</description>
</package>
<package name="66101611622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 16Pins</description>
</package>
<package name="689110131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 10Pins</description>
</package>
<package name="689105131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 5Pins</description>
</package>
<package name="689104131822">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Horizontal, SMT, 4Pins</description>
</package>
<package name="620110131822">
<description>&lt;b&gt;WR-WTB&lt;/b&gt;&lt;br&gt; 2.00 mm SMT Male Horizontal Shrouded Header,10 Pins</description>
</package>
<package name="689302124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 2Pins</description>
</package>
<package name="66102021622">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 20Pins</description>
</package>
<package name="689310124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 10Pins</description>
</package>
<package name="689312124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 12Pins</description>
</package>
<package name="689306124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 6Pins</description>
</package>
<package name="689304124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 4Pins</description>
</package>
<package name="689303124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 3Pins</description>
</package>
<package name="689308124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 8Pins</description>
</package>
<package name="689305124022">
<description>&lt;B&gt;WR-WTB 0.80 mm Male Header
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Vertical, SMT, 5Pins</description>
</package>
</packages>
<symbols>
<symbol name="7X2MT_1">
<description>7X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10MT_1">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="20X2MT">
<description>20X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="7MT_1">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2MT_1">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8MS_1">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4X2MT">
<description>4X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="18X2MT">
<description>18X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="2MS">
<description>2Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6MS">
<description>6Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5MT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4MS">
<description>4Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="7X2MT">
<description>7X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10MT">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8MT_1">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5X2MT_1">
<description>5X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2MT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6MT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3MT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="8MT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8X2MT_1">
<description>8X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="9MT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="9MS">
<description>9Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="7MS_1">
<description>7Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="18X2MT_1">
<description>18X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="8X2MT">
<description>8X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="19X2MT">
<description>19X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
</symbol>
<symbol name="2MS_1">
<description>2Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5MT_1">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="9MS_1">
<description>9Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="7MT">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="6X2MT">
<description>6X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6MT_1">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5X2MT">
<description>5X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7MS">
<description>7Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="5MS">
<description>5Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3MS">
<description>3Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="14MS">
<description>14Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="3MT_1">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="11X2MT">
<description>11X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="5MS_1">
<description>5Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4X2MT_1">
<description>4X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="20X2MT_1">
<description>20X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="3MS_1">
<description>3Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4MT_1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10MS_1">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6MS_1">
<description>6Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8MS">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12MS">
<description>12Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="11MS">
<description>11Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="9MT_1">
<description>9Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="4MS_1">
<description>4Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="15MS">
<description>15Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="13MS">
<description>13Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="10MS">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12X2MT">
<description>12X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="9X2MT">
<description>9X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="13X2MT">
<description>13X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="16X2MT">
<description>16X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="11X2MT_1">
<description>11X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="6X2MT_1">
<description>6X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="19X2MT_1">
<description>19X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
</symbol>
<symbol name="10X2MT">
<description>10X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="2X2MT_2">
<description>2X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10X2MT_1">
<description>10X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="17X2MT_1">
<description>17X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="12X2MT_1">
<description>12X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="14X2MT_1">
<description>14X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="16X2MT_1">
<description>16X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="13X2MT_1">
<description>13X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="14X2MT">
<description>14X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="17X2MT">
<description>17X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="4X2MT_2">
<description>4X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2MT_2">
<description>3X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="15X2MT_1">
<description>15X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="15X2MT">
<description>15X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="12MT">
<description>12Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5X2MT_2">
<description>5X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="14MT">
<description>16Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="9X2MT_1">
<description>9X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="12MS_1">
<description>12Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8X2MT_2">
<description>8X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="7X2MT_2">
<description>6X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="6X2MT_2">
<description>6X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="16MT">
<description>16Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="10X2MT_2">
<description>10X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="62401421622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="62401421622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401421622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401421622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62401421622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61901011121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="61901011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61901011121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61901011121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61901011121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648106131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="648106131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648106131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648106131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648106131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679308124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="679308124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679308124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679308124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679308124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645010117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="645010117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645010117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="39.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645010117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645010117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64600511622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="64600511622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64600511622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64600511622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64600511622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800211622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="68800211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800211622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800711722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT_1"/>
</gates>
<devices>
<device name="" package="68800711722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800711722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800711722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800711722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645008117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="645008117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645008117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="31.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645008117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645008117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800611622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="64800611622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800611622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="10.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800611622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800611622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62400821722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="62400821722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62400821722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="11.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62400821722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62400821722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62404021722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="62404021722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62404021722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="43.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62404021722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62404021722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648102131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="648102131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648102131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648102131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648102131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="62401021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="13.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62401021622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403621722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2MT"/>
</gates>
<devices>
<device name="" package="62403621722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403621722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="39.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403621722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62403621722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645002114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="645002114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645002114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="7.92mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645002114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645002114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900211121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="61900211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900211121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="5.08mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900211121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900211121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653104124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="653104124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653104124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653104124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653104124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653102131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="653102131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653102131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653102131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653102131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900511021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="61900511021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900511021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900511021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900511021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000411722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="62000411722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000411722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000411722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000411722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653006114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="653006114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653006114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653006114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653006114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000311622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="62000311622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000311622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000311622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000311622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62001011722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="62001011722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001011722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62001011722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62001011722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000311722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="62000311722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000311722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000311722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000311722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401421722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="62401421722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401421722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401421722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62401421722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645008114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="645008114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645008114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="31.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645008114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645008114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000211722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="62000211722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000211722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000211722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000211722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401621622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="62401621622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401621622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="19.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401621622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62401621622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900411021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="61900411021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900411021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10.16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900411021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900411021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100411622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="66100411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="9.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100411622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800911622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="64800911622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800911622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800911622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800911622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653109131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS"/>
</gates>
<devices>
<device name="" package="653109131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653109131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653109131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653109131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100211722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="66100211722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100211722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="4.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100211722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100211722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403621622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2MT_1"/>
</gates>
<devices>
<device name="" package="62403621622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403621622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="39.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403621622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62403621622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800411622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="64800411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800411622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679307124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS_1"/>
</gates>
<devices>
<device name="" package="679307124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679307124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679307124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679307124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000611722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="62000611722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000611722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="14mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000611722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000611722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401621722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="62401621722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401621722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="19.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401621722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62401621722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620302124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="620302124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620302124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620302124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620302124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100511722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="66100511722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100511722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100511722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100511722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900519521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="61900519521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900519521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900519521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900519521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679309124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS_1"/>
</gates>
<devices>
<device name="" package="679309124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679309124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="16.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679309124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679309124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403821722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="19X2MT"/>
</gates>
<devices>
<device name="" package="62403821722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403821722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="41.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403821722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 38 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62403821722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100511622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="66100511622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100511622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100511622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="5"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100511622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653007114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="653007114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653007114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653007114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653007114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900711121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="61900711121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900711121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900711121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900711121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000711622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="62000711622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000711622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000711622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000711622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900219521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="61900219521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900219521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="5.08mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900219521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900219521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900811121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="61900811121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900811121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900811121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900811121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653005117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="653005117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653005117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653005117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653005117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401221722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="62401221722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401221722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401221722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62401221722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645002117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="645002117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645002117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="7.92mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645002117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645002117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900619521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="61900619521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900619521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900619521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900619521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401021722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="62401021722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401021722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="13.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401021722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62401021722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620307124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS"/>
</gates>
<devices>
<device name="" package="620307124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620307124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620307124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620307124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64801011622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="64801011622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64801011622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="16.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64801011622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64801011622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000411622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="62000411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000411622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100311622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="66100311622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100311622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100311622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100311622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653105131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="653105131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653105131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653105131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653105131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000711722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="62000711722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000711722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000711722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000711722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620103131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="620103131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620103131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620103131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620103131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653114124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MS"/>
</gates>
<devices>
<device name="" package="653114124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653114124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="22.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653114124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653114124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653008117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="653008117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653008117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="11.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653008117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653008117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648103131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="648103131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648103131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648103131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648103131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620102131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="620102131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620102131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620102131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620102131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402221722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT"/>
</gates>
<devices>
<device name="" package="62402221722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402221722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402221722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62402221722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800311722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="68800311722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800311722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800311722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800311722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653104131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="653104131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653104131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653104131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653104131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653003117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="653003117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653003117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="5.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653003117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653003117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64600411622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="64600411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64600411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64600411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64600411622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900311021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="61900311021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900311021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.62mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900311021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900311021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620305124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="620305124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620305124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="14mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620305124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620305124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679302124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="679302124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679302124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679302124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679302124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645010114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="645010114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645010114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="39.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645010114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645010114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62400821622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="62400821622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62400821622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="11.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62400821622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62400821622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648104131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="648104131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648104131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648104131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648104131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68801011722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="68801011722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68801011722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="27.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68801011722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68801011722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653005114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="653005114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653005114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653005114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653005114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900211021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="61900211021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900211021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="5.08mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900211021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900211021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653004114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="653004114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653004114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653004114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653004114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620303124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="620303124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620303124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620303124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620303124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653002114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="653002114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653002114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="4.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="653002114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653002114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679303124022" prefix="K">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="679303124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679303124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679303124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679303124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62404021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="62404021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62404021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="43.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62404021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62404021622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648109131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS"/>
</gates>
<devices>
<device name="" package="648109131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648109131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="16.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648109131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648109131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653002117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="653002117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653002117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="4.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653002117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653002117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653004117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="653004117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653004117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653004117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653004117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645003114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="645003114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645003114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="11.88mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645003114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645003114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900819521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="61900819521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900819521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900819521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900819521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000911622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="62000911622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000911622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000911622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000911622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800211722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="68800211722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800211722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800211722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800211722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900611121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="61900611121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900611121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900611121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900611121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653003114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="653003114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653003114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="5.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="653003114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653003114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620310124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="620310124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620310124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="24mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620310124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620310124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64600711622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="64600711622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64600711622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64600711622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64600711622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653006117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="653006117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653006117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653006117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653006117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679306124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="679306124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679306124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679306124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679306124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101011722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58906v209%20Family_WR-WTB_Vertical_Shrouded_Header_6610xx11722_2.54_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58906v209%20Family_WR-WTB_Vertical_Shrouded_Header_6610xx11722_2.54_SW.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722"&gt;https://katalog.we-online.com/en/em/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-05
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="66101011722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101011722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101011722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66101011722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648108131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="648108131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648108131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648108131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648108131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64601011622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="64601011622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64601011622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="27.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64601011622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64601011622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653112124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS"/>
</gates>
<devices>
<device name="" package="653112124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653112124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="19.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653112124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653112124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648107131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS"/>
</gates>
<devices>
<device name="" package="648107131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648107131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648107131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648107131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653107131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS"/>
</gates>
<devices>
<device name="" package="653107131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653107131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653107131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653107131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653109124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS"/>
</gates>
<devices>
<device name="" package="653109124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653109124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653109124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653109124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653103131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="653103131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653103131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653103131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653103131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653111124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11MS"/>
</gates>
<devices>
<device name="" package="653111124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653111124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="18.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653111124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653111124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665303124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="665303124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665303124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665303124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665303124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653009117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_1"/>
</gates>
<devices>
<device name="" package="653009117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653009117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653009117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653009117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100411722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="66100411722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100411722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="9.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100411722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100411722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653111131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11MS"/>
</gates>
<devices>
<device name="" package="653111131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653111131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="18.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653111131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653111131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653112131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS"/>
</gates>
<devices>
<device name="" package="653112131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653112131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="19.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653112131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653112131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653108131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="653108131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653108131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="14.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653108131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653108131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653107124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS"/>
</gates>
<devices>
<device name="" package="653107124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653107124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653107124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653107124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665304124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="665304124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665304124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665304124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665304124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653106124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="653106124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653106124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653106124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653106124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653115131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MS"/>
</gates>
<devices>
<device name="" package="653115131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653115131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="23.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653115131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653115131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653113131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13MS"/>
</gates>
<devices>
<device name="" package="653113131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653113131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="21mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653113131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653113131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653110131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="653110131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653110131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="17.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653110131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653110131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653108124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="653108124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653108124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="14.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653108124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653108124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665302124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="665302124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665302124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665302124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665302124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653110124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="653110124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653110124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="17.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653110124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653110124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665110131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="665110131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665110131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665110131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665110131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665310124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="665310124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665310124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665310124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665310124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900411121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="61900411121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900411121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10.16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900411121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900411121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665306124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="665306124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665306124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665306124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665306124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665104131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="665104131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665104131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665104131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665104131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900511121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="61900511121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900511121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900511121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900511121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665308124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="665308124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665308124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665308124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665308124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402421722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT"/>
</gates>
<devices>
<device name="" package="62402421722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402421722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="27.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402421722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62402421722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900311121" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66; PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33345v209%206190xx11121_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_LOCKING_HEADER_6190XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="61900311121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900311121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.62mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900311121"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="61900311121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620304124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="620304124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620304124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620304124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620304124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648110131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="648110131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648110131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648110131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648110131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64600311622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="64600311622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64600311622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64600311622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64600311622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620109131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS"/>
</gates>
<devices>
<device name="" package="620109131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620109131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620109131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620109131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653010114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="653010114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653010114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="14.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653010114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653010114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800811722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="68800811722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800811722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="22.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800811722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800811722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100311722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="66100311722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100311722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100311722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="3"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100311722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800411622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="68800411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800411622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679304124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="679304124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679304124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679304124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679304124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653010117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="653010117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653010117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="14.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653010117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653010117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653009114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="653009114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653009114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653009114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653009114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653008114822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag; Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33370v209%20Multi-WR-WTB125-6530xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_VERTICAL_SHROUDED_HEADER_6530XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="653008114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653008114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="11.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653008114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653008114822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401821722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT"/>
</gates>
<devices>
<device name="" package="62401821722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401821722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="21.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401821722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62401821722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653103124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="653103124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653103124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653103124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653103124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653105124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="653105124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653105124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653105124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653105124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620306124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="620306124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620306124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620306124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620306124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403221722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2MT"/>
</gates>
<devices>
<device name="" package="62403221722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403221722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="35.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403221722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62403221722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402621722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="62402621722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402621722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="29.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402621722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62402621722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620308124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="620308124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620308124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620308124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620308124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900319521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="61900319521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900319521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.62mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900319521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900319521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800511722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="68800511722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800511722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800511722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800511722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645005114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="645005114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645005114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="19.8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645005114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645005114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800311622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="64800311622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800311622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800311622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800311622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620107131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS"/>
</gates>
<devices>
<device name="" package="620107131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620107131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620107131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620107131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100811622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="66100811622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100811622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.02mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100811622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100811622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620309124022" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	100 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33354v209%20Multi-WR-WTB200-6203xx124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6203XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS_1"/>
</gates>
<devices>
<device name="" package="620309124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620309124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="620309124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="620309124022"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64600211622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33364v209%20Multi-WR-WTB250-6460xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_MALE_SHROUDED_HEADER_6460XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="64600211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64600211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64600211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64600211622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653113124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13MS"/>
</gates>
<devices>
<device name="" package="653113124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653113124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="21mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653113124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653113124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000611622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="62000611622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000611622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="14mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000611622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000611622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800511622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="64800511622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800511622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800511622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800511622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620104131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="620104131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620104131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620104131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620104131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800611722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="68800611722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800611722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800611722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800611722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800711622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="64800711622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800711622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800711622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800711622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645004117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="645004117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645004117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="15.84mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645004117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645004117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679310124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="679310124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679310124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679310124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679310124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402221622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_1"/>
</gates>
<devices>
<device name="" package="62402221622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402221622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402221622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62402221622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401221622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="62401221622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401221622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401221622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62401221622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800911622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_1"/>
</gates>
<devices>
<device name="" package="68800911622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800911622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800911622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800911622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620105131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="620105131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620105131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="14mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620105131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620105131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000211622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="62000211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000211622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61901019521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="61901019521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61901019521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61901019521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61901019521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653007117322" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33371v209%20Multi-WR-WTB125-6530xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_MALE_HORIZONTAL_SHROUDED_HEADER_6530XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT_1"/>
</gates>
<devices>
<device name="" package="653007117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653007117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="653007117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653007117322"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403821622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="19X2MT_1"/>
</gates>
<devices>
<device name="" package="62403821622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403821622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="41.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403821622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 38 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62403821622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402021722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="62402021722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402021722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="23.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402021722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62402021722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800311622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="68800311622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800311622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800311622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800311622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="648105131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33368v209%20Multi-WR-WTB150-6481xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6481XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="648105131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/648105131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="648105131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="648105131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800811622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="64800811622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800811622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="13.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800811622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800811622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101011622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="66101011622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101011622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101011622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101011622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653114131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MS"/>
</gates>
<devices>
<device name="" package="653114131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653114131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="22.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653114131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653114131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653106131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Ivory
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;IR	1
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33373v209%20Multi-WR-WTB-6531xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6531XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="653106131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653106131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="12.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653106131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="653106131822"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900611021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="61900611021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900611021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900611021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900611021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68801011622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="68801011622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68801011622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="27.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68801011622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68801011622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665105131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="665105131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665105131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665105131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665105131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665305124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58873v209%206653xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_VERTICAL_SHROUDED_HEADER_6653XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="665305124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665305124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="665305124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="665305124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100811722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="66100811722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100811722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.02mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100811722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="8"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100811722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800911722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_1"/>
</gates>
<devices>
<device name="" package="68800911722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800911722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800911722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800911722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653115124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MS"/>
</gates>
<devices>
<device name="" package="653115124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653115124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="23.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653115124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653115124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000511722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="62000511722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000511722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000511722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000511722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620106131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="620106131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620106131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620106131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620106131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100421622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="66100421622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100421622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="9.96mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100421622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100421622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800811622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="68800811622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800811622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="22.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800811622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800811622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="64800211622" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33366v209%20Multi-WR-WTB150-6480xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_MALE_VERTICAL_SHROUDED_HEADER_6480XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="64800211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/64800211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="4.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="64800211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="64800211622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000911722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="62000911722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000911722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000911722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000911722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="679305124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.50 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33374v209%206793xx124022_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_50_SMT_MALE_VERTICAL_SHROUDED_HEADER_6793XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="679305124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/679305124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="679305124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="679305124022"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620108131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="620108131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620108131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620108131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620108131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000811622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="62000811622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000811622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000811622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000811622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="653102124022" prefix="J">
<description>&lt;b&gt;WR-WTB 1.25 mm SMT Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Ivory
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1.25 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33372v209%206531xx124022_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_25_SMT_MALE_VERTICAL_SHROUDED_HEADER_6531XX124022&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="653102124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/653102124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="7.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="653102124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.25mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="653102124022"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665102131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="665102131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665102131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665102131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665102131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900419521" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Top Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33347v209%206190xx19521_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_TOP_LOCKING_6190XX19521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="61900419521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900419521?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="10.16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900419521"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Top Locking"/>
<attribute name="VALUE" value="61900419521"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="62402021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="23.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62402021622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645004114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="645004114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645004114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="15.84mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645004114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645004114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403421622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="62403421622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403421622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="37.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403421622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62403421622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402421622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_1"/>
</gates>
<devices>
<device name="" package="62402421622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402421622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="27.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402421622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62402421622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665103131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="665103131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665103131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665103131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665103131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800611622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="68800611622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800611622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800611622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800611622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665108131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="665108131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665108131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665108131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665108131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402821622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2MT_1"/>
</gates>
<devices>
<device name="" package="62402821622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402821622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="31.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402821622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62402821622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403221622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2MT_1"/>
</gates>
<devices>
<device name="" package="62403221622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403221622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="35.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403221622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62403221622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000811722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	2 A
&lt;BR&gt;Working Voltage	125 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33352v209%206200xx11722_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="62000811722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000811722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="18mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000811722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62000811722"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100611622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="66100611622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100611622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="14.94mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100611622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100611622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402621622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="62402621622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402621622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="29.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402621622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62402621622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62001011622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="62001011622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001011622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62001011622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62001011622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403421722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="62403421722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403421722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="37.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403421722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62403421722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100821622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="66100821622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100821622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.12mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100821622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100821622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100911622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="66100911622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100911622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="22.56mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100911622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100911622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100621622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="66100621622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100621622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15.04mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100621622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100621622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="665106131822" prefix="J">
<description>&lt;b&gt;WR-WTB 1.00 mm SMT Male Horizontal Shrouded&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Beige
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
Compliance	RoHS
&lt;BR&gt;IR	1 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage [UL]	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Pitch	1 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58871v209%206651xx131822_Multi-Parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_1_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6651XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="665106131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/665106131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="665106131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="665106131822"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62402821722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2MT"/>
</gates>
<devices>
<device name="" package="62402821722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62402821722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="31.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62402821722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62402821722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MT_1"/>
</gates>
<devices>
<device name="" package="62403021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="33.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62403021622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800411722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33377v209%20Multi-WR-WTB250-6880xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_HORIZONTAL_MALE_SHROUDED_HEADER_6880XX11722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="68800411722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800411722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800411722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="68800411722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100211622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="66100211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="4.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100211622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62403021722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Horizontal Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Horizontal
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33359v209%20Family_WR-WTB_6240xx21722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_HORIZONTAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MT"/>
</gates>
<devices>
<device name="" package="62403021722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62403021722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="33.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62403021722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="62403021722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100711622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="66100711622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100711622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="17.48mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100711622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66100711622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645006114822" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Vertical Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33361v209%20Multi-WR-WTB396-6450xx114822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_LOCKING_HEADER_6450XX114822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="645006114822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645006114822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="23.76mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645006114822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="645006114822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800511622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="68800511622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800511622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="15mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800511622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800511622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101211622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MT"/>
</gates>
<devices>
<device name="" package="66101211622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101211622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="30.18mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101211622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101211622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="66101021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101021622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61901011021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="61901011021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61901011021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61901011021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61901011021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645003117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="645003117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645003117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="11.88mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645003117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645003117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62000511622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Top Locking
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33351v209%20Multi-WR-WTB200-6200xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="62000511622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000511622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="12mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000511622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62000511622"/>
<attribute name="WORKING-VOLTAGE" value="125V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="62401821622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm Male Dual Row Vertical Shrouded Header w. positive locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33358v209%20Family_WR-WTB_6240xx21622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_00_MALE_DUAL_ROW_VERTICAL_SHROUDED_HEADER_W_POSITIVE_LOCKING_6240XX21622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_1"/>
</gates>
<devices>
<device name="" package="62401821622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62401821622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="21.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62401821622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="62401821622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66100611722" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58906v209%20Multi-WR-WTB254-6610xx11722.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1722&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="66100611722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66100611722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="14.94mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66100611722"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66100611722"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689112131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS_1"/>
</gates>
<devices>
<device name="" package="689112131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689112131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="11.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689112131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689112131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101411622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MT"/>
</gates>
<devices>
<device name="" package="66101411622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101411622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="35.26mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101411622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101411622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101621622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="66101621622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101621622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="40.44mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101621622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101621622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68800711622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.50 mm “J” Type Vertical Male Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Brass
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-25 °C up to +85 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	800 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.5 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33376v209%20Multi-WR-WTB250-6880xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_50_J_TYPE_VERTICAL_MALE_SHROUDED_HEADER_6880XX11622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT_1"/>
</gates>
<devices>
<device name="" package="68800711622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/68800711622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="68800711622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="68800711622"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101421622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="66101421622">
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101421622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="35.36mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101421622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101421622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689108131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="689108131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689108131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="8.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689108131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689108131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101221622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="66101221622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101221622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="30.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101221622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101221622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689102131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="689102131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689102131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="3.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689102131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689102131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="645005117322" prefix="J">
<description>&lt;b&gt;WR-WTB 3.96 mm Male Right Angled Locking Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-2
&lt;BR&gt;Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	7 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	3.96 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61038v209%20Multi-WR-WTB396-6450xx117322.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_3_96_MALE_RIGHT_ANGLED_LOCKING_HEADER_6450XX117322&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="645005117322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/645005117322?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="19.8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="645005117322"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.96mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="645005117322"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689106131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="689106131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689106131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689106131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689106131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61900811021" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Right Angled Locking Header Bottom Locking&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Beige
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Right Angled Bottom Locking
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33344v209%206190xx11021_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_RIGHT_ANGLED_LOCKING_HEADER_BOTTOM_LOCKING&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="61900811021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61900811021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61900811021"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Right Angled Bottom Locking"/>
<attribute name="VALUE" value="61900811021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689103131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="689103131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689103131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="4.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689103131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689103131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66101611622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	co
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Phosphor Bronze
&lt;BR&gt;Contact Plating	Tin
&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	50 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Vertical
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58903v209%20Multi-WR-WTB254-6610xx11622.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16MT"/>
</gates>
<devices>
<device name="" package="66101611622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66101611622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="40.34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66101611622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66101611622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689110131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="689110131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689110131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="10.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689110131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689110131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689105131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="689105131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689105131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="6.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689105131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689105131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689104131822" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="689104131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689104131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689104131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="689104131822"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="620110131822" prefix="J">
<description>&lt;b&gt;WR-WTB 2.00 mm SMT Male Horizontal Shrouded Header&lt;/b&gt;&lt;BR&gt;


&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Beige 
&lt;BR&gt;Contact Material Copper Alloy 
&lt;BR&gt;Contact Plating Tin 
&lt;BR&gt;Contact Type Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage 800 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;cULus Approval E323964 
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tape and Reel 
&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33353v209%20Multi-WR-WTB200-6201xx131822.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WTB_2_00_SMT_MALE_HORIZONTAL_SHROUDED_HEADER_6201XX131822&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-07-05
&lt;BR&gt;2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="620110131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/620110131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="A"/>
<attribute name="L" value="24mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="620110131822"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="620110131822"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689302124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="689302124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689302124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="3.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689302124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689302124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66102021622" prefix="J">
<description>&lt;b&gt;WR-WTB 2.54 mm Male Vertical Shrouded Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:2.54 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Vertical
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Phosphor Bronze
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance: RoHS
&lt;BR&gt;IR:3A
&lt;BR&gt;Working Voltage:50 V (AC)
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Box
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58903v209%20Family_WR-WTB_6610xx11622_2%2054.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WTB_2_54_MALE_VERTICAL_SHROUDED_HEADER_GLOW_WIRE_PLASTIC_6610XXX1622&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-10-31
&lt;BR&gt;2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="66102021622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66102021622?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="50.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="66102021622"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66102021622"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689310124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="689310124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689310124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="10.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689310124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689310124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689312124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS_1"/>
</gates>
<devices>
<device name="" package="689312124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689312124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="11.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689312124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689312124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689306124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="689306124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689306124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689306124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689306124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689304124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="689304124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689304124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689304124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689304124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689303124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="689303124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689303124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="4.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689303124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689303124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689308124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="689308124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689308124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="8.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689308124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689308124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="689305124022" prefix="J">
<description>&lt;b&gt;WR-WTB 0.80 mm Male Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;Properties:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current: 0.5 A
&lt;BR&gt;Working Voltage: 30 V
&lt;BR&gt;Operating temperature: -25 °C to +85 °C
&lt;BR&gt;UL 94-V0
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Features:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Fine pitch
&lt;BR&gt;SMT soldering
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Microelectronic
&lt;BR&gt;Portable devices
&lt;BR&gt;Industry 4.0
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o841802v209%20Multi-WR-WTB080-689302124022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR-WTB_0_8_MALE_HEADER#/articles/WR-WTB_08_MM_MALE_SIZE_HORIZONTAL&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-03-06
&lt;BR&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="689305124022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/689305124022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="0.5A"/>
<attribute name="L" value="6.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="689305124022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="0.8mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="689305124022"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
