<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Resistors - Metal Plate Resistors - WRIS-PSMB&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-09-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WRIS-PSMB_1206_L3.2W1.6H0.28">
<description>&lt;B&gt;WRIS-PSMB Metal Plate Resistors
&lt;BR&gt;&lt;/B&gt;
&lt;BR&gt;Size : 12065, SMT, 2pins
&lt;BR&gt;LXWXHXFI=3.2X1.6X0.28X0.5</description>
</package>
<package name="WRIS-PSMB_2512_L6.3W3.1H0.35">
</package>
<package name="WRIS-PSMB_0603_L1.6W0.8H0.3">
<description>Hight= 0.3mm</description>
</package>
<package name="WRIS-PSMB_0603_L1.6W0.8H0.35">
<description>Hight= 0.35mm</description>
</package>
<package name="WRIS-PSMB_0805_L2W1.25H0.22">
</package>
</packages>
<symbols>
<symbol name="R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WRIS-PSMB_1206" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for enhanced current sensing up to 1 W
&lt;br&gt;Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 5 mΩ ‒ 10 mΩ
&lt;br&gt;Resistance tolerance: ±1%
&lt;br&gt;Rated Power: 0.33 W ‒ 1 W
&lt;br&gt;TCR: ±100 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0603 / 0805 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Motor control
&lt;br&gt;Battery pack
&lt;br&gt;DC/DC converter
&lt;br&gt;AC adapter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WRIS-PSMB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella 2025-09-24&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_L3.2W1.6H0.28" package="WRIS-PSMB_1206_L3.2W1.6H0.28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060732021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060732021?ae"/>
<attribute name="HEIGHT" value="0.28mm"/>
<attribute name="IR" value="10A"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060732021"/>
<attribute name="PRATED" value="1W"/>
<attribute name="R" value="10 mO"/>
<attribute name="SIZE" value="1206"/>
<attribute name="TCR-MAX" value="70ppm/°C"/>
<attribute name="TCR-MIN" value="-70ppm/°C"/>
<attribute name="VALUE" value="10 mO"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-PSMB_2512" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for enhanced current sensing up to 1 W
&lt;br&gt;Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 5 mΩ ‒ 10 mΩ
&lt;br&gt;Resistance tolerance: ±1%
&lt;br&gt;Rated Power: 0.33 W ‒ 1 W
&lt;br&gt;TCR: ±100 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0603 / 0805 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Motor control
&lt;br&gt;Battery pack
&lt;br&gt;DC/DC converter
&lt;br&gt;AC adapter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WRIS-PSMB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-09-24&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_L6.3W3.1H0.35" package="WRIS-PSMB_2512_L6.3W3.1H0.35">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060763005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060763005?ae"/>
<attribute name="HEIGHT" value="0.35mm"/>
<attribute name="IR" value="12A"/>
<attribute name="LENGTH" value="6.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060763005"/>
<attribute name="PRATED" value="1W"/>
<attribute name="R" value="7 mO"/>
<attribute name="SIZE" value="2512"/>
<attribute name="TCR-MAX" value="100ppm/°C"/>
<attribute name="TCR-MIN" value="100ppm/°C"/>
<attribute name="VALUE" value="7 mO"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-PSMB_0603" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for enhanced current sensing up to 1 W
&lt;br&gt;Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 5 mΩ ‒ 10 mΩ
&lt;br&gt;Resistance tolerance: ±1%
&lt;br&gt;Rated Power: 0.33 W ‒ 1 W
&lt;br&gt;TCR: ±100 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0603 / 0805 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Motor control
&lt;br&gt;Battery pack
&lt;br&gt;DC/DC converter
&lt;br&gt;AC adapter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WRIS-PSMB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-09-24&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_L1.6W0.8H0.3" package="WRIS-PSMB_0603_L1.6W0.8H0.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060716002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060716002?ae"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="IR" value="5.74A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060716002"/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="R" value="10 mO"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TCR-MAX" value="100ppm/°C"/>
<attribute name="TCR-MIN" value="-100ppm/°C"/>
<attribute name="VALUE" value="10 mO"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_L1.6W0.8H0.35" package="WRIS-PSMB_0603_L1.6W0.8H0.35">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060716001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060716001?ae"/>
<attribute name="HEIGHT" value="0.35mm"/>
<attribute name="IR" value="8.12A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060716001"/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="R" value="5 mO"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TCR-MAX" value="100ppm/°C"/>
<attribute name="TCR-MIN" value="-100ppm/°C"/>
<attribute name="VALUE" value="5 mO"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-PSMB_0805" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for enhanced current sensing up to 1 W
&lt;br&gt;Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 5 mΩ ‒ 10 mΩ
&lt;br&gt;Resistance tolerance: ±1%
&lt;br&gt;Rated Power: 0.33 W ‒ 1 W
&lt;br&gt;TCR: ±100 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0603 / 0805 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Motor control
&lt;br&gt;Battery pack
&lt;br&gt;DC/DC converter
&lt;br&gt;AC adapter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135743v209%20WRIS-PSMB_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WRIS-PSMB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-09-24&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_L2W1.25H0.22" package="WRIS-PSMB_0805_L2W1.25H0.22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060720003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060720003?ae"/>
<attribute name="HEIGHT" value="0.22mm"/>
<attribute name="IR" value="10A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060720003"/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="R" value="5 mO"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TCR-MAX" value="100ppm/°C"/>
<attribute name="TCR-MIN" value="-100ppm/°C"/>
<attribute name="VALUE" value="5 mO"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_580060720008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/580060720008?ae"/>
<attribute name="HEIGHT" value="0.22mm"/>
<attribute name="IR" value="7.07A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="580060720008"/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="R" value="10 mO"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TCR-MAX" value="100ppm/°C"/>
<attribute name="TCR-MIN" value="-100ppm/°C"/>
<attribute name="VALUE" value="10 mO"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
