<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Dip Switches - THT Dip Switch - WS-DITU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-01-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="418217270904A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,4Poles</description>
</package>
<package name="418217270906A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,6Poles</description>
</package>
<package name="418217270910A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,10Poles</description>
</package>
<package name="418217270908A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,8Poles</description>
</package>
<package name="418217270902A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,2Poles</description>
</package>
<package name="418217270903A">
<description>&lt;B&gt;WS-DITU&lt;/B&gt;&lt;BR&gt; Compact THT Right Angled with Raised Actuator 2.54 mm,3Poles</description>
</package>
</packages>
<symbols>
<symbol name="10POLES">
<description>This symbol is 10 pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="A10" direction="pas"/>
</symbol>
<symbol name="4POLES">
<description>This symbol is 4pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
</symbol>
<symbol name="6POLES">
<description>This symbol is 6pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
</symbol>
<symbol name="8POLES">
<description>This symbol is 8pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
</symbol>
<symbol name="3POLES">
<description>This symbol is 3pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
</symbol>
<symbol name="2POLES">
<description>This symbol is 2pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="418217270904A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418217270904A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270904A.pdf"/>
<attribute name="PART-NUMBER" value="418217270904A"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 44 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418217270910A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418217270910A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270910A.pdf"/>
<attribute name="PART-NUMBER" value="418217270910A"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 18 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418217270908A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418217270908A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270908A.pdf"/>
<attribute name="PART-NUMBER" value="418217270908A"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 23 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418217270906A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418217270906A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270906A.pdf"/>
<attribute name="PART-NUMBER" value="418217270906A"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 30 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418217270902A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418217270902A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270902A.pdf"/>
<attribute name="PART-NUMBER" value="418217270902A"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 82 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418217270903A" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DITU Compact THT Right Angled with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o93597v209%20Family_DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/"&gt;https://www.we-online.com/catalog/en/DITU_2_54_COMPACT_THT_RIGHT_ANGLED_WITH_RAISED_ACTUATOR_A_TYPE/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418217270903A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418217270903A.pdf"/>
<attribute name="PART-NUMBER" value="418217270903A"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 56 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
