<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Dip Switches - THT Dip Switch - WS-DITV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-03-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="418127160901">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,1poles</description>
</package>
<package name="418117270904">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,4 Pole</description>
</package>
<package name="418117270901">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,1Poles</description>
</package>
<package name="418117270907">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,7 Pole</description>
</package>
<package name="418127270909">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,9Poles</description>
</package>
<package name="418127160903">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,3poles</description>
</package>
<package name="418127270901">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,1Poles</description>
</package>
<package name="418117270909">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm, 9 Pole</description>
</package>
<package name="418127160909">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,9poles</description>
</package>
<package name="418127270902">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,2Poles</description>
</package>
<package name="418117170909">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 9 Pole</description>
</package>
<package name="418127270904">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,4Poles</description>
</package>
<package name="418117270903">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,3 Pole</description>
</package>
<package name="418127160905">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,5poles</description>
</package>
<package name="418127270907">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,7Poles</description>
</package>
<package name="418127270906">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,6Poles</description>
</package>
<package name="418117170905">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm,  5 Pole</description>
</package>
<package name="418127270910">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,10Poles</description>
</package>
<package name="418117170904">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 4 Pole</description>
</package>
<package name="418117170903">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 3 Pole</description>
</package>
<package name="418127270905">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,5Poles</description>
</package>
<package name="418117270908">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm, 8 Pole</description>
</package>
<package name="418127160910">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,10poles</description>
</package>
<package name="418117170907">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 7 Pole</description>
</package>
<package name="418127270903">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,3Poles</description>
</package>
<package name="418117270910">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,10 Pole</description>
</package>
<package name="418127160907">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,7poles</description>
</package>
<package name="418127160906">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,6poles</description>
</package>
<package name="418127160904">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,4poles</description>
</package>
<package name="418127160912">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,12poles</description>
</package>
<package name="418117170910">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 10 Pole</description>
</package>
<package name="418117170901">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 1 Pole</description>
</package>
<package name="418127160902">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,2poles</description>
</package>
<package name="418127270908">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,8Poles</description>
</package>
<package name="418127160908">
<description>&lt;b&gt;WS-DITV&lt;/b&gt; &lt;br&gt;Small Compact THT Flat Actuator with Top Tape 2.54 mm,8poles</description>
</package>
<package name="418117270905">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,5 Pole</description>
</package>
<package name="418117170902">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 2 Pole</description>
</package>
<package name="418117270912">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,12 Pole</description>
</package>
<package name="418127270912">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Small Compact THT with Raised Actuator 2.54 mm ,12Poles</description>
</package>
<package name="418117170908">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm,  8 Pole</description>
</package>
<package name="418117270902">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm,2 Pole</description>
</package>
<package name="418117170912">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 12 Poles</description>
</package>
<package name="418117170906">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Ccompact THT with Flat Actuator 2.54 mm, 7 Pole</description>
</package>
<package name="418117270906">
<description>&lt;b&gt;WS-DITV&lt;/b&gt;&lt;br&gt; Compact THT with Raised Actuator 2.54 mm, 6 Pole</description>
</package>
</packages>
<symbols>
<symbol name="1POLE">
<description>This symbol is 1pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="9POLES">
<description>This symbol is 9pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
</symbol>
<symbol name="4POLES">
<description>This symbol is 4pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
</symbol>
<symbol name="3POLES">
<description>This symbol is 3pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
</symbol>
<symbol name="7POLES">
<description>This symbol is 7pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
</symbol>
<symbol name="2POLES">
<description>This symbol is 2pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="6POLES">
<description>This symbol is 6pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
</symbol>
<symbol name="5POLES">
<description>This symbol is 5pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
</symbol>
<symbol name="10POLES">
<description>This symbol is 10 pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="A10" direction="pas"/>
</symbol>
<symbol name="8POLES">
<description>This symbol is 8pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
</symbol>
<symbol name="12POLES">
<description>This symbol is 12pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="418117270904" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418117270904">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270904.pdf"/>
<attribute name="PART-NUMBER" value="418117270904"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 45 "/>
<attribute name="VALUE" value="418117270904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270901" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418117270901">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270901.pdf"/>
<attribute name="PART-NUMBER" value="418117270901"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 130 "/>
<attribute name="VALUE" value="418117270901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270909" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418127270909">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270909.pdf"/>
<attribute name="PART-NUMBER" value="418127270909"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 21 "/>
<attribute name="VALUE" value="418127270909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270907" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418117270907">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270907.pdf"/>
<attribute name="PART-NUMBER" value="418117270907"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 26 "/>
<attribute name="VALUE" value="418117270907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160901" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418127160901">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160901.pdf"/>
<attribute name="PART-NUMBER" value="418127160901"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 145 "/>
<attribute name="VALUE" value="418127160901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160903" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418127160903">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160903.pdf"/>
<attribute name="PART-NUMBER" value="418127160903"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 59 "/>
<attribute name="VALUE" value="418127160903"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270901" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418127270901">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270901.pdf"/>
<attribute name="PART-NUMBER" value="418127270901"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 145 "/>
<attribute name="VALUE" value="418127270901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270909" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418117270909">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270909.pdf"/>
<attribute name="PART-NUMBER" value="418117270909"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 20 "/>
<attribute name="VALUE" value="418117270909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160909" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418127160909">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160909.pdf"/>
<attribute name="PART-NUMBER" value="418127160909"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 21 "/>
<attribute name="VALUE" value="418127160909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270902" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418127270902">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270902.pdf"/>
<attribute name="PART-NUMBER" value="418127270902"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 84 "/>
<attribute name="VALUE" value="418127270902"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170909" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418117170909">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170909.pdf"/>
<attribute name="PART-NUMBER" value="418117170909"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 20 "/>
<attribute name="VALUE" value="418117170909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270904" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418127270904">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270904.pdf"/>
<attribute name="PART-NUMBER" value="418127270904"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 45 "/>
<attribute name="VALUE" value="418127270904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270903" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418117270903">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270903.pdf"/>
<attribute name="PART-NUMBER" value="418117270903"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 56 "/>
<attribute name="VALUE" value="418117270903"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270907" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418127270907">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270907.pdf"/>
<attribute name="PART-NUMBER" value="418127270907"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 27 "/>
<attribute name="VALUE" value="418127270907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160905" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418127160905">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160905.pdf"/>
<attribute name="PART-NUMBER" value="418127160905"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 37 "/>
<attribute name="VALUE" value="418127160905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270906" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418127270906">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270906.pdf"/>
<attribute name="PART-NUMBER" value="418127270906"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 31 "/>
<attribute name="VALUE" value="418127270906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170905" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418117170905">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170905.pdf"/>
<attribute name="PART-NUMBER" value="418117170905"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 36 "/>
<attribute name="VALUE" value="418117170905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270910" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418127270910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270910.pdf"/>
<attribute name="PART-NUMBER" value="418127270910"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 19 "/>
<attribute name="VALUE" value="418127270910"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170904" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418117170904">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170904.pdf"/>
<attribute name="PART-NUMBER" value="418117170904"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 45 "/>
<attribute name="VALUE" value="418117170904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170903" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418117170903">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170903.pdf"/>
<attribute name="PART-NUMBER" value="418117170903"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 56 "/>
<attribute name="VALUE" value="418117170903"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270905" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418127270905">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270905.pdf"/>
<attribute name="PART-NUMBER" value="418127270905"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 37 "/>
<attribute name="VALUE" value="418127270905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270908" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418117270908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270908.pdf"/>
<attribute name="PART-NUMBER" value="418117270908"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 23 "/>
<attribute name="VALUE" value="418117270908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170907" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418117170907">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170907.pdf"/>
<attribute name="PART-NUMBER" value="418117170907"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 26 "/>
<attribute name="VALUE" value="418117170907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160910" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418127160910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160910.pdf"/>
<attribute name="PART-NUMBER" value="418127160910"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 19 "/>
<attribute name="VALUE" value="418127160910"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270903" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418127270903">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270903.pdf"/>
<attribute name="PART-NUMBER" value="418127270903"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 59 "/>
<attribute name="VALUE" value="418127270903"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270910" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418117270910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270910.pdf"/>
<attribute name="PART-NUMBER" value="418117270910"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 19 "/>
<attribute name="VALUE" value="418117270910"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160907" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418127160907">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160907.pdf"/>
<attribute name="PART-NUMBER" value="418127160907"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 27 "/>
<attribute name="VALUE" value="418127160907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160906" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418127160906">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160906.pdf"/>
<attribute name="PART-NUMBER" value="418127160906"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 31 "/>
<attribute name="VALUE" value="418127160906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160904" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418127160904">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160904.pdf"/>
<attribute name="PART-NUMBER" value="418127160904"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 45 "/>
<attribute name="VALUE" value="418127160904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160912" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418127160912">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160912.pdf"/>
<attribute name="PART-NUMBER" value="418127160912"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 16 "/>
<attribute name="VALUE" value="418127160912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170910" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418117170910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170910.pdf"/>
<attribute name="PART-NUMBER" value="418117170910"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 19 "/>
<attribute name="VALUE" value="418117170910"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170901" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418117170901">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170901.pdf"/>
<attribute name="PART-NUMBER" value="418117170901"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 130 "/>
<attribute name="VALUE" value="418117170901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160902" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418127160902">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160902.pdf"/>
<attribute name="PART-NUMBER" value="418127160902"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 84 "/>
<attribute name="VALUE" value="418127160902"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270908" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418127270908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270908.pdf"/>
<attribute name="PART-NUMBER" value="418127270908"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 24 "/>
<attribute name="VALUE" value="418127270908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127160908" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;
&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77514v209%20Family_WS-DITV_THT_FLAT_ACTUATOR_4181271609xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418127160908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127160908.pdf"/>
<attribute name="PART-NUMBER" value="418127160908"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 24 "/>
<attribute name="VALUE" value="418127160908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270905" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418117270905">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270905.pdf"/>
<attribute name="PART-NUMBER" value="418117270905"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 36 "/>
<attribute name="VALUE" value="418117270905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170902" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418117170902">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170902.pdf"/>
<attribute name="PART-NUMBER" value="418117170902"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 82 "/>
<attribute name="VALUE" value="418117170902"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270912" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418117270912">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270912.pdf"/>
<attribute name="PART-NUMBER" value="418117270912"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 15 "/>
<attribute name="VALUE" value="418117270912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418127270912" prefix="S">
<description>&lt;B&gt;WS-DITV Small Compact THT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA66
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77465v209%20Family_WS-DITV_THT_RAISED_ACTUATOR_4181272709xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_SMALL_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418127270912">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418127270912.pdf"/>
<attribute name="PART-NUMBER" value="418127270912"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 16 "/>
<attribute name="VALUE" value="418127270912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170908" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418117170908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170908.pdf"/>
<attribute name="PART-NUMBER" value="418117170908"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 23 "/>
<attribute name="VALUE" value="418117170908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270902" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418117270902">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270902.pdf"/>
<attribute name="PART-NUMBER" value="418117270902"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 82 "/>
<attribute name="VALUE" value="418117270902"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170912" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418117170912">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170912.pdf"/>
<attribute name="PART-NUMBER" value="418117170912"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 15 "/>
<attribute name="VALUE" value="418117170912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117170906" prefix="S">
<description>&lt;B&gt;WS-DITV Ccompact THT with Flat Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76752v209%20Family_WS-DITV_4181171709xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-23&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418117170906">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117170906.pdf"/>
<attribute name="PART-NUMBER" value="418117170906"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 30 "/>
<attribute name="VALUE" value="418117170906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418117270906" prefix="S">
<description>&lt;B&gt;WS-DITV Compact THT with Raised Actuator 2.54 mm  
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:800 g
&lt;BR&gt;Electrical Life:2000 Cycles
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PBT
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Red
&lt;BR&gt;Base Material:PBT
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PBT
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tube&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60896v209%20DITV_418117270908A_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-22&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418117270906">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418117270906.pdf"/>
<attribute name="PART-NUMBER" value="418117270906"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 30 "/>
<attribute name="VALUE" value="418117270906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
