<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - Micro Switches - WS-MITV&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="463092370402">
<description>&lt;B&gt;WS-MITV THT Terminal with Lever Micro Switch, 12.8 x 5.8 mm</description>
</package>
<package name="463092691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463091370403">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever Micro Switch, 19.8 x 6.4mm</description>
</package>
<package name="463093370403">
<description>&lt;b&gt;WS-MITV THT Terminal with Roller Lever Micro Switch, 19.8 x 6.4mm</description>
</package>
<package name="463093370402">
<description>&lt;B&gt;WS-MITV THT Terminal with Roller Lever Micro Switch, 12.8 x 5.8 mm</description>
</package>
<package name="463091691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Actuator, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463093691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Roller Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463092370403">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever Micro Switch, 19.8 x 6.4mm</description>
</package>
<package name="463091370402">
<description>&lt;B&gt;WS-MITV THT Terminal with Actuator Micro Switch, 12.8 x 5.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-MITV">
<description>WS-MITV</description>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="463092370402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.55 mm
&lt;BR&gt;Movement Differential	0.5 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o144915v209%20Single_WE-MITV_463093370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o144915v209%20Single_WE-MITV_463093370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_12_8X5_8_THT__LEVER_LEFT_55GF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_12_8X5_8_THT__LEVER_LEFT_55GF&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463092370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463092370402?ae"/>
<attribute name="OPERATING-POSITION" value="6.8mm"/>
<attribute name="OPERATION-FORCE" value="80g"/>
<attribute name="PART-NUMBER" value="463092370402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463092370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463092691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.55 mm
&lt;BR&gt;Movement Differential	0.5 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o320310v209 multi-WS-MITV-463092691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o320310v209 multi-WS-MITV-463092691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_THT_TERMINAL_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_THT_TERMINAL_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463092691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463092691402?ae"/>
<attribute name="OPERATING-POSITION" value="6.8mm"/>
<attribute name="OPERATION-FORCE" value="80g"/>
<attribute name="PART-NUMBER" value="463092691402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463092691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463091370403" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever Micro Switch, 19.8 x 6.4mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Actuator Material	PBT
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Moveable Contact Material	Silver
&lt;br&gt;Stationary Contact Material	Silver
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	0 °C up to +105 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval	E483308
&lt;br&gt;ENEC 15 Approval	ENEC-04881

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Contact Resistance Initial	30 mΩ
&lt;br&gt;Contact Resistance After Life Test	5 Ω
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	100000 Cycles
&lt;br&gt;Schematic	SPDT
&lt;br&gt;Over travel	0.6 mm
&lt;br&gt;Movement Differential	0.4 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray


&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o838187v209 multi-WS-MITV-463091370403.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o838187v209 multi-WS-MITV-463091370403.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_MITV_THT_TERMINAL_WITH_ACTUATOR_MICRO_SWITCH_19_8_X_6_4_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_MITV_THT_TERMINAL_WITH_ACTUATOR_MICRO_SWITCH_19_8_X_6_4_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463091370403">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463091370403?ae"/>
<attribute name="OPERATING-POSITION" value="8.4mm"/>
<attribute name="OPERATION-FORCE" value="240g"/>
<attribute name="PART-NUMBER" value="463091370403"/>
<attribute name="SIZE" value="19.8 x 6.4mm"/>
<attribute name="VALUE" value="463091370403"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463093370403" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Roller Lever Micro Switch, 19.8 x 6.4mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Actuator Material	PBT
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Moveable Contact Material	Silver
&lt;br&gt;Stationary Contact Material	Silver
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	0 °C up to +105 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval	E483308
&lt;br&gt;ENEC 15 Approval	ENEC-04881

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Contact Resistance Initial	30 mΩ
&lt;br&gt;Contact Resistance After Life Test	5 Ω
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	100000 Cycles
&lt;br&gt;Schematic	SPDT
&lt;br&gt;Over travel	0.8 mm
&lt;br&gt;Movement Differential	0.8 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray


&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828330v209 multi-WS-MITV-463093370403.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828330v209 multi-WS-MITV-463093370403.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_MITV_THT_TERMINAL_WITH_ROLLER_LEVER_MICRO_SWITCH_19_8_X_6_4_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_MITV_THT_TERMINAL_WITH_ROLLER_LEVER_MICRO_SWITCH_19_8_X_6_4_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463093370403">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463093370403?ae"/>
<attribute name="OPERATING-POSITION" value="14.9mm"/>
<attribute name="OPERATION-FORCE" value="55g"/>
<attribute name="PART-NUMBER" value="463093370403"/>
<attribute name="SIZE" value="19.8 x 6.4mm"/>
<attribute name="VALUE" value="463093370403"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463093370402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Roller Lever Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.55 mm
&lt;BR&gt;Movement Differential	0.5 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o144911v209%20Single_WE-MITV_463092370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o144911v209%20Single_WE-MITV_463092370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_12_8X5_8_THT_ROLLER_LEVER_RIGHT_55GF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_12_8X5_8_THT_ROLLER_LEVER_RIGHT_55GF&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463093370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463093370402?ae"/>
<attribute name="OPERATING-POSITION" value="13mm"/>
<attribute name="OPERATION-FORCE" value="80g"/>
<attribute name="PART-NUMBER" value="463093370402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463093370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463091691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Actuator, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.25 mm
&lt;BR&gt;Movement Differential	0.12 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o320306v209 multi-WS-MITV-463091691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o320306v209 multi-WS-MITV-463091691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_THT_TERMINAL_ACTUATOR_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_THT_TERMINAL_ACTUATOR_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463091691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463091691402?ae"/>
<attribute name="OPERATING-POSITION" value="5.5mm"/>
<attribute name="OPERATION-FORCE" value="150g"/>
<attribute name="PART-NUMBER" value="463091691402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463091691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463092370403" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever Micro Switch, 19.8 x 6.4mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Actuator Material	PBT
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Moveable Contact Material	Silver
&lt;br&gt;Stationary Contact Material	Silver
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	0 °C up to +105 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Certification
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval	E483308
&lt;br&gt;ENEC 15 Approval	ENEC-04881

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Contact Resistance Initial	30 mΩ
&lt;br&gt;Contact Resistance After Life Test	5 Ω
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	100000 Cycles
&lt;br&gt;Schematic	SPDT
&lt;br&gt;Over travel	1 mm
&lt;br&gt;Movement Differential	1.2 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray


&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828326v209 multi-WS-MITV-463092370403.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828326v209 multi-WS-MITV-463092370403.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_MITV_THT_TERMINAL_WITH_LEVER_MICRO_SWITCH_19_8_X_6_4__MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_MITV_THT_TERMINAL_WITH_LEVER_MICRO_SWITCH_19_8_X_6_4__MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463092370403">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463092370403?ae"/>
<attribute name="OPERATING-POSITION" value="9mm"/>
<attribute name="OPERATION-FORCE" value="55g"/>
<attribute name="PART-NUMBER" value="463092370403"/>
<attribute name="SIZE" value="19.8 x 6.4mm"/>
<attribute name="VALUE" value="463092370403"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463091370402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Actuator Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.25 mm
&lt;BR&gt;Movement Differential	0.12 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o144880v209%20Single_WE-MITV_463091370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o144880v209%20Single_WE-MITV_463091370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_12_8X5_8_THT_ACTUATOR_LEFT_240GF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_12_8X5_8_THT_ACTUATOR_LEFT_240GF&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463091370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463091370402?ae"/>
<attribute name="OPERATING-POSITION" value="5.5mm"/>
<attribute name="OPERATION-FORCE" value="150g"/>
<attribute name="PART-NUMBER" value="463091370402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463091370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463093691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Roller Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material	PBT
&lt;BR&gt; Actuator Flammability Rating	UL94 V-0
&lt;BR&gt; Frame Material	PBT
&lt;BR&gt; Frame Flammability Rating	UL94 V-0
&lt;BR&gt; Moveable Contact Material	Silver
&lt;BR&gt; Stationary Contact Material	Silver
&lt;BR&gt; Terminal Material	Copper Alloy
&lt;BR&gt; Terminal Plating	Silver
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;General Information
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	30 mΩ
&lt;BR&gt;Contact Resistance After Life Test	1 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life	10000 Cycles
&lt;BR&gt;Schematic	SPDT
&lt;BR&gt;Over travel	0.55 mm
&lt;BR&gt;Movement Differential	0.5 mm
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Certification&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E483308
&lt;BR&gt;ENEC 15 Approval	ENEC-03305
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o320308v209%20multi-WS-MITV-463093691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o320308v209%20multi-WS-MITV-463093691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MITV_THT_TERMINAL_ROLLER_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MITV_THT_TERMINAL_ROLLER_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463093691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/463093691402?ae"/>
<attribute name="OPERATING-POSITION" value="13mm"/>
<attribute name="OPERATION-FORCE" value="80g"/>
<attribute name="PART-NUMBER" value="463093691402"/>
<attribute name="SIZE" value="12.8 x 5.8 mm"/>
<attribute name="VALUE" value="463093691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
