<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Rotary Switches - WS-ROTU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="42942752091X_16POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt;&lt;br&gt; THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm</description>
</package>
<package name="42942752091X_10POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt;&lt;br&gt; THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm</description>
</package>
<package name="42942732091X_10POS">
<description>&lt;b&gt;WS-ROTU &lt;/b&gt;&lt;br&gt;THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm</description>
</package>
<package name="42842732091X_10POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt; &lt;br&gt;THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm</description>
</package>
<package name="42842732091X_16POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt; &lt;br&gt;THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm</description>
</package>
<package name="42842752091X_16POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt; &lt;br&gt;THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm</description>
</package>
<package name="42842752091X_10POS">
<description>&lt;b&gt;WS-ROTU&lt;/b&gt; &lt;br&gt;THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm</description>
</package>
<package name="42942732091X_16POS">
<description>&lt;b&gt;WS-ROTU &lt;/b&gt;&lt;br&gt;THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-ROTX">
<description>WS-ROTX</description>
<pin name="1" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="429427520917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427520917.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="429427520917"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427520916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427520916.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="429427520916"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427520911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427520911.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="429427520911"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427320911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427320911.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="429427320911"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427520910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 5.08 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61153v209%20Family_WS-ROTU_4294275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427520910.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="429427520910"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427320910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427320910.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="429427320910"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427320910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427320910.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428427320910"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427320916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427320916.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428427320916"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427320911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427320911.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428427320911"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427520917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427520917.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428427520917"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427520916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427520916.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428427520916"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427520911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427520911.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428427520911"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427520910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Cross Type Actuator, 2.54 mm Pitch, 10x10 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61145v209%20Family_WS-ROTU_4284275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_CROSS_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427520910.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428427520910"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427320917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427320917.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="429427320917"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="429427320916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 5.08 mm Pitch, 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61133v209%20Family_WS_RAT_10x10_THT_42942732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_5_08/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42942732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/429427320916.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="429427320916"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428427320917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTU THT Rotary Switch Right Angled with Arrow Type Actuator, 2.54 mm Pitch, 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61126v209%20Family_WS_RAT_10x10_THT_42842732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/"&gt;https://www.we-online.com/catalog/en/ROTU_10X10_WASHABLE_THT_RIGHT_ANGLED_ARROW_TYPE_PITCH_2_54/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42842732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/428427320917.pdf"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428427320917"/>
<attribute name="QTY" value="50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
