<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - Rotary Switches - WS-ROTV&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-03-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="42854732091X_16POS">
<description>&lt;B&gt;WS-ROTV&lt;/B&gt;&lt;BR&gt; THT Rotary Switch with Arrow Type Actuator 7x7 mm</description>
</package>
<package name="42852742091X_10POS">
<description>&lt;B&gt;WS-ROTV &lt;/B&gt;&lt;BR&gt;THT Rotary Switch with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="428517510911">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm</description>
</package>
<package name="428517510917">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm</description>
</package>
<package name="42854732091X_10POS">
<description>&lt;B&gt;WS-ROTV&lt;/B&gt;&lt;BR&gt; THT Rotary Switch with Arrow Type Actuator 7x7 mm</description>
</package>
<package name="428517510910">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm</description>
</package>
<package name="42852732090X_08POS">
<description>&lt;B&gt;WS-ROTV &lt;/B&gt;&lt;BR&gt;THT Rotary Switch with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="428517510916">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm</description>
</package>
<package name="428517310917">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="42852752091X_10POS">
<description>&lt;B&gt;WS-ROTV&lt;/B&gt; &lt;BR&gt;THT Rotary Switch with Cross Type Actuator 10x10 mm</description>
</package>
<package name="42852732091X_16POS">
<description>&lt;B&gt;WS-ROTV &lt;/B&gt;&lt;BR&gt;THT Rotary Switch with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="42852732091X_10POS">
<description>&lt;B&gt;WS-ROTV &lt;/B&gt;&lt;BR&gt;THT Rotary Switch with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="428517310916">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="42852752091X_16POS">
<description>&lt;B&gt;WS-ROTV&lt;/B&gt; &lt;BR&gt;THT Rotary Switch with Cross Type Actuator 10x10 mm</description>
</package>
<package name="428517310910">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="428517310911">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm</description>
</package>
<package name="42852752090X_08POS">
<description>&lt;B&gt;WS-ROTV&lt;/B&gt; &lt;BR&gt;THT Rotary Switch with Cross Type Actuator 10x10 mm</description>
</package>
<package name="42852742091X_16POS">
<description>&lt;B&gt;WS-ROTV &lt;/B&gt;&lt;BR&gt;THT Rotary Switch with Arrow Type Actuator 10x10 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-ROTX">
<description>WS-ROTX</description>
<pin name="1" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WS-ROTX_1COM">
<description>WS-ROTX</description>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="428547320916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 7x7 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :100 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material：LCP
&lt;BR&gt;Actuator Flammability Rating：UL94 V-0
&lt;BR&gt;Actuator Color：Grey; Ivory; Orange; Red
&lt;BR&gt;Base Material：LCP
&lt;BR&gt;Base Flammability Rating：UL94 V-0
&lt;BR&gt;Terminal Plating：Gold
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;VR：42 V (DC)
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：25000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-60 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42854732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428547320916?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428547320916"/>
<attribute name="QTY" value="70"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428547320917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 7x7 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :100 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material：LCP
&lt;BR&gt;Actuator Flammability Rating：UL94 V-0
&lt;BR&gt;Actuator Color：Grey; Ivory; Orange; Red
&lt;BR&gt;Base Material：LCP
&lt;BR&gt;Base Flammability Rating：UL94 V-0
&lt;BR&gt;Terminal Plating：Gold
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;VR：42 V (DC)
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：25000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-60 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42854732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428547320917?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428547320917"/>
<attribute name="QTY" value="70"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527420911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Shaft Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Shaft Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Shaft Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Shaft Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852742091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527420911?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527420911"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527420910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Shaft Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Shaft Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Shaft Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Shaft Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852742091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527420910?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527420910"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517510911" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Cross Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517510911">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Ivory"/>
<attribute name="CODE" value="Complement Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517510911?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value=" 428517510911 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517510917" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Cross Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517510917">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Ivory"/>
<attribute name="CODE" value="Complement Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517510917?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value=" 428517510917 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428547320911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 7x7 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :100 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material：LCP
&lt;BR&gt;Actuator Flammability Rating：UL94 V-0
&lt;BR&gt;Actuator Color：Grey; Ivory; Orange; Red
&lt;BR&gt;Base Material：LCP
&lt;BR&gt;Base Flammability Rating：UL94 V-0
&lt;BR&gt;Terminal Plating：Gold
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;VR：42 V (DC)
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：25000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-60 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42854732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428547320911?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428547320911"/>
<attribute name="QTY" value="70"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428547320910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 7x7 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :100 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material：LCP
&lt;BR&gt;Actuator Flammability Rating：UL94 V-0
&lt;BR&gt;Actuator Color：Grey; Ivory; Orange; Red
&lt;BR&gt;Base Material：LCP
&lt;BR&gt;Base Flammability Rating：UL94 V-0
&lt;BR&gt;Terminal Plating：Gold
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;VR：42 V (DC)
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：25000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-60 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55750v209%20Family_WS-ROtV_THT_Rotary_Switch_428547320910.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_7X7_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42854732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428547320910?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428547320910"/>
<attribute name="QTY" value="70"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320909" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732090X_08POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320909?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 8 "/>
<attribute name="PART-NUMBER" value="428527320909"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320908" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732090X_08POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320908?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 8 "/>
<attribute name="PART-NUMBER" value="428527320908"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517510910" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Cross Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517510910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Dark Grey"/>
<attribute name="CODE" value="Real Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517510910?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value=" 428517510910 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517510916" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Cross Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Cross Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783899v209%20Family-WS-ROTV-42851751091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_CROSS_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517510916">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Dark Grey"/>
<attribute name="CODE" value="Real Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517510916?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value=" 428517510916 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517310917" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Arrow Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517310917">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Ivory"/>
<attribute name="CODE" value="Complement Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517310917?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value=" 428517310917 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520911?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527520911"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520910?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527520910"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320917?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527320917"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320916?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527320916"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320911" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320911?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527320911"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517310916" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Arrow Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517310916">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Dark Grey"/>
<attribute name="CODE" value="Real Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517310916?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value=" 428517310916 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527320910" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Arrow Type Actuator 10x10 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Arrow Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Arrow Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Arrow Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55752v209%20Family_WS_RAT_10x10_THT_42852732091x_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_ARROW_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852732091X_10POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527320910?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value="428527320910"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520916?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527520916"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520917?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527520917"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517310910" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Arrow Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517310910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Dark Grey"/>
<attribute name="CODE" value="Real Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517310910?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value=" 428517310910 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428517310911" prefix="S">
<description>&lt;b&gt;WS-ROTV THT IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm&lt;br&gt;

&lt;br&gt;Material Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Cover Material	PA66
&lt;br&gt;Cover Flammability Rating	UL94 V-0
&lt;br&gt;Base Material	PA66
&lt;br&gt;Base Flammability Rating	UL94 V-0
&lt;br&gt;Actuator Material	POM
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Gold

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	Yes
&lt;br&gt;Ingress Protection Code	IP67
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	200 mA
&lt;br&gt;VR	42 V (DC)
&lt;br&gt;Contact Resistance Initial	80 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Electrical Life	10000 Steps
&lt;br&gt;Actuator Type	Arrow Type
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783849v209%20Family-WS-ROTV-42851731091x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_ROTV_THT_IP67_ROTARY_SWITCHES_4_X_1_TERMINAL_WITH_ARROW_TYPE_ACTUATOR_10_X_10_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-29&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX_1COM"/>
</gates>
<devices>
<device name="" package="428517310911">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Ivory"/>
<attribute name="CODE" value="Complement Code"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428517310911?ae"/>
<attribute name="INGRESS-PROTECTION-CODE" value="IP67"/>
<attribute name="NUMBER-OF-POSITION" value=" 10 "/>
<attribute name="PART-NUMBER" value=" 428517310911 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520908" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752090X_08POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520908?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 8 "/>
<attribute name="PART-NUMBER" value="428527520908"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527520909" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Cross Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Cross Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Cross Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Cross Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55754v209%20Family_WS-ROTV_THT_Rotary_Switch_4285275209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_CROSS_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852752090X_08POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527520909?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 8 "/>
<attribute name="PART-NUMBER" value="428527520909"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527420917" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Shaft Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Shaft Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Shaft Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Shaft Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852742091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527420917?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527420917"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="428527420916" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-ROTV THT Rotary Switch with Shaft Type Actuator 10x10 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : PA66
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1 :150 mA
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Materia:POM
&lt;BR&gt;Actuator Flammability Rating:UL94 HB
&lt;BR&gt;Actuator Color:Dark Grey; Ivory
&lt;BR&gt;Base Material:PA66
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;Actuator Type:Shaft Type
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;b&gt;Additional&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:150 mA
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life：10000 Steps
&lt;BR&gt;Actuator Type：Shaft Type
&lt;BR&gt;Code：Complement Code; Real Code
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Tableadditional&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Type：Shaft Type
&lt;BR&gt;Washable：Yes
&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61108v209%20Family_WS-ROTV_10x10mm_washable_THT_Rotary_Switch_4285274209xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/"&gt;https://www.we-online.com/catalog/en/ROTV_10X10_WASHABLE_THT_SHAFT_TYPE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-24
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ROTX"/>
</gates>
<devices>
<device name="" package="42852742091X_16POS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/428527420916?ae"/>
<attribute name="NUMBER-OF-POSITION" value=" 16 "/>
<attribute name="PART-NUMBER" value="428527420916"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
