<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Tact Switches - WS-TASU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-01-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="434331013822">
<description>&lt;B&gt;WS-TASU&lt;/B&gt;&lt;BR&gt; SMT Tact Switch 3.5x2.9 mm side push,4Pins</description>
</package>
<package name="4343X30458XX">
<description>&lt;b&gt;WS-TASU&lt;/b&gt;&lt;br&gt;3.5x4.7 mm side push J-Bend SMD Tact Switch, 4 pins</description>
</package>
<package name="4363X30458XX">
<description>&lt;b&gt;WS-TASU&lt;/b&gt;&lt;br&gt;3.5x4.7 mm side push J-Bend SMD Tact Switch with boss design, 4 pins</description>
</package>
<package name="434381035816">
<description>&lt;b&gt;WS-TASU&lt;/b&gt;&lt;br&gt; SMT Tact Switch 6.2x3.0 mm side push,6.2x3.0x3.5mm</description>
</package>
<package name="4363X10458XX">
<description>&lt;b&gt;WS-TASU&lt;/b&gt;&lt;br&gt;3.5x4.7 mm side push SMD Tact Switch with boss design, 4 pins</description>
</package>
<package name="436333033816">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch with Boss Design 4.5 x 3.4mm side push 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 4.5 x 3.4 x 3.3mm</description>
</package>
<package name="4343X10458XX">
<description>&lt;b&gt;WS-TASU&lt;/b&gt;&lt;br&gt;3.5x4.7 mm side push SMD Tact Switch, 4 pins</description>
</package>
</packages>
<symbols>
<symbol name="WS-TASX_4P">
<description>WS-TASU,4Pins</description>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WS_TASU_4P1">
<description>WS-TASU,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="436333033816">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="WS-TASX_2P">
<description>WS-TASX_2P</description>
<pin name="1"/>
<pin name="2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="434331013822" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch 3.5x2.9 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color:White22222
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:Black;
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3500
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.2mm
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64622v209%20Family_WS-TASU_434331013822_c.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64622v209%20Family_WS-TASU_434331013822_c.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X2_9_SMD_SIDE_PUSH/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X2_9_SMD_SIDE_PUSH/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS_TASU_4P1"/>
</gates>
<devices>
<device name="" package="434331013822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3 5"/>
<connect gate="G$1" pin="4" pad="4 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434331013822.pdf"/>
<attribute name="H" value="1.35mm"/>
<attribute name="OPERATION-FORCE" value="220g"/>
<attribute name="PART-NUMBER" value="434331013822"/>
<attribute name="QTY" value=" 3500 "/>
<attribute name="VALUE" value="434331013822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434353045816" prefix="S">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25mm,0.3mm
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61081v209%20Family_WS_TUS_Normal_SMD_J-Bend_4343x30458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61081v209%20Family_WS_TUS_Normal_SMD_J-Bend_4343x30458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4343X30458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434353045816.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434353045816"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="434353045816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="436353045816" prefix="S">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch with Boss Design 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:Black;
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25 mm; 0.3 mm
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH_BOSS_DESIGN/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH_BOSS_DESIGN/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4363X30458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/436353045816.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="436353045816"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="436353045816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434381035816" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch 6.2x3.0 mm side push
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Blue 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 15 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 2000 
&lt;br&gt;
&lt;br&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;Electrical Life:1000000 Times
&lt;br&gt;Stroke :0.15 mm&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158918v209%20WS-TASU-434381035816.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158918v209%20WS-TASU-434381035816.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASU_SMT_TACT_SWITCH_6_2_x_3_0/"&gt;https://www.we-online.com/catalog/en/WS_TASU_SMT_TACT_SWITCH_6_2_x_3_0/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434381035816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434381035816.pdf"/>
<attribute name="H" value="3.5mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434381035816"/>
<attribute name="QTY" value=" 2000 "/>
<attribute name="VALUE" value="434381035816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="436333045822" prefix="S">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch with Boss Design 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:Black;
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25 mm; 0.3 mm
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH_BOSS_DESIGN/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH_BOSS_DESIGN/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4363X30458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/436333045822.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="220g"/>
<attribute name="PART-NUMBER" value="436333045822"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="436333045822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="436333033816" prefix="S">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch with Boss Design 4.5 x 3.4mm side push
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Copper Alloy 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material HTN 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black 
&lt;br&gt;Frame Material HTN 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 500 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Electrical Life 100000 Cycles 
&lt;br&gt;Stroke (Value) 0.2 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable No 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o64618v209%20Family_WS-TASU_J-Bend_SMD_Tact_Switch_with_boss_design_436353045816.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/WS-TASU_J-BEND_SMT_TACT_SWITCH_SIDE_PUSH"&gt;https://www.we-online.de/katalog/en/WS-TASU_J-BEND_SMT_TACT_SWITCH_SIDE_PUSH&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2021-01-25&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="436333033816"/>
</gates>
<devices>
<device name="" package="436333033816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/436333033816.pdf"/>
<attribute name="H" value="3.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="436333033816"/>
<attribute name="VALUE" value="436333033816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="436331045822" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch with Boss Design 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:Black;White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25 mm; 0.3 mm
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61089v209%20Family_WS_TUS_Normal_SMD_J-Bend_4363x10458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61089v209%20Family_WS_TUS_Normal_SMD_J-Bend_4363x10458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH_BOSS_DESIGN/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH_BOSS_DESIGN/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4363X10458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/436331045822.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="220g"/>
<attribute name="PART-NUMBER" value="436331045822"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="436331045822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434333045822" prefix="S">
<description>&lt;b&gt;WS-TASU J-Bend SMT Tact Switch 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25mm,0.3mm
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61081v209%20Family_WS_TUS_Normal_SMD_J-Bend_4343x30458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61081v209%20Family_WS_TUS_Normal_SMD_J-Bend_4343x30458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_J-BEND_SIDE_PUSH/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4343X30458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434333045822.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="220g"/>
<attribute name="PART-NUMBER" value="434333045822"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="434333045822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434331045822" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61072v209%20Family_WS_TUS_Normal_SMD_Side-Push_4343x10458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61072v209%20Family_WS_TUS_Normal_SMD_Side-Push_4343x10458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4343X10458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434331045822.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="220g"/>
<attribute name="PART-NUMBER" value="434331045822"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="434331045822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="436351045816" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch with Boss Design 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:Black;White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Stroke:0.25 mm; 0.3 mm
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61089v209%20Family_WS_TUS_Normal_SMD_J-Bend_4363x10458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61089v209%20Family_WS_TUS_Normal_SMD_J-Bend_4363x10458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH_BOSS_DESIGN/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH_BOSS_DESIGN/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4363X10458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/436351045816.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="436351045816"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="436351045816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434351045816" prefix="S">
<description>&lt;b&gt;WS-TASU SMT Tact Switch 4.7x3.5 mm side push 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material:PA46
&lt;br&gt;Actuator Flammability Rating: UL94 HB
&lt;br&gt;Actuator Color: Black; White
&lt;br&gt;Frame Material: PA46
&lt;br&gt;Frame Flammability: UL94 HB
&lt;br&gt;Frame Color:White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 3300
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Washable:No
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61072v209%20Family_WS_TUS_Normal_SMD_Side-Push_4343x10458xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61072v209%20Family_WS_TUS_Normal_SMD_Side-Push_4343x10458xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH/"&gt;https://www.we-online.com/catalog/en/TASU_3_5X4_7_SMD_SIDE_PUSH/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun, Shan 2020-02-17&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="4343X10458XX">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/434351045816.pdf"/>
<attribute name="H" value="1.65mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434351045816"/>
<attribute name="QTY" value=" 3300 "/>
<attribute name="VALUE" value="434351045816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
