<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - Tact Switches - THT Tact Switch - WS-TATV&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-09-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="4301X60437X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="4304X60737X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="4304X60437X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="430156130736">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm</description>
</package>
<package name="430186130716">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm</description>
</package>
<package name="4301X60707X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="430156130726">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm</description>
</package>
<package name="4301X60507X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="4304X60857X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="4301X60957X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-TASX_4P1">
<description>WS-TASX_4P1</description>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="430156043726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156043726?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156043726"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156043726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156043736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156043736?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156043736"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156043736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456073736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430456073736?ae"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456073736"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430456073736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476073716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430476073716?ae"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476073716"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430476073716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186043716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430186043716?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186043716"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430186043716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456043736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430456043736?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456043736"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430456043736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466043726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430466043726?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466043726"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430466043726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476043716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430476043716?ae"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476043716"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430476043716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466073726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430466073726?ae"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466073726"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430466073726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156130736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Bulk

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TATV_6X6_THT_4301X6XXX7X6/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATV_6X6_THT_4301X6XXX7X6&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430156130736">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156130736?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156130736"/>
<attribute name="VALUE" value="430156130736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186130716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Bulk

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TATV_6X6_THT_4301X6XXX7X6/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATV_6X6_THT_4301X6XXX7X6&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430186130716">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430186130716?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186130716"/>
<attribute name="VALUE" value="430186130716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156070736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156070736?ae"/>
<attribute name="HEIGHT" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156070736"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156070736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156070726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156070726?ae"/>
<attribute name="HEIGHT" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156070726"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156070726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186070716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430186070716?ae"/>
<attribute name="HEIGHT" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186070716"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430186070716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156130726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Bulk

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TATV_6X6_THT_4301X6XXX7X6/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATV_6X6_THT_4301X6XXX7X6&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430156130726">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156130726?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156130726"/>
<attribute name="VALUE" value="430156130726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186050716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430186050716?ae"/>
<attribute name="HEIGHT" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186050716"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430186050716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156050736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156050736?ae"/>
<attribute name="HEIGHT" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156050736"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156050736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156050726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156050726?ae"/>
<attribute name="HEIGHT" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156050726"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156050726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466085726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430466085726?ae"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466085726"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430466085726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456085736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430456085736?ae"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456085736"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430456085736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476085716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430476085716?ae"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476085716"/>
<attribute name="QTY" value=" 50 "/>
<attribute name="VALUE" value="430476085716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186095716" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430186095716?ae"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186095716"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430186095716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156095726" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156095726?ae"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156095726"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156095726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156095736" prefix="S">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430156095736?ae"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156095736"/>
<attribute name="QTY" value=" 200 "/>
<attribute name="VALUE" value="430156095736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
