<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-MAPI

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-09-16
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MAPI_6030">
<description>WE-MAPI  SMD Power Inductorr

Size:6030,SMT,2pins

LXWXH=6.8X6.8X3.1mm</description>
</package>
<package name="WE-MAPI_3010">
<description>WE-MAPI  SMD Power Inductorr

Size:3010,SMT,2pins

LXWXH=3X3X1mm</description>
</package>
<package name="WE-MAPI_2010">
<description>WE-MAPI  SMD Power Inductorr

Size:2010,SMT,2pins

LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-MAPI_3012">
<description>WE-MAPI  SMD Power Inductorr

Size:3012,SMT,2pins

LXWXH=3X3X1.2mm</description>
</package>
<package name="WE-MAPI_4020">
<description>WE-MAPI  SMD Power Inductorr

Size:4020,SMT,2pins

LXWXH=4X4X2mm</description>
</package>
<package name="WE-MAPI_4020_IPC-7351">
<description>WE-MAPI  SMD Power Inductor

Size:4020,SMT,2pins

LXWXH=4X4X2mm</description>
</package>
<package name="WE-MAPI_2508">
<description>WE-MAPI  SMD Power Inductorr

Size:2508,SMT,2pins

LXWXH=2.5X2X0.8mm</description>
</package>
<package name="WE-MAPI_3020">
<description>WE-MAPI  SMD Power Inductorr

Size:3020,SMT,2pins

LXWXH=3X3X2mm</description>
</package>
<package name="WE-MAPI_2512">
<description>WE-MAPI  SMD Power Inductorr

Size:2512,SMT,2pins

LXWXH=2.5X2X1.2mm</description>
</package>
<package name="WE-MAPI_5030">
<description>WE-MAPI  SMD Power Inductorr

Size:5030,SMT,2pins

LXWXH=5.4X5.4X3.1mm</description>
</package>
<package name="WE-MAPI_3015">
<description>WE-MAPI  SMD Power Inductorr

Size:3015,SMT,2pins

LXWXH=3X3X1.5mm</description>
</package>
<package name="WE-MAPI_2510">
<description>WE-MAPI  SMD Power Inductorr

Size:2510,SMT,2pins

LXWXH=2.5X2X1mm</description>
</package>
<package name="WE-MAPI_4012_IPC-7351">
<description>WE-MAPI  SMD Power Inductor

Size:4012,SMT,2pins

LXWXH=4X4X1.2mm</description>
</package>
<package name="WE-MAPI_4012">
<description>WE-MAPI  SMD Power Inductor

Size:4012,SMT,2pins

LXWXH=4X4X1.2mm</description>
</package>
<package name="WE-MAPI_2506">
<description>WE-MAPI  SMD Power Inductorr

Size:2506,SMT,2pins

LXWXH=2.5X2X0.6mm</description>
</package>
<package name="WE-MAPI_1610">
<description>WE-MAPI  SMD Power Inductorr

Size:1610,SMT,2pins

LXWXH=1.6X1.6X1mm</description>
</package>
<package name="WE-MAPI_5020">
<description>WE-MAPI  SMD Power Inductorr

Size5020,SMT,2pins

LXWXH=5.4X5.4X2.1mm</description>
</package>
<package name="WE-MAPI_4030_IPC-7351">
<description>WE-MAPI  SMD Power Inductor

Size:4030,SMT,2pins

LXWXH=4X4X3.1mm</description>
</package>
<package name="WE-MAPI_4030">
<description>WE-MAPI  SMD Power Inductorr

Size:4030,SMT,2pins

LXW=4X4mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MAPI_6030" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383770033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383770033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="22.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="29 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="93 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383770033?ae"/>
</technology>
<technology name="_744383770068">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383770068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="18.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="23.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="3.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383770068?ae"/>
</technology>
<technology name="_74438377010">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="16.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="19.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="47 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377010?ae"/>
</technology>
<technology name="_74438377015">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="15.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377015?ae"/>
</technology>
<technology name="_74438377022">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="10.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377022?ae"/>
</technology>
<technology name="_74438377033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="15.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377033?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3010" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438333022">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438333022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="150 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438333022?ae"/>
</technology>
<technology name="_74438333033">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438333033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="232 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="38 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438333033?ae"/>
</technology>
<technology name="_74438333047">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438333047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="356 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438333047?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_6030HT" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383770030HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.3 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383770030HT"/>
<attribute name="INDUCTANCE" value="0.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="35 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="119 MHz"/>
<attribute name="OPERATING_VOLTAGE" value=""/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383770030HT?ae"/>
</technology>
<technology name="_744383770033HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383770033HT"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="21.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="27.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="96 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383770033HT?ae"/>
</technology>
<technology name="_744383770068HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383770068HT"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="16.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="21.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="55 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383770068HT?ae"/>
</technology>
<technology name="_74438377010HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="18 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="47 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377010HT?ae"/>
</technology>
<technology name="_74438377022HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="11.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377022HT?ae"/>
</technology>
<technology name="_74438377033HT">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="6.8mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438377033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="17.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438377033HT?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2010" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383430033">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383430033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="40 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="205 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383430033?ae"/>
</technology>
<technology name="_744383430047">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383430047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="49 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="175 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383430047?ae"/>
</technology>
<technology name="_744383430056">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383430056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="56 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="135 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383430056?ae"/>
</technology>
<technology name="_744383430068">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383430068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="65 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="130 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383430068?ae"/>
</technology>
<technology name="_744383430082">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383430082"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.35 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="71 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="125 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383430082?ae"/>
</technology>
<technology name="_74438343010">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438343010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="86 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="99 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438343010?ae"/>
</technology>
<technology name="_74438343012">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438343012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="114 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="96 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438343012?ae"/>
</technology>
<technology name="_74438343015">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438343015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.95 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="150 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438343015?ae"/>
</technology>
<technology name="_74438343022">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438343022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="225 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="70 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438343022?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3012" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383340033">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383340033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="19 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="140 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383340033?ae"/>
</technology>
<technology name="_744383340047">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383340047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="110 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383340047?ae"/>
</technology>
<technology name="_744383340056">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383340056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="108 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383340056?ae"/>
</technology>
<technology name="_744383340068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383340068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="36 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="100 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383340068?ae"/>
</technology>
<technology name="_74438334010">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="42.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="80 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334010?ae"/>
</technology>
<technology name="_74438334012">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="55 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="66 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334012?ae"/>
</technology>
<technology name="_74438334015">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="80 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334015?ae"/>
</technology>
<technology name="_74438334022">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="100 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334022?ae"/>
</technology>
<technology name="_74438334033">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="156.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="36 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334033?ae"/>
</technology>
<technology name="_74438334047">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="267.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334047?ae"/>
</technology>
<technology name="_74438334056">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="338.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334056?ae"/>
</technology>
<technology name="_74438334068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438334068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="368.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438334068?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4020" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2026-09-16
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="14.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="16.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="115 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560033?ae"/>
</technology>
<technology name="_744383560056">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560056?ae"/>
</technology>
<technology name="_744383560068">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="75 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560068?ae"/>
</technology>
<technology name="_74438356010">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="12 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="55 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356010?ae"/>
</technology>
<technology name="_74438356012">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="15 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="52 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356012?ae"/>
</technology>
<technology name="_74438356015">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="16 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="48 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356015?ae"/>
</technology>
<technology name="_74438356018">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356018"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="24.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="40 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356018?ae"/>
</technology>
<technology name="_74438356022">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="34 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356022?ae"/>
</technology>
<technology name="_74438356033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="39.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356033?ae"/>
</technology>
<technology name="_74438356047">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="63 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356047?ae"/>
</technology>
<technology name="_74438356056">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="68 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356056?ae"/>
</technology>
<technology name="_74438356150">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356150"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="200 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="14 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356150?ae"/>
</technology>
<technology name="_74438356220">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356220"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.45 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="250 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="11 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356220?ae"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MAPI_4020_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value=""/>
<attribute name="LENGTH" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="SIZE" value=""/>
<attribute name="VALUE" value=""/>
<attribute name="WIDTH" value=""/>
<attribute name="CATEGORY" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="INDUCTANCE" value=""/>
<attribute name="PERFORMANCE_RATED_CURRENT" value=""/>
<attribute name="SATURATION_CURRENT" value=""/>
<attribute name="DC_RESISTANCE_TYP" value=""/>
<attribute name="SELF_RESONANT_FREQUENCY" value=""/>
<attribute name="OPERATING_VOLTAGE" value=""/>
<attribute name="DATASHEET" value=""/>
</technology>
<technology name="_744383560033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="14.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="16.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="115 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560033?ae"/>
</technology>
<technology name="_744383560056">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560056?ae"/>
</technology>
<technology name="_744383560068">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="75 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560068?ae"/>
</technology>
<technology name="_74438356010">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="12 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="55 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356010?ae"/>
</technology>
<technology name="_74438356012">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="15 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="52 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356012?ae"/>
</technology>
<technology name="_74438356015">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="16 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="48 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356015?ae"/>
</technology>
<technology name="_74438356018">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356018"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="24.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="40 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356018?ae"/>
</technology>
<technology name="_74438356022">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="34 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356022?ae"/>
</technology>
<technology name="_74438356033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="39.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356033?ae"/>
</technology>
<technology name="_74438356047">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="63 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356047?ae"/>
</technology>
<technology name="_74438356056">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="68 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356056?ae"/>
</technology>
<technology name="_74438356150">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356150"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="200 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="14 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356150?ae"/>
</technology>
<technology name="_74438356220">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356220"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.45 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="250 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="11 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356220?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4020HT" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2026-09-16
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560033HT"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="98 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560033HT?ae"/>
</technology>
<technology name="_744383560047HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560047HT"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="83 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560047HT?ae"/>
</technology>
<technology name="_744383560056HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560056HT"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560056HT?ae"/>
</technology>
<technology name="_744383560068HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560068HT"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="67 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560068HT?ae"/>
</technology>
<technology name="_74438356010HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="13.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="46 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356010HT?ae"/>
</technology>
<technology name="_74438356012HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356012HT"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="16 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="45 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356012HT?ae"/>
</technology>
<technology name="_74438356015HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356015HT"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="40 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356015HT?ae"/>
</technology>
<technology name="_74438356018HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356018HT"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="26 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356018HT?ae"/>
</technology>
<technology name="_74438356022HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="28 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356022HT?ae"/>
</technology>
<technology name="_74438356033HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="45 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356033HT?ae"/>
</technology>
<technology name="_74438356047HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356047HT"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.05 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="65 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="18 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356047HT?ae"/>
</technology>
<technology name="_74438356056HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356056HT"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="70 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356056HT?ae"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MAPI_4020_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560033HT"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="98 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560033HT?ae"/>
</technology>
<technology name="_744383560047HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560047HT"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="83 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560047HT?ae"/>
</technology>
<technology name="_744383560056HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560056HT"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="7.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560056HT?ae"/>
</technology>
<technology name="_744383560068HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383560068HT"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="67 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383560068HT?ae"/>
</technology>
<technology name="_74438356010HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="13.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="46 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356010HT?ae"/>
</technology>
<technology name="_74438356012HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356012HT"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="16 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="45 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356012HT?ae"/>
</technology>
<technology name="_74438356015HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356015HT"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="40 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356015HT?ae"/>
</technology>
<technology name="_74438356018HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356018HT"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="26 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356018HT?ae"/>
</technology>
<technology name="_74438356022HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="28 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356022HT?ae"/>
</technology>
<technology name="_74438356033HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="45 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356033HT?ae"/>
</technology>
<technology name="_74438356047HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356047HT"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.05 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="65 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="18 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356047HT?ae"/>
</technology>
<technology name="_74438356056HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438356056HT"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="70 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438356056HT?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2508" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383220047">
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383220047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.65 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="70 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="160 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383220047?ae"/>
</technology>
<technology name="_74438322010">
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438322010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="107 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="100 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438322010?ae"/>
</technology>
<technology name="_74438322022">
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438322022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="252 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438322022?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3020" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383360033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383360033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="14 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="140 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383360033?ae"/>
</technology>
<technology name="_744383360047">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383360047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.55 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="99 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383360047?ae"/>
</technology>
<technology name="_744383360068">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383360068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383360068?ae"/>
</technology>
<technology name="_74438336010">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="26 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="67 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336010?ae"/>
</technology>
<technology name="_74438336012">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="30 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="57 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336012?ae"/>
</technology>
<technology name="_74438336015">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="33 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="51 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336015?ae"/>
</technology>
<technology name="_74438336022">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.55 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="67 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336022?ae"/>
</technology>
<technology name="_74438336033">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.35 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="99 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="39 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336033?ae"/>
</technology>
<technology name="_74438336047">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.15 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="137 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336047?ae"/>
</technology>
<technology name="_74438336068">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.15 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.65 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="168 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336068?ae"/>
</technology>
<technology name="_74438336100">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="280 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="18 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3020HT" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383360068HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383360068HT"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="24.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383360068HT?ae"/>
</technology>
<technology name="_74438336010HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="28.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="67 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336010HT?ae"/>
</technology>
<technology name="_74438336012HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336012HT"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="32.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336012HT?ae"/>
</technology>
<technology name="_74438336015HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336015HT"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="35.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="53 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336015HT?ae"/>
</technology>
<technology name="_74438336022HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="56.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="47 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336022HT?ae"/>
</technology>
<technology name="_74438336033HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="85.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336033HT?ae"/>
</technology>
<technology name="_74438336047HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336047HT"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="130.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336047HT?ae"/>
</technology>
<technology name="_74438336068HT">
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438336068HT"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="197.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438336068HT?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2512HT" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383240033HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240033HT"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="23.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="174 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240033HT?ae"/>
</technology>
<technology name="_744383240047HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240047HT"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="30.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="131 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240047HT?ae"/>
</technology>
<technology name="_744383240056HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240056HT"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="38.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="102 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240056HT?ae"/>
</technology>
<technology name="_74438324010HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="53.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="71 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324010HT?ae"/>
</technology>
<technology name="_74438324012HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324012HT"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="64.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="67 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324012HT?ae"/>
</technology>
<technology name="_74438324015HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324015HT"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="88.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="56 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324015HT?ae"/>
</technology>
<technology name="_74438324022HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="141.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="53 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324022HT?ae"/>
</technology>
<technology name="_74438324033HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="238.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324033HT?ae"/>
</technology>
<technology name="_74438324047HT">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="2.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324047HT"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="319.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="33 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324047HT?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_5030" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383670013">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.13 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383670013"/>
<attribute name="INDUCTANCE" value="0.13 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="27.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="30 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="189 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383670013?ae"/>
</technology>
<technology name="_744383670033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383670033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="21.6 A@40K"/>
<attribute name="SATURATION_CURRENT" value="26.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="108 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383670033?ae"/>
</technology>
<technology name="_744383670047">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383670047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="20.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="20 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="3.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383670047?ae"/>
</technology>
<technology name="_74438367010">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="10 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="44.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367010?ae"/>
</technology>
<technology name="_74438367022">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="14 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367022?ae"/>
</technology>
<technology name="_74438367033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="20 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367033?ae"/>
</technology>
<technology name="_74438367047">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="30 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="18.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367047?ae"/>
</technology>
<technology name="_74438367068">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="42 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367068?ae"/>
</technology>
<technology name="_74438367082">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="50 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="13 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367082?ae"/>
</technology>
<technology name="_74438367100">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438367100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="61 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="13 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438367100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2512" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383240047">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="30 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="145 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240047?ae"/>
</technology>
<technology name="_744383240056">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="37 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="120 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240056?ae"/>
</technology>
<technology name="_744383240068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383240068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="45 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="102 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383240068?ae"/>
</technology>
<technology name="_74438324010">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="49 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324010?ae"/>
</technology>
<technology name="_74438324012">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="67 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="80 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324012?ae"/>
</technology>
<technology name="_74438324015">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="82 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324015?ae"/>
</technology>
<technology name="_74438324022">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.65 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="123 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="57 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324022?ae"/>
</technology>
<technology name="_74438324033">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="226 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324033?ae"/>
</technology>
<technology name="_74438324047">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.65 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="300 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324047?ae"/>
</technology>
<technology name="_74438324056">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="405 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324056?ae"/>
</technology>
<technology name="_74438324068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.05 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="560 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="27 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324068?ae"/>
</technology>
<technology name="_74438324082">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="630 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324082?ae"/>
</technology>
<technology name="_74438324100">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438324100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="680 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438324100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3015" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383350047">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383350047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="20 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="105 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383350047?ae"/>
</technology>
<technology name="_744383350068">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383350068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="25 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="100 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383350068?ae"/>
</technology>
<technology name="_744383350082">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383350082"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="30 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383350082?ae"/>
</technology>
<technology name="_74438335010">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.95 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="39 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335010?ae"/>
</technology>
<technology name="_74438335022">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="94 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="45 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335022?ae"/>
</technology>
<technology name="_74438335033">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="114 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335033?ae"/>
</technology>
<technology name="_74438335047">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="141 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335047?ae"/>
</technology>
<technology name="_74438335068">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="250 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335068?ae"/>
</technology>
<technology name="_74438335100">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="446 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335100?ae"/>
</technology>
<technology name="_74438335150">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335150"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="720 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="14 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335150?ae"/>
</technology>
<technology name="_74438335220">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335220"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.95 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="940 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335220?ae"/>
</technology>
<technology name="_74438335330">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335330"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1210 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335330?ae"/>
</technology>
<technology name="_74438335470">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335470"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.55 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2090 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="8 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335470?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2510" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383230033">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383230033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="180 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383230033?ae"/>
</technology>
<technology name="_744383230047">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383230047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="37 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="170 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383230047?ae"/>
</technology>
<technology name="_744383230068">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383230068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="46 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="135 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383230068?ae"/>
</technology>
<technology name="_744383230082">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383230082"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.45 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="53 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="105 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383230082?ae"/>
</technology>
<technology name="_74438323010">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.55 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="63 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="80 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323010?ae"/>
</technology>
<technology name="_74438323012">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="82 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="75 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323012?ae"/>
</technology>
<technology name="_74438323015">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.85 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.75 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="92 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="65 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323015?ae"/>
</technology>
<technology name="_74438323022">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.55 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="147 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323022?ae"/>
</technology>
<technology name="_74438323033">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="220 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323033?ae"/>
</technology>
<technology name="_74438323047">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="338 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323047?ae"/>
</technology>
<technology name="_74438323068">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="563 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323068?ae"/>
</technology>
<technology name="_74438323082">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.85 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="646 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="27 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323082?ae"/>
</technology>
<technology name="_74438323100">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438323100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="1.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="733 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438323100?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3015HT" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383350056HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383350056HT"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.3 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="19.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="93 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383350056HT?ae"/>
</technology>
<technology name="_744383350068HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383350068HT"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="78 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383350068HT?ae"/>
</technology>
<technology name="_74438335010HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335010HT"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="46.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="73 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335010HT?ae"/>
</technology>
<technology name="_74438335022HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335022HT"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="83.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335022HT?ae"/>
</technology>
<technology name="_74438335033HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335033HT"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="115.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335033HT?ae"/>
</technology>
<technology name="_74438335047HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335047HT"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="162.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335047HT?ae"/>
</technology>
<technology name="_74438335068HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335068HT"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="270.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="22 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335068HT?ae"/>
</technology>
<technology name="_74438335100HT">
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438335100HT"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="2.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="477.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438335100HT?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4012" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2026-09-16
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443835400033">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.033 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7443835400033"/>
<attribute name="INDUCTANCE" value="0.033 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="33.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="40 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="0.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="682 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7443835400033?ae"/>
</technology>
<technology name="_7443835400068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.068 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7443835400068"/>
<attribute name="INDUCTANCE" value="0.068 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="27 A@40K"/>
<attribute name="SATURATION_CURRENT" value="38 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="374 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7443835400068?ae"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MAPI_4012_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443835400033">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.033 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7443835400033"/>
<attribute name="INDUCTANCE" value="0.033 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="33.5 A@40K"/>
<attribute name="SATURATION_CURRENT" value="40 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="0.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="682 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7443835400033?ae"/>
</technology>
<technology name="_7443835400068">
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.068 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7443835400068"/>
<attribute name="INDUCTANCE" value="0.068 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="27 A@40K"/>
<attribute name="SATURATION_CURRENT" value="38 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="374 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7443835400068?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2506" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383210047">
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2506"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383210047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.65 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="76 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="165 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383210047?ae"/>
</technology>
<technology name="_74438321010">
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="2506"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438321010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.25 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="163 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="90 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438321010?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_1610" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_1610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383130033">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383130033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="65 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="215 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
</technology>
<technology name="_744383130047">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383130047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.95 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="77 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="200 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383130047?ae"/>
</technology>
<technology name="_744383130056">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383130056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="90 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="150 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383130056?ae"/>
</technology>
<technology name="_744383130068">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383130068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.55 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="101 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="135 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383130068?ae"/>
</technology>
<technology name="_744383130082">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383130082"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.35 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="115 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="115 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383130082?ae"/>
</technology>
<technology name="_74438313010">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438313010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.25 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="127 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="111 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438313010?ae"/>
</technology>
<technology name="_74438313012">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438313012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="4.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="140 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="109 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438313012?ae"/>
</technology>
<technology name="_74438313015">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438313015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.45 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="189 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="90 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438313015?ae"/>
</technology>
<technology name="_74438313022">
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438313022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="3.25 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="337 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="70 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438313022?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_5020" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2024-11-14
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383660033">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383660033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="19.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="22.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="3.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="100 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383660033?ae"/>
</technology>
<technology name="_744383660047">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383660047"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="16 A@40K"/>
<attribute name="SATURATION_CURRENT" value="18.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="5.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383660047?ae"/>
</technology>
<technology name="_744383660068">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383660068"/>
<attribute name="INDUCTANCE" value="0.68 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="14.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="16.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="59 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383660068?ae"/>
</technology>
<technology name="_744383660082">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383660082"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="15.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="53.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383660082?ae"/>
</technology>
<technology name="_74438366010">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438366010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="11.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438366010?ae"/>
</technology>
<technology name="_74438366015">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438366015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438366015?ae"/>
</technology>
<technology name="_74438366022">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438366022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="23.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="31.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438366022?ae"/>
</technology>
<technology name="_74438366033">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438366033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="33.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438366033?ae"/>
</technology>
<technology name="_74438366047">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="5.6mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438366047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.65 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="54.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438366047?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4030" prefix="L">
<description>WE-MAPI SMT Power Inductor
Shielded

Characteristics
Magnetic iron alloy allows high rated currents
Compact design
Magnetically shielded
High current capability and handles high transient current spikes
Low acoustic noise and low leakage flux noise
AEC-Q 200 qualified
Operating temperature: –40 °C to 125 °C

WE-MAPI High Temperature Series
High Temperature Series with operating temperature from -55 °C to +150 °C

Applications
DC/DC-converter for high current power supplies
DC/DC-converter for Field Programmable Gate Array (FPGA)
POL-converters
Portable power like PDA, digital camera
Mainboards/graphic cards
Battery powered devices
Wireless communication devices
Power supplies for smartphones, tablet PCs and other mobile devices

Details see: www.we-online.com/components/products/WE-MAPI

Updated by Ella 2026-09-16
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383570033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383570033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="96 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383570033?ae"/>
</technology>
<technology name="_744383570056">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383570056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="5.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="79 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383570056?ae"/>
</technology>
<technology name="_74438357010">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="11.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="59 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357010?ae"/>
</technology>
<technology name="_74438357012">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="13.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="51 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357012?ae"/>
</technology>
<technology name="_74438357015">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="17.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="48 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357015?ae"/>
</technology>
<technology name="_74438357018">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357018"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357018?ae"/>
</technology>
<technology name="_74438357022">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357022?ae"/>
</technology>
<technology name="_74438357033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357033?ae"/>
</technology>
<technology name="_74438357047">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="39.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="24 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357047?ae"/>
</technology>
<technology name="_74438357056">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="46.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357056?ae"/>
</technology>
<technology name="_74438357068">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="69.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357068?ae"/>
</technology>
<technology name="_74438357082">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="81 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357082?ae"/>
</technology>
<technology name="_74438357100">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.95 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="100.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357100?ae"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MAPI_4030_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438357010">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.25 A@40K"/>
<attribute name="SATURATION_CURRENT" value="12.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="11.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="59 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357010?ae"/>
</technology>
<technology name="_74438357012">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="13.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="51 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357012?ae"/>
</technology>
<technology name="_74438357015">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.2 A@40K"/>
<attribute name="SATURATION_CURRENT" value="11 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="17.1 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="48 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357015?ae"/>
</technology>
<technology name="_74438357018">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357018"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.9 A@40K"/>
<attribute name="SATURATION_CURRENT" value="10.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="18 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357018?ae"/>
</technology>
<technology name="_74438357022">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="9.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357022?ae"/>
</technology>
<technology name="_74438357047">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="39.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="24 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357047?ae"/>
</technology>
<technology name="_74438357056">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.7 A@40K"/>
<attribute name="SATURATION_CURRENT" value="8.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="46.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357056?ae"/>
</technology>
<technology name="_74438357068">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.75 A@40K"/>
<attribute name="SATURATION_CURRENT" value="7.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="69.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19.5 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357068?ae"/>
</technology>
<technology name="_74438357082">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.45 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="81 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357082?ae"/>
</technology>
<technology name="_74438357100">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357100"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.05 A@40K"/>
<attribute name="SATURATION_CURRENT" value="5.95 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="100.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357100?ae"/>
</technology>
<technology name="_74438357033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74438357033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="SATURATION_CURRENT" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="29 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74438357033?ae"/>
</technology>
<technology name="_744383570033">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383570033"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.8 A@40K"/>
<attribute name="SATURATION_CURRENT" value="14.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="96 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383570033?ae"/>
</technology>
<technology name="_744383570056">
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="4.3mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744383570056"/>
<attribute name="INDUCTANCE" value="0.56 uH"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13.4 A@40K"/>
<attribute name="SATURATION_CURRENT" value="13.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="5.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="79 MHz"/>
<attribute name="OPERATING_VOLTAGE" value="80 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744383570056?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
