<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-MJ Modular Jacks

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-06-29
Copyright: Würth Elektronik</description>
<packages>
<package name="615006144121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Vertical</description>
</package>
<package name="615008144221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615008140121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008149521M">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615006143421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615008142521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Angled</description>
</package>
<package name="615008138321">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615004143821">
<description>WR-MJ Cat 3 Modular Jacks – THT, 4P4C, Horizontal</description>
</package>
<package name="615008150121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008143521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615012143921">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615006138421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615032149521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634108149621">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Vertical</description>
</package>
<package name="615008160421">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="634008138121">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Vertical</description>
</package>
<package name="615006143221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615002138421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P2C, Horizontal</description>
</package>
<package name="615008137121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615016245421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615006138521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Vertical</description>
</package>
<package name="615008160321">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615008143721">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615024143921">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615096243321">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615024149421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615016137621">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008185221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634108185321">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Vertical</description>
</package>
<package name="615004141121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P4C, Horizontal</description>
</package>
<package name="615008160221">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634108185421">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615024149521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008140421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615016149521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634008149721">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615008149521R">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615004144121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P4C, Vertical</description>
</package>
<package name="615006141121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615008185121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008160621">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Angled</description>
</package>
<package name="615032137921">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615012149421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="634008137221">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615008142121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008160721">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Angled</description>
</package>
<package name="615018149421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="634108185521">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615008138221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615004144021">
<description>WR-MJ Cat 3 Modular Jacks – THT, 4P4C, Vertical</description>
</package>
<package name="61500814221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008141321">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615016137721">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008149521L">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615004138421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P4C, Horizontal</description>
</package>
<package name="615008138021">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615008160521">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Vertical</description>
</package>
<package name="615006149421R">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615008142621">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008140621">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615006143621">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615008145521">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008148521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634008137521">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615032243321">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634104149621">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 4P4C, Vertical</description>
</package>
<package name="615016240521">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615006149421M">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="634106149621">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 6P6C, Vertical</description>
</package>
<package name="615008150021">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008160121">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634008149821">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615108150221R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Angled</description>
</package>
<package name="615108137421R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615064243321">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008160021">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615032137821">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="615008137421">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Horizontal</description>
</package>
<package name="634108150321">
<description>WR-MJ Cat 3 Modular Jacks – SMT, 8P8C, Horizontal</description>
</package>
<package name="615006149421L">
<description>WR-MJ Cat 3 Modular Jacks – THT, 6P6C, Horizontal</description>
</package>
<package name="615008145221">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Angled</description>
</package>
<package name="615008145121">
<description>WR-MJ Cat 3 Modular Jacks – THT, 8P8C, Angled</description>
</package>
<package name="615032137921R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615108138321R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615108140621R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615108137121R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615108140121R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615108144221R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615108140421R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615108138021R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615108145121R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Angled</description>
</package>
<package name="615106141121R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 6P6C, Horizontal</description>
</package>
<package name="615108137621R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615106138521R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615108138221R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Vertical</description>
</package>
<package name="615116137721R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
<package name="615108137221R">
<description>WR-MJ Cat 3 Modular Jacks – THR, 8P8C, Horizontal</description>
</package>
</packages>
<symbols>
<symbol name="6P6C">
<description>6P6C</description>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8P8C_2">
<description>8P8C</description>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="6P6C_S">
<description>6P6C</description>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_S">
<description>8P8C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_S_LEDYG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="6P4C">
<description>6P4C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8P8C_LEDYG">
<description>8P8C With LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="6P2C">
<description>6P2C</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="8P8C_S1">
<description>8p8c</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8P8C_S_2LEDYG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="G+Y-_1" direction="pas"/>
<pin name="G-Y+_1" direction="pas"/>
<pin name="G+Y-_2" direction="pas"/>
<pin name="G-Y+_2" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="6P4C_S">
<description>4P4C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="SHILED" direction="pas"/>
</symbol>
<symbol name="8P8C_S_2LEDRG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="R-G+_1" direction="pas"/>
<pin name="R+G-_1" direction="pas"/>
<pin name="G+R-_2" direction="pas"/>
<pin name="G-R+_2" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_2LEDRG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="R-G+_1" direction="pas"/>
<pin name="R+G-_1" direction="pas"/>
<pin name="G+R-_2" direction="pas"/>
<pin name="G-R+_2" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="8P8C_S_LEDYG-1">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_S-1">
<description>8P8C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_S1-1">
<description>8p8c</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6P6C-1">
<description>6P6C</description>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8P8C_S_2LEDYG_2">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="G+Y-_1" direction="pas"/>
<pin name="G-Y+_1" direction="pas"/>
<pin name="G+Y-_2" direction="pas"/>
<pin name="G-Y+_2" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="615006144121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006144121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615006144121"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006144121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006144121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008144221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008144221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008144221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008144221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008144221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140121">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008140121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008140121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008140121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521M" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008149521M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521M"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008149521M?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008149521M"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006143421">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006143421"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Half-shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006143421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006143421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008142521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615008142521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="45°"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008142521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008142521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008138321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008138321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008138321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008138321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004143821" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004143821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615004143821"/>
<attribute name="XPXC" value="4P4C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615004143821?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615004143821"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008150121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_LEDYG"/>
</gates>
<devices>
<device name="" package="615008150121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008150121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="Mid Mount"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008150121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008150121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008143521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008143521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008143521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Half-shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008143521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008143521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615012143921" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C"/>
<gate name="B" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615012143921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615012143921"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615012143921?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615012143921"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006138421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006138421"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006138421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006138421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032149521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_2"/>
<gate name="C" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615032149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615032149521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615032149521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615032149521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108149621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="634108149621"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Soldering Tab"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634108149621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634108149621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008138121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="634008138121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="634008138121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634008138121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634008138121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160421" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008160421"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006143221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006143221"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006143221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006143221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615002138421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P2C"/>
</gates>
<devices>
<device name="" package="615002138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615002138421"/>
<attribute name="XPXC" value="6P2C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615002138421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615002138421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008137121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008137121">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008137121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008137121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008137121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016245421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615016245421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A11"/>
<connect gate="A" pin="G-" pad="A12"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="A" pin="Y+" pad="A9"/>
<connect gate="A" pin="Y-" pad="A10"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B11"/>
<connect gate="B" pin="G-" pad="B12"/>
<connect gate="B" pin="SHIELD" pad="S3 S4"/>
<connect gate="B" pin="Y+" pad="B9"/>
<connect gate="B" pin="Y-" pad="B10"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615016245421"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up &amp; Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="2x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615016245421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615016245421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006138521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006138521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615006138521"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006138521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006138521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160321" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008160321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008143721" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008143721">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008143721"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008143721?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008143721"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024143921" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C"/>
<gate name="B" symbol="6P6C"/>
<gate name="C" symbol="6P6C"/>
<gate name="D" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615024143921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615024143921"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615024143921?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615024143921"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024149421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="D" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C"/>
<gate name="C" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615024149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615024149421"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615024149421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615024149421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615096243321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="E" symbol="8P8C_S"/>
<gate name="F" symbol="8P8C_S"/>
<gate name="G" symbol="8P8C_S"/>
<gate name="L" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S1"/>
<gate name="H" symbol="8P8C_S1"/>
<gate name="I" symbol="8P8C_S1"/>
<gate name="J" symbol="8P8C_S1"/>
<gate name="K" symbol="8P8C_S1"/>
</gates>
<devices>
<device name="" package="615096243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S4"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S5"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="E" pin="1" pad="E1"/>
<connect gate="E" pin="2" pad="E2"/>
<connect gate="E" pin="3" pad="E3"/>
<connect gate="E" pin="4" pad="E4"/>
<connect gate="E" pin="5" pad="E5"/>
<connect gate="E" pin="6" pad="E6"/>
<connect gate="E" pin="7" pad="E7"/>
<connect gate="E" pin="8" pad="E8"/>
<connect gate="E" pin="SHIELD" pad="S6"/>
<connect gate="F" pin="1" pad="F1"/>
<connect gate="F" pin="2" pad="F2"/>
<connect gate="F" pin="3" pad="F3"/>
<connect gate="F" pin="4" pad="F4"/>
<connect gate="F" pin="5" pad="F5"/>
<connect gate="F" pin="6" pad="F6"/>
<connect gate="F" pin="7" pad="F7"/>
<connect gate="F" pin="8" pad="F8"/>
<connect gate="F" pin="SHIELD" pad="S7"/>
<connect gate="G" pin="1" pad="G1"/>
<connect gate="G" pin="2" pad="G2"/>
<connect gate="G" pin="3" pad="G3"/>
<connect gate="G" pin="4" pad="G4"/>
<connect gate="G" pin="5" pad="G5"/>
<connect gate="G" pin="6" pad="G6"/>
<connect gate="G" pin="7" pad="G7"/>
<connect gate="G" pin="8" pad="G8"/>
<connect gate="G" pin="SHIELD" pad="S8 S9"/>
<connect gate="H" pin="1" pad="H1"/>
<connect gate="H" pin="2" pad="H2"/>
<connect gate="H" pin="3" pad="H3"/>
<connect gate="H" pin="4" pad="H4"/>
<connect gate="H" pin="5" pad="H5"/>
<connect gate="H" pin="6" pad="H6"/>
<connect gate="H" pin="7" pad="H7"/>
<connect gate="H" pin="8" pad="H8"/>
<connect gate="I" pin="1" pad="I1"/>
<connect gate="I" pin="2" pad="I2"/>
<connect gate="I" pin="3" pad="I3"/>
<connect gate="I" pin="4" pad="I4"/>
<connect gate="I" pin="5" pad="I5"/>
<connect gate="I" pin="6" pad="I6"/>
<connect gate="I" pin="7" pad="I7"/>
<connect gate="I" pin="8" pad="I8"/>
<connect gate="J" pin="1" pad="J1"/>
<connect gate="J" pin="2" pad="J2"/>
<connect gate="J" pin="3" pad="J3"/>
<connect gate="J" pin="4" pad="J4"/>
<connect gate="J" pin="5" pad="J5"/>
<connect gate="J" pin="6" pad="J6"/>
<connect gate="J" pin="7" pad="J7"/>
<connect gate="J" pin="8" pad="J8"/>
<connect gate="K" pin="1" pad="K1"/>
<connect gate="K" pin="2" pad="K2"/>
<connect gate="K" pin="3" pad="K3"/>
<connect gate="K" pin="4" pad="K4"/>
<connect gate="K" pin="5" pad="K5"/>
<connect gate="K" pin="6" pad="K6"/>
<connect gate="K" pin="7" pad="K7"/>
<connect gate="K" pin="8" pad="K8"/>
<connect gate="L" pin="1" pad="L1"/>
<connect gate="L" pin="2" pad="L2"/>
<connect gate="L" pin="3" pad="L3"/>
<connect gate="L" pin="4" pad="L4"/>
<connect gate="L" pin="5" pad="L5"/>
<connect gate="L" pin="6" pad="L6"/>
<connect gate="L" pin="7" pad="L7"/>
<connect gate="L" pin="8" pad="L8"/>
<connect gate="L" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615096243321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up &amp; Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="2x6"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615096243321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615096243321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016137621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016137621">
<connects>
<connect gate="A" pin="1" pad="A8"/>
<connect gate="A" pin="2" pad="A7"/>
<connect gate="A" pin="3" pad="A6"/>
<connect gate="A" pin="4" pad="A5"/>
<connect gate="A" pin="5" pad="A4"/>
<connect gate="A" pin="6" pad="A3"/>
<connect gate="A" pin="7" pad="A2"/>
<connect gate="A" pin="8" pad="A1"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="B" pin="1" pad="B8"/>
<connect gate="B" pin="2" pad="B7"/>
<connect gate="B" pin="3" pad="B6"/>
<connect gate="B" pin="4" pad="B5"/>
<connect gate="B" pin="5" pad="B4"/>
<connect gate="B" pin="6" pad="B3"/>
<connect gate="B" pin="7" pad="B2"/>
<connect gate="B" pin="8" pad="B1"/>
<connect gate="B" pin="SHIELD" pad="S3"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615016137621"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615016137621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615016137621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008185221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008185221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008185221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008185221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008185221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="634108185321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="with Soldering Tab"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634108185321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634108185321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004141121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004141121">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615004141121"/>
<attribute name="XPXC" value="6P4C"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615004141121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615004141121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634108185421"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634108185421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634108185421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160221" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008160221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="150 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024149521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615024149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615024149521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x3"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615024149521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615024149521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008140421"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008140421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008140421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016149521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615016149521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615016149521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615016149521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008149721" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634008149721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634008149721"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634008149721?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634008149721"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008149521R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008149521R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008149521R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004144121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004144121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615004144121"/>
<attribute name="XPXC" value="6P4C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615004144121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615004144121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006141121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006141121">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006141121"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006141121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006141121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008185121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008185121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008185121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="Low Profile"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008185121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008185121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160621" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615008160621"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TYPE" value="47.5°"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615012149421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615012149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615012149421"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615012149421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615012149421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032137921" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
<gate name="C" symbol="8P8C_S_LEDYG"/>
<gate name="D" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615032137921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A10"/>
<connect gate="A" pin="G-" pad="A9"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="A" pin="Y+" pad="A12"/>
<connect gate="A" pin="Y-" pad="A11"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B10"/>
<connect gate="B" pin="G-" pad="B9"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="B" pin="Y+" pad="B12"/>
<connect gate="B" pin="Y-" pad="B11"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="G+" pad="C10"/>
<connect gate="C" pin="G-" pad="C9"/>
<connect gate="C" pin="SHIELD" pad="S3"/>
<connect gate="C" pin="Y+" pad="C12"/>
<connect gate="C" pin="Y-" pad="C11"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="G+" pad="D10"/>
<connect gate="D" pin="G-" pad="D9"/>
<connect gate="D" pin="SHIELD" pad="S4"/>
<connect gate="D" pin="Y+" pad="D12"/>
<connect gate="D" pin="Y-" pad="D11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615032137921"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615032137921?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615032137921"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008137221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="634008137221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634008137221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634008137221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634008137221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_2LEDYG"/>
</gates>
<devices>
<device name="" package="615008142121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+Y-_1" pad="11"/>
<connect gate="G$1" pin="G+Y-_2" pad="9"/>
<connect gate="G$1" pin="G-Y+_1" pad="12"/>
<connect gate="G$1" pin="G-Y+_2" pad="10"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="2xBipolar Y/G"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008142121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008142121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008142121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160721" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615008160721"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TYPE" value="47.5°"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160721?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160721"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615018149421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="C" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615018149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615018149421"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x3"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615018149421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615018149421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634108185521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634108185521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634108185521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008138221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008138221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008138221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008138221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004144021" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004144021">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615004144021"/>
<attribute name="XPXC" value="4P4C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Panel Stop"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615004144021?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615004144021"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61500814221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="61500814221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="61500814221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/61500814221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="61500814221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008141321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_2LEDYG"/>
</gates>
<devices>
<device name="" package="615008141321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+Y-_1" pad="12"/>
<connect gate="G$1" pin="G+Y-_2" pad="10"/>
<connect gate="G$1" pin="G-Y+_1" pad="11"/>
<connect gate="G$1" pin="G-Y+_2" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="2xBipolar Y/G"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008141321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008141321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008141321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016137721" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615016137721">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A10"/>
<connect gate="A" pin="G-" pad="A9"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="A" pin="Y+" pad="A12"/>
<connect gate="A" pin="Y-" pad="A11"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B10"/>
<connect gate="B" pin="G-" pad="B9"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="B" pin="Y+" pad="B12"/>
<connect gate="B" pin="Y-" pad="B11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615016137721"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615016137721?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615016137721"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521L" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008149521L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521L"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008149521L?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008149521L"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004138421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615004138421"/>
<attribute name="XPXC" value="6P4C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615004138421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615004138421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138021" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008138021">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008138021"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008138021?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008138021"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160521" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615008160521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6a"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006149421R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421R"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006149421R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006149421R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008142621">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008142621"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008142621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008142621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008140621"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008140621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008140621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006143621">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006143621"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006143621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006143621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145521" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008145521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 5e"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008145521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008145521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008148521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008148521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008148521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008148521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008148521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634104149621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C_S"/>
</gates>
<devices>
<device name="" package="634104149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SHILED" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="634104149621"/>
<attribute name="XPXC" value="4P4C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Soldering Tab"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634104149621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634104149621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032243321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615032243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3 S4"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S5"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S6 S7"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615032243321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up &amp; Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="2x2"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615032243321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615032243321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016240521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016240521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S3 S4 S5 S6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615016240521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up &amp; Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="2x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615016240521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615016240521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008137521" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="634008137521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="11"/>
<connect gate="G$1" pin="G-" pad="12"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="9"/>
<connect gate="G$1" pin="Y-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634008137521"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634008137521?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634008137521"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421M" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006149421M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421M"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006149421M?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006149421M"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634106149621" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="634106149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="634106149621"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Soldering Tab"/>
<attribute name="PACKAGING" value="Tape and Reel &amp; Mylar"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634106149621?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634106149621"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008150021" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008150021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008150021"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="Mid Mount"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008150021?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008150021"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160121" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008160121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008149821" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634008149821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634008149821"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634008149821?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634008149821"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108150221R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Ella 2026-09-08
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615108150221R">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615108150221R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="Mid Mount"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108150221R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108150221R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108137421R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Ella 2026-09-08
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615108137421R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108137421R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="THR Compatible"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108137421R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108137421R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615064243321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S1"/>
<gate name="C" symbol="8P8C_S1"/>
<gate name="F" symbol="8P8C_S1"/>
<gate name="G" symbol="8P8C_S1"/>
<gate name="H" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="E" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615064243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S4"/>
<connect gate="E" pin="1" pad="E1"/>
<connect gate="E" pin="2" pad="E2"/>
<connect gate="E" pin="3" pad="E3"/>
<connect gate="E" pin="4" pad="E4"/>
<connect gate="E" pin="5" pad="E5"/>
<connect gate="E" pin="6" pad="E6"/>
<connect gate="E" pin="7" pad="E7"/>
<connect gate="E" pin="8" pad="E8"/>
<connect gate="E" pin="SHIELD" pad="S5 S6"/>
<connect gate="F" pin="1" pad="F1"/>
<connect gate="F" pin="2" pad="F2"/>
<connect gate="F" pin="3" pad="F3"/>
<connect gate="F" pin="4" pad="F4"/>
<connect gate="F" pin="5" pad="F5"/>
<connect gate="F" pin="6" pad="F6"/>
<connect gate="F" pin="7" pad="F7"/>
<connect gate="F" pin="8" pad="F8"/>
<connect gate="G" pin="1" pad="G1"/>
<connect gate="G" pin="2" pad="G2"/>
<connect gate="G" pin="3" pad="G3"/>
<connect gate="G" pin="4" pad="G4"/>
<connect gate="G" pin="5" pad="G5"/>
<connect gate="G" pin="6" pad="G6"/>
<connect gate="G" pin="7" pad="G7"/>
<connect gate="G" pin="8" pad="G8"/>
<connect gate="H" pin="1" pad="H1"/>
<connect gate="H" pin="2" pad="H2"/>
<connect gate="H" pin="3" pad="H3"/>
<connect gate="H" pin="4" pad="H4"/>
<connect gate="H" pin="5" pad="H5"/>
<connect gate="H" pin="6" pad="H6"/>
<connect gate="H" pin="7" pad="H7"/>
<connect gate="H" pin="8" pad="H8"/>
<connect gate="H" pin="SHIELD" pad="S1 S2" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615064243321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up &amp; Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="2x4"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615064243321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615064243321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160021" prefix="J">
<description>WR-MJ Gigabit Ethernet Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Angled, vertical and horizontal orientations

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 5e to 6A

Applications

Telecommunications
Computing
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008160021"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 6"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="150 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008160021?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008160021"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032137821" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S1"/>
</gates>
<devices>
<device name="" package="615032137821">
<connects>
<connect gate="A" pin="1" pad="A8"/>
<connect gate="A" pin="2" pad="A7"/>
<connect gate="A" pin="3" pad="A6"/>
<connect gate="A" pin="4" pad="A5"/>
<connect gate="A" pin="5" pad="A4"/>
<connect gate="A" pin="6" pad="A3"/>
<connect gate="A" pin="7" pad="A2"/>
<connect gate="A" pin="8" pad="A1"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B8"/>
<connect gate="B" pin="2" pad="B7"/>
<connect gate="B" pin="3" pad="B6"/>
<connect gate="B" pin="4" pad="B5"/>
<connect gate="B" pin="5" pad="B4"/>
<connect gate="B" pin="6" pad="B3"/>
<connect gate="B" pin="7" pad="B2"/>
<connect gate="B" pin="8" pad="B1"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="C" pin="1" pad="C8"/>
<connect gate="C" pin="2" pad="C7"/>
<connect gate="C" pin="3" pad="C6"/>
<connect gate="C" pin="4" pad="C5"/>
<connect gate="C" pin="5" pad="C4"/>
<connect gate="C" pin="6" pad="C3"/>
<connect gate="C" pin="7" pad="C2"/>
<connect gate="C" pin="8" pad="C1"/>
<connect gate="D" pin="1" pad="D8"/>
<connect gate="D" pin="2" pad="D7"/>
<connect gate="D" pin="3" pad="D6"/>
<connect gate="D" pin="4" pad="D5"/>
<connect gate="D" pin="5" pad="D4"/>
<connect gate="D" pin="6" pad="D3"/>
<connect gate="D" pin="7" pad="D2"/>
<connect gate="D" pin="8" pad="D1"/>
<connect gate="D" pin="SHIELD" pad="S3"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615032137821"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Down"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615032137821?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615032137821"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008137421" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008137421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="Yes"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615008137421"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008137421?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008137421"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108150321" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – SMT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Tape &amp; Reel packaging for pick-and-place assembly

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-03
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108150321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="634108150321"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="VARIANT" value="Mid Mount"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/634108150321?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="634108150321"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421L" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006149421L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421L"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="TAB" value="Up"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="PORTS" value="1xX"/>
<attribute name="SHIELDING" value="Plastic"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Peg Assembly"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615006149421L?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615006149421L"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145121" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615008145121"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="45°"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Post Tail"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008145121?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008145121"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145221" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THT

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Angled, vertical and horizontal orientation
Stacked and assembled configurations
Properties

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Updated by Yingchun Shan 2020-01-06
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name="">
<attribute name="EMI" value="No"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615008145221"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="45°"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELDING" value="Shielded"/>
<attribute name="WORKING-VOLTAGE" value="120 V (AC)"/>
<attribute name="VARIANT" value="with Metal Post Tail"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615008145221?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615008145221"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032137921R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_2LEDRG"/>
<gate name="B" symbol="8P8C_2LEDRG"/>
<gate name="C" symbol="8P8C_2LEDRG"/>
<gate name="D" symbol="8P8C_2LEDRG"/>
</gates>
<devices>
<device name="" package="615032137921R">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+R-_2" pad="A11"/>
<connect gate="A" pin="G-R+_2" pad="A12"/>
<connect gate="A" pin="R+G-_1" pad="A10"/>
<connect gate="A" pin="R-G+_1" pad="A9"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+R-_2" pad="B11"/>
<connect gate="B" pin="G-R+_2" pad="B12"/>
<connect gate="B" pin="R+G-_1" pad="B10"/>
<connect gate="B" pin="R-G+_1" pad="B9"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="G+R-_2" pad="C11"/>
<connect gate="C" pin="G-R+_2" pad="C12"/>
<connect gate="C" pin="R+G-_1" pad="C10"/>
<connect gate="C" pin="R-G+_1" pad="C9"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="G+R-_2" pad="D11"/>
<connect gate="D" pin="G-R+_2" pad="D12"/>
<connect gate="D" pin="R+G-_1" pad="D10"/>
<connect gate="D" pin="R-G+_1" pad="D9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615032137921R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615032137921R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615032137921R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108138321R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG-1"/>
</gates>
<devices>
<device name="" package="615108138321R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615108138321R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108138321R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108138321R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108140621R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S-1"/>
</gates>
<devices>
<device name="" package="615108140621R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108140621R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108140621R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108140621R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108137121R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S1-1"/>
</gates>
<devices>
<device name="" package="615108137121R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108137121R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108137121R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108137121R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108140121R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S-1"/>
</gates>
<devices>
<device name="" package="615108140121R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108140121R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108140121R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108140121R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108144221R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S1-1"/>
</gates>
<devices>
<device name="" package="615108144221R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615108144221R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108144221R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108144221R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108140421R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S-1"/>
</gates>
<devices>
<device name="" package="615108140421R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615108140421R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108140421R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108140421R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108138021R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S1-1"/>
</gates>
<devices>
<device name="" package="615108138021R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615108138021R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108138021R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108138021R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108145121R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S-1"/>
</gates>
<devices>
<device name="" package="615108145121R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Angled"/>
<attribute name="VALUE" value="615108145121R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108145121R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108145121R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615106141121R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C-1"/>
</gates>
<devices>
<device name="" package="615106141121R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615106141121R"/>
<attribute name="XPXC" value="6P6C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615106141121R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615106141121R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108137621R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG-1"/>
</gates>
<devices>
<device name="" package="615108137621R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108137621R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108137621R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108137621R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615106138521R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C-1"/>
</gates>
<devices>
<device name="" package="615106138521R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615106138521R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615106138521R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615106138521R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108138221R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S-1"/>
</gates>
<devices>
<device name="" package="615108138221R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Vertical"/>
<attribute name="VALUE" value="615108138221R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108138221R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108138221R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615116137721R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_2LEDYG_2"/>
<gate name="B" symbol="8P8C_S_2LEDYG_2"/>
</gates>
<devices>
<device name="" package="615116137721R">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+Y-_1" pad="A9"/>
<connect gate="A" pin="G+Y-_2" pad="A11"/>
<connect gate="A" pin="G-Y+_1" pad="A10"/>
<connect gate="A" pin="G-Y+_2" pad="A12"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+Y-_1" pad="B9"/>
<connect gate="B" pin="G+Y-_2" pad="B11"/>
<connect gate="B" pin="G-Y+_1" pad="B10"/>
<connect gate="B" pin="G-Y+_2" pad="B12"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615116137721R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615116137721R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615116137721R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108137221R" prefix="J">
<description>WR-MJ Cat 3 Modular Jacks – THR

Characteristics

Shieldingless and shielded with EMI-spring option
Optional LEDs in various sequences
Vertical and horizontal orientation
Stacked and assembled configurations
Tape &amp; Reel packaging for pick-and-place assembly (Tray for larger stacks)

Properties

PoE++ compatible up to 100 W (IEEE 802.3bt)
UL and cULus certified
UL94-V0 reflow-compatible insulator material
Ethernet Category 3 – Category 5 under conditions

Applications

Networks
Internet of Things
Smart buildings

Created by Ella 2026-06-26
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG-1"/>
</gates>
<devices>
<device name="" package="615108137221R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MOUNT" value="THR"/>
<attribute name="SIZE" value="Horizontal"/>
<attribute name="VALUE" value="615108137221R"/>
<attribute name="XPXC" value="8P8C"/>
<attribute name="APPLICATION-SYSTEM" value="CAT 3"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="WORKING-VOLTAGE" value="125 V (AC)"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/615108137221R?ae"/>
<attribute name="CATEGORY" value="Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="615108137221R"/>
<attribute name="RATED-CURRENT" value="1.5 A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
