<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-PD4&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD4_S">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD4 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;S</description>
</package>
<package name="WE-PD4_L">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD4 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;L</description>
</package>
<package name="WE-PD4_X">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD4 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;X</description>
</package>
<package name="WE-PD4_XL">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD4 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;XL</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD4_L" prefix="L">
<description>&lt;b&gt;WE-PD4 SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current loading up to 38 A
&lt;br&gt;Compact size
&lt;br&gt;&lt;br&gt;Low-loss ferrite core
&lt;br&gt;Application frequency range up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression, EMI Filter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, 
 &lt;br&gt;Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, &lt;br&gt;Analogic Tech and Diodes

&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD4"&gt;https://katalog.we-online.com/en/pbs/WE-PD4&lt;/a&gt;&lt;p&gt;


Updated  by Yingchun,Shan 2019-08-05&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD4_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445601">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445601.pdf"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="14.25A"/>
<attribute name="PART-NUMBER" value=" 7445601 "/>
<attribute name="RDC-MAX" value="0.007Ohm"/>
<attribute name="RDC-TYP" value="0.004Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74456015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456015.pdf"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="10.7A"/>
<attribute name="PART-NUMBER" value=" 74456015 "/>
<attribute name="RDC-MAX" value="0.009Ohm"/>
<attribute name="RDC-TYP" value="0.006Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74456022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456022.pdf"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="PART-NUMBER" value=" 74456022 "/>
<attribute name="RDC-MAX" value="0.011Ohm"/>
<attribute name="RDC-TYP" value="0.007Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74456025">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456025.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="PART-NUMBER" value=" 74456025 "/>
<attribute name="RDC-MAX" value="0.012Ohm"/>
<attribute name="RDC-TYP" value="0.009Ohm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_74456033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456033.pdf"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="PART-NUMBER" value=" 74456033 "/>
<attribute name="RDC-MAX" value="0.015Ohm"/>
<attribute name="RDC-TYP" value="0.011Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74456047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456047.pdf"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74456047 "/>
<attribute name="RDC-MAX" value="0.019Ohm"/>
<attribute name="RDC-TYP" value="0.015Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74456056">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456056.pdf"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74456056 "/>
<attribute name="RDC-MAX" value="0.032Ohm"/>
<attribute name="RDC-TYP" value="0.024Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74456068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456068.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="PART-NUMBER" value=" 74456068 "/>
<attribute name="RDC-MAX" value="0.034Ohm"/>
<attribute name="RDC-TYP" value="0.026Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74456082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456082.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="PART-NUMBER" value=" 74456082 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.034Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7445610">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445610.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="PART-NUMBER" value=" 7445610 "/>
<attribute name="RDC-MAX" value="0.045Ohm"/>
<attribute name="RDC-TYP" value="0.035Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74456115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456115.pdf"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="PART-NUMBER" value=" 74456115 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="RDC-TYP" value="0.043Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74456122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456122.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="PART-NUMBER" value=" 74456122 "/>
<attribute name="RDC-MAX" value="0.095Ohm"/>
<attribute name="RDC-TYP" value="0.071Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74456133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456133.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="PART-NUMBER" value=" 74456133 "/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="RDC-TYP" value="0.094Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74456147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456147.pdf"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2.14A"/>
<attribute name="PART-NUMBER" value=" 74456147 "/>
<attribute name="RDC-MAX" value="0.19Ohm"/>
<attribute name="RDC-TYP" value="0.142Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74456168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456168.pdf"/>
<attribute name="FRES" value="8.5MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 74456168 "/>
<attribute name="RDC-MAX" value="0.24Ohm"/>
<attribute name="RDC-TYP" value="0.187Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445620">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445620.pdf"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 7445620 "/>
<attribute name="RDC-MAX" value="0.33Ohm"/>
<attribute name="RDC-TYP" value="0.253Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74456215">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456215.pdf"/>
<attribute name="FRES" value="5.3MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 74456215 "/>
<attribute name="RDC-MAX" value="0.59Ohm"/>
<attribute name="RDC-TYP" value="0.448Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74456222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456222.pdf"/>
<attribute name="FRES" value="4.7MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 74456222 "/>
<attribute name="RDC-MAX" value="0.78Ohm"/>
<attribute name="RDC-TYP" value="0.601Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74456233">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456233.pdf"/>
<attribute name="FRES" value="3.7MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 74456233 "/>
<attribute name="RDC-MAX" value="1.15Ohm"/>
<attribute name="RDC-TYP" value="0.893Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74456247">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456247.pdf"/>
<attribute name="FRES" value="3.1MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="PART-NUMBER" value=" 74456247 "/>
<attribute name="RDC-MAX" value="1.7Ohm"/>
<attribute name="RDC-TYP" value="1.315Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74456268">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456268.pdf"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 74456268 "/>
<attribute name="RDC-MAX" value="2.6Ohm"/>
<attribute name="RDC-TYP" value="1.942Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7445630">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445630.pdf"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.52A"/>
<attribute name="PART-NUMBER" value=" 7445630 "/>
<attribute name="RDC-MAX" value="3.9Ohm"/>
<attribute name="RDC-TYP" value="2.94Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_74456322">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456322.pdf"/>
<attribute name="FRES" value="1.2MHz"/>
<attribute name="IR" value="0.1A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="PART-NUMBER" value=" 74456322 "/>
<attribute name="RDC-MAX" value="8.2Ohm"/>
<attribute name="RDC-TYP" value="6.26Ohm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
<technology name="_74456347">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456347.pdf"/>
<attribute name="FRES" value="0.9MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="PART-NUMBER" value=" 74456347 "/>
<attribute name="RDC-MAX" value="17Ohm"/>
<attribute name="RDC-TYP" value="13.3Ohm"/>
<attribute name="VALUE" value="4700uH"/>
</technology>
<technology name="_74456382">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74456382.pdf"/>
<attribute name="FRES" value="0.7MHz"/>
<attribute name="IR" value="0.11A"/>
<attribute name="ISAT" value="0.17A"/>
<attribute name="PART-NUMBER" value=" 74456382 "/>
<attribute name="RDC-MAX" value="35Ohm"/>
<attribute name="RDC-TYP" value="28Ohm"/>
<attribute name="VALUE" value="8200uH"/>
</technology>
<technology name="_7445640">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445640.pdf"/>
<attribute name="FRES" value="0.6MHz"/>
<attribute name="IR" value="0.1A"/>
<attribute name="ISAT" value="0.15A"/>
<attribute name="PART-NUMBER" value=" 7445640 "/>
<attribute name="RDC-MAX" value="39Ohm"/>
<attribute name="RDC-TYP" value="29.9Ohm"/>
<attribute name="VALUE" value="10000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_S" prefix="L">
<description>&lt;b&gt;WE-PD4 SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current loading up to 38 A
&lt;br&gt;Compact size
&lt;br&gt;&lt;br&gt;Low-loss ferrite core
&lt;br&gt;Application frequency range up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression, EMI Filter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, 
 &lt;br&gt;Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, &lt;br&gt;Analogic Tech and Diodes

&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD4"&gt;https://katalog.we-online.com/en/pbs/WE-PD4&lt;/a&gt;&lt;p&gt;


Updated  by Yingchun,Shan 2019-08-05&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD4_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445501">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445501.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="PART-NUMBER" value=" 7445501 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="RDC-TYP" value="0.017Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74455015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455015.pdf"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="PART-NUMBER" value=" 74455015 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="RDC-TYP" value="0.02Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74455022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455022.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 74455022 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.028Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74455033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455033.pdf"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="PART-NUMBER" value=" 74455033 "/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="RDC-TYP" value="0.044Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74455047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455047.pdf"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 74455047 "/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="RDC-TYP" value="0.063Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74455068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455068.pdf"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 74455068 "/>
<attribute name="RDC-MAX" value="0.13Ohm"/>
<attribute name="RDC-TYP" value="0.092Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7445510">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445510.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7445510 "/>
<attribute name="RDC-MAX" value="0.16Ohm"/>
<attribute name="RDC-TYP" value="0.121Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74455115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455115.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 74455115 "/>
<attribute name="RDC-MAX" value="0.23Ohm"/>
<attribute name="RDC-TYP" value="0.176Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74455122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455122.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 74455122 "/>
<attribute name="RDC-MAX" value="0.37Ohm"/>
<attribute name="RDC-TYP" value="0.255Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74455133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455133.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.58A"/>
<attribute name="PART-NUMBER" value=" 74455133 "/>
<attribute name="RDC-MAX" value="0.51Ohm"/>
<attribute name="RDC-TYP" value="0.362Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74455147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455147.pdf"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 74455147 "/>
<attribute name="RDC-MAX" value="0.64Ohm"/>
<attribute name="RDC-TYP" value="0.556Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74455168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455168.pdf"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="PART-NUMBER" value=" 74455168 "/>
<attribute name="RDC-MAX" value="0.86Ohm"/>
<attribute name="RDC-TYP" value="0.79Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445520">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445520.pdf"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.31A"/>
<attribute name="PART-NUMBER" value=" 7445520 "/>
<attribute name="RDC-MAX" value="1.27Ohm"/>
<attribute name="RDC-TYP" value="1.08Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74455215">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455215.pdf"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.27A"/>
<attribute name="PART-NUMBER" value=" 74455215 "/>
<attribute name="RDC-MAX" value="2Ohm"/>
<attribute name="RDC-TYP" value="1.45Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74455222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455222.pdf"/>
<attribute name="FRES" value="4.8MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="PART-NUMBER" value=" 74455222 "/>
<attribute name="RDC-MAX" value="3.11Ohm"/>
<attribute name="RDC-TYP" value="2.58Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74455233">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455233.pdf"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.16A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="PART-NUMBER" value=" 74455233 "/>
<attribute name="RDC-MAX" value="5Ohm"/>
<attribute name="RDC-TYP" value="4.15Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74455247">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74455247.pdf"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.16A"/>
<attribute name="ISAT" value="0.15A"/>
<attribute name="PART-NUMBER" value=" 74455247 "/>
<attribute name="RDC-MAX" value="6.8Ohm"/>
<attribute name="RDC-TYP" value="5.58Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_7445530">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445530.pdf"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.07A"/>
<attribute name="ISAT" value="0.1A"/>
<attribute name="PART-NUMBER" value=" 7445530 "/>
<attribute name="RDC-MAX" value="13.8Ohm"/>
<attribute name="RDC-TYP" value="11.5Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_X" prefix="L">
<description>&lt;b&gt;WE-PD4 SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current loading up to 38 A
&lt;br&gt;Compact size
&lt;br&gt;&lt;br&gt;Low-loss ferrite core
&lt;br&gt;Application frequency range up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression, EMI Filter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, 
 &lt;br&gt;Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, &lt;br&gt;Analogic Tech and Diodes

&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD4"&gt;https://katalog.we-online.com/en/pbs/WE-PD4&lt;/a&gt;&lt;p&gt;


Updated  by Yingchun,Shan 2019-08-05&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD4_X">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74458001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458001.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="PART-NUMBER" value=" 74458001 "/>
<attribute name="RDC-MAX" value="0.009Ohm"/>
<attribute name="RDC-TYP" value="0.005Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74458002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458002.pdf"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="20.3A"/>
<attribute name="PART-NUMBER" value=" 74458002 "/>
<attribute name="RDC-MAX" value="0.014Ohm"/>
<attribute name="RDC-TYP" value="0.008Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74458003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458003.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="15.8A"/>
<attribute name="PART-NUMBER" value=" 74458003 "/>
<attribute name="RDC-MAX" value="0.018Ohm"/>
<attribute name="RDC-TYP" value="0.01Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74458005">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458005.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="13.1A"/>
<attribute name="PART-NUMBER" value=" 74458005 "/>
<attribute name="RDC-MAX" value="0.02Ohm"/>
<attribute name="RDC-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74458010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458010.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="PART-NUMBER" value=" 74458010 "/>
<attribute name="RDC-MAX" value="0.031Ohm"/>
<attribute name="RDC-TYP" value="0.021Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74458115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458115.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="PART-NUMBER" value=" 74458115 "/>
<attribute name="RDC-MAX" value="0.036Ohm"/>
<attribute name="RDC-TYP" value="0.03Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74458122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458122.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="PART-NUMBER" value=" 74458122 "/>
<attribute name="RDC-MAX" value="0.047Ohm"/>
<attribute name="RDC-TYP" value="0.043Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74458133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458133.pdf"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="PART-NUMBER" value=" 74458133 "/>
<attribute name="RDC-MAX" value="0.066Ohm"/>
<attribute name="RDC-TYP" value="0.06Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74458147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458147.pdf"/>
<attribute name="FRES" value="8.4MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 74458147 "/>
<attribute name="RDC-MAX" value="0.086Ohm"/>
<attribute name="RDC-TYP" value="0.076Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74458168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458168.pdf"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="PART-NUMBER" value=" 74458168 "/>
<attribute name="RDC-MAX" value="0.13Ohm"/>
<attribute name="RDC-TYP" value="0.11Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445820">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445820.pdf"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="PART-NUMBER" value=" 7445820 "/>
<attribute name="RDC-MAX" value="0.19Ohm"/>
<attribute name="RDC-TYP" value="0.141Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74458215">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458215.pdf"/>
<attribute name="FRES" value="4.6MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 74458215 "/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="RDC-TYP" value="0.21Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74458220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458220.pdf"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 74458220 "/>
<attribute name="RDC-MAX" value="0.38Ohm"/>
<attribute name="RDC-TYP" value="0.326Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74458233">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458233.pdf"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 74458233 "/>
<attribute name="RDC-MAX" value="0.56Ohm"/>
<attribute name="RDC-TYP" value="0.431Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74458247">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458247.pdf"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 74458247 "/>
<attribute name="RDC-MAX" value="0.85Ohm"/>
<attribute name="RDC-TYP" value="0.633Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74458268">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74458268.pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 74458268 "/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="RDC-TYP" value="0.954Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7445830">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445830.pdf"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7445830 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="1.37Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_XL" prefix="L">
<description>&lt;b&gt;WE-PD4 SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current loading up to 38 A
&lt;br&gt;Compact size
&lt;br&gt;&lt;br&gt;Low-loss ferrite core
&lt;br&gt;Application frequency range up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression, EMI Filter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, 
 &lt;br&gt;Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, &lt;br&gt;Analogic Tech and Diodes

&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14832v209%20Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD4"&gt;https://katalog.we-online.com/en/pbs/WE-PD4&lt;/a&gt;&lt;p&gt;


Updated  by Yingchun,Shan 2019-08-05&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD4_XL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74457006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457006.pdf"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="ISAT" value="38A"/>
<attribute name="PART-NUMBER" value=" 74457006 "/>
<attribute name="RDC-MAX" value="0.002Ohm"/>
<attribute name="RDC-TYP" value="0.001Ohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74457008">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457008.pdf"/>
<attribute name="FRES" value="92MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="35A"/>
<attribute name="PART-NUMBER" value=" 74457008 "/>
<attribute name="RDC-MAX" value="0.003Ohm"/>
<attribute name="RDC-TYP" value="0.002Ohm"/>
<attribute name="VALUE" value="0.8uH"/>
</technology>
<technology name="_74457010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457010.pdf"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="PART-NUMBER" value=" 74457010 "/>
<attribute name="RDC-MAX" value="0.004Ohm"/>
<attribute name="RDC-TYP" value="0.003Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74457012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457012.pdf"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="PART-NUMBER" value=" 74457012 "/>
<attribute name="RDC-MAX" value="0.004Ohm"/>
<attribute name="RDC-TYP" value="0.003Ohm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74457018">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457018.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="PART-NUMBER" value=" 74457018 "/>
<attribute name="RDC-MAX" value="0.005Ohm"/>
<attribute name="RDC-TYP" value="0.005Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_74457027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457027.pdf"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="PART-NUMBER" value=" 74457027 "/>
<attribute name="RDC-MAX" value="0.008Ohm"/>
<attribute name="RDC-TYP" value="0.007Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74457033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457033.pdf"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="PART-NUMBER" value=" 74457033 "/>
<attribute name="RDC-MAX" value="0.009Ohm"/>
<attribute name="RDC-TYP" value="0.008Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74457047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457047.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="PART-NUMBER" value=" 74457047 "/>
<attribute name="RDC-MAX" value="0.011Ohm"/>
<attribute name="RDC-TYP" value="0.009Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74457056">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457056.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="PART-NUMBER" value=" 74457056 "/>
<attribute name="RDC-MAX" value="0.015Ohm"/>
<attribute name="RDC-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74457068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457068.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="PART-NUMBER" value=" 74457068 "/>
<attribute name="RDC-MAX" value="0.017Ohm"/>
<attribute name="RDC-TYP" value="0.014Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74457082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457082.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="PART-NUMBER" value=" 74457082 "/>
<attribute name="RDC-MAX" value="0.019Ohm"/>
<attribute name="RDC-TYP" value="0.016Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7445710">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445710.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="PART-NUMBER" value=" 7445710 "/>
<attribute name="RDC-MAX" value="0.021Ohm"/>
<attribute name="RDC-TYP" value="0.017Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74457112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457112.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="PART-NUMBER" value=" 74457112 "/>
<attribute name="RDC-MAX" value="0.028Ohm"/>
<attribute name="RDC-TYP" value="0.024Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_74457115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457115.pdf"/>
<attribute name="FRES" value="15MHzv"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="PART-NUMBER" value=" 74457115 "/>
<attribute name="RDC-MAX" value="0.035Ohm"/>
<attribute name="RDC-TYP" value="0.029Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74457118">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457118.pdf"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="PART-NUMBER" value=" 74457118 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.033Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_74457122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457122.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="PART-NUMBER" value=" 74457122 "/>
<attribute name="RDC-MAX" value="0.047Ohm"/>
<attribute name="RDC-TYP" value="0.039Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74457127">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457127.pdf"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74457127 "/>
<attribute name="RDC-MAX" value="0.052Ohm"/>
<attribute name="RDC-TYP" value="0.044Ohm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_74457133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457133.pdf"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="PART-NUMBER" value=" 74457133 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.058Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74457139">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457139.pdf"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="PART-NUMBER" value=" 74457139 "/>
<attribute name="RDC-MAX" value="0.078Ohm"/>
<attribute name="RDC-TYP" value="0.065Ohm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_74457147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457147.pdf"/>
<attribute name="FRES" value="9.2MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="PART-NUMBER" value=" 74457147 "/>
<attribute name="RDC-MAX" value="0.109Ohm"/>
<attribute name="RDC-TYP" value="0.091Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74457156">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457156.pdf"/>
<attribute name="FRES" value="8.8MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 74457156 "/>
<attribute name="RDC-MAX" value="0.116Ohm"/>
<attribute name="RDC-TYP" value="0.097Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_74457168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457168.pdf"/>
<attribute name="FRES" value="7.6MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 74457168 "/>
<attribute name="RDC-MAX" value="0.134Ohm"/>
<attribute name="RDC-TYP" value="0.112Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74457182">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457182.pdf"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="PART-NUMBER" value=" 74457182 "/>
<attribute name="RDC-MAX" value="0.173Ohm"/>
<attribute name="RDC-TYP" value="0.144Ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_7445720">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7445720.pdf"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 7445720 "/>
<attribute name="RDC-MAX" value="0.202Ohm"/>
<attribute name="RDC-TYP" value="0.168Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74457212">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457212.pdf"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 74457212 "/>
<attribute name="RDC-MAX" value="0.235Ohm"/>
<attribute name="RDC-TYP" value="0.196Ohm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_74457215">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457215.pdf"/>
<attribute name="FRES" value="4.1MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="PART-NUMBER" value=" 74457215 "/>
<attribute name="RDC-MAX" value="0.268Ohm"/>
<attribute name="RDC-TYP" value="0.223Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74457218">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457218.pdf"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="PART-NUMBER" value=" 74457218 "/>
<attribute name="RDC-MAX" value="0.307Ohm"/>
<attribute name="RDC-TYP" value="0.256Ohm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_74457222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457222.pdf"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 74457222 "/>
<attribute name="RDC-MAX" value="0.388Ohm"/>
<attribute name="RDC-TYP" value="0.323Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74457227">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457227.pdf"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="PART-NUMBER" value=" 74457227 "/>
<attribute name="RDC-MAX" value="0.479Ohm"/>
<attribute name="RDC-TYP" value="0.399Ohm"/>
<attribute name="VALUE" value="270uH"/>
</technology>
<technology name="_74457230">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457230.pdf"/>
<attribute name="FRES" value="1.4MHz"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 74457230 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="1.506Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_74457233">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457233.pdf"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 74457233 "/>
<attribute name="RDC-MAX" value="0.564Ohm"/>
<attribute name="RDC-TYP" value="0.47Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74457239">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457239.pdf"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 74457239 "/>
<attribute name="RDC-MAX" value="0.67Ohm"/>
<attribute name="RDC-TYP" value="0.558Ohm"/>
<attribute name="VALUE" value="390uH"/>
</technology>
<technology name="_74457247">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457247.pdf"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 74457247 "/>
<attribute name="RDC-MAX" value="0.809Ohm"/>
<attribute name="RDC-TYP" value="0.674Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74457256">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457256.pdf"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.78A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 74457256 "/>
<attribute name="RDC-MAX" value="1.026Ohm"/>
<attribute name="RDC-TYP" value="0.855Ohm"/>
<attribute name="VALUE" value="560uH"/>
</technology>
<technology name="_74457268">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457268.pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 74457268 "/>
<attribute name="RDC-MAX" value="1.2Ohm"/>
<attribute name="RDC-TYP" value="1.002Ohm"/>
<attribute name="VALUE" value="680uHV"/>
</technology>
<technology name="_74457282">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74457282.pdf"/>
<attribute name="FRES" value="1.7MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 74457282 "/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="RDC-TYP" value="1.172Ohm"/>
<attribute name="VALUE" value="820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
