<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Unshielded Power Inductors - WE-PD2&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-02-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD2_5848">
<description>&lt;b&gt;WE-PD2 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5848, SMT, 2pins
&lt;br&gt;LXWXH=5.2X5.8X4.5mm</description>
</package>
<package name="WE-PD2_7850">
<description>&lt;b&gt;WE-PD2 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7850, SMT, 2pins
&lt;br&gt;LXWXH=7X7.8X5mm</description>
</package>
<package name="WE-PD2_4532">
<description>&lt;b&gt;WE-PD2 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4532, SMT, 2pins
&lt;br&gt;LXWXH=4X4.5X3.2mm</description>
</package>
<package name="WE-PD2_1054">
<description>&lt;b&gt;WE-PD2 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1054, SMT, 2pins
&lt;br&gt;LXWXH=9X10X5.4mm</description>
</package>
<package name="WE-PD2_3521">
<description>&lt;b&gt;WE-PD2 SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 3521, SMT, 2pins
&lt;br&gt;LXWXH=3X3.5X2.1mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD2_4532" prefix="L">
<description>&lt;b&gt;WE-PD2 SMT Power Inductor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;Saturation currents up to 14 A
&lt;br&gt;Low tolerances at high inductance values
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
&lt;br&gt;Integrated DC/DC converter
&lt;br&gt;Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD2"&gt;www.we-online.com/en/components/products/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated by Ella 2023-02-20&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447730">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447730?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="5.72A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447730 "/>
<attribute name="RDC-MAX" value="0.049Ohm"/>
<attribute name="RDC-TYP" value="0.014Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744773014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773014?ae"/>
<attribute name="FRES" value="103MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="5.04A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773014 "/>
<attribute name="RDC-MAX" value="0.056Ohm"/>
<attribute name="RDC-TYP" value="0.022Ohm"/>
<attribute name="VALUE" value="1.4uH"/>
</technology>
<technology name="_744773018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773018?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773018 "/>
<attribute name="RDC-MAX" value="0.064Ohm"/>
<attribute name="RDC-TYP" value="0.028Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744773022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773022?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="3.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773022 "/>
<attribute name="RDC-MAX" value="0.071Ohm"/>
<attribute name="RDC-TYP" value="0.034Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744773027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773027?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="2.25A"/>
<attribute name="ISAT" value="2.97A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773027 "/>
<attribute name="RDC-MAX" value="0.079Ohm"/>
<attribute name="RDC-TYP" value="0.039Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_744773033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773033?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.88A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773033 "/>
<attribute name="RDC-MAX" value="0.086Ohm"/>
<attribute name="RDC-TYP" value="0.041Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744773039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773039?ae"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="1.88A"/>
<attribute name="ISAT" value="2.57A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773039 "/>
<attribute name="RDC-MAX" value="0.094Ohm"/>
<attribute name="RDC-TYP" value="0.054Ohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744773047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773047?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="1.82A"/>
<attribute name="ISAT" value="2.46A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773047 "/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="RDC-TYP" value="0.059Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744773056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773056?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="1.58A"/>
<attribute name="ISAT" value="2.43A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773056 "/>
<attribute name="RDC-MAX" value="0.126Ohm"/>
<attribute name="RDC-TYP" value="0.069Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744773068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773068?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="1.54A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773068 "/>
<attribute name="RDC-MAX" value="0.131Ohm"/>
<attribute name="RDC-TYP" value="0.076Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744773082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773082?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773082 "/>
<attribute name="RDC-MAX" value="0.146Ohm"/>
<attribute name="RDC-TYP" value="0.116Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74477310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477310?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.74A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477310 "/>
<attribute name="RDC-MAX" value="0.182Ohm"/>
<attribute name="RDC-TYP" value="0.118Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744773112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773112?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="1.28A"/>
<attribute name="ISAT" value="1.62A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773112 "/>
<attribute name="RDC-MAX" value="0.21Ohm"/>
<attribute name="RDC-TYP" value="0.156Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744773115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773115?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.46A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773115 "/>
<attribute name="RDC-MAX" value="0.235Ohm"/>
<attribute name="RDC-TYP" value="0.204Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744773118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773118?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.29A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773118 "/>
<attribute name="RDC-MAX" value="0.338Ohm"/>
<attribute name="RDC-TYP" value="0.225Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744773122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773122?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773122 "/>
<attribute name="RDC-MAX" value="0.37Ohm"/>
<attribute name="RDC-TYP" value="0.261Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744773127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773127?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="0.94A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773127 "/>
<attribute name="RDC-MAX" value="0.522Ohm"/>
<attribute name="RDC-TYP" value="0.328Ohm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744773133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773133?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.86A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773133 "/>
<attribute name="RDC-MAX" value="0.54Ohm"/>
<attribute name="RDC-TYP" value="0.37Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744773139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773139?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.77A"/>
<attribute name="ISAT" value="0.87A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773139 "/>
<attribute name="RDC-MAX" value="0.587Ohm"/>
<attribute name="RDC-TYP" value="0.418Ohm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_744773147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773147?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="0.68A"/>
<attribute name="ISAT" value="0.77A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773147 "/>
<attribute name="RDC-MAX" value="0.844Ohm"/>
<attribute name="RDC-TYP" value="0.523Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744773156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773156?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773156 "/>
<attribute name="RDC-MAX" value="0.937Ohm"/>
<attribute name="RDC-TYP" value="0.714Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_744773168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744773168?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744773168 "/>
<attribute name="RDC-MAX" value="1.117Ohm"/>
<attribute name="RDC-TYP" value="0.754Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74477330A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477330A?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="0.12A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74477330A"/>
<attribute name="RDC-MAX" value="15Ohm"/>
<attribute name="RDC-TYP" value="12.5Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_7850" prefix="L">
<description>&lt;b&gt;WE-PD2 SMT Power Inductor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;Saturation currents up to 14 A
&lt;br&gt;Low tolerances at high inductance values
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
&lt;br&gt;Integrated DC/DC converter
&lt;br&gt;Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD2"&gt;www.we-online.com/en/components/products/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated by Ella 2023-02-20&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744775022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775022?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775022 "/>
<attribute name="RDC-MAX" value="0.015Ohm"/>
<attribute name="RDC-TYP" value="0.008Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744775033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775033?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="4.9A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775033 "/>
<attribute name="RDC-MAX" value="0.018Ohm"/>
<attribute name="RDC-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744775047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775047?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775047 "/>
<attribute name="RDC-MAX" value="0.019Ohm"/>
<attribute name="RDC-TYP" value="0.016Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744775056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775056?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775056 "/>
<attribute name="RDC-MAX" value="0.022Ohm"/>
<attribute name="RDC-TYP" value="0.018Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744775068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775068?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775068 "/>
<attribute name="RDC-MAX" value="0.026Ohm"/>
<attribute name="RDC-TYP" value="0.022Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744775082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775082?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775082 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.029Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74477510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477510?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477510 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.044Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744775112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775112?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2.18A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775112 "/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="RDC-TYP" value="0.042Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744775115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775115?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.93A"/>
<attribute name="ISAT" value="2.23A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775115 "/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="RDC-TYP" value="0.044Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744775118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775118?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.89A"/>
<attribute name="ISAT" value="2.14A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775118 "/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="RDC-TYP" value="0.053Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744775122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775122?ae"/>
<attribute name="FRES" value="17.5MHz"/>
<attribute name="IR" value="1.76A"/>
<attribute name="ISAT" value="1.81A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775122 "/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="RDC-TYP" value="0.065Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744775127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775127?ae"/>
<attribute name="FRES" value="15.5MHz"/>
<attribute name="IR" value="1.48A"/>
<attribute name="ISAT" value="1.62A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775127 "/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="RDC-TYP" value="0.074Ohm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744775133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775133?ae"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.47A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775133 "/>
<attribute name="RDC-MAX" value="0.13Ohm"/>
<attribute name="RDC-TYP" value="0.088Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744775139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775139?ae"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.33A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775139 "/>
<attribute name="RDC-MAX" value="0.16Ohm"/>
<attribute name="RDC-TYP" value="0.116Ohm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_744775147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775147?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.17A"/>
<attribute name="ISAT" value="1.24A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775147 "/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="RDC-TYP" value="0.134Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744775156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775156?ae"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="IR" value="1.04A"/>
<attribute name="ISAT" value="1.14A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775156 "/>
<attribute name="RDC-MAX" value="0.24Ohm"/>
<attribute name="RDC-TYP" value="0.189Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_744775168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775168?ae"/>
<attribute name="FRES" value="9.7MHz"/>
<attribute name="IR" value="0.99A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775168 "/>
<attribute name="RDC-MAX" value="0.28Ohm"/>
<attribute name="RDC-TYP" value="0.218Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744775182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775182?ae"/>
<attribute name="FRES" value="8.6MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775182 "/>
<attribute name="RDC-MAX" value="0.37Ohm"/>
<attribute name="RDC-TYP" value="0.248Ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_74477520">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477520?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.77A"/>
<attribute name="ISAT" value="0.86A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477520 "/>
<attribute name="RDC-MAX" value="0.43Ohm"/>
<attribute name="RDC-TYP" value="0.208Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744775210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775210?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.67A"/>
<attribute name="ISAT" value="0.81A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775210 "/>
<attribute name="RDC-MAX" value="0.47Ohm"/>
<attribute name="RDC-TYP" value="0.308Ohm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_744775215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775215?ae"/>
<attribute name="FRES" value="6.2MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.71A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775215 "/>
<attribute name="RDC-MAX" value="0.64Ohm"/>
<attribute name="RDC-TYP" value="0.467Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744775218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775218?ae"/>
<attribute name="FRES" value="5.8MHz"/>
<attribute name="IR" value="0.55A"/>
<attribute name="ISAT" value="0.57A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775218 "/>
<attribute name="RDC-MAX" value="0.71Ohm"/>
<attribute name="RDC-TYP" value="0.574Ohm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_744775222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775222?ae"/>
<attribute name="FRES" value="5.4MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775222 "/>
<attribute name="RDC-MAX" value="0.96Ohm"/>
<attribute name="RDC-TYP" value="0.614Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744775227">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775227?ae"/>
<attribute name="FRES" value="4.7MHz"/>
<attribute name="IR" value="0.47A"/>
<attribute name="ISAT" value="0.51A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775227 "/>
<attribute name="RDC-MAX" value="1.11Ohm"/>
<attribute name="RDC-TYP" value="0.699Ohm"/>
<attribute name="VALUE" value="270uH"/>
</technology>
<technology name="_744775233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775233?ae"/>
<attribute name="FRES" value="4.2MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.48A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775233 "/>
<attribute name="RDC-MAX" value="1.26Ohm"/>
<attribute name="RDC-TYP" value="0.81Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_744775239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775239?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="IR" value="0.38A"/>
<attribute name="ISAT" value="0.43A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775239 "/>
<attribute name="RDC-MAX" value="1.77Ohm"/>
<attribute name="RDC-TYP" value="1.151Ohm"/>
<attribute name="VALUE" value="390uH"/>
</technology>
<technology name="_744775247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744775247?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775247 "/>
<attribute name="RDC-MAX" value="1.96Ohm"/>
<attribute name="RDC-TYP" value="1.37Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74477530">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477530?ae"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477530 "/>
<attribute name="RDC-MAX" value="3.3Ohm"/>
<attribute name="RDC-TYP" value="2.78Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_5848" prefix="L">
<description>&lt;b&gt;WE-PD2 SMT Power Inductor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;Saturation currents up to 14 A
&lt;br&gt;Low tolerances at high inductance values
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
&lt;br&gt;Integrated DC/DC converter
&lt;br&gt;Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD2"&gt;www.we-online.com/en/components/products/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated by Ella 2023-02-20&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_5848">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744774003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774003?ae"/>
<attribute name="FRES" value="295MHz"/>
<attribute name="IR" value="10.8A"/>
<attribute name="ISAT" value="15.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774003 "/>
<attribute name="RDC-MAX" value="0.008Ohm"/>
<attribute name="RDC-TYP" value="0.006Ohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744774022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774022?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="8.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774022 "/>
<attribute name="RDC-MAX" value="0.041Ohm"/>
<attribute name="RDC-TYP" value="0.026Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744774027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774027?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774027 "/>
<attribute name="RDC-MAX" value="0.045Ohm"/>
<attribute name="RDC-TYP" value="0.032Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_744774033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774033?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774033 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="RDC-TYP" value="0.042Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744774047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774047?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774047 "/>
<attribute name="RDC-MAX" value="0.071Ohm"/>
<attribute name="RDC-TYP" value="0.056Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744774068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774068?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774068 "/>
<attribute name="RDC-MAX" value="0.082Ohm"/>
<attribute name="RDC-TYP" value="0.071Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74477410">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477410?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477410 "/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="RDC-TYP" value="0.078Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744774112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774112?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.94A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774112 "/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="RDC-TYP" value="0.082Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744774115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774115?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.53A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774115 "/>
<attribute name="RDC-MAX" value="0.14Ohm"/>
<attribute name="RDC-TYP" value="0.089Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744774118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774118?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.69A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774118 "/>
<attribute name="RDC-MAX" value="0.15Ohm"/>
<attribute name="RDC-TYP" value="0.104Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744774122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774122?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.28A"/>
<attribute name="ISAT" value="1.53A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774122 "/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="RDC-TYP" value="0.109Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744774127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774127?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.19A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774127 "/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="RDC-TYP" value="0.133Ohm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744774133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774133?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="1.09A"/>
<attribute name="ISAT" value="1.17A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774133 "/>
<attribute name="RDC-MAX" value="0.23Ohm"/>
<attribute name="RDC-TYP" value="0.15Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744774139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774139?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.94A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774139 "/>
<attribute name="RDC-MAX" value="0.32Ohm"/>
<attribute name="RDC-TYP" value="0.215Ohm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_744774147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774147?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="0.86A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774147 "/>
<attribute name="RDC-MAX" value="0.37Ohm"/>
<attribute name="RDC-TYP" value="0.26Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744774156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774156?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.77A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774156 "/>
<attribute name="RDC-MAX" value="0.42Ohm"/>
<attribute name="RDC-TYP" value="0.298Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_744774168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774168?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="0.86A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774168 "/>
<attribute name="RDC-MAX" value="0.46Ohm"/>
<attribute name="RDC-TYP" value="0.313Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744774182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774182?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.72A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774182 "/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="RDC-TYP" value="0.475Ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_74477420">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477420?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="0.57A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477420 "/>
<attribute name="RDC-MAX" value="0.65Ohm"/>
<attribute name="RDC-TYP" value="0.51Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744774212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774212?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="0.63A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774212 "/>
<attribute name="RDC-MAX" value="0.93Ohm"/>
<attribute name="RDC-TYP" value="0.66Ohm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_744774215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774215?ae"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="0.46A"/>
<attribute name="ISAT" value="0.54A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774215 "/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="RDC-TYP" value="0.72Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744774218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774218?ae"/>
<attribute name="FRES" value="5.8MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774218 "/>
<attribute name="RDC-MAX" value="1.38Ohm"/>
<attribute name="RDC-TYP" value="0.85Ohm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_744774222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744774222?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744774222 "/>
<attribute name="RDC-MAX" value="1.57Ohm"/>
<attribute name="RDC-TYP" value="0.945Ohm"/>
<attribute name="VALUE" value="20uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_1054" prefix="L">
<description>&lt;b&gt;WE-PD2 SMT Power Inductor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;Saturation currents up to 14 A
&lt;br&gt;Low tolerances at high inductance values
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
&lt;br&gt;Integrated DC/DC converter
&lt;br&gt;Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD2"&gt;www.we-online.com/en/components/products/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated by Ella 2023-02-20&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744776012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776012?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="7.4A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776012 "/>
<attribute name="RDC-MAX" value="0.006Ohm"/>
<attribute name="RDC-TYP" value="0.004Ohm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744776022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776022?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776022 "/>
<attribute name="RDC-MAX" value="0.01Ohm"/>
<attribute name="RDC-TYP" value="0.007Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744776033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776033?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776033 "/>
<attribute name="RDC-MAX" value="0.015Ohm"/>
<attribute name="RDC-TYP" value="0.009Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744776047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776047?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776047 "/>
<attribute name="RDC-MAX" value="0.017Ohm"/>
<attribute name="RDC-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744776056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776056?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776056 "/>
<attribute name="RDC-MAX" value="0.019Ohm"/>
<attribute name="RDC-TYP" value="0.015Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744776068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776068?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="4.4A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776068 "/>
<attribute name="RDC-MAX" value="0.022Ohm"/>
<attribute name="RDC-TYP" value="0.016Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744776082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776082?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="4.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776082 "/>
<attribute name="RDC-MAX" value="0.026Ohm"/>
<attribute name="RDC-TYP" value="0.02Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74477610">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477610?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="2.98A"/>
<attribute name="ISAT" value="3.24A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477610 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="RDC-TYP" value="0.028Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744776112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776112?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="2.72A"/>
<attribute name="ISAT" value="3.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776112 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.033Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744776115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776115?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.47A"/>
<attribute name="ISAT" value="2.88A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776115 "/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="RDC-TYP" value="0.034Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744776118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776118?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="2.36A"/>
<attribute name="ISAT" value="2.43A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776118 "/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="RDC-TYP" value="0.043Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744776122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776122?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.04A"/>
<attribute name="ISAT" value="2.07A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776122 "/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="RDC-TYP" value="0.051Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744776127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776127?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.95A"/>
<attribute name="ISAT" value="1.98A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776127 "/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="RDC-TYP" value="0.063Ohm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744776133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776133?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="1.78A"/>
<attribute name="ISAT" value="1.89A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776133 "/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="RDC-TYP" value="0.083Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744776139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776139?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.62A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776139 "/>
<attribute name="RDC-MAX" value="0.14Ohm"/>
<attribute name="RDC-TYP" value="0.098Ohm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_744776147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776147?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.62A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776147 "/>
<attribute name="RDC-MAX" value="0.17Ohm"/>
<attribute name="RDC-TYP" value="0.095Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744776156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776156?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.36A"/>
<attribute name="ISAT" value="1.53A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776156 "/>
<attribute name="RDC-MAX" value="0.19Ohm"/>
<attribute name="RDC-TYP" value="0.112Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_744776168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776168?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="1.19A"/>
<attribute name="ISAT" value="1.49A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776168 "/>
<attribute name="RDC-MAX" value="0.22Ohm"/>
<attribute name="RDC-TYP" value="0.138Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744776182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776182?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.11A"/>
<attribute name="ISAT" value="1.17A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776182 "/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="RDC-TYP" value="0.15Ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_74477620">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477620?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="1.02A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477620 "/>
<attribute name="RDC-MAX" value="0.35Ohm"/>
<attribute name="RDC-TYP" value="0.2Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744776212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776212?ae"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="0.94A"/>
<attribute name="ISAT" value="0.99A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776212 "/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="RDC-TYP" value="0.243Ohm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_744776215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776215?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.81A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776215 "/>
<attribute name="RDC-MAX" value="0.47Ohm"/>
<attribute name="RDC-TYP" value="0.3Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744776218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776218?ae"/>
<attribute name="FRES" value="5.4MHz"/>
<attribute name="IR" value="0.76A"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776218 "/>
<attribute name="RDC-MAX" value="0.63Ohm"/>
<attribute name="RDC-TYP" value="0.32Ohm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_744776222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776222?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.67A"/>
<attribute name="ISAT" value="0.77A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776222 "/>
<attribute name="RDC-MAX" value="0.73Ohm"/>
<attribute name="RDC-TYP" value="0.451Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744776227">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776227?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776227 "/>
<attribute name="RDC-MAX" value="0.97Ohm"/>
<attribute name="RDC-TYP" value="0.5Ohm"/>
<attribute name="VALUE" value="270uH"/>
</technology>
<technology name="_744776233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776233?ae"/>
<attribute name="FRES" value="4.1MHz"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="0.59A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776233 "/>
<attribute name="RDC-MAX" value="1.15Ohm"/>
<attribute name="RDC-TYP" value="0.75Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_744776239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776239?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="0.54A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776239 "/>
<attribute name="RDC-MAX" value="1.3Ohm"/>
<attribute name="RDC-TYP" value="0.794Ohm"/>
<attribute name="VALUE" value="390uH"/>
</technology>
<technology name="_744776247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776247?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.44A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776247 "/>
<attribute name="RDC-MAX" value="1.48Ohm"/>
<attribute name="RDC-TYP" value="0.969Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_744776256">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776256?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776256 "/>
<attribute name="RDC-MAX" value="1.9Ohm"/>
<attribute name="RDC-TYP" value="1.047Ohm"/>
<attribute name="VALUE" value="560uH"/>
</technology>
<technology name="_744776260">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776260?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776260 "/>
<attribute name="RDC-MAX" value="1.39Ohm"/>
<attribute name="RDC-TYP" value="1.17Ohm"/>
<attribute name="VALUE" value="600uH"/>
</technology>
<technology name="_744776268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776268?ae"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.43A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776268 "/>
<attribute name="RDC-MAX" value="2.25Ohm"/>
<attribute name="RDC-TYP" value="1.245Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_744776282">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776282?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.41A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776282 "/>
<attribute name="RDC-MAX" value="2.55Ohm"/>
<attribute name="RDC-TYP" value="1.42Ohm"/>
<attribute name="VALUE" value="820uH"/>
</technology>
<technology name="_74477630">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477630?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477630 "/>
<attribute name="RDC-MAX" value="2.6Ohm"/>
<attribute name="RDC-TYP" value="2.2Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_744776312">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776312?ae"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776312 "/>
<attribute name="RDC-MAX" value="3Ohm"/>
<attribute name="RDC-TYP" value="2.48Ohm"/>
<attribute name="VALUE" value="1200uH"/>
</technology>
<technology name="_744776322">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744776322?ae"/>
<attribute name="FRES" value="1.4MHz"/>
<attribute name="IR" value="0.18A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776322 "/>
<attribute name="RDC-MAX" value="5.3Ohm"/>
<attribute name="RDC-TYP" value="4.4Ohm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_3521" prefix="L">
<description>&lt;b&gt;WE-PD2 SMT Power Inductor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;Saturation currents up to 14 A
&lt;br&gt;Low tolerances at high inductance values
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
&lt;br&gt;Integrated DC/DC converter
&lt;br&gt;Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o97350v209%20Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD2"&gt;www.we-online.com/en/components/products/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated by Ella 2023-02-20&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_3521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447732010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732010?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="2.55A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732010 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="RDC-TYP" value="0.039Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7447732015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732015?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="2.08A"/>
<attribute name="ISAT" value="3.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732015 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.054Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7447732022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732022?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="1.71A"/>
<attribute name="ISAT" value="2.54A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732022 "/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="RDC-TYP" value="0.07Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7447732033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732033?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="1.39A"/>
<attribute name="ISAT" value="2.09A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732033 "/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="RDC-TYP" value="0.091Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7447732047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732047?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.16A"/>
<attribute name="ISAT" value="1.77A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732047 "/>
<attribute name="RDC-MAX" value="0.16Ohm"/>
<attribute name="RDC-TYP" value="0.125Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7447732068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732068?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="0.96A"/>
<attribute name="ISAT" value="1.48A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732068 "/>
<attribute name="RDC-MAX" value="0.21Ohm"/>
<attribute name="RDC-TYP" value="0.17Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7447732110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732110?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.23A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732110 "/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="RDC-TYP" value="0.237Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7447732115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732115?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="1.01A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732115 "/>
<attribute name="RDC-MAX" value="0.43Ohm"/>
<attribute name="RDC-TYP" value="0.347Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7447732122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732122?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="0.53A"/>
<attribute name="ISAT" value="0.84A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732122 "/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="RDC-TYP" value="0.561Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7447732133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732133?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732133 "/>
<attribute name="RDC-MAX" value="0.97Ohm"/>
<attribute name="RDC-TYP" value="0.778Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7447732147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732147?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.59A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732147 "/>
<attribute name="RDC-MAX" value="1.33Ohm"/>
<attribute name="RDC-TYP" value="1.11Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7447732168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732168?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.49A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732168 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="1.57Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7447732210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447732210?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.24A"/>
<attribute name="ISAT" value="0.41A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447732210 "/>
<attribute name="RDC-MAX" value="2.8Ohm"/>
<attribute name="RDC-TYP" value="2.42Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
