<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - V-Chip SMT - WCAP-ASLI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-10-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASLI_D6.3L6.1">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X6.1X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D6.3L7.7">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D8L6.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,&lt;BR&gt;8X6.5X2.3(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D8L10.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X10.5X3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D12.5L14">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,12.5X14X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D5L5.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,&lt;BR&gt;5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D10L10.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X10.5X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D16L17">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,&lt;BR&gt;16X17X6.6(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_D4L5.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLI_D6.3L5.5">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASLI_D6.3L6.1" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D6.3L6.1">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080864003">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080864003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="LENGTH" value="6.1mm"/>
<attribute name="PART-NUMBER" value="865080864003"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="3800mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D6.3L7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D6.3L7.7">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080145010">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080145010?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080145010"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865080245009">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080245009?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080245009"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865080345010">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080345010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="265mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080345010"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="450mohm"/>
</technology>
<technology name="_865080345012">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080345012?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080345012"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="430mohm"/>
</technology>
<technology name="_865080445010">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080445010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="290mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080445010"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="380mohm"/>
</technology>
<technology name="_865080545010">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080545010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080545010"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="490mohm"/>
</technology>
<technology name="_865080545011">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080545011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="265mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080545011"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="400mohm"/>
</technology>
<technology name="_865080545012">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080545012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080545012"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="380mohm"/>
</technology>
<technology name="_865080645009">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080645009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="13.5uA"/>
<attribute name="I-RIPPLE" value="180mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080645009"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="1200mohm"/>
</technology>
<technology name="_865080645010">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080645010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080645010"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="710mohm"/>
</technology>
<technology name="_865080645012">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080645012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080645012"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="700mohm"/>
</technology>
<technology name="_865080745011">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080745011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080745011"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="1026mohm"/>
</technology>
<technology name="_865080845004">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080845004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080845004"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="3142mohm"/>
</technology>
<technology name="_865080845005">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080845005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865080845005"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="3178mohm"/>
</technology>
<technology name="_865081745005">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081745005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865081745005"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="2661mohm"/>
</technology>
<technology name="_865081745006">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081745006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="17.6uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865081745006"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="2347mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D8L6.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D8L6.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080149011">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080149011?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="290mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080149011"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="340mohm"/>
</technology>
<technology name="_865080249010">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080249010?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="285mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080249010"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="400mohm"/>
</technology>
<technology name="_865080349011">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080349011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080349011"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865080349013">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080349013?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="285mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080349013"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="410mohm"/>
</technology>
<technology name="_865080449011">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080449011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080449011"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865080649011">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080649011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080649011"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="700mohm"/>
</technology>
<technology name="_865080649013">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080649013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865080649013"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="690mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D5L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D5L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080142005">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080142005?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.528uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080142005"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="1100mohm"/>
</technology>
<technology name="_865080142006">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080142006?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4.284uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080142006"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="900mohm"/>
</technology>
<technology name="_865080142007">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080142007?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080142007"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865080242002">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080242002?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080242002"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="1900mohm"/>
</technology>
<technology name="_865080242004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080242004?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="165mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080242004"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="1100mohm"/>
</technology>
<technology name="_865080342004">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080342004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4.32uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080342004"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="740mohm"/>
</technology>
<technology name="_865080342006">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080342006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="195mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080342006"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="1050mohm"/>
</technology>
<technology name="_865080442003">
<attribute name="C" value="15 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080442003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.75uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080442003"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="1900mohm"/>
</technology>
<technology name="_865080442004">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080442004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080442004"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="1200mohm"/>
</technology>
<technology name="_865080442006">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080442006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080442006"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="1050mohm"/>
</technology>
<technology name="_865080542005">
<attribute name="C" value="15 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080542005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.25uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080542005"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="1200mohm"/>
</technology>
<technology name="_865080542006">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080542006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080542006"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="1100mohm"/>
</technology>
<technology name="_865080642005">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080642005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080642005"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="3800mohm"/>
</technology>
<technology name="_865080642006">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080642006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="95mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080642006"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="2800mohm"/>
</technology>
<technology name="_865080742008">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080742008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="14mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080742008"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="4236mohm"/>
</technology>
<technology name="_865080742009">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080742009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="22mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080742009"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="4193mohm"/>
</technology>
<technology name="_865081742002">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081742002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865081742002"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="10386mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D10L10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D10L10.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080157015">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080157015?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080157015"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="160mohm"/>
</technology>
<technology name="_865080157016">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080157016?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080157016"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="130mohm"/>
</technology>
<technology name="_865080257013">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080257013?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080257013"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="200mohm"/>
</technology>
<technology name="_865080257014">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080257014?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080257014"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="150mohm"/>
</technology>
<technology name="_865080357016">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080357016?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="720mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080357016"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="160mohm"/>
</technology>
<technology name="_865080457015">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080457015?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080457015"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="150mohm"/>
</technology>
<technology name="_865080557015">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080557015?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080557015"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="150mohm"/>
</technology>
<technology name="_865080657017">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080657017?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080657017"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080657018">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080657018?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080657018"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="230mohm"/>
</technology>
<technology name="_865080757014">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080757014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080757014"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="346mohm"/>
</technology>
<technology name="_865080857007">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080857007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="135mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080857007"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="1031mohm"/>
</technology>
<technology name="_865081757008">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081757008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="37.6uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865081757008"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="1159mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D12.5L14" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D12.5L14">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080162017">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080162017?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080162017"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080262015">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080262015?ae"/>
<attribute name="DF" value="21%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080262015"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080362017">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080362017?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080362017"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080462016">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080462016?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080462016"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080562016">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080562016?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080562016"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080562017">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080562017?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080562017"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="80mohm"/>
</technology>
<technology name="_865080662019">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080662019?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080662019"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="210mohm"/>
</technology>
<technology name="_865080762015">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080762015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080762015"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="152mohm"/>
</technology>
<technology name="_865080862008">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080862008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865080862008"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="349mohm"/>
</technology>
<technology name="_865081762009">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081762009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="80uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="PART-NUMBER" value="865081762009"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="493mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D8L10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D8L10.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080153012">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080153012?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080153012"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="280mohm"/>
</technology>
<technology name="_865080153013">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080153013?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080153013"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080153014">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080153014?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="530mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080153014"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="200mohm"/>
</technology>
<technology name="_865080253011">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080253011?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080253011"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080253012">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080253012?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080253012"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080353014">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080353014?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080353014"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080353015">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080353015?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="590mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080353015"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="220mohm"/>
</technology>
<technology name="_865080453012">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080453012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080453012"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865080453013">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080453013?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="530mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080453013"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="220mohm"/>
</technology>
<technology name="_865080453014">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080453014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080453014"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="200mohm"/>
</technology>
<technology name="_865080553013">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080553013?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="510mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080553013"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="240mohm"/>
</technology>
<technology name="_865080553014">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080553014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080553014"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="210mohm"/>
</technology>
<technology name="_865080653014">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080653014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080653014"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="520mohm"/>
</technology>
<technology name="_865080653015">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080653015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080653015"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="500mohm"/>
</technology>
<technology name="_865080653016">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080653016?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080653016"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="460mohm"/>
</technology>
<technology name="_865080753012">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080753012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="112mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080753012"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="452mohm"/>
</technology>
<technology name="_865080753013">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080753013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="119mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080753013"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="591mohm"/>
</technology>
<technology name="_865080853006">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080853006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865080853006"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="1298mohm"/>
</technology>
<technology name="_865081753007">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081753007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="112mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value="865081753007"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="1542mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D4L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D4L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080140001">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080140001?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080140001"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="2200mohm"/>
</technology>
<technology name="_865080140002">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080140002?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="79mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080140002"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="1980mohm"/>
</technology>
<technology name="_865080140003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080140003?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="82mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080140003"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="1900mohm"/>
</technology>
<technology name="_865080140004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080140004?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="86mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080140004"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="1880mohm"/>
</technology>
<technology name="_865080240001">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080240001?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080240001"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="2200mohm"/>
</technology>
<technology name="_865080240003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080240003?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080240003"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="1850mohm"/>
</technology>
<technology name="_865080340001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080340001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080340001"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="2200mohm"/>
</technology>
<technology name="_865080340002">
<attribute name="C" value="15 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080340002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080340002"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="2000mohm"/>
</technology>
<technology name="_865080340003">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080340003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080340003"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="1980mohm"/>
</technology>
<technology name="_865080440001">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080440001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080440001"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="2800mohm"/>
</technology>
<technology name="_865080440002">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080440002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080440002"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="2100mohm"/>
</technology>
<technology name="_865080540001">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080540001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080540001"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="2800mohm"/>
</technology>
<technology name="_865080540002">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080540002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080540002"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="2500mohm"/>
</technology>
<technology name="_865080540003">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080540003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="88mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080540003"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="2200mohm"/>
</technology>
<technology name="_865080540004">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080540004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080540004"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="2000mohm"/>
</technology>
<technology name="_865080640001">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080640001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080640001"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="4500mohm"/>
</technology>
<technology name="_865080640002">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080640002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080640002"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="4500mohm"/>
</technology>
<technology name="_865080640003">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080640003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080640003"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="4500mohm"/>
</technology>
<technology name="_865080640004">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080640004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080640004"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="4500mohm"/>
</technology>
<technology name="_865080740005">
<attribute name="C" value="0.47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080740005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3.5mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080740005"/>
<attribute name="VALUE" value="0.47 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="21017mohm"/>
</technology>
<technology name="_865080740006">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080740006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080740006"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="20749mohm"/>
</technology>
<technology name="_865080740007">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080740007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="11mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080740007"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="6111mohm"/>
</technology>
<technology name="_865080840001">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080840001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080840001"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="20381mohm"/>
</technology>
<technology name="_865081740001">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081740001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865081740001"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="21618mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D16L17" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D16L17">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080163018">
<attribute name="C" value="6800 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080163018?ae"/>
<attribute name="DF" value="34%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080163018"/>
<attribute name="VALUE" value="6800 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="52mohm"/>
</technology>
<technology name="_865080263016">
<attribute name="C" value="4700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080263016?ae"/>
<attribute name="DF" value="25%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080263016"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="52mohm"/>
</technology>
<technology name="_865080363018">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080363018?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080363018"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="52mohm"/>
</technology>
<technology name="_865080463017">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080463017?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080463017"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="52mohm"/>
</technology>
<technology name="_865080563018">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080563018?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080563018"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="52mohm"/>
</technology>
<technology name="_865080663020">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080663020?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080663020"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="78mohm"/>
</technology>
<technology name="_865080763016">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080763016?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="630mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080763016"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="125mohm"/>
</technology>
<technology name="_865080863009">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080863009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865080863009"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="267mohm"/>
</technology>
<technology name="_865081763010">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081763010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865081763010"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="257mohm"/>
</technology>
<technology name="_865081763011">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081763011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="176uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="17mm"/>
<attribute name="PART-NUMBER" value="865081763011"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="224mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_D6.3L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_D6.3L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080143008">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080143008?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="235mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080143008"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="510mohm"/>
</technology>
<technology name="_865080143009">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080143009?ae"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080143009"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="6.3VDC"/>
<attribute name="Z" value="480mohm"/>
</technology>
<technology name="_865080243005">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080243005?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.6uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080243005"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="570mohm"/>
</technology>
<technology name="_865080243006">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080243006?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080243006"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="550mohm"/>
</technology>
<technology name="_865080243007">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080243007?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080243007"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="530mohm"/>
</technology>
<technology name="_865080243008">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080243008?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080243008"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="10VDC"/>
<attribute name="Z" value="490mohm"/>
</technology>
<technology name="_865080343005">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080343005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080343005"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="600mohm"/>
</technology>
<technology name="_865080343007">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080343007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080343007"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="560mohm"/>
</technology>
<technology name="_865080343008">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080343008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080343008"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="540mohm"/>
</technology>
<technology name="_865080343009">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080343009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="255mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080343009"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16VDC"/>
<attribute name="Z" value="520mohm"/>
</technology>
<technology name="_865080443005">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080443005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.75uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080443005"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="620mohm"/>
</technology>
<technology name="_865080443007">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080443007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080443007"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="560mohm"/>
</technology>
<technology name="_865080443008">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080443008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080443008"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="540mohm"/>
</technology>
<technology name="_865080443009">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080443009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080443009"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="480mohm"/>
</technology>
<technology name="_865080543007">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080543007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080543007"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="600mohm"/>
</technology>
<technology name="_865080543008">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080543008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080543008"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="540mohm"/>
</technology>
<technology name="_865080543009">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080543009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080543009"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35VDC"/>
<attribute name="Z" value="530mohm"/>
</technology>
<technology name="_865080643007">
<attribute name="C" value="15 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080643007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="7.5uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080643007"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="1600mohm"/>
</technology>
<technology name="_865080643008">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080643008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080643008"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50VDC"/>
<attribute name="Z" value="1300mohm"/>
</technology>
<technology name="_865080743010">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080743010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080743010"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="63VDC"/>
<attribute name="Z" value="1928mohm"/>
</technology>
<technology name="_865080843002">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865080843002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865080843002"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="Z" value="5267mohm"/>
</technology>
<technology name="_865081743003">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081743003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865081743003"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="7260mohm"/>
</technology>
<technology name="_865081743004">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865081743004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.76uA"/>
<attribute name="I-RIPPLE" value="25mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865081743004"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="80VDC"/>
<attribute name="Z" value="6328mohm"/>
</technology>
<technology name="_S8650804430071">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/S8650804430071?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="S8650804430071"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
<attribute name="Z" value="560mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
