<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Radial THT - WCAP-AT1H&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-10-30&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AT1H_D13L50">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;13X50X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D8L11.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D10L20">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;10X20X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D18L35.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D10L16">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;10X16X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D13L25">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;13X25X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D18L31.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D8L16">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;8X16X3.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D16L31.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D6.3L11">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D16L21">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X21X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D5L11">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,&lt;BR&gt;5X11X2X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D10L12.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,&lt;BR&gt;10X12.5X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D18L21">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X21X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D18L25">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D13L20">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,&lt;BR&gt;13X20X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D16L35.5">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_D16L25">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AT1H_D13L50" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D13L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241978002">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241978002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="615uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PART-NUMBER" value="860241978002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="420VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D8L11.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D8L11.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240274006">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240274006?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240274006"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240374004">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240374004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="245mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240374004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240374005">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240374005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240374005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240374006">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240374006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240374006"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240474004">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240474004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240474004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240474005">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240474005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="327mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240474005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240574004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240574004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240574004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240574005">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240574005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240574005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240674004">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240674004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="241mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240674004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240674005">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240674005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="287mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860240674005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D10L20" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D10L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240475008">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240475008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="805mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240475008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240475009">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240475009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="950mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240475009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240575008">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240575008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240575008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240675008">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240675008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="747mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240675008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240975001">
<attribute name="C" value=""/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240975001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value=""/>
<attribute name="I-LEAK" value="164uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="LENGTH" value=""/>
<attribute name="PART-NUMBER" value=" 860240975001 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860240975002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240975002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="240.8uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240975002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241075003">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241075003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241075003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241075004">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241075004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="276uA"/>
<attribute name="I-RIPPLE" value="470mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241075004"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241175001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241175001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="200uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241175001"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241175002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241175002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="320uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241175002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D18L35.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D18L35.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241081001">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241081001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="2740uA"/>
<attribute name="I-RIPPLE" value="3220mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860241081001"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D13L25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D13L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240478010">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240478010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1552mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240478010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240578010">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240578010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240578010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240678010">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240678010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240678010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240978005">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240978005?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="535.2uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240978005"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241178003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241178003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="430uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241178003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241478004">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241478004?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="496uA"/>
<attribute name="I-RIPPLE" value="632mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241478004"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D18L31.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D18L31.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240681012">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240681012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="2093mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860240681012"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860241081009">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241081009?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1860uA"/>
<attribute name="I-RIPPLE" value="2350mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860241081009"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241181007">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241181007?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="1870mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860241181007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241381006">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241381006?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1188uA"/>
<attribute name="I-RIPPLE" value="1460mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860241381006"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_860241481007">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241481007?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="946uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860241481007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D8L16" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D8L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240374007">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240374007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240374007"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D16L31.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D16L31.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240480011">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240480011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860240480011"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240580011">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240580011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="1932mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860240580011"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D10L16" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D10L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240275008">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240275008?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240275008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240375008">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240375008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="730mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240375008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240475007">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240475007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="580mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240475007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240575007">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240575007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="632mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240575007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240675007">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240675007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240675007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240975001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240975001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="164uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860240975001"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241375002">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241375002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="260uA"/>
<attribute name="I-RIPPLE" value="274mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860241375002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_860241475018">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241475018?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="185uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860241475018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D16L21" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D16L21">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241180004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241180004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="570uA"/>
<attribute name="I-RIPPLE" value="930mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241180004"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241480005">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241480005?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="496uA"/>
<attribute name="I-RIPPLE" value="685mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241480005"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D5L11" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D5L11">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240272001">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240272001?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240272001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240272002">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240272002?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240272002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240372001">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240372001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="115mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240372001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240372002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240372002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240372002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240472001">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240472001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240472001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240472002">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240472002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240472002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240572001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240572001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240572001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240572002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240572002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240572002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240672001">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240672001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240672001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240672002">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240672002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="97mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240672002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D6.3L11" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D6.3L11">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240273003">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240273003?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240273003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240273004">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240273004?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240273004"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240273005">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240273005?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240273005"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240373003">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240373003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240373003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240473003">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240473003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240473003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240573003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240573003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="178mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240573003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240673003">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240673003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860240673003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D10L12.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D10L12.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240275007">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240275007?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860240275007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240475006">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240475006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860240475006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860240575006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240575006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860240575006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240675006">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240675006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="356mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860240675006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860241375001">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241375001?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="208.8uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860241375001"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D18L21" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D18L21">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240981006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240981006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="740uA"/>
<attribute name="I-RIPPLE" value="1310mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860240981006"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241081007">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241081007?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241081007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241181005">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241181005?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="780uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241181005"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241381004">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241381004?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="628uA"/>
<attribute name="I-RIPPLE" value="870mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241381004"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_860241381005">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241381005?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="852uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241381005"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_860241481006">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241481006?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="694uA"/>
<attribute name="I-RIPPLE" value="883mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860241481006"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D18L25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D18L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240981007">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240981007?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1060uA"/>
<attribute name="I-RIPPLE" value="1780mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240981007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860240981008">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240981008?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1508uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240981008"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241081008">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241081008?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1300uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241081008"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241181006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241181006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241181006"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241381008">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241381008?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1412uA"/>
<attribute name="I-RIPPLE" value="1530mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241381008"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D13L20" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D13L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240278009">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240278009?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1540mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240278009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240378009">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240378009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1173mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240378009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240578009">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240578009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1035mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240578009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860240678009">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240678009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="977mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240678009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860240978003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240978003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="311.2uA"/>
<attribute name="I-RIPPLE" value="610mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240978003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860240978004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240978004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="400.8uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860240978004"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
<technology name="_860241078002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241078002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="476uA"/>
<attribute name="I-RIPPLE" value="980mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241078002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241078005">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241078005?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="364uA"/>
<attribute name="I-RIPPLE" value="620mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241078005"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241178002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241178002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="320uA"/>
<attribute name="I-RIPPLE" value="490mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241178002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="250VDC"/>
</technology>
<technology name="_860241378003">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241378003?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="452uA"/>
<attribute name="I-RIPPLE" value="557mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241378003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_860241478002">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241478002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="222.4uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241478002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_860241478003">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241478003?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860241478003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D16L35.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D16L35.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241480001">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241480001?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="1900uA"/>
<attribute name="I-RIPPLE" value="610mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860241480001"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_D16L25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683504v209%20family-wcap-at1h-860240672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AT1H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AT1H&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_D16L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240280010">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240280010?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240280010"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860240380010">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240380010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2093mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240380010"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860240680011">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860240680011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1552mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860240680011"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860241080006">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241080006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="644uA"/>
<attribute name="I-RIPPLE" value="1190mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241080006"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_860241380015">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860241380015?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="852uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860241380015"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
