<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Radial THT - WCAP-ATUL&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-10-28&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATUL_D10L25">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D18L31.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D18L35.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L30">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D6.3L11">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D16L21">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X21X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D10L12.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D16L41">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X41X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D18L25">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D10L16">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L35">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X35X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L40">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X40X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L16">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D18L40">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X40X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D16L25">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D8L20">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X20X3.5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L25">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D16L35.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D18L41">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X41X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D8L16">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D13L20">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D5L11">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D10L20">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D10L30">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D16L31.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D8L11.5">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_D10L30_HORIZONTAL">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATUL_D18L31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D18L31.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040581020">
<attribute name="C" value="2700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040581020?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3850mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040581020"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="2700 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040781018">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781018?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040781018"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040881012">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881012?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040881012"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D6.3L11" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D6.3L11">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040273002">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040273002?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="4000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040273002"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040273003">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040273003?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="4000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040273003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040373002">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040373002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040373002"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040373003">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040373003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040373003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040473003">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040473003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040473003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040573003">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040573003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040573003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040573004">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040573004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040573004"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040673002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040673002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040673002"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040673003">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040673003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040673003"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040773001">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040773001?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040773001"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L30" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278015">
<attribute name="C" value="3900 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278015?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040278015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="3900 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040378016">
<attribute name="C" value="2700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378016?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040378016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2700 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040478014">
<attribute name="C" value="1800 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040478014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1800 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040578015">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040578015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040778013">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778013?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040778013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D16L21" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D16L21">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040580016">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580016?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="PART-NUMBER" value="860040580016"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D18L35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D18L35.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040781020">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781020?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860040781020"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040881013">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881013?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860040881013"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D16L41" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D16L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040780019">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780019?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="2920mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="860040780019"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D10L12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D10L12.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275006">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275006?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040275006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040375007">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040375007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040475006">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="826mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040475006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040575007">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040575007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040675006">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040675006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040775005">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775005?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040775005"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040775006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775006?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040775006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040875002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875002?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value="860040875002"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D18L25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D18L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040381018">
<attribute name="C" value="4700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040381018?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040381018"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040881010">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881010?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1740mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040881010"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D10L16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D10L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275007">
<attribute name="C" value="820 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275007?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="920mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040275007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="820 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040275009">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275009?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1110mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040275009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040475008">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1210mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040475008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040575009">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040575009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040675008">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040675008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040775008">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775008?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040775008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040875003">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875003?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040875003"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D18L40" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D18L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040381001">
<attribute name="C" value="10000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040381001?ae"/>
<attribute name="DF" value="34%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="4290mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PART-NUMBER" value="860040381001"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="10000 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040881015">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881015?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1000uA"/>
<attribute name="I-RIPPLE" value="2580mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PART-NUMBER" value="860040881015"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L35" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040378017">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378017?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="2860mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PART-NUMBER" value="860040378017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040478015">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478015?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2880mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PART-NUMBER" value="860040478015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040578017">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578017?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PART-NUMBER" value="860040578017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D16L25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D16L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040480016">
<attribute name="C" value="2700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040480016?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="2820mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040480016"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="2700 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040580018">
<attribute name="C" value="1800 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580018?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040580018"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1800 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040780014">
<attribute name="C" value="560 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780014?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="352.8uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040780014"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040880007">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880007?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040880007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040378011">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1420mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040378011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L40" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040778015">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778015?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PART-NUMBER" value="860040778015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040878008">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878008?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PART-NUMBER" value="860040878008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278014">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278014?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2120mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040278014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040378014">
<attribute name="C" value="1800 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378014?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="2030mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040378014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1800 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040378015">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378015?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040378015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040478013">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478013?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="2240mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040478013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040578014">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040578014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040678012">
<attribute name="C" value="560 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040678012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="1950mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040678012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040778012">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778012?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040778012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040878017">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878017?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="2220mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040878017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D8L20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D8L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274008">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274008?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040274008"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040374008">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040374008"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040474007">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1020mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040474007"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040574008">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="1180mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040574008"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040674007">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040674007"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040774007">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774007?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040774007"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D16L35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D16L35.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040580019">
<attribute name="C" value="2700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580019?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860040580019"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="2700 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040780017">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780017?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860040780017"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040880011">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880011?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1880mA"/>
<attribute name="LENGTH" value="35.5mm"/>
<attribute name="PART-NUMBER" value="860040880011"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D18L41" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D18L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040581021">
<attribute name="C" value="4700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040581021?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="1645uA"/>
<attribute name="I-RIPPLE" value="5350mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="860040581021"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040781021">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781021?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3200mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="860040781021"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040881014">
<attribute name="C" value="820 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881014?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="820uA"/>
<attribute name="I-RIPPLE" value="2340mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="860040881014"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="820 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D8L16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D8L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274005">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274005?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040274005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040374006">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="780mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040374006"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040474005">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040474005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040574006">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040574006"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040674005">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040674005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040774004">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774004?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040774004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040774029">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774029?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="9000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="990mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="860040774029"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D10L20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D10L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275010">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275010?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040275010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040375009">
<attribute name="C" value="820 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040375009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="820 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040375010">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040375010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040475009">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040475009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040575010">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040575010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040675009">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="135uA"/>
<attribute name="I-RIPPLE" value="1350mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040675009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040775009">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775009?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="113.4uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040775009"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040875004">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875004?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040875004"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D5L11" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D5L11">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040272001">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040272001?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="4000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="215mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040272001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040372001">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040372001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040372001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040472001">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040472001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040472001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040472002">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040472002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040472002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040572001">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040572001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040572001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040572002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040572002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040572002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040672001">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040672001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="860040672001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D10L25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D10L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275011">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275011?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="1550mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040275011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040375012">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375012?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="1560mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040375012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040475010">
<attribute name="C" value="820 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="1580mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040475010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="820 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040575011">
<attribute name="C" value="560 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040575011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040675010">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040675010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040775010">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775010?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040775010"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040875005">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875005?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="860040875005"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D13L20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D13L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278013">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278013?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="8000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040278013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040378013">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378013?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040378013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040478012">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040478012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040578013">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040578013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040778011">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778011?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="170.1uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040778011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040878006">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878006?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value="860040878006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D16L31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D16L31.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040680013">
<attribute name="C" value="1200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040680013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2870mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040680013"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="1200 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040780016">
<attribute name="C" value="820 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780016?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040780016"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="820 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040880009">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880009?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1700mA"/>
<attribute name="LENGTH" value="31.5mm"/>
<attribute name="PART-NUMBER" value="860040880009"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D8L11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D8L11.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274004">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274004?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040274004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040374004">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040374004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040374005">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040374005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_860040474004">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="590mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040474004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040574005">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040574005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040674004">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040674004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_860040774002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774002?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040774002"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040774003">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774003?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="35.28uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040774003"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_860040874001">
<attribute name="C" value="27 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040874001?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="27uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value="860040874001"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="VALUE" value="27 µF"/>
<attribute name="VR" value="100VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_D10L30" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series
&lt;BR&gt;Mounting style: THT Radial
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATUL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_D10L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275012">
<attribute name="C" value="2200 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275012?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="6000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1880mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040275012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_860040475011">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1820mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040475011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_860040575012">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040575012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_860040675011">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="860040675011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
<device name="_HORIZONTAL" package="WCAP-ATUL_D10L30_HORIZONTAL">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_S860040675011">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/S860040675011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="7000h"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="S860040675011"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
