<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Super Capacitors (EDLCs) - WCAP-SISC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-03-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-SISC_D35XH61XP24.3">
<description>&lt;b&gt;WCAP-SISC Supercapacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X61X24.3(Diameter X Length X Pitch), THT, 4pins</description>
</package>
<package name="WCAP-SISC_D22XH46XP10">
<description>&lt;b&gt;WCAP-SISC Supercapacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X46X10(Diameter X Length X Pitch), THT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C-POLAR">
<description>C-POLAR</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-SISC_D35XH61XP24.3" prefix="C">
<description>&lt;b&gt; WCAP-SISC Supercapacitors (EDLCs)
&lt;br&gt;Standard Cylindrical – Snap-In
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Product series with snap-in contacts
&lt;br&gt;Higher energy density than usual capacitors
&lt;br&gt;Mounting style: Radial snap-in
&lt;br&gt;Capacitance range: 100 F, 350 F
&lt;br&gt;Capacitance tolerance: -10 % / +30 %
&lt;br&gt;Rated Voltage: 2.7 V(DC)
&lt;br&gt;Load Life: 500000 Cycles
&lt;br&gt;Operating temperature: -40 °C up to +65 °C
&lt;br&gt;Dimensions (DxL) in mm: 22 x 46 up to 35 x 61
&lt;br&gt;Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy Harvesting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o668222v209%20Family_WCAP-SISC_100F_350F_22x45x10.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o668222v209%20Family_WCAP-SISC_100F_350F_22x45x10.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-SISC"&gt;https://www.we-online.com/catalog/en/WCAP-SISC&lt;/a&gt;&lt;p&gt;

&lt;/a&gt;&lt;p&gt;Created by Ella.Wu 2022-03-23
&lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-SISC_D35XH61XP24.3">
<connects>
<connect gate="G$1" pin="+" pad="1 2 3"/>
<connect gate="G$1" pin="-" pad="4"/>
</connects>
<technologies>
<technology name="_851617034001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/851617034001.pdf"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENERGY-DENSITY" value="5.4Wh/ kg"/>
<attribute name="ILEAK" value="1.5mA"/>
<attribute name="IMAX" value="212A"/>
<attribute name="IRATED" value="75A"/>
<attribute name="LENGTH" value="61mm"/>
<attribute name="LIFE-CYCLE" value="500000 Cycles"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +65 °C"/>
<attribute name="PART-NUMBER" value=" 851617034001 "/>
<attribute name="PITCH" value="24.3mm"/>
<attribute name="POWER-DENSITY" value="8.01kW/ kg"/>
<attribute name="RESR-AC" value="3.2mohm"/>
<attribute name="RESR-DC" value="3.5mohm"/>
<attribute name="VALUE" value="350F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-SISC_D22XH46XP10" prefix="C">
<description>&lt;b&gt; WCAP-SISC Supercapacitors (EDLCs)
&lt;br&gt;Standard Cylindrical – Snap-In
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Product series with snap-in contacts
&lt;br&gt;Higher energy density than usual capacitors
&lt;br&gt;Mounting style: Radial snap-in
&lt;br&gt;Capacitance range: 100 F, 350 F
&lt;br&gt;Capacitance tolerance: -10 % / +30 %
&lt;br&gt;Rated Voltage: 2.7 V(DC)
&lt;br&gt;Load Life: 500000 Cycles
&lt;br&gt;Operating temperature: -40 °C up to +65 °C
&lt;br&gt;Dimensions (DxL) in mm: 22 x 46 up to 35 x 61
&lt;br&gt;Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy Harvesting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o668222v209%20Family_WCAP-SISC_100F_350F_22x45x10.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o668222v209%20Family_WCAP-SISC_100F_350F_22x45x10.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-SISC"&gt;https://www.we-online.com/catalog/en/WCAP-SISC&lt;/a&gt;&lt;p&gt;

&lt;/a&gt;&lt;p&gt;Created by Ella.Wu 2022-03-23
&lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-SISC_D22XH46XP10">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_851617031001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/851617031001.pdf"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENERGY-DENSITY" value="4.8Wh/ kg"/>
<attribute name="ILEAK" value="0.55mA"/>
<attribute name="IMAX" value="61.3A"/>
<attribute name="IRATED" value="21.7A"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="LIFE-CYCLE" value="500000 Cycles"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +65 °C"/>
<attribute name="PART-NUMBER" value=" 851617031001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="POWER-DENSITY" value="7.23kW/ kg"/>
<attribute name="RESR-AC" value="9mohm"/>
<attribute name="RESR-DC" value="12mohm"/>
<attribute name="VALUE" value="100F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
