<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - RF Inductors - WE-AC HC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-ACHC_7449152022">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1212</description>
</package>
<package name="WE-ACHC_7449152111">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1212</description>
</package>
<package name="WE-ACHC_7449152042">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1212</description>
</package>
<package name="WE-ACHC_7449152066">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1212</description>
</package>
<package name="WE-ACHC_7449152090">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1212</description>
</package>
<package name="WE-ACHC_7449150079">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1010</description>
</package>
<package name="WE-ACHC_7449150111">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1010</description>
</package>
<package name="WE-ACHC_7449150046">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1010</description>
</package>
<package name="WE-ACHC_7449150146">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1010</description>
</package>
<package name="WE-ACHC_7449150023">
<description>&lt;B&gt;WE-AC HC High current air coil
&lt;BR&gt;&lt;/B&gt;Size:1010</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-ACHC_1212" prefix="L">
<description>&lt;b&gt;WE-AC HC High current air coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;High quality factor Q
&lt;br&gt;Hight currents
&lt;br&gt;Inductance tolerances +-20 %
&lt;br&gt;Operating temperature: -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;&lt;br&gt;
&lt;br&gt;High power filter
&lt;br&gt;RF-Voltage regulator
&lt;br&gt;High current applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97652v209%20Family_WE-AC_HC_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97652v209%20Family_WE-AC_HC_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-ACHC"&gt;https://katalog.we-online.com/en/pbs/WE-ACHC&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2019-08-19 &lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_7449152111" package="WE-ACHC_7449152111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449152111.pdf"/>
<attribute name="FRES" value="345Mhz"/>
<attribute name="IR" value="32A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449152111 "/>
<attribute name="Q-FACTOR" value=" 211 "/>
<attribute name="RDC" value="1.43mOhm"/>
<attribute name="VALUE" value="117nH"/>
</technology>
</technologies>
</device>
<device name="_7449152022" package="WE-ACHC_7449152022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449152022.pdf"/>
<attribute name="FRES" value="867Mhz"/>
<attribute name="IR" value="40A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449152022 "/>
<attribute name="Q-FACTOR" value=" 280 "/>
<attribute name="RDC" value="0.55mOhm"/>
<attribute name="VALUE" value="22nH"/>
</technology>
</technologies>
</device>
<device name="_7449152042" package="WE-ACHC_7449152042">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449152042.pdf"/>
<attribute name="FRES" value="605Mhz"/>
<attribute name="IR" value="34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449152042 "/>
<attribute name="Q-FACTOR" value=" 240 "/>
<attribute name="RDC" value="0.77mOhm"/>
<attribute name="VALUE" value="42nH"/>
</technology>
</technologies>
</device>
<device name="_7449152066" package="WE-ACHC_7449152066">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449152066.pdf"/>
<attribute name="FRES" value="457Mhz"/>
<attribute name="IR" value="32A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449152066 "/>
<attribute name="Q-FACTOR" value=" 245 "/>
<attribute name="RDC" value="0.99mOhm"/>
<attribute name="VALUE" value="66nH"/>
</technology>
</technologies>
</device>
<device name="_7449152090" package="WE-ACHC_7449152090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449152090.pdf"/>
<attribute name="FRES" value="359Mhz"/>
<attribute name="IR" value="30A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449152090 "/>
<attribute name="Q-FACTOR" value=" 226 "/>
<attribute name="RDC" value="1.21mOhm"/>
<attribute name="VALUE" value="90nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ACHC_1010" prefix="L">
<description>&lt;b&gt;WE-AC HC High current air coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;High quality factor Q
&lt;br&gt;Hight currents
&lt;br&gt;Inductance tolerances +-20 %
&lt;br&gt;Operating temperature: -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;&lt;br&gt;
&lt;br&gt;High power filter
&lt;br&gt;RF-Voltage regulator
&lt;br&gt;High current applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97652v209%20Family_WE-AC_HC_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97652v209%20Family_WE-AC_HC_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-ACHC"&gt;https://katalog.we-online.com/en/pbs/WE-ACHC&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2019-08-19 &lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_7449150023" package="WE-ACHC_7449150023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449150023.pdf"/>
<attribute name="FRES" value="867Mhz"/>
<attribute name="IR" value="30A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449150023 "/>
<attribute name="Q-FACTOR" value=" 191 "/>
<attribute name="RDC" value="1.2mOhm"/>
<attribute name="VALUE" value="23nH"/>
</technology>
</technologies>
</device>
<device name="_7449150046" package="WE-ACHC_7449150046">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449150046.pdf"/>
<attribute name="FRES" value="581Mhz"/>
<attribute name="IR" value="28A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449150046 "/>
<attribute name="Q-FACTOR" value=" 223 "/>
<attribute name="RDC" value="1.62mOhm"/>
<attribute name="VALUE" value="46.5nH"/>
</technology>
</technologies>
</device>
<device name="_7449150079" package="WE-ACHC_7449150079">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449150079.pdf"/>
<attribute name="FRES" value="422Mhz"/>
<attribute name="IR" value="23A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449150079 "/>
<attribute name="Q-FACTOR" value=" 184 "/>
<attribute name="RDC" value="2.11mOhm"/>
<attribute name="VALUE" value="79nH"/>
</technology>
</technologies>
</device>
<device name="_7449150111" package="WE-ACHC_7449150111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449150111.pdf"/>
<attribute name="FRES" value="374Mhz"/>
<attribute name="IR" value="22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449150111 "/>
<attribute name="Q-FACTOR" value=" 186 "/>
<attribute name="RDC" value="2.11mOhm"/>
<attribute name="VALUE" value="111nH"/>
</technology>
</technologies>
</device>
<device name="_7449150146" package="WE-ACHC_7449150146">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7449150146.pdf"/>
<attribute name="FRES" value="332Mhz"/>
<attribute name="IR" value="19A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7449150146 "/>
<attribute name="Q-FACTOR" value=" 163 "/>
<attribute name="RDC" value="3.33mOhm"/>
<attribute name="VALUE" value="146nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
