<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Power Transformer - WE-AGDA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-05-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-AGDA_EP7">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: EP7, SMT, 8pins
&lt;br&gt;LXWXH=11.3X109.5X11.94mm</description>
</package>
</packages>
<symbols>
<symbol name="789318208">
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="789317893">
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="789318616">
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="789318207">
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="789318114">
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="789317894">
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="789318131">
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="789317893" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789317893"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="6.8 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789317893?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="1.95 A"/>
<attribute name="L" value="18 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value="789317893"/>
<attribute name="PO" value="3 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="9 - 18 Vin, 19 Vout"/>
<attribute name="VIN" value="9 - 18 V"/>
<attribute name="VOUT1" value="19 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789318208" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789318208"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="7 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789318208?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="1.5 A"/>
<attribute name="L" value="27 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.5:3.5:1"/>
<attribute name="PART-NUMBER" value="789318208"/>
<attribute name="PO" value="5 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="18 - 36 Vin, 15 Vout"/>
<attribute name="VIN" value="18 - 36 V"/>
<attribute name="VOUT1" value="15 V"/>
<attribute name="VOUT2" value="-4 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789318616" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789318616"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="3.25 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789318616?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="1.85 A"/>
<attribute name="L" value="10 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.2:2:1"/>
<attribute name="PART-NUMBER" value="789318616"/>
<attribute name="PO" value="2.7 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="7 - 31 Vin, 27 Vout"/>
<attribute name="VAUX" value="13 V"/>
<attribute name="VIN" value="7 - 31 V"/>
<attribute name="VOUT1" value="27 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789318207" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789318207"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="8.2 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789318207?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="2 A"/>
<attribute name="L" value="27 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.2"/>
<attribute name="PART-NUMBER" value="789318207"/>
<attribute name="PO" value="5 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="18 - 36 Vin, 19 Vout"/>
<attribute name="VIN" value="18 - 36 V"/>
<attribute name="VOUT1" value="19 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789318114" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789318114"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="6.8 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789318114?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="6.2 A"/>
<attribute name="L" value="6 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value="789318114"/>
<attribute name="PO" value="6 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="9 - 18 Vin, 19 Vout"/>
<attribute name="VIN" value="9 - 18 V"/>
<attribute name="VOUT1" value="19 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789317894" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789317894"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="7 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789317894?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="1.6 A"/>
<attribute name="L" value="18 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.25:3.5:1"/>
<attribute name="PART-NUMBER" value="789317894"/>
<attribute name="PO" value="3 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="9 - 18 Vin, 15 Vout"/>
<attribute name="VIN" value="9 - 18 V"/>
<attribute name="VOUT1" value="15 V"/>
<attribute name="VOUT2" value="-4 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="789318131" prefix="T">
<description>&lt;b&gt;WE-AGDA Auxiliary Gate Drive Transformer Automotive&lt;br&gt;
&lt;/b&gt;for SiC-MOSFET and IGBT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Interwinding capacitance down to &lt;3 pF
&lt;br&gt;Tiny surface mount EP7 package
&lt;br&gt;Dielectric insulation up to 4 kV AC
&lt;br&gt;Basic insulation for 568 Vrms / 800 Vpk
&lt;br&gt;AEC-Q200 qualification
&lt;br&gt;Common control voltages for SiC MOSFET’s
&lt;br&gt;Up to 6 W output power
&lt;br&gt;Wide range input voltages 7 V to 36 V
&lt;br&gt;Different unipolar and bipolar voltages available
&lt;br&gt;Operating temperature: -40 °C up to +130 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Motor inverters
&lt;br&gt;OBCs
&lt;br&gt;Active power factor correction
&lt;br&gt;Flyback, LLC, Half- and Full Bridge topologies
&lt;br&gt;SiC-MOSFET based power converter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o893879v209%20multi-78931xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-AGDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-AGDA&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-05-12 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="789318131"/>
</gates>
<devices>
<device name="" package="WE-AGDA_EP7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="7.5 pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/789318131?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="11.94mm"/>
<attribute name="ISAT" value="5 A"/>
<attribute name="L" value="7 uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.25:3.5:1"/>
<attribute name="PART-NUMBER" value="789318131"/>
<attribute name="PO" value="6 W"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="9 - 18 Vin, 15 Vout"/>
<attribute name="VIN" value="9 - 18 V"/>
<attribute name="VOUT1" value="15 V"/>
<attribute name="VOUT2" value="-4 V"/>
<attribute name="WIDTH" value="10.95mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
