<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - AS-Interace Inductors - WE-ASI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2019-05-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-ASI_L">
<description>&lt;b&gt;WE-ASI SMD Wire Wound Inductor&lt;/b&gt;&lt;p&gt;
Size : L</description>
</package>
<package name="WE-ASI_M">
<description>&lt;b&gt;WE-ASI SMD Wire Wound Inductor&lt;/b&gt;&lt;p&gt;
Size : M</description>
</package>
<package name="WE-ASI_SENSOR">
<description>&lt;b&gt;WE-ASI SMD Wire Wound Inductor&lt;/b&gt;&lt;p&gt;
Size : Sensor</description>
</package>
</packages>
<symbols>
<symbol name="WE-ASI">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-ASI_M" prefix="L">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Specially designed for sensors and actuators
&lt;br&gt;Highest possible current in the smallest case size
&lt;br&gt;High self resonant frequency
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-ASI"&gt;https://katalog.we-online.com/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2020-05-29&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-ASI"/>
</gates>
<devices>
<device name="" package="WE-ASI_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744776333">
<attribute name="C" value="10  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744776333.pdf"/>
<attribute name="FRES" value="900Mhz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776333 "/>
<attribute name="RDC" value="0.02Ohm"/>
<attribute name="RDC-MAX" value="7Ohm"/>
<attribute name="RDC-TYP" value="5.6Ohm"/>
<attribute name="VALUE" value="3mH"/>
</technology>
<technology name="_744776347">
<attribute name="C" value="13  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744776347.pdf"/>
<attribute name="FRES" value="650Mhz"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776347 "/>
<attribute name="RDC" value="0.015Ohm"/>
<attribute name="RDC-MAX" value="12Ohm"/>
<attribute name="RDC-TYP" value="11.5Ohm"/>
<attribute name="VALUE" value="4.7mH"/>
</technology>
<technology name="_744776360">
<attribute name="C" value="13  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744776360.pdf"/>
<attribute name="FRES" value="570Mhz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.27A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776360 "/>
<attribute name="RDC" value="0.015Ohm"/>
<attribute name="RDC-MAX" value="14Ohm"/>
<attribute name="RDC-TYP" value="14Ohm"/>
<attribute name="VALUE" value="6mH"/>
</technology>
<technology name="_744776381">
<attribute name="C" value="13  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744776381.pdf"/>
<attribute name="FRES" value="500Mhz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744776381 "/>
<attribute name="RDC" value="0.03Ohm"/>
<attribute name="RDC-MAX" value="16Ohm"/>
<attribute name="RDC-TYP" value="15.4Ohm"/>
<attribute name="VALUE" value="8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ASI_L" prefix="L">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Specially designed for sensors and actuators
&lt;br&gt;Highest possible current in the smallest case size
&lt;br&gt;High self resonant frequency
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-ASI"&gt;https://katalog.we-online.com/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2020-05-29&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-ASI"/>
</gates>
<devices>
<device name="" package="WE-ASI_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74458303">
<attribute name="C" value="21  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74458303.pdf"/>
<attribute name="FRES" value="630Mhz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74458303 "/>
<attribute name="RDC" value="0.045Ohm"/>
<attribute name="RDC-MAX" value="3.5Ohm"/>
<attribute name="RDC-TYP" value="2.9Ohm"/>
<attribute name="VALUE" value="3mH"/>
</technology>
<technology name="_74458304">
<attribute name="C" value="22  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74458304.pdf"/>
<attribute name="FRES" value="500Mhz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74458304 "/>
<attribute name="RDC" value="0.015Ohm"/>
<attribute name="RDC-MAX" value="4.8Ohm"/>
<attribute name="RDC-TYP" value="4Ohm"/>
<attribute name="VALUE" value="4.7mH"/>
</technology>
<technology name="_74458306">
<attribute name="C" value="20  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74458306.pdf"/>
<attribute name="FRES" value="470Mhz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74458306 "/>
<attribute name="RDC" value="0.04Ohm"/>
<attribute name="RDC-MAX" value="6Ohm"/>
<attribute name="RDC-TYP" value="5.2Ohm"/>
<attribute name="VALUE" value="6mH"/>
</technology>
<technology name="_74458308">
<attribute name="C" value="19  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74458308.pdf"/>
<attribute name="FRES" value="410Mhz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74458308 "/>
<attribute name="RDC" value="0.045Ohm"/>
<attribute name="RDC-MAX" value="8Ohm"/>
<attribute name="RDC-TYP" value="6.8Ohm"/>
<attribute name="VALUE" value="8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ASI_SENSOR" prefix="L">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Specially designed for sensors and actuators
&lt;br&gt;Highest possible current in the smallest case size
&lt;br&gt;High self resonant frequency
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14747v209%20Family_WE-ASI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-ASI"&gt;https://katalog.we-online.com/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2020-05-29&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-ASI"/>
</gates>
<devices>
<device name="" package="WE-ASI_SENSOR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744775318">
<attribute name="C" value="9  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744775318.pdf"/>
<attribute name="FRES" value="400Mhz"/>
<attribute name="IR" value="0.08A"/>
<attribute name="ISAT" value="0.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775318 "/>
<attribute name="RDC" value="0.02Ohm"/>
<attribute name="RDC-MAX" value="72Ohm"/>
<attribute name="RDC-TYP" value="57.7Ohm"/>
<attribute name="VALUE" value="18mH"/>
</technology>
<technology name="_744775330">
<attribute name="C" value="10  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744775330.pdf"/>
<attribute name="FRES" value="900Mhz"/>
<attribute name="IR" value="0.24A"/>
<attribute name="ISAT" value="0.12A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775330 "/>
<attribute name="RDC" value="0.01Ohm"/>
<attribute name="RDC-MAX" value="10Ohm"/>
<attribute name="RDC-TYP" value="8.2Ohm"/>
<attribute name="VALUE" value="3mH"/>
</technology>
<technology name="_744775347">
<attribute name="C" value="11  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744775347.pdf"/>
<attribute name="FRES" value="700Mhz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775347 "/>
<attribute name="RDC" value="0.02Ohm"/>
<attribute name="RDC-MAX" value="13.8Ohm"/>
<attribute name="RDC-TYP" value="11.5Ohm"/>
<attribute name="VALUE" value="4.7mH"/>
</technology>
<technology name="_744775360">
<attribute name="C" value="12  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744775360.pdf"/>
<attribute name="FRES" value="600Mhz"/>
<attribute name="IR" value="0.18A"/>
<attribute name="ISAT" value="0.09A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775360 "/>
<attribute name="RDC" value="0.03Ohm"/>
<attribute name="RDC-MAX" value="18Ohm"/>
<attribute name="RDC-TYP" value="16.7Ohm"/>
<attribute name="VALUE" value="6mH"/>
</technology>
<technology name="_744775380">
<attribute name="C" value="11  pF "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744775380.pdf"/>
<attribute name="FRES" value="700Mhz"/>
<attribute name="IR" value="0.14A"/>
<attribute name="ISAT" value="0.09A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744775380 "/>
<attribute name="RDC" value="0.025Ohm"/>
<attribute name="RDC-MAX" value="25Ohm"/>
<attribute name="RDC-TYP" value="23.3Ohm"/>
<attribute name="VALUE" value="8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
