<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - RF Inductors - WE-CAIR&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CAIR_1322">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 1322</description>
</package>
<package name="WE-CAIR_5910">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 5910</description>
</package>
<package name="WE-CAIR_3168">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 3168</description>
</package>
<package name="WE-CAIR_3136">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 3136</description>
</package>
<package name="WE-CAIR_1340">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 1340</description>
</package>
<package name="WE-CAIR_4248">
<description>&lt;b&gt;WE-CAIR Air coil
&lt;/b&gt;&lt;br&gt;Size: 4248</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CAIR_5910" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_5910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744918190">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918190.pdf"/>
<attribute name="FRES" value="1140GHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918190 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="90nH"/>
</technology>
<technology name="_744918211">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918211.pdf"/>
<attribute name="FRES" value="1020GHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918211 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="111nH"/>
</technology>
<technology name="_744918213">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918213.pdf"/>
<attribute name="FRES" value="900GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918213 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="130nH"/>
</technology>
<technology name="_744918217">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918217.pdf"/>
<attribute name="FRES" value="875GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918217 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="VALUE" value="169nH"/>
</technology>
<technology name="_744918220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918220.pdf"/>
<attribute name="FRES" value="800GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918220 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="206nH"/>
</technology>
<technology name="_744918222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918222.pdf"/>
<attribute name="FRES" value="730GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918222 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="222nH"/>
</technology>
<technology name="_744918224">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918224.pdf"/>
<attribute name="FRES" value="685GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918224 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="246nH"/>
</technology>
<technology name="_744918230">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918230.pdf"/>
<attribute name="FRES" value="660GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918230 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="307nH"/>
</technology>
<technology name="_744918238">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918238.pdf"/>
<attribute name="FRES" value="590GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918238 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="380nH"/>
</technology>
<technology name="_744918242">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918242.pdf"/>
<attribute name="FRES" value="540GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918242 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="422nH"/>
</technology>
<technology name="_744918249">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918249.pdf"/>
<attribute name="FRES" value="535GHz"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918249 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="65mOhm"/>
<attribute name="VALUE" value="491nH"/>
</technology>
<technology name="_744918254">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744918254.pdf"/>
<attribute name="FRES" value="490GHz"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744918254 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="VALUE" value="538nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_3136" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_3136">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744913025">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913025.pdf"/>
<attribute name="FRES" value="12.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744913025 "/>
<attribute name="Q-FACTOR" value=" 140 "/>
<attribute name="RDC" value="1.1mOhm"/>
<attribute name="VALUE" value="2.5nH"/>
</technology>
<technology name="_744913050">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913050.pdf"/>
<attribute name="FRES" value="6.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744913050 "/>
<attribute name="Q-FACTOR" value=" 140 "/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="VALUE" value="5nH"/>
</technology>
<technology name="_744913050G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913050G.pdf"/>
<attribute name="FRES" value="6.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744913050G"/>
<attribute name="Q-FACTOR" value=" 140 "/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="VALUE" value="5nH"/>
</technology>
<technology name="_744913080">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913080.pdf"/>
<attribute name="FRES" value="5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744913080 "/>
<attribute name="Q-FACTOR" value=" 140 "/>
<attribute name="RDC" value="2.6mOhm"/>
<attribute name="VALUE" value="8nH"/>
</technology>
<technology name="_744913080G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913080G.pdf"/>
<attribute name="FRES" value="5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744913080G"/>
<attribute name="Q-FACTOR" value=" 140 "/>
<attribute name="RDC" value="2.6mOhm"/>
<attribute name="VALUE" value="8nH"/>
</technology>
<technology name="_744913112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913112.pdf"/>
<attribute name="FRES" value="3.3GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744913112 "/>
<attribute name="Q-FACTOR" value=" 137 "/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="VALUE" value="12.5nH"/>
</technology>
<technology name="_744913112G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913112G.pdf"/>
<attribute name="FRES" value="3.3GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744913112G"/>
<attribute name="Q-FACTOR" value=" 137 "/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="VALUE" value="12.5nH"/>
</technology>
<technology name="_744913118">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913118.pdf"/>
<attribute name="FRES" value="2.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744913118 "/>
<attribute name="Q-FACTOR" value=" 132 "/>
<attribute name="RDC" value="3.9mOhm"/>
<attribute name="VALUE" value="18.5nH"/>
</technology>
<technology name="_744913118G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744913118G.pdf"/>
<attribute name="FRES" value="2.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744913118G"/>
<attribute name="Q-FACTOR" value=" 132 "/>
<attribute name="RDC" value="3.9mOhm"/>
<attribute name="VALUE" value="18.5nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_1322" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_1322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744910016">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744910016.pdf"/>
<attribute name="FRES" value="10GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744910016 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4mOhm"/>
<attribute name="VALUE" value="1.65nH"/>
</technology>
<technology name="_744910025">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744910025.pdf"/>
<attribute name="FRES" value="8.2GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744910025 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="5mOhm"/>
<attribute name="VALUE" value="2.55nH"/>
</technology>
<technology name="_744910038">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744910038.pdf"/>
<attribute name="FRES" value="7.5GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744910038 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="6mOhm"/>
<attribute name="VALUE" value="3.85nH"/>
</technology>
<technology name="_744910054">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744910054.pdf"/>
<attribute name="FRES" value="7GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744910054 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="8mOhm"/>
<attribute name="VALUE" value="5.45nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_1340" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_1340">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744911056">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744911056.pdf"/>
<attribute name="FRES" value="6.5GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744911056 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="VALUE" value="5.6nH"/>
</technology>
<technology name="_744911071">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744911071.pdf"/>
<attribute name="FRES" value="6GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744911071 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="7.15nH"/>
</technology>
<technology name="_744911088">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744911088.pdf"/>
<attribute name="FRES" value="6GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744911088 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="12mOhm"/>
<attribute name="VALUE" value="8.8nH"/>
</technology>
<technology name="_744911098">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744911098.pdf"/>
<attribute name="FRES" value="5.2GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744911098 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="VALUE" value="9.85nH"/>
</technology>
<technology name="_744911112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744911112.pdf"/>
<attribute name="FRES" value="4.6GHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744911112 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="14mOhm"/>
<attribute name="VALUE" value="12.55nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_4248" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_4248">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744912122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912122.pdf"/>
<attribute name="FRES" value="3.2GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912122 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.2mOhm"/>
<attribute name="VALUE" value="22nH"/>
</technology>
<technology name="_744912122G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912122G.pdf"/>
<attribute name="FRES" value="3.2GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912122G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.2mOhm"/>
<attribute name="VALUE" value="22nH"/>
</technology>
<technology name="_744912127">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912127.pdf"/>
<attribute name="FRES" value="2.7GHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912127 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4mOhm"/>
<attribute name="VALUE" value="27nH"/>
</technology>
<technology name="_744912127G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912127G.pdf"/>
<attribute name="FRES" value="2.7GHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912127G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4mOhm"/>
<attribute name="VALUE" value="27nH"/>
</technology>
<technology name="_744912133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912133.pdf"/>
<attribute name="FRES" value="2.5GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912133 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.8mOhm"/>
<attribute name="VALUE" value="33nH"/>
</technology>
<technology name="_744912133G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912133G.pdf"/>
<attribute name="FRES" value="2.5GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912133G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.8mOhm"/>
<attribute name="VALUE" value="33nH"/>
</technology>
<technology name="_744912139">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912139.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912139 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.4mOhm"/>
<attribute name="VALUE" value="39nH"/>
</technology>
<technology name="_744912139G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912139G.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912139G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.4mOhm"/>
<attribute name="VALUE" value="39nH"/>
</technology>
<technology name="_744912147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912147.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912147 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="5.6mOhm"/>
<attribute name="VALUE" value="47nH"/>
</technology>
<technology name="_744912147G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912147G.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912147G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="5.6mOhm"/>
<attribute name="VALUE" value="47nH"/>
</technology>
<technology name="_744912156">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912156.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912156 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="6.2mOhm"/>
<attribute name="VALUE" value="56nH"/>
</technology>
<technology name="_744912156G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912156G.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912156G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="6.2mOhm"/>
<attribute name="VALUE" value="56nH"/>
</technology>
<technology name="_744912168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912168.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912168 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="8.2mOhm"/>
<attribute name="VALUE" value="68nH"/>
</technology>
<technology name="_744912168G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912168G.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912168G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="8.2mOhm"/>
<attribute name="VALUE" value="68nH"/>
</technology>
<technology name="_744912182">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912182.pdf"/>
<attribute name="FRES" value="1.3GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912182 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="9.4mOhm"/>
<attribute name="VALUE" value="82nH"/>
</technology>
<technology name="_744912182G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912182G.pdf"/>
<attribute name="FRES" value="1.3GHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912182G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="9.4mOhm"/>
<attribute name="VALUE" value="82nH"/>
</technology>
<technology name="_744912210">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912210.pdf"/>
<attribute name="FRES" value="1.2GHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912210 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="12.3mOhm"/>
<attribute name="VALUE" value="100nH"/>
</technology>
<technology name="_744912210G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912210G.pdf"/>
<attribute name="FRES" value="1.2GHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912210G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="12.3mOhm"/>
<attribute name="VALUE" value="100nH"/>
</technology>
<technology name="_744912212">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912212.pdf"/>
<attribute name="FRES" value="1.1GHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744912212 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="17.3mOhm"/>
<attribute name="VALUE" value="120nH"/>
</technology>
<technology name="_744912212G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744912212G.pdf"/>
<attribute name="FRES" value="1.1GHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744912212G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="17.3mOhm"/>
<attribute name="VALUE" value="120nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_3168" prefix="L">
<description>&lt;B&gt;WE-CAIR Air coil
&lt;BR&gt;
&lt;BR&gt;Characteristics
&lt;BR&gt;
&lt;BR&gt;
&lt;/B&gt;Inductance values from 1.65 nH up to 120 nH
&lt;BR&gt;Very high quality factor &gt;100
&lt;BR&gt;High self-resonant frequency
&lt;BR&gt;Hight currents up to 3.5 A
&lt;BR&gt;Inductance tolerances 5% and 10%
&lt;BR&gt;Pick and place-process possible
&lt;BR&gt;Good solderability (tinned connector pins)
&lt;BR&gt;Operating temperature: -40°C to +125°C
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Applications &lt;BR&gt;
&lt;BR&gt;&lt;/B&gt;Especially for RF applications
&lt;BR&gt;Ideal for high current applications
&lt;BR&gt;Broad band filter
&lt;BR&gt;RF-Decoupling
&lt;BR&gt;&lt;BR&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14750v209%20Family_WE-CAIR_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-CAIR"&gt;https://katalog.we-online.com/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-19&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_3168">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744914117">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914117.pdf"/>
<attribute name="FRES" value="2.2GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744914117 "/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.5mOhm"/>
<attribute name="VALUE" value="17.5nH"/>
</technology>
<technology name="_744914117G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914117G.pdf"/>
<attribute name="FRES" value="2.2GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744914117G"/>
<attribute name="Q-FACTOR" value=" 100 "/>
<attribute name="RDC" value="4.5mOhm"/>
<attribute name="VALUE" value="17.5nH"/>
</technology>
<technology name="_744914122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914122.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744914122 "/>
<attribute name="Q-FACTOR" value=" 102 "/>
<attribute name="RDC" value="5.2mOhm"/>
<attribute name="VALUE" value="22nH"/>
</technology>
<technology name="_744914122G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914122G.pdf"/>
<attribute name="FRES" value="2.1GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744914122G"/>
<attribute name="Q-FACTOR" value=" 102 "/>
<attribute name="RDC" value="5.2mOhm"/>
<attribute name="VALUE" value="22nH"/>
</technology>
<technology name="_744914128">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914128.pdf"/>
<attribute name="FRES" value="1.8GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744914128 "/>
<attribute name="Q-FACTOR" value=" 105 "/>
<attribute name="RDC" value="6mOhm"/>
<attribute name="VALUE" value="28nH"/>
</technology>
<technology name="_744914128G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914128G.pdf"/>
<attribute name="FRES" value="1.8GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744914128G"/>
<attribute name="Q-FACTOR" value=" 105 "/>
<attribute name="RDC" value="6mOhm"/>
<attribute name="VALUE" value="28nH"/>
</technology>
<technology name="_744914135">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914135.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744914135 "/>
<attribute name="Q-FACTOR" value=" 112 "/>
<attribute name="RDC" value="6.8mOhm"/>
<attribute name="VALUE" value="35.5nH"/>
</technology>
<technology name="_744914135G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914135G.pdf"/>
<attribute name="FRES" value="1.5GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744914135G"/>
<attribute name="Q-FACTOR" value=" 112 "/>
<attribute name="RDC" value="6.8mOhm"/>
<attribute name="VALUE" value="35.5nH"/>
</technology>
<technology name="_744914143">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914143.pdf"/>
<attribute name="FRES" value="1.2GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744914143 "/>
<attribute name="Q-FACTOR" value=" 106 "/>
<attribute name="RDC" value="7.9mOhm"/>
<attribute name="VALUE" value="43nH"/>
</technology>
<technology name="_744914143G">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744914143G.pdf"/>
<attribute name="FRES" value="1.2GHz"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744914143G"/>
<attribute name="Q-FACTOR" value=" 106 "/>
<attribute name="RDC" value="7.9mOhm"/>
<attribute name="VALUE" value="43nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
