<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-CHSA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-04-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CHSA_1212P">
<description>&lt;B&gt;WE-CHSA Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1212, SMT, 2pins
&lt;BR&gt;L X W X H = 12.2mm X 12.2mm X 11.75mm</description>
</package>
<package name="WE-CHSA_1011">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1011, SMT, 2pins
&lt;BR&gt;L X W X H = 10.6mm X 10.6mm X 11mm</description>
</package>
<package name="WE-CHSA_8090P">
<description>&lt;B&gt;WE-CHSA Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 8090, SMT, 2pins
&lt;BR&gt;L X W X H = 8.1mm X 8.1mm X 9mm</description>
</package>
<package name="WE-CHSA_8090">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 8090, SMT, 2pins
&lt;BR&gt;L X W X H = 8.1mm X 8.1mm X 9mm</description>
</package>
<package name="WE-CHSA_1212">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1212, SMT, 2pins
&lt;BR&gt;L X W X H = 12.2mm X 12.2mm X 11.75mm</description>
</package>
<package name="WE-CHSA_1011P">
<description>&lt;B&gt;WE-CHSA Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1011, SMT, 2pins
&lt;BR&gt;L X W X H = 10.6mm X 10.6mm X 11mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CHSA_1212P" prefix="L">
<description>&lt;b&gt;WE-CHSA Performance SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Saturation current up to 48.5 A
&lt;br&gt;Iron alloy core leads to soft saturation
&lt;br&gt;AEC-Q200
&lt;br&gt;Excellent coplanarity due to the plastic base
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA-/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA-&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04--03&lt;br&gt;
2026 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1212P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433290200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290200?ae"/>
<attribute name="FRES" value="64 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="16.2 A"/>
<attribute name="ISAT" value="29 A"/>
<attribute name="L" value="2 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290200 "/>
<attribute name="RDC-MAX" value="4.7 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="2 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290240?ae"/>
<attribute name="FRES" value="60 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="13.8 A"/>
<attribute name="ISAT" value="24.8 A"/>
<attribute name="L" value="2.4 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290240 "/>
<attribute name="RDC-MAX" value="6.4 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="2.4 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290360">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290360?ae"/>
<attribute name="FRES" value="48 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="12.2 A"/>
<attribute name="ISAT" value="20.6 A"/>
<attribute name="L" value="3.6 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290360 "/>
<attribute name="RDC-MAX" value="8.2 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="3.6 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290510?ae"/>
<attribute name="FRES" value="40 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="9.8 A"/>
<attribute name="ISAT" value="17 A"/>
<attribute name="L" value="5.1 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290510 "/>
<attribute name="RDC-MAX" value="11.9 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="5.1 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290620">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290620?ae"/>
<attribute name="FRES" value="37 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="8.8 A"/>
<attribute name="ISAT" value="16 A"/>
<attribute name="L" value="6.2 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290620 "/>
<attribute name="RDC-MAX" value="15 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="6.2 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290750">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290750?ae"/>
<attribute name="FRES" value="34 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="7.8 A"/>
<attribute name="ISAT" value="14.6 A"/>
<attribute name="L" value="7.5 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290750 "/>
<attribute name="RDC-MAX" value="20.35 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="7.5 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433290820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433290820?ae"/>
<attribute name="FRES" value="32 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="7.1 A"/>
<attribute name="ISAT" value="13.7 A"/>
<attribute name="L" value="8.2 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433290820 "/>
<attribute name="RDC-MAX" value="21.5 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_78433291500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433291500?ae"/>
<attribute name="FRES" value="23 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="5.4 A"/>
<attribute name="ISAT" value="9.8 A"/>
<attribute name="L" value="15 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433291500 "/>
<attribute name="RDC-MAX" value="43.1 mohm"/>
<attribute name="SIZE" value="1212P"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_1011" prefix="L">
<description>&lt;b&gt;WE-CHSA SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt; Operating temperature: -55°C to +150°C
&lt;BR&gt; Current capability up to 28A
&lt;BR&gt; Ideal coplanarity due to embedded solder pads
&lt;BR&gt; Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04-03&lt;br&gt;
2026 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843330033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330033?ae"/>
<attribute name="FRES" value="230 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="26 A"/>
<attribute name="ISAT" value="54.5 A"/>
<attribute name="L" value="0.33 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330033"/>
<attribute name="RDC-MAX" value="1.7 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330056?ae"/>
<attribute name="FRES" value="100 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="23.5 A"/>
<attribute name="ISAT" value="43.4 A"/>
<attribute name="L" value="0.56 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330056"/>
<attribute name="RDC-MAX" value="2.05 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330100?ae"/>
<attribute name="FRES" value="88 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="20.3 A"/>
<attribute name="ISAT" value="34.8 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330100"/>
<attribute name="RDC-MAX" value="2.9 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330180?ae"/>
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="16 A"/>
<attribute name="ISAT" value="25.9 A"/>
<attribute name="L" value="1.8 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330180"/>
<attribute name="RDC-MAX" value="4.7 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330330?ae"/>
<attribute name="FRES" value="55 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="13.8 A"/>
<attribute name="ISAT" value="20.5 A"/>
<attribute name="L" value="3.3 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330330"/>
<attribute name="RDC-MAX" value="6.5 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330390?ae"/>
<attribute name="FRES" value="50 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="11.2 A"/>
<attribute name="ISAT" value="17.8 A"/>
<attribute name="L" value="3.9 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330390"/>
<attribute name="RDC-MAX" value="8.7 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="3.9 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330560?ae"/>
<attribute name="FRES" value="41 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="9.2 A"/>
<attribute name="ISAT" value="14.9 A"/>
<attribute name="L" value="5.6 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330560"/>
<attribute name="RDC-MAX" value="13 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843330820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843330820?ae"/>
<attribute name="FRES" value="34 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="7.2 A"/>
<attribute name="ISAT" value="12.8 A"/>
<attribute name="L" value="8.2 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843330820"/>
<attribute name="RDC-MAX" value="19.1 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843331000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843331000?ae"/>
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="6.7 A"/>
<attribute name="ISAT" value="10.7 A"/>
<attribute name="L" value="10 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843331000"/>
<attribute name="RDC-MAX" value="25.8 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843331200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843331200?ae"/>
<attribute name="FRES" value="28 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="5.6 A"/>
<attribute name="ISAT" value="9.1 A"/>
<attribute name="L" value="12 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843331200"/>
<attribute name="RDC-MAX" value="33.2 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843331800">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843331800?ae"/>
<attribute name="FRES" value="23 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="5.1 A"/>
<attribute name="ISAT" value="8.5 A"/>
<attribute name="L" value="18 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843331800"/>
<attribute name="RDC-MAX" value="41.1 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_7843332000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843332000?ae"/>
<attribute name="FRES" value="20 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="4.3 A"/>
<attribute name="ISAT" value="7 A"/>
<attribute name="L" value="20 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843332000"/>
<attribute name="RDC-MAX" value="60.9 mohm"/>
<attribute name="SIZE" value=" 1011 "/>
<attribute name="VALUE" value="20 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_8090P" prefix="L">
<description>&lt;b&gt;WE-CHSA Performance SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Saturation current up to 48.5 A
&lt;br&gt;Iron alloy core leads to soft saturation
&lt;br&gt;AEC-Q200
&lt;br&gt;Excellent coplanarity due to the plastic base
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA-/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA-&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04--03&lt;br&gt;
2026 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_8090P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433490036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490036?ae"/>
<attribute name="FRES" value="218 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="19 A"/>
<attribute name="ISAT" value="48.5 A"/>
<attribute name="L" value="0.36 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490036 "/>
<attribute name="RDC-MAX" value="2.8 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="0.36 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_78433490056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490056?ae"/>
<attribute name="FRES" value="184 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="15.6 A"/>
<attribute name="ISAT" value="40.5 A"/>
<attribute name="L" value="0.56 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490056 "/>
<attribute name="RDC-MAX" value="4.1 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="0.56 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_78433490075">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490075?ae"/>
<attribute name="FRES" value="154 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="12.8 A"/>
<attribute name="ISAT" value="34.5 A"/>
<attribute name="L" value="0.75 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490075 "/>
<attribute name="RDC-MAX" value="5.9 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="0.75 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_78433490160">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490160?ae"/>
<attribute name="FRES" value="93 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="8.4 A"/>
<attribute name="ISAT" value="22.3 A"/>
<attribute name="L" value="1.6 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490160 "/>
<attribute name="RDC-MAX" value="12 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="1.6 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_78433490240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490240?ae"/>
<attribute name="FRES" value="80 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="6.8 A"/>
<attribute name="ISAT" value="18.4 A"/>
<attribute name="L" value="2.4 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490240 "/>
<attribute name="RDC-MAX" value="18.4 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="2.4 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_78433490390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433490390?ae"/>
<attribute name="FRES" value="65 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="5 A"/>
<attribute name="ISAT" value="14.6 A"/>
<attribute name="L" value="3.9 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433490390 "/>
<attribute name="RDC-MAX" value="28.9 mohm"/>
<attribute name="SIZE" value="8090P"/>
<attribute name="VALUE" value="3.9 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_8090" prefix="L">
<description>&lt;b&gt;WE-CHSA SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt; Operating temperature: -55°C to +150°C
&lt;BR&gt; Current capability up to 28A
&lt;BR&gt; Ideal coplanarity due to embedded solder pads
&lt;BR&gt; Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04-03&lt;br&gt;
2026 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_8090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340033?ae"/>
<attribute name="FRES" value="196 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="21 A"/>
<attribute name="ISAT" value="36 A"/>
<attribute name="L" value="0.33 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340033"/>
<attribute name="RDC-MAX" value="2.1 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340047?ae"/>
<attribute name="FRES" value="146 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="19 A"/>
<attribute name="ISAT" value="29.7 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340047"/>
<attribute name="RDC-MAX" value="2.8 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340068?ae"/>
<attribute name="FRES" value="132 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="15.6 A"/>
<attribute name="ISAT" value="24.8 A"/>
<attribute name="L" value="0.68 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340068"/>
<attribute name="RDC-MAX" value="4.1 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340100?ae"/>
<attribute name="FRES" value="100 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="12.8 A"/>
<attribute name="ISAT" value="21.3 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340100"/>
<attribute name="RDC-MAX" value="5.9 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340220?ae"/>
<attribute name="FRES" value="80 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="8.4 A"/>
<attribute name="ISAT" value="14.7 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340220"/>
<attribute name="RDC-MAX" value="12 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340330?ae"/>
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="6.8 A"/>
<attribute name="ISAT" value="12.3 A"/>
<attribute name="L" value="3.3 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340330"/>
<attribute name="RDC-MAX" value="18.4 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7843340470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843340470?ae"/>
<attribute name="FRES" value="50 MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="5 A"/>
<attribute name="ISAT" value="9.6 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="8.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843340470"/>
<attribute name="RDC-MAX" value="28.9 mohm"/>
<attribute name="SIZE" value=" 8090 "/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_1212" prefix="L">
<description>&lt;b&gt;WE-CHSA SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt; Operating temperature: -55°C to +150°C
&lt;BR&gt; Current capability up to 28A
&lt;BR&gt; Ideal coplanarity due to embedded solder pads
&lt;BR&gt; Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107952v209%20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04-03&lt;br&gt;
2026 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843320039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320039?ae"/>
<attribute name="FRES" value="100 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="28 A"/>
<attribute name="ISAT" value="57 A"/>
<attribute name="L" value="0.39 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320039"/>
<attribute name="RDC-MAX" value="1.65 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="0.39 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320068?ae"/>
<attribute name="FRES" value="88 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="25.3 A"/>
<attribute name="ISAT" value="41.4 A"/>
<attribute name="L" value="0.68 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320068"/>
<attribute name="RDC-MAX" value="2.05 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320100?ae"/>
<attribute name="FRES" value="81 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="22.5 A"/>
<attribute name="ISAT" value="33.7 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320100"/>
<attribute name="RDC-MAX" value="2.4 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320150?ae"/>
<attribute name="FRES" value="74 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="19.7 A"/>
<attribute name="ISAT" value="28.2 A"/>
<attribute name="L" value="1.5 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320150"/>
<attribute name="RDC-MAX" value="3.3 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320270?ae"/>
<attribute name="FRES" value="50 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="16.2 A"/>
<attribute name="ISAT" value="21.6 A"/>
<attribute name="L" value="2.7 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320270"/>
<attribute name="RDC-MAX" value="4.7 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="2.7 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320330?ae"/>
<attribute name="FRES" value="45 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="13.8 A"/>
<attribute name="ISAT" value="19 A"/>
<attribute name="L" value="3.3 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320330"/>
<attribute name="RDC-MAX" value="6.4 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320470?ae"/>
<attribute name="FRES" value="37 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="12.2 A"/>
<attribute name="ISAT" value="15.3 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320470"/>
<attribute name="RDC-MAX" value="8.2 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320680?ae"/>
<attribute name="FRES" value="34 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="9.8 A"/>
<attribute name="ISAT" value="13 A"/>
<attribute name="L" value="6.8 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320680"/>
<attribute name="RDC-MAX" value="11.9 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843320820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843320820?ae"/>
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="8.8 A"/>
<attribute name="ISAT" value="12.1 A"/>
<attribute name="L" value="8.2 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843320820"/>
<attribute name="RDC-MAX" value="15 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843321000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843321000?ae"/>
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="7.8 A"/>
<attribute name="ISAT" value="10.8 A"/>
<attribute name="L" value="10 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843321000"/>
<attribute name="RDC-MAX" value="20.35 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843321200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843321200?ae"/>
<attribute name="FRES" value="28 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="7.1 A"/>
<attribute name="ISAT" value="10.3 A"/>
<attribute name="L" value="12 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843321200"/>
<attribute name="RDC-MAX" value="21.5 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843321800">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843321800?ae"/>
<attribute name="FRES" value="21 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="5.5 A"/>
<attribute name="ISAT" value="7.7 A"/>
<attribute name="L" value="18 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843321800"/>
<attribute name="RDC-MAX" value="38.4 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
<technology name="_7843322000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843322000?ae"/>
<attribute name="FRES" value="19 MHz"/>
<attribute name="HEIGHT" value="11.75mm"/>
<attribute name="IR" value="5.4 A"/>
<attribute name="ISAT" value="7 A"/>
<attribute name="L" value="20 uH"/>
<attribute name="LENGTH" value="12.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843322000"/>
<attribute name="RDC-MAX" value="43.1 mohm"/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="VALUE" value="20 uH"/>
<attribute name="WIDTH" value="12.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_1011P" prefix="L">
<description>&lt;b&gt;WE-CHSA Performance SMT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Saturation current up to 48.5 A
&lt;br&gt;Iron alloy core leads to soft saturation
&lt;br&gt;AEC-Q200
&lt;br&gt;Excellent coplanarity due to the plastic base
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CHSA-/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CHSA-&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-04--03&lt;br&gt;
2026 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1011P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433390150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390150?ae"/>
<attribute name="FRES" value="80 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="16 A"/>
<attribute name="ISAT" value="37.4 A"/>
<attribute name="L" value="1.5 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390150 "/>
<attribute name="RDC-MAX" value="4.7 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433390240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390240?ae"/>
<attribute name="FRES" value="60 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="13.8 A"/>
<attribute name="ISAT" value="28.7 A"/>
<attribute name="L" value="2.4 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390240 "/>
<attribute name="RDC-MAX" value="6.5 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="2.4 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433390300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390300?ae"/>
<attribute name="FRES" value="55 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="11.2 A"/>
<attribute name="ISAT" value="26.2 A"/>
<attribute name="L" value="3 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390300 "/>
<attribute name="RDC-MAX" value="8.7 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="3 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433390430">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390430?ae"/>
<attribute name="FRES" value="41 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="9.2 A"/>
<attribute name="ISAT" value="20.6 A"/>
<attribute name="L" value="4.3 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390430 "/>
<attribute name="RDC-MAX" value="13 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="4.3 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433390620">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390620?ae"/>
<attribute name="FRES" value="34 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="7.2 A"/>
<attribute name="ISAT" value="18 A"/>
<attribute name="L" value="6.2 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390620 "/>
<attribute name="RDC-MAX" value="19.1 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="6.2 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433390820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433390820?ae"/>
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="6.7 A"/>
<attribute name="ISAT" value="15.6 A"/>
<attribute name="L" value="8.2 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433390820 "/>
<attribute name="RDC-MAX" value="25.8 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433391000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433391000?ae"/>
<attribute name="FRES" value="28 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="5.6 A"/>
<attribute name="ISAT" value="14.4 A"/>
<attribute name="L" value="10 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433391000 "/>
<attribute name="RDC-MAX" value="33.2 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_78433391500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78433391500?ae"/>
<attribute name="FRES" value="20 MHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IR" value="4.3 A"/>
<attribute name="ISAT" value="11.3 A"/>
<attribute name="L" value="15 uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MOUNT" value="SMT "/>
<attribute name="PART-NUMBER" value=" 78433391500 "/>
<attribute name="RDC-MAX" value="60.9 mohm"/>
<attribute name="SIZE" value="1011P"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
