<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Common Mode Chokes for Mains Power Lines - WE-CMAHV&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-04-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMAHV_XXL_784831010205">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=46.5X28X44.5mm</description>
</package>
<package name="WE-CMAHV_XXL_784831034090">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=44.5X28X44.5mm</description>
</package>
<package name="WE-CMAHV_XXL_784831016164">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=46.5X28X44.5mm</description>
</package>
<package name="WE-CMAHV_XXL_784831020133">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=45.5X28X44.5mm</description>
</package>
<package name="WE-CMAHV_XL_784830010185">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=41.5X23X39.5mm</description>
</package>
<package name="WE-CMAHV_XL_784830025103">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=39.5X23X39.5mm</description>
</package>
<package name="WE-CMAHV_XL_784830017132">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=40X23X39.5mm</description>
</package>
<package name="WE-CMAHV_XL_784830007215">
<description>&lt;B&gt;WE-CMA HV Common Mode Power Line Choke Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=42.5X23X39.5mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-CMA_HV">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMAHV_XXL" prefix="L">
<description>&lt;b&gt;WE-CMAHV Common Mode Choke Automotive High Voltage&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;High permeability MnZn core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;Rated currents up to 22 A
&lt;br&gt;Applications up to 1000 VAC/1250 VDC
&lt;br&gt;Operating temperature: -40°C to +125°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line filter
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;DC/DC converters for hybrid and electric cars
&lt;br&gt;Onboard charger and motor inverter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o890967v209%20MODEL-WE-CMAHV-01.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o890967v209%20MODEL-WE-CMAHV-01.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMAHV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMAHV&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-04-09&lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMA_HV"/>
</gates>
<devices>
<device name="_784831010205" package="WE-CMAHV_XXL_784831010205">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784831010205?ae"/>
<attribute name="HEIGHT" value="44.5 mm"/>
<attribute name="IR" value="20.5 A"/>
<attribute name="L" value="1 mH"/>
<attribute name="LENGTH" value="46.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784831010205"/>
<attribute name="RDC" value="5.5 mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="1 mH"/>
<attribute name="WIDTH" value="28 mm"/>
</technology>
</technologies>
</device>
<device name="_784831016164" package="WE-CMAHV_XXL_784831016164">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784831016164?ae"/>
<attribute name="HEIGHT" value="44.5 mm"/>
<attribute name="IR" value="16.4 A"/>
<attribute name="L" value="1.6 mH"/>
<attribute name="LENGTH" value="46.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784831016164"/>
<attribute name="RDC" value="8.5 mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="1.6 mH"/>
<attribute name="WIDTH" value="28 mm"/>
</technology>
</technologies>
</device>
<device name="_784831020133" package="WE-CMAHV_XXL_784831020133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784831020133?ae"/>
<attribute name="HEIGHT" value="44.5 mm"/>
<attribute name="IR" value="13.3 A"/>
<attribute name="L" value="2 mH"/>
<attribute name="LENGTH" value="45.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784831020133"/>
<attribute name="RDC" value="13 mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="2 mH"/>
<attribute name="WIDTH" value="28 mm"/>
</technology>
</technologies>
</device>
<device name="_784831034090" package="WE-CMAHV_XXL_784831034090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784831034090?ae"/>
<attribute name="HEIGHT" value="44.5 mm"/>
<attribute name="IR" value="9 A"/>
<attribute name="L" value="3.4 mH"/>
<attribute name="LENGTH" value="44.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784831034090"/>
<attribute name="RDC" value="27 mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="3.4 mH"/>
<attribute name="WIDTH" value="28 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMAHV_XL" prefix="L">
<description>&lt;b&gt;WE-CMAHV Common Mode Choke Automotive High Voltage&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;High permeability MnZn core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;Rated currents up to 22 A
&lt;br&gt;Applications up to 1000 VAC/1250 VDC
&lt;br&gt;Operating temperature: -40°C to +125°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line filter
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;DC/DC converters for hybrid and electric cars
&lt;br&gt;Onboard charger and motor inverter
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o890967v209%20MODEL-WE-CMAHV-01.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o890967v209%20MODEL-WE-CMAHV-01.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMAHV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMAHV&lt;/a&gt;&lt;p&gt;

Created by Ella 2026-04-09&lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMA_HV"/>
</gates>
<devices>
<device name="_784830007215" package="WE-CMAHV_XL_784830007215">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784830007215?ae"/>
<attribute name="HEIGHT" value="39.5 mm"/>
<attribute name="IR" value="21.5 A"/>
<attribute name="L" value="0.7 mH"/>
<attribute name="LENGTH" value="42.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784830007215"/>
<attribute name="RDC" value="3.8 mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="0.7 mH"/>
<attribute name="WIDTH" value="23 mm"/>
</technology>
</technologies>
</device>
<device name="_784830010185" package="WE-CMAHV_XL_784830010185">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784830010185?ae"/>
<attribute name="HEIGHT" value="39.5 mm"/>
<attribute name="IR" value="18.5 A"/>
<attribute name="L" value="1 mH"/>
<attribute name="LENGTH" value="41.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784830010185"/>
<attribute name="RDC" value="5.5 mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="1 mH"/>
<attribute name="WIDTH" value="23 mm"/>
</technology>
</technologies>
</device>
<device name="_784830017132" package="WE-CMAHV_XL_784830017132">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784830017132?ae"/>
<attribute name="HEIGHT" value="39.5 mm"/>
<attribute name="IR" value="13.2 A"/>
<attribute name="L" value="1.7 mH"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784830017132"/>
<attribute name="RDC" value="10 mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="1.7 mH"/>
<attribute name="WIDTH" value="23 mm"/>
</technology>
</technologies>
</device>
<device name="_784830025103" package="WE-CMAHV_XL_784830025103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784830025103?ae"/>
<attribute name="HEIGHT" value="39.5 mm"/>
<attribute name="IR" value="10.3 A"/>
<attribute name="L" value="2.5 mH"/>
<attribute name="LENGTH" value="39.5 mm"/>
<attribute name="MATERIAL" value=" MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="784830025103"/>
<attribute name="RDC" value="18 mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="2.5 mH"/>
<attribute name="WIDTH" value="23 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
