<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Common Mode Chokes for Mains Power Lines - WE-CMANC&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMANC_M_7848030333">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: M, THT, 4pins
&lt;br&gt;LXWXH=23X13.5X26mm</description>
</package>
<package name="WE-CMANC_M_7848030509">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: M, THT, 4pins
&lt;br&gt;LXWXH=23X13.5X26mm</description>
</package>
<package name="WE-CMANC_M_7848031002">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: M, THT, 4pins
&lt;br&gt;LXWXH=24X17X25mm</description>
</package>
<package name="WE-CMANC_M_7848031501">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: M, THT, 4pins
&lt;br&gt;LXWXH=24X17X25mm</description>
</package>
<package name="WE-CMANC_M_7848030417">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: M, THT, 4pins
&lt;br&gt;LXWXH=23X13.5X26mm</description>
</package>
<package name="WE-CMANC_XL_7848050530">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=33X23X33mm</description>
</package>
<package name="WE-CMANC_XL_7848050219">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=33X19X38mm</description>
</package>
<package name="WE-CMANC_XL_7848050490">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=33X19X39mm</description>
</package>
<package name="WE-CMANC_XL_7848051012">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=34X23X33mm</description>
</package>
<package name="WE-CMANC_XL_7848051804">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=36X23X34mm</description>
</package>
<package name="WE-CMANC_XL_7848053201">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 12pins
&lt;br&gt;LXWXH=37X23X34mm</description>
</package>
<package name="WE-CMANC_L_7848040382">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=27.5X18X32mm</description>
</package>
<package name="WE-CMANC_XL_7848052502">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=36X23X34mm</description>
</package>
<package name="WE-CMANC_XL_7848052303">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XL, THT, 4pins
&lt;br&gt;LXWXH=36X23X33mm</description>
</package>
<package name="WE-CMANC_L_7848040435">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive

&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=27.5X18X32mm</description>
</package>
<package name="WE-CMANC_L_7848040515">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=28X19X32mm</description>
</package>
<package name="WE-CMANC_L_7848040707">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=29X19X32mm</description>
</package>
<package name="WE-CMANC_L_7848041801">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=30X19X28mm</description>
</package>
<package name="WE-CMANC_L_7848041104">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=29X19X28mm</description>
</package>
<package name="WE-CMANC_L_7848041502">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=29X19X28mm</description>
</package>
<package name="WE-CMANC_L_7848042001">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: L, THT, 4pins
&lt;br&gt;LXWXH=30X19X28mm</description>
</package>
<package name="WE-CMANC_XXL_7848060535">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=43X27X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848060620">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=43X27X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848061309">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=45X27X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848060814">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=43.5X27X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848061507">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=46.5X27.5X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848062105">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=46.5X27.5X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848062603">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 4pins
&lt;br&gt;LXWXH=47X27.5X46mm</description>
</package>
<package name="WE-CMANC_XXL_7848063801">
<description>&lt;B&gt;WE-CMANC Common Mode Choke Nanocrystalline Automotive
&lt;/b&gt;&lt;br&gt;&lt;br&gt; Size: XXL, THT, 12pins
&lt;br&gt;LXWXH=48X27.5X46mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-CMBNC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMANC_M" prefix="L">
<description>&lt;b&gt;WE-CMANC Common Mode Power Line Choke Nanocrystalline&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Very high permeability nanocrystalline core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;High and stable inductance values up to 150 °C
&lt;br&gt;High rated currents
&lt;br&gt;Broadband suppression
&lt;br&gt;Small size
&lt;br&gt;Frequency range: 1 kHz-300 MHz
&lt;br&gt;Climatic category: 55/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Operating temperature: -55 °C to +125 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Radio interference suppression in motors
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMANC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMANC&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-04 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMBNC"/>
</gates>
<devices>
<device name="_7848030333" package="WE-CMANC_M_7848030333">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848030333?ae"/>
<attribute name="HEIGHT" value="26mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="33mH"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848030333"/>
<attribute name="RDC-MAX" value="94mohm"/>
<attribute name="SIZE" value="M"/>
<attribute name="VALUE" value="33mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848030417" package="WE-CMANC_M_7848030417">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848030417?ae"/>
<attribute name="HEIGHT" value="26mm"/>
<attribute name="IR" value="4A"/>
<attribute name="L" value="17mH"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848030417"/>
<attribute name="RDC-MAX" value="52mohm"/>
<attribute name="SIZE" value="M"/>
<attribute name="VALUE" value="17mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848030509" package="WE-CMANC_M_7848030509">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848030509?ae"/>
<attribute name="HEIGHT" value="26mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="9mH"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848030509"/>
<attribute name="RDC-MAX" value="32mohm"/>
<attribute name="SIZE" value="M"/>
<attribute name="VALUE" value="9mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848031002" package="WE-CMANC_M_7848031002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848031002?ae"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="IR" value="10A"/>
<attribute name="L" value="2mH"/>
<attribute name="LENGTH" value="24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848031002"/>
<attribute name="RDC-MAX" value="6.3mohm"/>
<attribute name="SIZE" value="M"/>
<attribute name="VALUE" value="2mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="17mm"/>
</technology>
</technologies>
</device>
<device name="_7848031501" package="WE-CMANC_M_7848031501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848031501?ae"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="IR" value="15A"/>
<attribute name="L" value="1mH"/>
<attribute name="LENGTH" value="24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848031501"/>
<attribute name="RDC-MAX" value="3.2mohm"/>
<attribute name="SIZE" value="M"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="17mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMANC_XL" prefix="L">
<description>&lt;b&gt;WE-CMANC Common Mode Power Line Choke Nanocrystalline&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Very high permeability nanocrystalline core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;High and stable inductance values up to 150 °C
&lt;br&gt;High rated currents
&lt;br&gt;Broadband suppression
&lt;br&gt;Small size
&lt;br&gt;Frequency range: 1 kHz-300 MHz
&lt;br&gt;Climatic category: 55/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Operating temperature: -55 °C to +125 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Radio interference suppression in motors
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMANC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMANC&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-04 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMBNC"/>
</gates>
<devices>
<device name="_7848050219" package="WE-CMANC_XL_7848050219">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848050219?ae"/>
<attribute name="HEIGHT" value="38mm"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="190mH"/>
<attribute name="LENGTH" value="33mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848050219"/>
<attribute name="RDC-MAX" value="310mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="190mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848050490" package="WE-CMANC_XL_7848050490">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848050490?ae"/>
<attribute name="HEIGHT" value="39mm"/>
<attribute name="IR" value="3.5A"/>
<attribute name="L" value="90mH"/>
<attribute name="LENGTH" value="33mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848050490"/>
<attribute name="RDC-MAX" value="110mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="90mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848050530" package="WE-CMANC_XL_7848050530">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848050530?ae"/>
<attribute name="HEIGHT" value="33mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="30mH"/>
<attribute name="LENGTH" value="33mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848050530"/>
<attribute name="RDC-MAX" value="46mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="30mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
<device name="_7848051012" package="WE-CMANC_XL_7848051012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848051012?ae"/>
<attribute name="HEIGHT" value="33mm"/>
<attribute name="IR" value="10A"/>
<attribute name="L" value="12mH"/>
<attribute name="LENGTH" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848051012"/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="12mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
<device name="_7848051804" package="WE-CMANC_XL_7848051804">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848051804?ae"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="IR" value="18A"/>
<attribute name="L" value="4.5mH"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848051804"/>
<attribute name="RDC-MAX" value="4.2mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="4.5mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
<device name="_7848052303" package="WE-CMANC_XL_7848052303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848052303?ae"/>
<attribute name="HEIGHT" value="33mm"/>
<attribute name="IR" value="23A"/>
<attribute name="L" value="3mH"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848052303"/>
<attribute name="RDC-MAX" value="3mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="3mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
<device name="_7848052502" package="WE-CMANC_XL_7848052502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848052502?ae"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="IR" value="25A"/>
<attribute name="L" value="2.5mH"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848052502"/>
<attribute name="RDC-MAX" value="2.2mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="2.5mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
<device name="_7848053201" package="WE-CMANC_XL_7848053201">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3"/>
<connect gate="G$1" pin="2" pad="4 5 6"/>
<connect gate="G$1" pin="3" pad="7 8 9"/>
<connect gate="G$1" pin="4" pad="10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848053201?ae"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="IR" value="32A"/>
<attribute name="L" value="0.9mH"/>
<attribute name="LENGTH" value="37mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848053201"/>
<attribute name="RDC-MAX" value="1.1mohm"/>
<attribute name="SIZE" value="XL"/>
<attribute name="VALUE" value="0.9mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMANC_L" prefix="L">
<description>&lt;b&gt;WE-CMANC Common Mode Power Line Choke Nanocrystalline&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Very high permeability nanocrystalline core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;High and stable inductance values up to 150 °C
&lt;br&gt;High rated currents
&lt;br&gt;Broadband suppression
&lt;br&gt;Small size
&lt;br&gt;Frequency range: 1 kHz-300 MHz
&lt;br&gt;Climatic category: 55/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Operating temperature: -55 °C to +125 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Radio interference suppression in motors
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMANC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMANC&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-04 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMBNC"/>
</gates>
<devices>
<device name="_7848040382" package="WE-CMANC_L_7848040382">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848040382?ae"/>
<attribute name="HEIGHT" value="32mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="82mH"/>
<attribute name="LENGTH" value="27mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848040382"/>
<attribute name="RDC-MAX" value="170mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="82mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
</technologies>
</device>
<device name="_7848040435" package="WE-CMANC_L_7848040435">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848040435?ae"/>
<attribute name="HEIGHT" value="32mm"/>
<attribute name="IR" value="3.5A"/>
<attribute name="L" value="35mH"/>
<attribute name="LENGTH" value="27mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848040435"/>
<attribute name="RDC-MAX" value="80mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="35mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
</technologies>
</device>
<device name="_7848040515" package="WE-CMANC_L_7848040515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848040515?ae"/>
<attribute name="HEIGHT" value="32mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="15mH"/>
<attribute name="LENGTH" value="27mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848040515"/>
<attribute name="RDC-MAX" value="40mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="15mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
</technologies>
</device>
<device name="_7848040707" package="WE-CMANC_L_7848040707">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848040707?ae"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="7mH"/>
<attribute name="LENGTH" value="29mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848040707"/>
<attribute name="RDC-MAX" value="22mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="7mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848041104" package="WE-CMANC_L_7848041104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848041104?ae"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="11A"/>
<attribute name="L" value="4mH"/>
<attribute name="LENGTH" value="29mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848041104"/>
<attribute name="RDC-MAX" value="8.8mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="4mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848041502" package="WE-CMANC_L_7848041502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848041502?ae"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="15A"/>
<attribute name="L" value="2mH"/>
<attribute name="LENGTH" value="29mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848041502"/>
<attribute name="RDC-MAX" value="5mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="2mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848041801" package="WE-CMANC_L_7848041801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848041801?ae"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="18A"/>
<attribute name="L" value="1.5mH"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848041801"/>
<attribute name="RDC-MAX" value="3.2mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="1.5mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_7848042001" package="WE-CMANC_L_7848042001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848042001?ae"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="20A"/>
<attribute name="L" value="1mH"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848042001"/>
<attribute name="RDC-MAX" value="2.4mohm"/>
<attribute name="SIZE" value="L"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMANC_XXL" prefix="L">
<description>&lt;b&gt;WE-CMANC Common Mode Power Line Choke Nanocrystalline&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Very high permeability nanocrystalline core material
&lt;br&gt;Improved isolation through plastic case and winding spacer
&lt;br&gt;High and stable inductance values up to 150 °C
&lt;br&gt;High rated currents
&lt;br&gt;Broadband suppression
&lt;br&gt;Small size
&lt;br&gt;Frequency range: 1 kHz-300 MHz
&lt;br&gt;Climatic category: 55/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Operating temperature: -55 °C to +125 °C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Radio interference suppression in motors
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o876244v209%20family-WE-IndCMBNC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMANC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMANC&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-04 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMBNC"/>
</gates>
<devices>
<device name="_7848060535" package="WE-CMANC_XXL_7848060535">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848060535?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="35mH"/>
<attribute name="LENGTH" value="43mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848060535"/>
<attribute name="RDC-MAX" value="90mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="35mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27mm"/>
</technology>
</technologies>
</device>
<device name="_7848060620" package="WE-CMANC_XXL_7848060620">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848060620?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="20mH"/>
<attribute name="LENGTH" value="43mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848060620"/>
<attribute name="RDC-MAX" value="45mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27mm"/>
</technology>
</technologies>
</device>
<device name="_7848060814" package="WE-CMANC_XXL_7848060814">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848060814?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="14mH"/>
<attribute name="LENGTH" value="43.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848060814"/>
<attribute name="RDC-MAX" value="27mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="14mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27mm"/>
</technology>
</technologies>
</device>
<device name="_7848061309" package="WE-CMANC_XXL_7848061309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848061309?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="13A"/>
<attribute name="L" value="9mH"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848061309"/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="9mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27mm"/>
</technology>
</technologies>
</device>
<device name="_7848061507" package="WE-CMANC_XXL_7848061507">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848061507?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="15A"/>
<attribute name="L" value="7mH"/>
<attribute name="LENGTH" value="46.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848061507"/>
<attribute name="RDC-MAX" value="9.5mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="7mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848062105" package="WE-CMANC_XXL_7848062105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848062105?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="21A"/>
<attribute name="L" value="5mH"/>
<attribute name="LENGTH" value="46.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848062105"/>
<attribute name="RDC-MAX" value="6.5mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="5mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848062603" package="WE-CMANC_XXL_7848062603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848062603?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="26A"/>
<attribute name="L" value="3mH"/>
<attribute name="LENGTH" value="47mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848062603"/>
<attribute name="RDC-MAX" value="4.5mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="3mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27.5mm"/>
</technology>
</technologies>
</device>
<device name="_7848063801" package="WE-CMANC_XXL_7848063801">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3"/>
<connect gate="G$1" pin="2" pad="4 5 6"/>
<connect gate="G$1" pin="3" pad="7 8 9"/>
<connect gate="G$1" pin="4" pad="10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7848063801?ae"/>
<attribute name="HEIGHT" value="46mm"/>
<attribute name="IR" value="38A"/>
<attribute name="L" value="1.5mH"/>
<attribute name="LENGTH" value="48mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7848063801"/>
<attribute name="RDC-MAX" value="2.3mohm"/>
<attribute name="SIZE" value="XXL"/>
<attribute name="VALUE" value="1.5mH"/>
<attribute name="VR" value="300VAC"/>
<attribute name="VT" value="2100VAC"/>
<attribute name="WIDTH" value="27.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
