<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Mains Power Lines - WE-CMB&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021d, 2021-11-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMB_XXL_7448261418">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XXL, THT, 4pins
&lt;br&gt;L X W X H=43mm X 23.5mm X 43mm</description>
</package>
<package name="WE-CMB_L">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : L, THT, 4pins
&lt;br&gt;L X W X H=27.5mm X 18.5mm X 33mm</description>
</package>
<package name="WE-CMB_XXL_7448262510">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XXL, THT, 4pins
&lt;br&gt;L X W X H=44mm X 23.5mm X 43mm</description>
</package>
<package name="WE-CMB_XXL_7448263505">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XXL, THT, 4pins
&lt;br&gt;L X W X H=47mm X 23.5mm X 43mm</description>
</package>
<package name="WE-CMB_XXL_7448262013">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XXL, THT, 4pins
&lt;br&gt;L X W X H=43.5mm X 23.5mm X 43mm</description>
</package>
<package name="WE-CMB_S">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : S, THT, 4pins
&lt;br&gt;L X W X H=17.5mm X 13mm X 22mm</description>
</package>
<package name="WE-CMB_XS_744821120">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XS, THT, 4pins
&lt;br&gt;L X W X H=15mm X 7.8mm X 17.5mm</description>
</package>
<package name="WE-CMB_XS">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XS, THT, 4pins
&lt;br&gt;L X W X H=15mm X 7.5mm X 18mm</description>
</package>
<package name="WE-CMB_XS_744821150">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XS, THT, 4pins
&lt;br&gt;L X W X H=15mm X 7.8mm X 18mm</description>
</package>
<package name="WE-CMB_M_744823333">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : L, THT, 4pins
&lt;br&gt;L X W X H=23.5mm X 13mm X 25.5mm</description>
</package>
<package name="WE-CMB_XS_744821240">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XS, THT, 4pins
&lt;br&gt;L X W X H=15.8mm X 8mm X 18mm</description>
</package>
<package name="WE-CMB_M">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : M, THT, 4pins
&lt;br&gt;L X W X H=23mm X 13.8mm X 25.5mm</description>
</package>
<package name="WE-CMB_M_744823601">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : L, THT, 4pins
&lt;br&gt;L X W X H=25mm X 17mm X 26.5mm</description>
</package>
<package name="WE-CMB_XL_7448251201">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XL, THT, 4pins
&lt;br&gt;L X W X H=31mm X 22mm X 35mm</description>
</package>
<package name="WE-CMB_M_744823422">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : L, THT, 4pins
&lt;br&gt;L X W X H=23.5mm X 13.8mm X 25.5mm</description>
</package>
<package name="WE-CMB_XL">
<description>&lt;b&gt;WE-CMB Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : XL, THT, 4pins
&lt;br&gt;L X W X H=30mm X 21mm X 35mm</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMB_L" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2021-04-022&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744824220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824220.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824220 "/>
<attribute name="RDC" value="220mOhm"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824310.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824310 "/>
<attribute name="RDC" value="105mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824405">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824405.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824405 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="5mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824407">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824407.pdf"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824407 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="7mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824433">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824433.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824433 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824622">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824622.pdf"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824622 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744824801">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744824801.pdf"/>
<attribute name="IR" value="7.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744824801 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_S" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2020-12-07&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744822110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744822110.pdf"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744822110 "/>
<attribute name="RDC" value="360mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744822120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744822120.pdf"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744822120 "/>
<attribute name="RDC" value="540mOhm"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744822222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744822222.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744822222 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744822233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744822233.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744822233 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744822301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744822301.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744822301 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_XXL" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2020-12-07&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="_7448261418" package="WE-CMB_XXL_7448261418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448261418.pdf"/>
<attribute name="IR" value="14A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448261418 "/>
<attribute name="RDC" value="9.5mOhm"/>
<attribute name="VALUE" value="1.8mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_7448262013" package="WE-CMB_XXL_7448262013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448262013.pdf"/>
<attribute name="IR" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448262013 "/>
<attribute name="RDC" value="6.2mOhm"/>
<attribute name="VALUE" value="1.3mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_7448262510" package="WE-CMB_XXL_7448262510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448262510.pdf"/>
<attribute name="IR" value="25A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448262510 "/>
<attribute name="RDC" value="4.5mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_7448263505" package="WE-CMB_XXL_7448263505">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448263505.pdf"/>
<attribute name="IR" value="35A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448263505 "/>
<attribute name="RDC" value="2.3mOhm"/>
<attribute name="VALUE" value="0.5mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_XS" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2021-11-12&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744821039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821039.pdf"/>
<attribute name="IR" value="0.3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821039 "/>
<attribute name="RDC" value="3000mOhm"/>
<attribute name="VALUE" value="39mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744821110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821110.pdf"/>
<attribute name="IR" value="0.7A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821110 "/>
<attribute name="RDC" value="350mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744821201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821201.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821201 "/>
<attribute name="RDC" value="45mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_744821120" package="WE-CMB_XS_744821120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821120.pdf"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821120 "/>
<attribute name="RDC" value="1000mOhm"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_744821150" package="WE-CMB_XS_744821150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821150.pdf"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821150 "/>
<attribute name="RDC" value="220mOhm"/>
<attribute name="VALUE" value="5mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_744821240" package="WE-CMB_XS_744821240">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744821240.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744821240 "/>
<attribute name="RDC" value="140mOhm"/>
<attribute name="VALUE" value="4mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_XL" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2021-03-05&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="_7448251201" package="WE-CMB_XL_7448251201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448251201.pdf"/>
<attribute name="IR" value="12A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448251201 "/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="" package="WE-CMB_XL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744825320">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744825320.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744825320 "/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744825410">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744825410.pdf"/>
<attribute name="IR" value="4.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744825410 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744825433">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744825433.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744825433 "/>
<attribute name="RDC" value="210mOhm"/>
<attribute name="VALUE" value="33mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7448256033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448256033.pdf"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448256033 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744825605">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744825605.pdf"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744825605 "/>
<attribute name="RDC" value="45mOhm"/>
<attribute name="VALUE" value="5mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7448258022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448258022.pdf"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448258022 "/>
<attribute name="RDC" value="14mOhm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_M" prefix="L">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2

&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filterring of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14763v209%20Family_WE-CMB_XS-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB"&gt;https://www.we-online.com/katalog/en/WE-CMB&lt;/a&gt;&lt;p&gt;


Updated by  Ella Wu 2020-12-07&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="_744823601" package="WE-CMB_M_744823601">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823601.pdf"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823601 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="" package="WE-CMB_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744823210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823210.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823210 "/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744823220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823220.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823220 "/>
<attribute name="RDC" value="270mOhm"/>
<attribute name="VALUE" value="20mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744823305">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823305.pdf"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823305 "/>
<attribute name="RDC" value="95mOhm"/>
<attribute name="VALUE" value="5mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_744823333" package="WE-CMB_M_744823333">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823333.pdf"/>
<attribute name="IR" value="2.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823333 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
<device name="_744823422" package="WE-CMB_M_744823422">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744823422.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744823422 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
