<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Mains Power Lines - WE-CMB NiZn&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021b, 2021-04-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMB_NIZN_XS">
<description>&lt;B&gt;WE-CMB NiZn Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : Type XS, THT, 4pins
&lt;br&gt;L X W X H=16mm X 17.5mm X 7.5mm</description>
</package>
<package name="WE-CMB_NIZN_S">
<description>&lt;B&gt;WE-CMB NiZn Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : Type S, THT, 4pins
&lt;br&gt;L X W X H=18.5mm X 22mm X 14.5mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-CMB_NIZN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMB_NIZN_XS" prefix="L">
<description>&lt;b&gt;WE-CMB NiZn Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: Nickel-Zinc Ferrite
&lt;br&gt;High suppression rates of asymmetrical interferences at high and middle frequencies
&lt;br&gt;High interference stability against RF interference and burst signals
&lt;br&gt;Compact design
&lt;br&gt;Noise suppression up to 300 MHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Optimized for burst signals
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o14762v209%20Family_WE-CMB_NiZn.jpg"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o14762v209%20Family_WE-CMB_NiZn.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB-NIZN"&gt;https://www.we-online.com/katalog/en/WE-CMB-NIZN&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu  2020-12-07&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMB_NIZN"/>
</gates>
<devices>
<device name="" package="WE-CMB_NIZN_XS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744841210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744841210.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744841210 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744841247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744841247.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744841247 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744841330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744841330.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744841330 "/>
<attribute name="RDC" value="26mOhm"/>
<attribute name="VALUE" value="30uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744841414">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744841414.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744841414 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="14uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_NIZN_S" prefix="L">
<description>&lt;b&gt;WE-CMB NiZn Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: Nickel-Zinc Ferrite
&lt;br&gt;High suppression rates of asymmetrical interferences at high and middle frequencies
&lt;br&gt;High interference stability against RF interference and burst signals
&lt;br&gt;Compact design
&lt;br&gt;Noise suppression up to 300 MHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Optimized for burst signals
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o14762v209%20Family_WE-CMB_NiZn.jpg"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o14762v209%20Family_WE-CMB_NiZn.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB-NIZN"&gt;https://www.we-online.com/katalog/en/WE-CMB-NIZN&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu  2021-04-02&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CMB_NIZN"/>
</gates>
<devices>
<device name="" package="WE-CMB_NIZN_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744842311">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744842311.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744842311 "/>
<attribute name="RDC" value="31mOhm"/>
<attribute name="VALUE" value="110uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744842565">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744842565.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744842565 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="VALUE" value="65uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744842632">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744842632.pdf"/>
<attribute name="IR" value="5.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744842632 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="32uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744842742">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744842742.pdf"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744842742 "/>
<attribute name="RDC" value="8.1mOhm"/>
<attribute name="VALUE" value="42uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_744842816">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744842816.pdf"/>
<attribute name="IR" value="7.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 744842816 "/>
<attribute name="RDC" value="5mOhm"/>
<attribute name="VALUE" value="16uH"/>
<attribute name="VR" value="250  V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
