<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - Common Mode Chokes for Extra-low Voltage and Data Lines - WE-CMDC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-12-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMDC_9070">
<description>&lt;b&gt;WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size: 9070, SMT, 4pins
&lt;br&gt;L X W X H X FI = 9mm X 7mm X 4.5mm X 1.3mm</description>
</package>
<package name="WE-CMDC_7060">
<description>&lt;b&gt;WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size: 7060, SMT, 4pins
&lt;br&gt;L X W X H X FI = 7mm X 6mm X 3.5mm X 1.3mm</description>
</package>
<package name="WE-CMDC_1211">
<description>&lt;b&gt;WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size: 1211, SMT, 4pins
&lt;br&gt;L X W X H X FI = 12mm X 11mm X 6mm X 2.3mm</description>
</package>
<package name="WE-CMDC_1513">
<description>&lt;b&gt;WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size: 1513, SMT, 4pins
&lt;br&gt;L X W X H X FI = 15mm X 13mm X 6mm X 2.3mm</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMDC_9070" prefix="L">
<description>&lt;b&gt; WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High current up to 8 A
&lt;br&gt; High impedance up to 1500 Ω
&lt;br&gt;Low profile in SMT construction
&lt;br&gt; Compact case
&lt;br&gt; AEC-Q200 qualification
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt; DC low voltage power lines
&lt;br&gt; Data and signal lines
 &lt;br&gt;Power supply systems
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMDC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMDC&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-12-18&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMDC_9070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744239252">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744239252?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="1.9A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744239252"/>
<attribute name="RDC" value="71mOhm"/>
<attribute name="SIZE" value=" 9070 "/>
<attribute name="VALUE" value="45uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="2500Ohm"/>
</technology>
<technology name="_744239301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744239301?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="4.5uH"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744239301"/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="SIZE" value=" 9070 "/>
<attribute name="VALUE" value="4.5uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="300Ohm"/>
</technology>
<technology name="_744239701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744239701?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="8uH"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744239701"/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="SIZE" value=" 9070 "/>
<attribute name="VALUE" value="8uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="700Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMDC_7060" prefix="L">
<description>&lt;b&gt; WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High current up to 8 A
&lt;br&gt; High impedance up to 1500 Ω
&lt;br&gt;Low profile in SMT construction
&lt;br&gt; Compact case
&lt;br&gt; AEC-Q200 qualification
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt; DC low voltage power lines
&lt;br&gt; Data and signal lines
 &lt;br&gt;Power supply systems
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMDC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMDC&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-12-18&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMDC_7060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744238102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238102?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238102"/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="12.5uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="1000Ohm"/>
</technology>
<technology name="_744238132">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238132?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="14uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238132"/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="14uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="1300Ohm"/>
</technology>
<technology name="_744238182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238182?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="20uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238182"/>
<attribute name="RDC" value="53mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="20uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="1800Ohm"/>
</technology>
<technology name="_744238202">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238202?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="L" value="23.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238202"/>
<attribute name="RDC" value="63mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="23.5uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="2000Ohm"/>
</technology>
<technology name="_744238252">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238252?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="1.2A"/>
<attribute name="L" value="27uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238252"/>
<attribute name="RDC" value="72mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="2500Ohm"/>
</technology>
<technology name="_744238301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238301?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="4uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238301"/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="4uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="300Ohm"/>
</technology>
<technology name="_744238501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238501?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="4.5A"/>
<attribute name="L" value="7uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238501"/>
<attribute name="RDC" value="14mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="7uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="500Ohm"/>
</technology>
<technology name="_744238701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744238701?ae"/>
<attribute name="FI" value="1.3mm"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="4A"/>
<attribute name="L" value="9uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744238701"/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="SIZE" value=" 7060 "/>
<attribute name="VALUE" value="9uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="700Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMDC_1211" prefix="L">
<description>&lt;b&gt; WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High current up to 8 A
&lt;br&gt; High impedance up to 1500 Ω
&lt;br&gt;Low profile in SMT construction
&lt;br&gt; Compact case
&lt;br&gt; AEC-Q200 qualification
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt; DC low voltage power lines
&lt;br&gt; Data and signal lines
 &lt;br&gt;Power supply systems
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMDC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMDC&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-12-18&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMDC_1211">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744237102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744237102?ae"/>
<attribute name="FI" value="2.3mm"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="13uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744237102"/>
<attribute name="RDC" value="14mOhm"/>
<attribute name="SIZE" value="1211"/>
<attribute name="VALUE" value="13uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="1000Ohm"/>
</technology>
<technology name="_744237152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744237152?ae"/>
<attribute name="FI" value="2.3mm"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="4.5A"/>
<attribute name="L" value="17uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744237152"/>
<attribute name="RDC" value="21mOhm"/>
<attribute name="SIZE" value="1211"/>
<attribute name="VALUE" value="17uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="1500Ohm"/>
</technology>
<technology name="_744237701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744237701?ae"/>
<attribute name="FI" value="2.3mm"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="9uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744237701"/>
<attribute name="RDC" value="6mOhm"/>
<attribute name="SIZE" value="1211"/>
<attribute name="VALUE" value="9uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
<attribute name="WINDING-STYLE" value="sectional"/>
<attribute name="Z" value="700Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMDC_1513" prefix="L">
<description>&lt;b&gt; WE-CMDC Common Mode Data Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High current up to 8 A
&lt;br&gt; High impedance up to 1500 Ω
&lt;br&gt;Low profile in SMT construction
&lt;br&gt; Compact case
&lt;br&gt; AEC-Q200 qualification
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt; DC low voltage power lines
&lt;br&gt; Data and signal lines
 &lt;br&gt;Power supply systems
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o182610v209%20Model.4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CMDC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CMDC&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-12-18&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMDC_1513">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744240202">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744240202?ae"/>
<attribute name="FI" value="2.3mm"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="31.5uH"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744240202"/>
<attribute name="RDC" value="21mOhm"/>
<attribute name="SIZE" value=" 1513 "/>
<attribute name="VALUE" value="31.5uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="13mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="2000Ohm"/>
</technology>
<technology name="_744240501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744240501?ae"/>
<attribute name="FI" value="2.3mm"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="10A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744240501"/>
<attribute name="RDC" value="5.6mOhm"/>
<attribute name="SIZE" value=" 1513 "/>
<attribute name="VALUE" value="6.3uH"/>
<attribute name="VR" value="80V(DC)"/>
<attribute name="WIDTH" value="13mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="500Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
