<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Common Mode Chokes for Extra-low Voltage and Data Lines - WE-CNSA&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-07-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CNSA_0805">
<description>&lt;b&gt;WE-CNSA SMD Common Mode Power Line Choke
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 4pins
&lt;br&gt;L X W X H=2mm X 1.2mm X 1.2mm</description>
</package>
<package name="WE-CNSA_1210">
<description>&lt;b&gt;WE-CNSA SMD Common Mode Power Line Choke
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1210, SMT, 4pins
&lt;br&gt;L X W X H=3.2mm X 2.5mm X 2.5mm</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H_SINGLELINE">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CM2W-H">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CNSA_1210" prefix="L">
<description>&lt;b&gt;WE-CNSA SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current compensated data line filter
&lt;BR&gt; High common mode noise suppression at high frequencies
&lt;BR&gt; Low RDC design
&lt;BR&gt; AEC-Q200
&lt;BR&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Car infotainment
&lt;BR&gt;Flex ray
&lt;BR&gt;High speed data lines
&lt;BR&gt;IEEE 1394 (Firewire)
&lt;BR&gt;LVDS
&lt;BR&gt;USB 2.0 &amp; 3.0
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o639517v209%20784231xxx_0805_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o639517v209%20784231xxx_0805_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CNSA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2023-07-24&lt;br&gt;
2023 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="CM2W-H_SINGLELINE"/>
</gates>
<devices>
<device name="" package="WE-CNSA_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_784234101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784234101?ae"/>
<attribute name="IR" value="100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784234101 "/>
<attribute name="RDC" value="3.36ohm"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VR" value="80V (DC)"/>
<attribute name="VT" value="125V (DC)"/>
<attribute name="WINDING-STYLE" value="bifilar"/>
<attribute name="Z1" value="4890ohm@10MHz"/>
<attribute name="Z2" value="9850ohm@100MHz"/>
</technology>
<technology name="_784234201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784234201?ae"/>
<attribute name="IR" value="70mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784234201 "/>
<attribute name="RDC" value="5.5ohm"/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VR" value="80V (DC)"/>
<attribute name="VT" value="125V (DC)"/>
<attribute name="WINDING-STYLE" value="bifilar"/>
<attribute name="Z1" value="10640ohm@10MHz"/>
<attribute name="Z2" value="10500ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSA_0805" prefix="L">
<description>&lt;b&gt;WE-CNSA SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Current compensated data line filter
&lt;BR&gt; High common mode noise suppression at high frequencies
&lt;BR&gt; Low RDC design
&lt;BR&gt; AEC-Q200
&lt;BR&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Car infotainment
&lt;BR&gt;Flex ray
&lt;BR&gt;High speed data lines
&lt;BR&gt;IEEE 1394 (Firewire)
&lt;BR&gt;LVDS
&lt;BR&gt;USB 2.0 &amp; 3.0
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o639517v209%20784231xxx_0805_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o639517v209%20784231xxx_0805_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CNSA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-01-26&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSA_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_784231061">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231061?ae"/>
<attribute name="IR" value="400mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231061 "/>
<attribute name="RDC" value="0.25ohm"/>
<attribute name="VALUE" value="0.088uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="10ohm@10MHz"/>
<attribute name="Z2" value="67ohm@100MHz"/>
</technology>
<technology name="_784231091">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231091?ae"/>
<attribute name="IR" value="370mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231091 "/>
<attribute name="RDC" value="0.3ohm"/>
<attribute name="VALUE" value="0.131uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="12ohm@10MHz"/>
<attribute name="Z2" value="90ohm@100MHz"/>
</technology>
<technology name="_784231121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231121?ae"/>
<attribute name="IR" value="370mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231121 "/>
<attribute name="RDC" value="0.3ohm"/>
<attribute name="VALUE" value="0.166uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="18ohm@10MHz"/>
<attribute name="Z2" value="120ohm@100MHz"/>
</technology>
<technology name="_784231181">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231181?ae"/>
<attribute name="IR" value="330mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231181 "/>
<attribute name="RDC" value="0.35ohm"/>
<attribute name="VALUE" value="0.252uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="28ohm@10MHz"/>
<attribute name="Z2" value="180ohm@100MHz"/>
</technology>
<technology name="_784231261">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231261?ae"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231261 "/>
<attribute name="RDC" value="0.4ohm"/>
<attribute name="VALUE" value="0.367uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="36ohm@10MHz"/>
<attribute name="Z2" value="260ohm@100MHz"/>
</technology>
<technology name="_784231371">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784231371?ae"/>
<attribute name="IR" value="280mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784231371 "/>
<attribute name="RDC" value="0.45ohm"/>
<attribute name="VALUE" value="0.478uH"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="VT" value="125V (AC)"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z1" value="54ohm@10MHz"/>
<attribute name="Z2" value="370ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
