<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Current Sense Transformers - WE-CSTLF&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-07-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CSTLF_EI187">
</package>
</packages>
<symbols>
<symbol name="WE-CSTLF_EI187">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CSTLF_EI187" prefix="T">
<description>&lt;b&gt;WE-CSTLF Line Frequency Current Sense Transformer&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Primary current rating to 45A
&lt;br&gt;Frequency 47Hz - 400Hz
&lt;br&gt;UL Class F 155°C Insulation System
&lt;br&gt;Operating temperature: -40 °C to +125 °C
&lt;br&gt;Low profile, compact, THT form factor
&lt;br&gt;Dielectric isolation 4kV AC
&lt;br&gt;Safety: IEC62368-1 / IEC61558-2-16
&lt;br&gt;AEC-Q200 qualification

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;AC current detection
&lt;br&gt;Fixed chargers on streets and garages (EV charging infrastructure)
&lt;br&gt;Overload sensing
&lt;br&gt;Load drop/shutdown detection
&lt;br&gt;Industrial automation
&lt;br&gt;Control and monitoring applications
&lt;br&gt;Motor Controls
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o783729v209%20multi-WE-CST-7492551000.178.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o783729v209%20multi-WE-CST-7492551000.178.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CSTLF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-CSTLF&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CSTLF_EI187"/>
</gates>
<devices>
<device name="" package="WE-CSTLF_EI187">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7492550500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492550500.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:500"/>
<attribute name="PART-NUMBER" value=" 7492550500 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="16.2Ohm"/>
<attribute name="VALUE" value="400mH"/>
<attribute name="VDT" value="10uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
<technology name="_7492551000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492551000.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:1000"/>
<attribute name="PART-NUMBER" value=" 7492551000 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="78.7Ohm"/>
<attribute name="VALUE" value="1600mH"/>
<attribute name="VDT" value="15uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
<technology name="_7492551500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492551500.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:1500"/>
<attribute name="PART-NUMBER" value=" 7492551500 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="178Ohm"/>
<attribute name="VALUE" value="3600mH"/>
<attribute name="VDT" value="20uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
<technology name="_7492552000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492552000.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:2000"/>
<attribute name="PART-NUMBER" value=" 7492552000 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="317Ohm"/>
<attribute name="VALUE" value="6400mH"/>
<attribute name="VDT" value="25uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
<technology name="_7492552500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492552500.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:2500"/>
<attribute name="PART-NUMBER" value=" 7492552500 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="468Ohm"/>
<attribute name="VALUE" value="10000mH"/>
<attribute name="VDT" value="30uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
<technology name="_7492553000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7492553000.pdf"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="45A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="N" value="1:3000"/>
<attribute name="PART-NUMBER" value=" 7492553000 "/>
<attribute name="RDC1" value="0.27mOhm"/>
<attribute name="RDC2" value="747Ohm"/>
<attribute name="VALUE" value="14400mH"/>
<attribute name="VDT" value="35uVs"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="16.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
