<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-DD&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-DD_1210">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1210</description>
</package>
<package name="WE-DD_1280_CROSSED">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280 crossed</description>
</package>
<package name="WE-DD_7332">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7332</description>
</package>
<package name="WE-DD_7345">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7345</description>
</package>
<package name="WE-DD_1260">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1260</description>
</package>
<package name="WE-DD_1260_CROSSED">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1260 crossed</description>
</package>
<package name="WE-DD_1280">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DD SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280</description>
</package>
</packages>
<symbols>
<symbol name="WE-DD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-DD_1210" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448709022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709022.pdf"/>
<attribute name="FRE" value="45MHz"/>
<attribute name="IR1" value="4.1A"/>
<attribute name="IR2" value="4.1A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="PART-NUMBER" value=" 7448709022 "/>
<attribute name="RDC1-MAX" value="0.017Ohm"/>
<attribute name="RDC1-TYP" value="0.015Ohm"/>
<attribute name="RDC2-MAX" value="0.017Ohm"/>
<attribute name="RDC2-TYP" value="0.015Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448709033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709033.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="3.7A"/>
<attribute name="IR2" value="3.7A"/>
<attribute name="ISAT" value="15.5A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 7448709033 "/>
<attribute name="RDC1-MAX" value="0.02Ohm"/>
<attribute name="RDC1-TYP" value="0.017Ohm"/>
<attribute name="RDC2-MAX" value="0.02Ohm"/>
<attribute name="RDC2-TYP" value="0.017Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448709047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709047.pdf"/>
<attribute name="FRE" value="30MHz"/>
<attribute name="IR1" value="3.6A"/>
<attribute name="IR2" value="3.6A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 7448709047 "/>
<attribute name="RDC1-MAX" value="0.023Ohm"/>
<attribute name="RDC1-TYP" value="0.019Ohm"/>
<attribute name="RDC2-MAX" value="0.023Ohm"/>
<attribute name="RDC2-TYP" value="0.019Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448709068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709068.pdf"/>
<attribute name="FRE" value="23MHz"/>
<attribute name="IR1" value="3.3A"/>
<attribute name="IR2" value="3.3A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 7448709068 "/>
<attribute name="RDC1-MAX" value="0.031Ohm"/>
<attribute name="RDC1-TYP" value="0.026Ohm"/>
<attribute name="RDC2-MAX" value="0.031Ohm"/>
<attribute name="RDC2-TYP" value="0.026Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448709100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709100.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="3.2A"/>
<attribute name="IR2" value="3.2A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 7448709100 "/>
<attribute name="RDC1-MAX" value="0.04Ohm"/>
<attribute name="RDC1-TYP" value="0.033Ohm"/>
<attribute name="RDC2-MAX" value="0.04Ohm"/>
<attribute name="RDC2-TYP" value="0.033Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448709220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709220.pdf"/>
<attribute name="FRE" value="10MHz"/>
<attribute name="IR1" value="3.5A"/>
<attribute name="IR2" value="3.5A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 7448709220 "/>
<attribute name="RDC1-MAX" value="0.08Ohm"/>
<attribute name="RDC1-TYP" value="0.064Ohm"/>
<attribute name="RDC2-MAX" value="0.08Ohm"/>
<attribute name="RDC2-TYP" value="0.064Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448709330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709330.pdf"/>
<attribute name="FRE" value="6MHz"/>
<attribute name="IR1" value="2A"/>
<attribute name="IR2" value="2A"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="L2" value="33uH"/>
<attribute name="PART-NUMBER" value=" 7448709330 "/>
<attribute name="RDC1-MAX" value="0.1Ohm"/>
<attribute name="RDC1-TYP" value="0.08Ohm"/>
<attribute name="RDC2-MAX" value="0.1Ohm"/>
<attribute name="RDC2-TYP" value="0.08Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448709470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448709470.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR1" value="1.9A"/>
<attribute name="IR2" value="1.9A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 7448709470 "/>
<attribute name="RDC1-MAX" value="0.13Ohm"/>
<attribute name="RDC1-TYP" value="0.106Ohm"/>
<attribute name="RDC2-MAX" value="0.13Ohm"/>
<attribute name="RDC2-TYP" value="0.106Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1280_CROSSED" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_1280_CROSSED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448700015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448700015.pdf"/>
<attribute name="FRE" value="60MHz"/>
<attribute name="IR1" value="8.6A"/>
<attribute name="IR2" value="8.6A"/>
<attribute name="ISAT" value="17.5A"/>
<attribute name="L2" value="0.5uH"/>
<attribute name="PART-NUMBER" value=" 7448700015 "/>
<attribute name="RDC1-MAX" value="0.016Ohm"/>
<attribute name="RDC1-TYP" value="0.012Ohm"/>
<attribute name="RDC2-MAX" value="0.016Ohm"/>
<attribute name="RDC2-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="0.5uH"/>
</technology>
<technology name="_744870002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870002.pdf"/>
<attribute name="FRE" value="40MHz"/>
<attribute name="IR1" value="7.8A"/>
<attribute name="IR2" value="7.8A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="L2" value="2.4uH"/>
<attribute name="PART-NUMBER" value=" 744870002 "/>
<attribute name="RDC1-MAX" value="0.018Ohm"/>
<attribute name="RDC1-TYP" value="0.014Ohm"/>
<attribute name="RDC2-MAX" value="0.018Ohm"/>
<attribute name="RDC2-TYP" value="0.014Ohm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744870003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870003.pdf"/>
<attribute name="FRE" value="30MHz"/>
<attribute name="IR1" value="7.1A"/>
<attribute name="IR2" value="7.1A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 744870003 "/>
<attribute name="RDC1-MAX" value="0.021Ohm"/>
<attribute name="RDC1-TYP" value="0.016Ohm"/>
<attribute name="RDC2-MAX" value="0.021Ohm"/>
<attribute name="RDC2-TYP" value="0.016Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744870004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870004.pdf"/>
<attribute name="FRE" value="34MHz"/>
<attribute name="IR1" value="3.6A"/>
<attribute name="IR2" value="3.6A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744870004 "/>
<attribute name="RDC1-MAX" value="0.03Ohm"/>
<attribute name="RDC1-TYP" value="0.025Ohm"/>
<attribute name="RDC2-MAX" value="0.03Ohm"/>
<attribute name="RDC2-TYP" value="0.025Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744870006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870006.pdf"/>
<attribute name="FRE" value="18MHz"/>
<attribute name="IR1" value="3.2A"/>
<attribute name="IR2" value="3.2A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 744870006 "/>
<attribute name="RDC1-MAX" value="0.035Ohm"/>
<attribute name="RDC1-TYP" value="0.027Ohm"/>
<attribute name="RDC2-MAX" value="0.035Ohm"/>
<attribute name="RDC2-TYP" value="0.027Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744870100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870100.pdf"/>
<attribute name="FRE" value="18MHz"/>
<attribute name="IR1" value="2.7A"/>
<attribute name="IR2" value="2.7A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744870100 "/>
<attribute name="RDC1-MAX" value="0.044Ohm"/>
<attribute name="RDC1-TYP" value="0.038Ohm"/>
<attribute name="RDC2-MAX" value="0.044Ohm"/>
<attribute name="RDC2-TYP" value="0.038Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744870101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870101.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="IR2" value="1.4A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744870101 "/>
<attribute name="RDC1-MAX" value="0.3Ohm"/>
<attribute name="RDC1-TYP" value="0.23Ohm"/>
<attribute name="RDC2-MAX" value="0.3Ohm"/>
<attribute name="RDC2-TYP" value="0.23Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744870151">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870151.pdf"/>
<attribute name="FRE" value="2.3MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L2" value="150uH"/>
<attribute name="PART-NUMBER" value=" 744870151 "/>
<attribute name="RDC1-MAX" value="0.4Ohm"/>
<attribute name="RDC1-TYP" value="0.34Ohm"/>
<attribute name="RDC2-MAX" value="0.4Ohm"/>
<attribute name="RDC2-TYP" value="0.34Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744870220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870220.pdf"/>
<attribute name="FRE" value="10MHz"/>
<attribute name="IR1" value="2.45A"/>
<attribute name="IR2" value="2.45A"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744870220 "/>
<attribute name="RDC1-MAX" value="0.08Ohm"/>
<attribute name="RDC1-TYP" value="0.062Ohm"/>
<attribute name="RDC2-MAX" value="0.08Ohm"/>
<attribute name="RDC2-TYP" value="0.062Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744870221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870221.pdf"/>
<attribute name="FRE" value="2MHz"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="IR2" value="0.9A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L2" value="220uH"/>
<attribute name="PART-NUMBER" value=" 744870221 "/>
<attribute name="RDC1-MAX" value="0.65Ohm"/>
<attribute name="RDC1-TYP" value="0.53Ohm"/>
<attribute name="RDC2-MAX" value="0.65Ohm"/>
<attribute name="RDC2-TYP" value="0.53Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744870470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870470.pdf"/>
<attribute name="FRE" value="5MHz"/>
<attribute name="IR1" value="1.45A"/>
<attribute name="IR2" value="1.45A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 744870470 "/>
<attribute name="RDC1-MAX" value="0.15Ohm"/>
<attribute name="RDC1-TYP" value="0.125Ohm"/>
<attribute name="RDC2-MAX" value="0.15Ohm"/>
<attribute name="RDC2-TYP" value="0.125Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744870471">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870471.pdf"/>
<attribute name="FRE" value="0.65MHz"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.7A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L2" value="470uH"/>
<attribute name="PART-NUMBER" value=" 744870471 "/>
<attribute name="RDC1-MAX" value="1.2Ohm"/>
<attribute name="RDC1-TYP" value="1Ohm"/>
<attribute name="RDC2-MAX" value="1.2Ohm"/>
<attribute name="RDC2-TYP" value="1Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_744870680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744870680.pdf"/>
<attribute name="FRE" value="3.7MHz"/>
<attribute name="IR1" value="1.35A"/>
<attribute name="IR2" value="1.35A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L2" value="68uH"/>
<attribute name="PART-NUMBER" value=" 744870680 "/>
<attribute name="RDC1-MAX" value="0.215Ohm"/>
<attribute name="RDC1-TYP" value="0.17Ohm"/>
<attribute name="RDC2-MAX" value="0.215Ohm"/>
<attribute name="RDC2-TYP" value="0.17Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_7332" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744878001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878001.pdf"/>
<attribute name="FRE" value="60MHz"/>
<attribute name="IR1" value="4.4A"/>
<attribute name="IR2" value="4.4A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="L2" value="1.3uH"/>
<attribute name="PART-NUMBER" value=" 744878001 "/>
<attribute name="RDC1-MAX" value="0.035Ohm"/>
<attribute name="RDC1-TYP" value="0.027Ohm"/>
<attribute name="RDC2-MAX" value="0.035Ohm"/>
<attribute name="RDC2-TYP" value="0.027Ohm"/>
<attribute name="VALUE" value="1.3uH"/>
</technology>
<technology name="_744878002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878002.pdf"/>
<attribute name="FRE" value="53MHz"/>
<attribute name="IR1" value="3.6A"/>
<attribute name="IR2" value="3.6A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="L2" value="2.4uH"/>
<attribute name="PART-NUMBER" value=" 744878002 "/>
<attribute name="RDC1-MAX" value="0.052Ohm"/>
<attribute name="RDC1-TYP" value="0.042Ohm"/>
<attribute name="RDC2-MAX" value="0.052Ohm"/>
<attribute name="RDC2-TYP" value="0.042Ohm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744878003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878003.pdf"/>
<attribute name="FRE" value="49MHz"/>
<attribute name="IR1" value="3.3A"/>
<attribute name="IR2" value="3.3A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 744878003 "/>
<attribute name="RDC1-MAX" value="0.064Ohm"/>
<attribute name="RDC1-TYP" value="0.052Ohm"/>
<attribute name="RDC2-MAX" value="0.064Ohm"/>
<attribute name="RDC2-TYP" value="0.052Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744878004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878004.pdf"/>
<attribute name="FRE" value="46MHz"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744878004 "/>
<attribute name="RDC1-MAX" value="0.075Ohm"/>
<attribute name="RDC1-TYP" value="0.065Ohm"/>
<attribute name="RDC2-MAX" value="0.075Ohm"/>
<attribute name="RDC2-TYP" value="0.065Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744878005">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878005.pdf"/>
<attribute name="FRE" value="26MHz"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="IR2" value="1.5A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L2" value="5.6uH"/>
<attribute name="PART-NUMBER" value=" 744878005 "/>
<attribute name="RDC1-MAX" value="0.12Ohm"/>
<attribute name="RDC1-TYP" value="0.095Ohm"/>
<attribute name="RDC2-MAX" value="0.12Ohm"/>
<attribute name="RDC2-TYP" value="0.095Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744878006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878006.pdf"/>
<attribute name="FRE" value="25MHz"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="IR2" value="1.4A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 744878006 "/>
<attribute name="RDC1-MAX" value="0.135Ohm"/>
<attribute name="RDC1-TYP" value="0.11Ohm"/>
<attribute name="RDC2-MAX" value="0.135Ohm"/>
<attribute name="RDC2-TYP" value="0.11Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744878008">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878008.pdf"/>
<attribute name="FRE" value="22MHz"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="PART-NUMBER" value=" 744878008 "/>
<attribute name="RDC1-MAX" value="0.14Ohm"/>
<attribute name="RDC1-TYP" value="0.115Ohm"/>
<attribute name="RDC2-MAX" value="0.14Ohm"/>
<attribute name="RDC2-TYP" value="0.115Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744878100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878100.pdf"/>
<attribute name="FRE" value="30MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744878100 "/>
<attribute name="RDC1-MAX" value="0.15Ohm"/>
<attribute name="RDC1-TYP" value="0.125Ohm"/>
<attribute name="RDC2-MAX" value="0.15Ohm"/>
<attribute name="RDC2-TYP" value="0.125Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744878101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878101.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR1" value="0.3A"/>
<attribute name="IR2" value="0.3A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744878101 "/>
<attribute name="RDC1-MAX" value="1.73Ohm"/>
<attribute name="RDC1-TYP" value="1.4Ohm"/>
<attribute name="RDC2-MAX" value="1.73Ohm"/>
<attribute name="RDC2-TYP" value="1.4Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744878220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878220.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.7A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744878220 "/>
<attribute name="RDC1-MAX" value="0.3Ohm"/>
<attribute name="RDC1-TYP" value="0.245Ohm"/>
<attribute name="RDC2-MAX" value="0.3Ohm"/>
<attribute name="RDC2-TYP" value="0.245Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744878470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744878470.pdf"/>
<attribute name="FRE" value="8MHz"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="IR2" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 744878470 "/>
<attribute name="RDC1-MAX" value="0.75Ohm"/>
<attribute name="RDC1-TYP" value="0.6Ohm"/>
<attribute name="RDC2-MAX" value="0.75Ohm"/>
<attribute name="RDC2-TYP" value="0.6Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1260" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_1260">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744874001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874001.pdf"/>
<attribute name="FRE" value="70MHz"/>
<attribute name="IR1" value="5.85A"/>
<attribute name="IR2" value="5.85A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="L2" value="1.5uH"/>
<attribute name="PART-NUMBER" value=" 744874001 "/>
<attribute name="RDC1-MAX" value="0.016Ohm"/>
<attribute name="RDC1-TYP" value="0.012Ohm"/>
<attribute name="RDC2-MAX" value="0.016Ohm"/>
<attribute name="RDC2-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744874002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874002.pdf"/>
<attribute name="FRE" value="54MHz"/>
<attribute name="IR1" value="5.5A"/>
<attribute name="IR2" value="5.5A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="L2" value="2.4uH"/>
<attribute name="PART-NUMBER" value=" 744874002 "/>
<attribute name="RDC1-MAX" value="0.017Ohm"/>
<attribute name="RDC1-TYP" value="0.013Ohm"/>
<attribute name="RDC2-MAX" value="0.017Ohm"/>
<attribute name="RDC2-TYP" value="0.013Ohm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744874003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874003.pdf"/>
<attribute name="FRE" value="45MHz"/>
<attribute name="IR1" value="4.91A"/>
<attribute name="IR2" value="4.91A"/>
<attribute name="ISAT" value="8.9A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 744874003 "/>
<attribute name="RDC1-MAX" value="0.021Ohm"/>
<attribute name="RDC1-TYP" value="0.017Ohm"/>
<attribute name="RDC2-MAX" value="0.021Ohm"/>
<attribute name="RDC2-TYP" value="0.017Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744874004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874004.pdf"/>
<attribute name="FRE" value="39MHz"/>
<attribute name="IR1" value="4.22A"/>
<attribute name="IR2" value="4.22A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744874004 "/>
<attribute name="RDC1-MAX" value="0.028Ohm"/>
<attribute name="RDC1-TYP" value="0.023Ohm"/>
<attribute name="RDC2-MAX" value="0.028Ohm"/>
<attribute name="RDC2-TYP" value="0.023Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744874006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874006.pdf"/>
<attribute name="FRE" value="33MHz"/>
<attribute name="IR1" value="3.9A"/>
<attribute name="IR2" value="3.9A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 744874006 "/>
<attribute name="RDC1-MAX" value="0.032Ohm"/>
<attribute name="RDC1-TYP" value="0.027Ohm"/>
<attribute name="RDC2-MAX" value="0.032Ohm"/>
<attribute name="RDC2-TYP" value="0.027Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744874100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874100.pdf"/>
<attribute name="FRE" value="24MHz"/>
<attribute name="IR1" value="3.28A"/>
<attribute name="IR2" value="3.28A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744874100 "/>
<attribute name="RDC1-MAX" value="0.044Ohm"/>
<attribute name="RDC1-TYP" value="0.038Ohm"/>
<attribute name="RDC2-MAX" value="0.044Ohm"/>
<attribute name="RDC2-TYP" value="0.038Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744874101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874101.pdf"/>
<attribute name="FRE" value="6MHz"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="IR2" value="1.2A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744874101 "/>
<attribute name="RDC1-MAX" value="0.32Ohm"/>
<attribute name="RDC1-TYP" value="0.285Ohm"/>
<attribute name="RDC2-MAX" value="0.32Ohm"/>
<attribute name="RDC2-TYP" value="0.285Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744874220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874220.pdf"/>
<attribute name="FRE" value="15.5MHz"/>
<attribute name="IR1" value="2.47A"/>
<attribute name="IR2" value="2.47A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744874220 "/>
<attribute name="RDC1-MAX" value="0.08Ohm"/>
<attribute name="RDC1-TYP" value="0.067Ohm"/>
<attribute name="RDC2-MAX" value="0.08Ohm"/>
<attribute name="RDC2-TYP" value="0.067Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744874470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744874470.pdf"/>
<attribute name="FRE" value="11MHz"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="IR2" value="1.8A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 744874470 "/>
<attribute name="RDC1-MAX" value="0.15Ohm"/>
<attribute name="RDC1-TYP" value="0.13Ohm"/>
<attribute name="RDC2-MAX" value="0.15Ohm"/>
<attribute name="RDC2-TYP" value="0.13Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_7345" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744877001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877001.pdf"/>
<attribute name="FRE" value="58MHz"/>
<attribute name="IR1" value="4.7A"/>
<attribute name="IR2" value="4.7A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="L2" value="1.8uH"/>
<attribute name="PART-NUMBER" value=" 744877001 "/>
<attribute name="RDC1-MAX" value="0.034Ohm"/>
<attribute name="RDC1-TYP" value="0.025Ohm"/>
<attribute name="RDC2-MAX" value="0.034Ohm"/>
<attribute name="RDC2-TYP" value="0.025Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744877002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877002.pdf"/>
<attribute name="FRE" value="50MHz"/>
<attribute name="IR1" value="4.2A"/>
<attribute name="IR2" value="4.2A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="L2" value="2.4uH"/>
<attribute name="PART-NUMBER" value=" 744877002 "/>
<attribute name="RDC1-MAX" value="0.042Ohm"/>
<attribute name="RDC1-TYP" value="0.031Ohm"/>
<attribute name="RDC2-MAX" value="0.042Ohm"/>
<attribute name="RDC2-TYP" value="0.031Ohm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744877003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877003.pdf"/>
<attribute name="FRE" value="46MHz"/>
<attribute name="IR1" value="3.7A"/>
<attribute name="IR2" value="3.7A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 744877003 "/>
<attribute name="RDC1-MAX" value="0.052Ohm"/>
<attribute name="RDC1-TYP" value="0.04Ohm"/>
<attribute name="RDC2-MAX" value="0.052Ohm"/>
<attribute name="RDC2-TYP" value="0.04Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744877004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877004.pdf"/>
<attribute name="FRE" value="42MHz"/>
<attribute name="IR1" value="2.55A"/>
<attribute name="IR2" value="2.55A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744877004 "/>
<attribute name="RDC1-MAX" value="0.064Ohm"/>
<attribute name="RDC1-TYP" value="0.052Ohm"/>
<attribute name="RDC2-MAX" value="0.064Ohm"/>
<attribute name="RDC2-TYP" value="0.052Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744877005">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877005.pdf"/>
<attribute name="FRE" value="23MHz"/>
<attribute name="IR1" value="1.9A"/>
<attribute name="IR2" value="1.9A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="L2" value="5.6uH"/>
<attribute name="PART-NUMBER" value=" 744877005 "/>
<attribute name="RDC1-MAX" value="0.095Ohm"/>
<attribute name="RDC1-TYP" value="0.08Ohm"/>
<attribute name="RDC2-MAX" value="0.095Ohm"/>
<attribute name="RDC2-TYP" value="0.08Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744877006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877006.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="IR2" value="1.8A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 744877006 "/>
<attribute name="RDC1-MAX" value="0.102Ohm"/>
<attribute name="RDC1-TYP" value="0.085Ohm"/>
<attribute name="RDC2-MAX" value="0.102Ohm"/>
<attribute name="RDC2-TYP" value="0.085Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744877008">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877008.pdf"/>
<attribute name="FRE" value="17MHz"/>
<attribute name="IR1" value="1.7A"/>
<attribute name="IR2" value="1.7A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="PART-NUMBER" value=" 744877008 "/>
<attribute name="RDC1-MAX" value="0.11Ohm"/>
<attribute name="RDC1-TYP" value="0.091Ohm"/>
<attribute name="RDC2-MAX" value="0.11Ohm"/>
<attribute name="RDC2-TYP" value="0.091Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744877100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877100.pdf"/>
<attribute name="FRE" value="27MHz"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="IR2" value="1.1A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744877100 "/>
<attribute name="RDC1-MAX" value="0.12Ohm"/>
<attribute name="RDC1-TYP" value="0.11Ohm"/>
<attribute name="RDC2-MAX" value="0.12Ohm"/>
<attribute name="RDC2-TYP" value="0.11Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744877101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877101.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR1" value="0.65A"/>
<attribute name="IR2" value="0.65A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744877101 "/>
<attribute name="RDC1-MAX" value="1.3Ohm"/>
<attribute name="RDC1-TYP" value="1.029Ohm"/>
<attribute name="RDC2-MAX" value="1.3Ohm"/>
<attribute name="RDC2-TYP" value="1.029Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744877220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877220.pdf"/>
<attribute name="FRE" value="16MHz"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="IR2" value="0.8A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744877220 "/>
<attribute name="RDC1-MAX" value="0.26Ohm"/>
<attribute name="RDC1-TYP" value="0.215Ohm"/>
<attribute name="RDC2-MAX" value="0.26Ohm"/>
<attribute name="RDC2-TYP" value="0.215Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744877330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744877330.pdf"/>
<attribute name="FRE" value="8MHz"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.7A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="33uH"/>
<attribute name="PART-NUMBER" value=" 744877330 "/>
<attribute name="RDC1-MAX" value="0.5Ohm"/>
<attribute name="RDC1-TYP" value="0.4Ohm"/>
<attribute name="RDC2-MAX" value="0.5Ohm"/>
<attribute name="RDC2-TYP" value="0.4Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1260_CROSSED" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_1260_CROSSED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744871004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871004.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="3A"/>
<attribute name="IR2" value="3A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744871004 "/>
<attribute name="RDC1-MAX" value="0.028Ohm"/>
<attribute name="RDC1-TYP" value="0.023Ohm"/>
<attribute name="RDC2-MAX" value="0.028Ohm"/>
<attribute name="RDC2-TYP" value="0.023Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744871006">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871006.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="2.8A"/>
<attribute name="IR2" value="2.8A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 744871006 "/>
<attribute name="RDC1-MAX" value="0.04Ohm"/>
<attribute name="RDC1-TYP" value="0.035Ohm"/>
<attribute name="RDC2-MAX" value="0.04Ohm"/>
<attribute name="RDC2-TYP" value="0.035Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744871100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871100.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="2A"/>
<attribute name="IR2" value="2A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744871100 "/>
<attribute name="RDC1-MAX" value="0.05Ohm"/>
<attribute name="RDC1-TYP" value="0.044Ohm"/>
<attribute name="RDC2-MAX" value="0.05Ohm"/>
<attribute name="RDC2-TYP" value="0.044Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744871101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871101.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="IR2" value="1.5A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744871101 "/>
<attribute name="RDC1-MAX" value="0.36Ohm"/>
<attribute name="RDC1-TYP" value="0.293Ohm"/>
<attribute name="RDC2-MAX" value="0.36Ohm"/>
<attribute name="RDC2-TYP" value="0.293Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744871220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871220.pdf"/>
<attribute name="FRE" value="14MHz"/>
<attribute name="IR1" value="1.85A"/>
<attribute name="IR2" value="1.85A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744871220 "/>
<attribute name="RDC1-MAX" value="0.09Ohm"/>
<attribute name="RDC1-TYP" value="0.067Ohm"/>
<attribute name="RDC2-MAX" value="0.09Ohm"/>
<attribute name="RDC2-TYP" value="0.067Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744871330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871330.pdf"/>
<attribute name="FRE" value="6MHz"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="IR2" value="1.2A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="L2" value="33uH"/>
<attribute name="PART-NUMBER" value=" 744871330 "/>
<attribute name="RDC1-MAX" value="0.17Ohm"/>
<attribute name="RDC1-TYP" value="0.125Ohm"/>
<attribute name="RDC2-MAX" value="0.17Ohm"/>
<attribute name="RDC2-TYP" value="0.125Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744871470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744871470.pdf"/>
<attribute name="FRE" value="5MHz"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="IR2" value="1.1A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 744871470 "/>
<attribute name="RDC1-MAX" value="0.18Ohm"/>
<attribute name="RDC1-TYP" value="0.145Ohm"/>
<attribute name="RDC2-MAX" value="0.18Ohm"/>
<attribute name="RDC2-TYP" value="0.145Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1280" prefix="L">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14775v209%20Family_WE-DD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DD"&gt;https://katalog.we-online.com/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DD"/>
</gates>
<devices>
<device name="" package="WE-DD_1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744873001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873001.pdf"/>
<attribute name="FRE" value="75MHz"/>
<attribute name="IR1" value="6.25A"/>
<attribute name="IR2" value="6.25A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="L2" value="1.5uH"/>
<attribute name="PART-NUMBER" value=" 744873001 "/>
<attribute name="RDC1-MAX" value="0.015Ohm"/>
<attribute name="RDC1-TYP" value="0.011Ohm"/>
<attribute name="RDC2-MAX" value="0.015Ohm"/>
<attribute name="RDC2-TYP" value="0.011Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744873002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873002.pdf"/>
<attribute name="FRE" value="54MHz"/>
<attribute name="IR1" value="6A"/>
<attribute name="IR2" value="6A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="L2" value="2.4uH"/>
<attribute name="PART-NUMBER" value=" 744873002 "/>
<attribute name="RDC1-MAX" value="0.016Ohm"/>
<attribute name="RDC1-TYP" value="0.012Ohm"/>
<attribute name="RDC2-MAX" value="0.016Ohm"/>
<attribute name="RDC2-TYP" value="0.012Ohm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744873003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873003.pdf"/>
<attribute name="FRE" value="41MHz"/>
<attribute name="IR1" value="5.14A"/>
<attribute name="IR2" value="5.14A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="PART-NUMBER" value=" 744873003 "/>
<attribute name="RDC1-MAX" value="0.022Ohm"/>
<attribute name="RDC1-TYP" value="0.017Ohm"/>
<attribute name="RDC2-MAX" value="0.022Ohm"/>
<attribute name="RDC2-TYP" value="0.017Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744873004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873004.pdf"/>
<attribute name="FRE" value="32MHz"/>
<attribute name="IR1" value="4.87A"/>
<attribute name="IR2" value="4.87A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 744873004 "/>
<attribute name="RDC1-MAX" value="0.024Ohm"/>
<attribute name="RDC1-TYP" value="0.019Ohm"/>
<attribute name="RDC2-MAX" value="0.024Ohm"/>
<attribute name="RDC2-TYP" value="0.019Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744873100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873100.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="4.2A"/>
<attribute name="IR2" value="4.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 744873100 "/>
<attribute name="RDC1-MAX" value="0.042Ohm"/>
<attribute name="RDC1-TYP" value="0.031Ohm"/>
<attribute name="RDC2-MAX" value="0.042Ohm"/>
<attribute name="RDC2-TYP" value="0.031Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744873101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873101.pdf"/>
<attribute name="FRE" value="4.4MHz"/>
<attribute name="IR1" value="1.38A"/>
<attribute name="IR2" value="1.38A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L2" value="100uH"/>
<attribute name="PART-NUMBER" value=" 744873101 "/>
<attribute name="RDC1-MAX" value="0.255Ohm"/>
<attribute name="RDC1-TYP" value="0.235Ohm"/>
<attribute name="RDC2-MAX" value="0.255Ohm"/>
<attribute name="RDC2-TYP" value="0.235Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744873150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873150.pdf"/>
<attribute name="FRE" value="14MHz"/>
<attribute name="IR1" value="3.3A"/>
<attribute name="IR2" value="3.3A"/>
<attribute name="ISAT" value="6.1A"/>
<attribute name="L2" value="15uH"/>
<attribute name="PART-NUMBER" value=" 744873150 "/>
<attribute name="RDC1-MAX" value="0.055Ohm"/>
<attribute name="RDC1-TYP" value="0.041Ohm"/>
<attribute name="RDC2-MAX" value="0.055Ohm"/>
<attribute name="RDC2-TYP" value="0.041Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744873220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873220.pdf"/>
<attribute name="FRE" value="11.5MHz"/>
<attribute name="IR1" value="2.79A"/>
<attribute name="IR2" value="2.79A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 744873220 "/>
<attribute name="RDC1-MAX" value="0.07Ohm"/>
<attribute name="RDC1-TYP" value="0.058Ohm"/>
<attribute name="RDC2-MAX" value="0.07Ohm"/>
<attribute name="RDC2-TYP" value="0.058Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744873221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873221.pdf"/>
<attribute name="FRE" value="2.8MHz"/>
<attribute name="IR1" value="0.91A"/>
<attribute name="IR2" value="0.91A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L2" value="220uH"/>
<attribute name="PART-NUMBER" value=" 744873221 "/>
<attribute name="RDC1-MAX" value="0.58Ohm"/>
<attribute name="RDC1-TYP" value="0.54Ohm"/>
<attribute name="RDC2-MAX" value="0.58Ohm"/>
<attribute name="RDC2-TYP" value="0.54Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744873330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873330.pdf"/>
<attribute name="FRE" value="8.9MHz"/>
<attribute name="IR1" value="2.25A"/>
<attribute name="IR2" value="2.25A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="L2" value="33uH"/>
<attribute name="PART-NUMBER" value=" 744873330 "/>
<attribute name="RDC1-MAX" value="0.105Ohm"/>
<attribute name="RDC1-TYP" value="0.087Ohm"/>
<attribute name="RDC2-MAX" value="0.105Ohm"/>
<attribute name="RDC2-TYP" value="0.087Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744873470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873470.pdf"/>
<attribute name="FRE" value="7.8MHz"/>
<attribute name="IR1" value="2.02A"/>
<attribute name="IR2" value="2.02A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="L2" value="47uH"/>
<attribute name="PART-NUMBER" value=" 744873470 "/>
<attribute name="RDC1-MAX" value="0.12Ohm"/>
<attribute name="RDC1-TYP" value="0.11Ohm"/>
<attribute name="RDC2-MAX" value="0.12Ohm"/>
<attribute name="RDC2-TYP" value="0.11Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744873680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744873680.pdf"/>
<attribute name="FRE" value="5.5MHz"/>
<attribute name="IR1" value="1.66A"/>
<attribute name="IR2" value="1.66A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="L2" value="68uH"/>
<attribute name="PART-NUMBER" value=" 744873680 "/>
<attribute name="RDC1-MAX" value="0.18Ohm"/>
<attribute name="RDC1-TYP" value="0.163Ohm"/>
<attribute name="RDC2-MAX" value="0.18Ohm"/>
<attribute name="RDC2-TYP" value="0.163Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
