<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-DPC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-DPC_4818">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DPC SMD Dual Powerchoke&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4818</description>
</package>
<package name="WE-DPC_4828">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DPC SMD Dual Powerchoke&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4828</description>
</package>
<package name="WE-DPC_5838">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DPC SMD Dual Powerchoke&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5838</description>
</package>
</packages>
<symbols>
<symbol name="WE-DPC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-DPC_4828" prefix="L">
<description>&lt;b&gt; WE-DPC SMD Dual Powerchoke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Characteristics Tiny package: our smalles double choke
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;More variants due to parallel and series connection
&lt;br&gt;Operating temperature: -40 °C to +125 °C

&lt;br&gt; 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Applications Flyback applications
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulators with secondary unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DPC"&gt;https://katalog.we-online.com/en/pbs/WE-DPC&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC"/>
</gates>
<devices>
<device name="" package="WE-DPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448843010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843010.pdf"/>
<attribute name="FRE" value="65MHz"/>
<attribute name="IR1" value="2.95A"/>
<attribute name="IR2" value="2.95A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843010 "/>
<attribute name="RDC1-MAX" value="36mOhm"/>
<attribute name="RDC1-TYP" value="30mOhm"/>
<attribute name="RDC2-MAX" value="36mOhm"/>
<attribute name="RDC2-TYP" value="30mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448843022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843022.pdf"/>
<attribute name="FRE" value="50MHz"/>
<attribute name="IR1" value="2.25A"/>
<attribute name="IR2" value="2.25A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843022 "/>
<attribute name="RDC1-MAX" value="53mOhm"/>
<attribute name="RDC1-TYP" value="45mOhm"/>
<attribute name="RDC2-MAX" value="53mOhm"/>
<attribute name="RDC2-TYP" value="45mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448843033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843033.pdf"/>
<attribute name="FRE" value="45MHz"/>
<attribute name="IR1" value="1.95A"/>
<attribute name="IR2" value="1.95A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843033 "/>
<attribute name="RDC1-MAX" value="80mOhm"/>
<attribute name="RDC1-TYP" value="67mOhm"/>
<attribute name="RDC2-MAX" value="80mOhm"/>
<attribute name="RDC2-TYP" value="67mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448843047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843047.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="IR2" value="1.8A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843047 "/>
<attribute name="RDC1-MAX" value="100mOhm"/>
<attribute name="RDC1-TYP" value="84mOhm"/>
<attribute name="RDC2-MAX" value="100mOhm"/>
<attribute name="RDC2-TYP" value="84mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448843068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843068.pdf"/>
<attribute name="FRE" value="32MHz"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="IR2" value="1.5A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843068 "/>
<attribute name="RDC1-MAX" value="137mOhm"/>
<attribute name="RDC1-TYP" value="115mOhm"/>
<attribute name="RDC2-MAX" value="137mOhm"/>
<attribute name="RDC2-TYP" value="115mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448843082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843082.pdf"/>
<attribute name="FRE" value="27MHz"/>
<attribute name="IR1" value="1.15A"/>
<attribute name="IR2" value="1.15A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843082 "/>
<attribute name="RDC1-MAX" value="216mOhm"/>
<attribute name="RDC1-TYP" value="180mOhm"/>
<attribute name="RDC2-MAX" value="216mOhm"/>
<attribute name="RDC2-TYP" value="180mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7448843100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843100.pdf"/>
<attribute name="FRE" value="24MHz"/>
<attribute name="IR1" value="1.08A"/>
<attribute name="IR2" value="1.08A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843100 "/>
<attribute name="RDC1-MAX" value="248mOhm"/>
<attribute name="RDC1-TYP" value="205mOhm"/>
<attribute name="RDC2-MAX" value="248mOhm"/>
<attribute name="RDC2-TYP" value="205mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448843150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843150.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L2" value="15uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843150 "/>
<attribute name="RDC1-MAX" value="321mOhm"/>
<attribute name="RDC1-TYP" value="265mOhm"/>
<attribute name="RDC2-MAX" value="321mOhm"/>
<attribute name="RDC2-TYP" value="265mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7448843220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843220.pdf"/>
<attribute name="FRE" value="16MHz"/>
<attribute name="IR1" value="0.78A"/>
<attribute name="IR2" value="0.78A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="22uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843220 "/>
<attribute name="RDC1-MAX" value="455mOhm"/>
<attribute name="RDC1-TYP" value="382mOhm"/>
<attribute name="RDC2-MAX" value="455mOhm"/>
<attribute name="RDC2-TYP" value="382mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448843330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843330.pdf"/>
<attribute name="FRE" value="12MHz"/>
<attribute name="IR1" value="0.65A"/>
<attribute name="IR2" value="0.65A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L2" value="33uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843330 "/>
<attribute name="RDC1-MAX" value="667mOhm"/>
<attribute name="RDC1-TYP" value="560mOhm"/>
<attribute name="RDC2-MAX" value="667mOhm"/>
<attribute name="RDC2-TYP" value="560mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448843470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843470.pdf"/>
<attribute name="FRE" value="10MHz"/>
<attribute name="IR1" value="0.54A"/>
<attribute name="IR2" value="0.54A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L2" value="47uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843470 "/>
<attribute name="RDC1-MAX" value="959mOhm"/>
<attribute name="RDC1-TYP" value="800mOhm"/>
<attribute name="RDC2-MAX" value="959mOhm"/>
<attribute name="RDC2-TYP" value="800mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7448843680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448843680.pdf"/>
<attribute name="FRE" value="9MHz"/>
<attribute name="IR1" value="0.45A"/>
<attribute name="IR2" value="0.45A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="L2" value="68uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448843680 "/>
<attribute name="RDC1-MAX" value="1400mOhm"/>
<attribute name="RDC1-TYP" value="1160mOhm"/>
<attribute name="RDC2-MAX" value="1400mOhm"/>
<attribute name="RDC2-TYP" value="1160mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DPC_4818" prefix="L">
<description>&lt;b&gt; WE-DPC SMD Dual Powerchoke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Characteristics Tiny package: our smalles double choke
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;More variants due to parallel and series connection
&lt;br&gt;Operating temperature: -40 °C to +125 °C

&lt;br&gt; 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Applications Flyback applications
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulators with secondary unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DPC"&gt;https://katalog.we-online.com/en/pbs/WE-DPC&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC"/>
</gates>
<devices>
<device name="" package="WE-DPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448842010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842010.pdf"/>
<attribute name="FRE" value="80MHz"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="IR2" value="1.8A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842010 "/>
<attribute name="RDC1-MAX" value="90mOhm"/>
<attribute name="RDC1-TYP" value="75mOhm"/>
<attribute name="RDC2-MAX" value="90mOhm"/>
<attribute name="RDC2-TYP" value="75mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448842022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842022.pdf"/>
<attribute name="FRE" value="65MHz"/>
<attribute name="IR1" value="1.68A"/>
<attribute name="IR2" value="1.68A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842022 "/>
<attribute name="RDC1-MAX" value="163mOhm"/>
<attribute name="RDC1-TYP" value="135mOhm"/>
<attribute name="RDC2-MAX" value="163mOhm"/>
<attribute name="RDC2-TYP" value="135mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448842033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842033.pdf"/>
<attribute name="FRE" value="55MHz"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842033 "/>
<attribute name="RDC1-MAX" value="205mOhm"/>
<attribute name="RDC1-TYP" value="170mOhm"/>
<attribute name="RDC2-MAX" value="205mOhm"/>
<attribute name="RDC2-TYP" value="170mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448842047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842047.pdf"/>
<attribute name="FRE" value="47MHz"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="IR2" value="1.1A"/>
<attribute name="ISAT" value="2.25A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842047 "/>
<attribute name="RDC1-MAX" value="253.5mOhm"/>
<attribute name="RDC1-TYP" value="210mOhm"/>
<attribute name="RDC2-MAX" value="253.5mOhm"/>
<attribute name="RDC2-TYP" value="210mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448842068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842068.pdf"/>
<attribute name="FRE" value="41MHz"/>
<attribute name="IR1" value="1.05A"/>
<attribute name="IR2" value="1.05A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842068 "/>
<attribute name="RDC1-MAX" value="462.5mOhm"/>
<attribute name="RDC1-TYP" value="390mOhm"/>
<attribute name="RDC2-MAX" value="462.5mOhm"/>
<attribute name="RDC2-TYP" value="390mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448842082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842082.pdf"/>
<attribute name="FRE" value="38MHz"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="IR2" value="0.9A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842082 "/>
<attribute name="RDC1-MAX" value="494.5mOhm"/>
<attribute name="RDC1-TYP" value="415mOhm"/>
<attribute name="RDC2-MAX" value="494.5mOhm"/>
<attribute name="RDC2-TYP" value="415mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7448842100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448842100.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="IR2" value="0.8A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448842100 "/>
<attribute name="RDC1-MAX" value="562mOhm"/>
<attribute name="RDC1-TYP" value="475mOhm"/>
<attribute name="RDC2-MAX" value="562mOhm"/>
<attribute name="RDC2-TYP" value="475mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DPC_5838" prefix="L">
<description>&lt;b&gt; WE-DPC SMD Dual Powerchoke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Characteristics Tiny package: our smalles double choke
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;More variants due to parallel and series connection
&lt;br&gt;Operating temperature: -40 °C to +125 °C

&lt;br&gt; 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Applications Flyback applications
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulators with secondary unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o35281v209%20Family_WE-DPC_5838_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DPC"&gt;https://katalog.we-online.com/en/pbs/WE-DPC&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by Yingchun,Shan 2019-08-14&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC"/>
</gates>
<devices>
<device name="" package="WE-DPC_5838">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448844010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844010.pdf"/>
<attribute name="FRE" value="150MHz"/>
<attribute name="IR1" value="4.5A"/>
<attribute name="IR2" value="4.5A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844010 "/>
<attribute name="RDC1-MAX" value="35mOhm"/>
<attribute name="RDC1-TYP" value="25mOhm"/>
<attribute name="RDC2-MAX" value="35mOhm"/>
<attribute name="RDC2-TYP" value="25mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448844022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844022.pdf"/>
<attribute name="FRE" value="80MHz"/>
<attribute name="IR1" value="3.9A"/>
<attribute name="IR2" value="3.9A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844022 "/>
<attribute name="RDC1-MAX" value="47mOhm"/>
<attribute name="RDC1-TYP" value="33mOhm"/>
<attribute name="RDC2-MAX" value="47mOhm"/>
<attribute name="RDC2-TYP" value="33mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448844033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844033.pdf"/>
<attribute name="FRE" value="56MHz"/>
<attribute name="IR1" value="3.5A"/>
<attribute name="IR2" value="3.5A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844033 "/>
<attribute name="RDC1-MAX" value="57mOhm"/>
<attribute name="RDC1-TYP" value="40mOhm"/>
<attribute name="RDC2-MAX" value="57mOhm"/>
<attribute name="RDC2-TYP" value="40mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448844047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844047.pdf"/>
<attribute name="FRE" value="46MHz"/>
<attribute name="IR1" value="3.1A"/>
<attribute name="IR2" value="3.1A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844047 "/>
<attribute name="RDC1-MAX" value="62mOhm"/>
<attribute name="RDC1-TYP" value="44mOhm"/>
<attribute name="RDC2-MAX" value="62mOhm"/>
<attribute name="RDC2-TYP" value="44mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448844068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844068.pdf"/>
<attribute name="FRE" value="42MHz"/>
<attribute name="IR1" value="2.3A"/>
<attribute name="IR2" value="2.3A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844068 "/>
<attribute name="RDC1-MAX" value="85mOhm"/>
<attribute name="RDC1-TYP" value="60mOhm"/>
<attribute name="RDC2-MAX" value="85mOhm"/>
<attribute name="RDC2-TYP" value="60mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448844100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844100.pdf"/>
<attribute name="FRE" value="34MHz"/>
<attribute name="IR1" value="2A"/>
<attribute name="IR2" value="2A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844100 "/>
<attribute name="RDC1-MAX" value="100mOhm"/>
<attribute name="RDC1-TYP" value="70mOhm"/>
<attribute name="RDC2-MAX" value="100mOhm"/>
<attribute name="RDC2-TYP" value="70mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448844150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844150.pdf"/>
<attribute name="FRE" value="28MHz"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="IR2" value="1.8A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L2" value="15uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844150 "/>
<attribute name="RDC1-MAX" value="120mOhm"/>
<attribute name="RDC1-TYP" value="84mOhm"/>
<attribute name="RDC2-MAX" value="120mOhm"/>
<attribute name="RDC2-TYP" value="84mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7448844220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844220.pdf"/>
<attribute name="FRE" value="19MHz"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="IR2" value="1.2A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="L2" value="22uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844220 "/>
<attribute name="RDC1-MAX" value="220mOhm"/>
<attribute name="RDC1-TYP" value="154mOhm"/>
<attribute name="RDC2-MAX" value="220mOhm"/>
<attribute name="RDC2-TYP" value="154mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448844330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844330.pdf"/>
<attribute name="FRE" value="14MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L2" value="33uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844330 "/>
<attribute name="RDC1-MAX" value="240mOhm"/>
<attribute name="RDC1-TYP" value="168mOhm"/>
<attribute name="RDC2-MAX" value="240mOhm"/>
<attribute name="RDC2-TYP" value="168mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448844470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448844470.pdf"/>
<attribute name="FRE" value="12MHz"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="IR2" value="0.9A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L2" value="47uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448844470 "/>
<attribute name="RDC1-MAX" value="350mOhm"/>
<attribute name="RDC1-TYP" value="245mOhm"/>
<attribute name="RDC2-MAX" value="350mOhm"/>
<attribute name="RDC2-TYP" value="245mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
