<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-DPC HV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-DPCHV_5030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-DPC HV SMD Dual Powerchoke&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5030</description>
</package>
</packages>
<symbols>
<symbol name="WE-DPC_HV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-DPCHV_5030" prefix="L">
<description>&lt;b&gt;WE-DPC HV SMD Dual Powerchokel&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Our smallest double choke with 1.5kV isolation
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 Transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;Operation temperature: -40 °C to +125 °C

&lt;br&gt;


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;High density Isolated converter application (i.e Flyback converter) 
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Can be used as single inductor with series and parallel connection


&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97635v209%20Family_WE-DPC_HV_5030.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97635v209%20Family_WE-DPC_HV_5030.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-DPCHV"&gt;https://katalog.we-online.com/en/pbs/WE-DPCHV&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;updated by Yingchun Shan 2019-08-15 &lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC_HV"/>
</gates>
<devices>
<device name="" package="WE-DPCHV_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448441100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448441100.pdf"/>
<attribute name="FRE" value="MHz"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="IR2" value="1.2A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448441100 "/>
<attribute name="RDC1-MAX" value="300mOhm"/>
<attribute name="RDC1-TYP" value="210mOhm"/>
<attribute name="RDC2-MAX" value="300mOhm"/>
<attribute name="RDC2-TYP" value="210mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448841010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841010.pdf"/>
<attribute name="FRE" value="190MHz"/>
<attribute name="IR1" value="2.9A"/>
<attribute name="IR2" value="2.9A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841010 "/>
<attribute name="RDC1-MAX" value="45mOhm"/>
<attribute name="RDC1-TYP" value="32mOhm"/>
<attribute name="RDC2-MAX" value="45mOhm"/>
<attribute name="RDC2-TYP" value="32mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448841015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841015.pdf"/>
<attribute name="FRE" value="110MHz"/>
<attribute name="IR1" value="2.7A"/>
<attribute name="IR2" value="2.7A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="L2" value="1.5uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841015 "/>
<attribute name="RDC1-MAX" value="68mOhm"/>
<attribute name="RDC1-TYP" value="48mOhm"/>
<attribute name="RDC2-MAX" value="68mOhm"/>
<attribute name="RDC2-TYP" value="48mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7448841022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841022.pdf"/>
<attribute name="FRE" value="95MHz"/>
<attribute name="IR1" value="2.5A"/>
<attribute name="IR2" value="2.5A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841022 "/>
<attribute name="RDC1-MAX" value="72mOhm"/>
<attribute name="RDC1-TYP" value="50mOhm"/>
<attribute name="RDC2-MAX" value="72mOhm"/>
<attribute name="RDC2-TYP" value="50mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448841033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841033.pdf"/>
<attribute name="FRE" value="50MHz"/>
<attribute name="IR1" value="1.9A"/>
<attribute name="IR2" value="1.9A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841033 "/>
<attribute name="RDC1-MAX" value="120mOhm"/>
<attribute name="RDC1-TYP" value="84mOhm"/>
<attribute name="RDC2-MAX" value="120mOhm"/>
<attribute name="RDC2-TYP" value="84mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448841047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841047.pdf"/>
<attribute name="FRE" value="45MHz"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="IR2" value="1.6A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841047 "/>
<attribute name="RDC1-MAX" value="145mOhm"/>
<attribute name="RDC1-TYP" value="102mOhm"/>
<attribute name="RDC2-MAX" value="145mOhm"/>
<attribute name="RDC2-TYP" value="102mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448841068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841068.pdf"/>
<attribute name="FRE" value="42MHz"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="IR2" value="1.4A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841068 "/>
<attribute name="RDC1-MAX" value="240mOhm"/>
<attribute name="RDC1-TYP" value="168mOhm"/>
<attribute name="RDC2-MAX" value="240mOhm"/>
<attribute name="RDC2-TYP" value="168mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448841082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841082.pdf"/>
<attribute name="FRE" value="40MHz"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841082 "/>
<attribute name="RDC1-MAX" value="265mOhm"/>
<attribute name="RDC1-TYP" value="180mOhm"/>
<attribute name="RDC2-MAX" value="265mOhm"/>
<attribute name="RDC2-TYP" value="180mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7448841100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841100.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="IR2" value="1.2A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841100 "/>
<attribute name="RDC1-MAX" value="300mOhm"/>
<attribute name="RDC1-TYP" value="210mOhm"/>
<attribute name="RDC2-MAX" value="300mOhm"/>
<attribute name="RDC2-TYP" value="210mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448841150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841150.pdf"/>
<attribute name="FRE" value="24MHz"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="IR2" value="0.9A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L2" value="15uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841150 "/>
<attribute name="RDC1-MAX" value="465mOhm"/>
<attribute name="RDC1-TYP" value="325mOhm"/>
<attribute name="RDC2-MAX" value="465mOhm"/>
<attribute name="RDC2-TYP" value="325mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7448841220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841220.pdf"/>
<attribute name="FRE" value="21MHz"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="IR2" value="0.8A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="22uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841220 "/>
<attribute name="RDC1-MAX" value="650mOhm"/>
<attribute name="RDC1-TYP" value="455mOhm"/>
<attribute name="RDC2-MAX" value="650mOhm"/>
<attribute name="RDC2-TYP" value="455mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448841330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841330.pdf"/>
<attribute name="FRE" value="19MHz"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.7A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L2" value="33uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841330 "/>
<attribute name="RDC1-MAX" value="1025mOhm"/>
<attribute name="RDC1-TYP" value="718mOhm"/>
<attribute name="RDC2-MAX" value="1025mOhm"/>
<attribute name="RDC2-TYP" value="718mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448841470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7448841470.pdf"/>
<attribute name="FRE" value="18MHz"/>
<attribute name="IR1" value="0.6A"/>
<attribute name="IR2" value="0.6A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L2" value="47uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448841470 "/>
<attribute name="RDC1-MAX" value="1200mOhm"/>
<attribute name="RDC1-TYP" value="840mOhm"/>
<attribute name="RDC2-MAX" value="1200mOhm"/>
<attribute name="RDC2-TYP" value="840mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
