<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-FAMI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FAMI_1280_0.7WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280,0.7mm wire</description>
</package>
<package name="WE-FAMI_1280_0.6WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280,0.6mm wire</description>
</package>
<package name="WE-FAMI_1280_0.8WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280,0.8mm wire</description>
</package>
<package name="WE-FAMI_1415_0.9WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1415,0.9mm wire</description>
</package>
<package name="WE-FAMI_1012_0.7WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1012,0.7mm wire</description>
</package>
<package name="WE-FAMI_1415_1.2WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1415,1.2mm wire</description>
</package>
<package name="WE-FAMI_1012_0.8WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1012,0.8mm wire</description>
</package>
<package name="WE-FAMI_1280_0.55WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280,0.55 mm wire</description>
</package>
<package name="WE-FAMI_8010_0.5WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8010,0.5mm wire</description>
</package>
<package name="WE-FAMI_1280_0.65WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1280,0.65mm wire</description>
</package>
<package name="WE-FAMI_1410_1.1WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1410,1.1mm wire</description>
</package>
<package name="WE-FAMI_8010_0.65WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8010,0.65 mm wire</description>
</package>
<package name="WE-FAMI_1410_1.0WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1410,1.0mm wire</description>
</package>
<package name="WE-FAMI_8010_0.55WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8010,0.55mm wire</description>
</package>
<package name="WE-FAMI_1410_0.9WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1410,0.9mm wire</description>
</package>
<package name="WE-FAMI_1215_1.0WRIE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1215,1.0mm wire</description>
</package>
<package name="WE-FAMI_1215_0.9WIRE">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FAMI THT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1215,0.9 mm wire</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-FAMI_1012" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_0.8WIRE" package="WE-FAMI_1012_0.8WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750340047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750340047.pdf"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="14.4A"/>
<attribute name="PART-NUMBER" value="744750340047"/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="RDC-TYPE" value="6.6mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
<device name="_0.7WIRE" package="WE-FAMI_1012_0.7WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750340150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750340150.pdf"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="PART-NUMBER" value="744750340150"/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="RDC-TYPE" value="17.2mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI_1415" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_0.9WIRE" package="WE-FAMI_1415_0.9WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750560220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750560220.pdf"/>
<attribute name="IR" value="7.7A"/>
<attribute name="ISAT" value="8.9A"/>
<attribute name="PART-NUMBER" value="744750560220"/>
<attribute name="RDC-MAX" value="14.5mOhm"/>
<attribute name="RDC-TYPE" value="12.6mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
<device name="_1.2WIRE" package="WE-FAMI_1415_1.2WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750560047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750560047.pdf"/>
<attribute name="IR" value="14.5A"/>
<attribute name="ISAT" value="19.7A"/>
<attribute name="PART-NUMBER" value="744750560047"/>
<attribute name="RDC-MAX" value="3.8mOhm"/>
<attribute name="RDC-TYPE" value="3.1mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744750560100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750560100.pdf"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="13.4A"/>
<attribute name="PART-NUMBER" value="744750560100"/>
<attribute name="RDC-MAX" value="6.8mOhm"/>
<attribute name="RDC-TYPE" value="5.4mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI_1280" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_0.7WIRE" package="WE-FAMI_1280_0.7WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750420068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750420068.pdf"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="11.4A"/>
<attribute name="PART-NUMBER" value="744750420068"/>
<attribute name="RDC-MAX" value="12mOhm"/>
<attribute name="RDC-TYPE" value="9.4mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
<device name="_0.8WIRE" package="WE-FAMI_1280_0.8WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750420047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750420047.pdf"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="PART-NUMBER" value="744750420047"/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
<device name="_0.65WIRE" package="WE-FAMI_1280_0.65WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750420100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750420100.pdf"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="PART-NUMBER" value="744750420100"/>
<attribute name="RDC-MAX" value="15.5mOhm"/>
<attribute name="RDC-TYPE" value="12.9mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_0.6WIRE" package="WE-FAMI_1280_0.6WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750420150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750420150.pdf"/>
<attribute name="IR" value="5.1A"/>
<attribute name="ISAT" value="7.9A"/>
<attribute name="PART-NUMBER" value="744750420150"/>
<attribute name="RDC-MAX" value="25mOhm"/>
<attribute name="RDC-TYPE" value="21.3mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
<device name="_0.55WIRE" package="WE-FAMI_1280_0.55WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750420220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750420220.pdf"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="6.7A"/>
<attribute name="PART-NUMBER" value="744750420220"/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="RDC-TYPE" value="30.9mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI_8010" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_0.65WIRE" package="WE-FAMI_8010_0.65WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750230030">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750230030.pdf"/>
<attribute name="IR" value="7.6A"/>
<attribute name="ISAT" value="11.7A"/>
<attribute name="PART-NUMBER" value="744750230030"/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
<technology name="_744750230047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750230047.pdf"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="PART-NUMBER" value="744750230047"/>
<attribute name="RDC-MAX" value="12.5mOhm"/>
<attribute name="RDC-TYPE" value="9.7mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744750230068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750230068.pdf"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="8.1A"/>
<attribute name="PART-NUMBER" value="744750230068"/>
<attribute name="RDC-MAX" value="16mOhm"/>
<attribute name="RDC-TYPE" value="12.2mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
<device name="_0.55WIRE" package="WE-FAMI_8010_0.55WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750230100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750230100.pdf"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="PART-NUMBER" value="744750230100"/>
<attribute name="RDC-MAX" value="23mOhm"/>
<attribute name="RDC-TYPE" value="18.6mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_0.5WIRE" package="WE-FAMI_8010_0.5WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750230150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750230150.pdf"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="PART-NUMBER" value="744750230150"/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="RDC-TYPE" value="27.9mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI_1410" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_1.1WIRE" package="WE-FAMI_1410_1.1WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750530047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750530047.pdf"/>
<attribute name="IR" value="11.8A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="PART-NUMBER" value="744750530047"/>
<attribute name="RDC-MAX" value="4.8mOhm"/>
<attribute name="RDC-TYPE" value="4.1mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
<device name="_1.0WIRE" package="WE-FAMI_1410_1.0WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750530068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750530068.pdf"/>
<attribute name="IR" value="10.7A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="PART-NUMBER" value="744750530068"/>
<attribute name="RDC-MAX" value="6.5mOhm"/>
<attribute name="RDC-TYPE" value="5.3mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
<device name="_0.9WIRE" package="WE-FAMI_1410_0.9WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750530100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750530100.pdf"/>
<attribute name="IR" value="8.9A"/>
<attribute name="ISAT" value="12.4A"/>
<attribute name="PART-NUMBER" value="744750530100"/>
<attribute name="RDC-MAX" value="9.5mOhm"/>
<attribute name="RDC-TYPE" value="8mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI_1215" prefix="L">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Optimization of material composition causes high performance
&lt;br&gt;Up to 19.7 A Saturation Current
&lt;br&gt;RDC values starting at 3.8 mΩ
&lt;br&gt;Shielded design
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C to +125 °C&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;DC/DC converters
&lt;br&gt;Power supplies and battery chargers
&lt;br&gt;Home Entertainment Systems
&lt;br&gt;Portable devices like notebooks
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14778v209%20Family_WE-FAMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FAMI"&gt;https://katalog.we-online.com/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated bY Yingchun Shan  2019-08-09&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_1.0WIRE" package="WE-FAMI_1215_1.0WRIE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750460100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750460100.pdf"/>
<attribute name="IR" value="9.2A"/>
<attribute name="ISAT" value="11.3A"/>
<attribute name="PART-NUMBER" value="744750460100"/>
<attribute name="RDC-MAX" value="8.6mOhm"/>
<attribute name="RDC-TYPE" value="6.7mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744750460150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750460150.pdf"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="PART-NUMBER" value="744750460150"/>
<attribute name="RDC-MAX" value="12mOhm"/>
<attribute name="RDC-TYPE" value="9.3mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
<device name="_0.9WIRE" package="WE-FAMI_1215_0.9WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744750460220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744750460220.pdf"/>
<attribute name="IR" value="6.9A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value="744750460220"/>
<attribute name="RDC-MAX" value="16mOhm"/>
<attribute name="RDC-TYPE" value="12.4mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
