<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - Common Mode Chokes for Low Voltage and Data Lines - WE-FCLP&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-09-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FCLP_FT16H">
<description>&lt;b&gt;WE-FCLP Common Mode Power Line Choke
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size: FT16H, THT, 4pins
&lt;br&gt;L X W X H = 24.5mm X 15.5mm X 14.5mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-FCLP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-FCLP_FT16H" prefix="L">
<description>&lt;b&gt;WE-FCLP Common Mode Power Line Choke 
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suppression of common mode noise up to 90 dB
&lt;br&gt; High leakage inductance for differential filtering
&lt;br&gt; Low profile with high inductance
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mains operated LED drivers
&lt;br&gt; Electronic ballasts
&lt;br&gt; Switched-mode power supplies
&lt;br&gt; Mains filter

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o183897v209%20WE-LPFC_744869161xxx_Group.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o183897v209%20WE-LPFC_744869161xxx_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-FCLP"&gt;https://www.we-online.com/catalog/en/WE-FCLP&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-03-12&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FCLP"/>
</gates>
<devices>
<device name="" package="WE-FCLP_FT16H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744869161063">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161063?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="2A"/>
<attribute name="IR2" value="2.4A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="120uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161063"/>
<attribute name="RDC" value="220mOhm"/>
<attribute name="VALUE" value="6mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161103">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161103?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="IR2" value="1.7A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="200uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161103"/>
<attribute name="RDC" value="330mOhm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161104">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161104?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="0.4A"/>
<attribute name="IR2" value="0.5A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="1930uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161104"/>
<attribute name="RDC" value="3470mOhm"/>
<attribute name="VALUE" value="100mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161153">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161153?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="290uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161153"/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="VALUE" value="15mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161273">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161273?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="IR2" value="1A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="520uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161273"/>
<attribute name="RDC" value="1000mOhm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161393">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161393?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.85A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="760uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161393"/>
<attribute name="RDC" value="1430mOhm"/>
<attribute name="VALUE" value="39mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161473">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161473?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="0.65A"/>
<attribute name="IR2" value="0.8A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="920uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161473"/>
<attribute name="RDC" value="1630mOhm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
<technology name="_744869161683">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744869161683?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR1" value="0.55A"/>
<attribute name="IR2" value="0.65A"/>
<attribute name="LENGTH" value="24.5mm"/>
<attribute name="LS" value="1340uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="744869161683"/>
<attribute name="RDC" value="2560mOhm"/>
<attribute name="VALUE" value="68mH"/>
<attribute name="VR" value="250 V (AC) "/>
<attribute name="VT" value="1.5KV"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
