<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Flexible Transformers for SMPS - WE-FLEX HV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FLEXHV_EFD15">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;EFD15  SMD 12Pin</description>
</package>
<package name="WE-FLEXHV_EFD20">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;EFD20  SMD 12Pin</description>
</package>
<package name="WE-FLEXHV_ER11/5">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;ER11/5  SMD 12Pin</description>
</package>
<package name="WE-FLEXHV_ER14.5/6">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;ER14.5/6  SMD 12Pin</description>
</package>
</packages>
<symbols>
<symbol name="WE-FLEXHV">
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-FLEXHV_EFD15" prefix="T">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
&lt;br&gt;SEPIC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3"&gt;https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan 2019-08-19 &lt;br&gt;
&lt;br&gt;20179(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196308">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196308.pdf"/>
<attribute name="IRBASE" value="0.83A"/>
<attribute name="ISATBASE" value="0.06A"/>
<attribute name="LSBASE" value="0.13uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196308 "/>
<attribute name="RDCBASE" value="145mOhm"/>
<attribute name="VALUE" value="153.8uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="61.3uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196318">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196318.pdf"/>
<attribute name="IRBASE" value="0.83A"/>
<attribute name="ISATBASE" value="0.43A"/>
<attribute name="LSBASE" value="0.13uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196318 "/>
<attribute name="RDCBASE" value="145mOhm"/>
<attribute name="VALUE" value="23.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="61.3uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196328">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196328.pdf"/>
<attribute name="IRBASE" value="0.83A"/>
<attribute name="ISATBASE" value="0.72A"/>
<attribute name="LSBASE" value="0.13uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196328 "/>
<attribute name="RDCBASE" value="145mOhm"/>
<attribute name="VALUE" value="14.2uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="61.3uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196338">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196338.pdf"/>
<attribute name="IRBASE" value="0.83A"/>
<attribute name="ISATBASE" value="1.13A"/>
<attribute name="LSBASE" value="0.13uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196338 "/>
<attribute name="RDCBASE" value="145mOhm"/>
<attribute name="VALUE" value="9.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="61.3uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196348">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196348.pdf"/>
<attribute name="IRBASE" value="0.83A"/>
<attribute name="ISATBASE" value="1.41A"/>
<attribute name="LSBASE" value="0.13uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196348 "/>
<attribute name="RDCBASE" value="145mOhm"/>
<attribute name="VALUE" value="7.9uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="61.3uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_ER11/5" prefix="T">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
&lt;br&gt;SEPIC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3"&gt;https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan 2019-08-19 &lt;br&gt;
&lt;br&gt;20179(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_ER11/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="11"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="9" pad="8"/>
</connects>
<technologies>
<technology name="_749196108">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196108.pdf"/>
<attribute name="IRBASE" value="0.5A"/>
<attribute name="ISATBASE" value="0.04A"/>
<attribute name="LSBASE" value="0.3uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196108 "/>
<attribute name="RDCBASE" value="344mOhm"/>
<attribute name="VALUE" value="224.6uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="49.3uVs"/>
</technology>
<technology name="_749196118">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196118.pdf"/>
<attribute name="IRBASE" value="0.5A"/>
<attribute name="ISATBASE" value="0.29A"/>
<attribute name="LSBASE" value="0.3uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196118 "/>
<attribute name="RDCBASE" value="344mOhm"/>
<attribute name="VALUE" value="27.4uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="49.3uVs"/>
</technology>
<technology name="_749196128">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196128.pdf"/>
<attribute name="IRBASE" value="0.5A"/>
<attribute name="ISATBASE" value="0.55A"/>
<attribute name="LSBASE" value="0.3uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196128 "/>
<attribute name="RDCBASE" value="344mOhm"/>
<attribute name="VALUE" value="14.7uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="49.3uVs"/>
</technology>
<technology name="_749196138">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196138.pdf"/>
<attribute name="IRBASE" value="0.5A"/>
<attribute name="ISATBASE" value="0.8A"/>
<attribute name="LSBASE" value="0.3uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196138 "/>
<attribute name="RDCBASE" value="344mOhm"/>
<attribute name="VALUE" value="10.9uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="49.3uVs"/>
</technology>
<technology name="_749196148">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196148.pdf"/>
<attribute name="IRBASE" value="0.5A"/>
<attribute name="ISATBASE" value="1.02A"/>
<attribute name="LSBASE" value="0.3uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196148 "/>
<attribute name="RDCBASE" value="344mOhm"/>
<attribute name="VALUE" value="8.5uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="49.3uVs"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_EFD20" prefix="T">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
&lt;br&gt;SEPIC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3"&gt;https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan 2019-08-19 &lt;br&gt;
&lt;br&gt;20179(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196507">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196507.pdf"/>
<attribute name="IRBASE" value="2.3A"/>
<attribute name="ISATBASE" value="0.16A"/>
<attribute name="LSBASE" value="0.18uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196507 "/>
<attribute name="RDCBASE" value="36mOhm"/>
<attribute name="VALUE" value="87.1uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="83.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196508">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196508.pdf"/>
<attribute name="IRBASE" value="1.35A"/>
<attribute name="ISATBASE" value="0.1A"/>
<attribute name="LSBASE" value="0.24uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196508 "/>
<attribute name="RDCBASE" value="102mOhm"/>
<attribute name="VALUE" value="196uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="123.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196517">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196517.pdf"/>
<attribute name="IRBASE" value="2.3A"/>
<attribute name="ISATBASE" value="1.35A"/>
<attribute name="LSBASE" value="0.18uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196517 "/>
<attribute name="RDCBASE" value="36mOhm"/>
<attribute name="VALUE" value="9.9uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="83.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196518">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196518.pdf"/>
<attribute name="IRBASE" value="1.35A"/>
<attribute name="ISATBASE" value="0.93A"/>
<attribute name="LSBASE" value="0.24uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196518 "/>
<attribute name="RDCBASE" value="102mOhm"/>
<attribute name="VALUE" value="22.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="123.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196527">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196527.pdf"/>
<attribute name="IRBASE" value="2.3A"/>
<attribute name="ISATBASE" value="2.81A"/>
<attribute name="LSBASE" value="0.18uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196527 "/>
<attribute name="RDCBASE" value="36mOhm"/>
<attribute name="VALUE" value="5.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="83.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196528">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196528.pdf"/>
<attribute name="IRBASE" value="1.35A"/>
<attribute name="ISATBASE" value="1.71A"/>
<attribute name="LSBASE" value="0.24uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196528 "/>
<attribute name="RDCBASE" value="102mOhm"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="123.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196537">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196537.pdf"/>
<attribute name="IRBASE" value="2.3A"/>
<attribute name="ISATBASE" value="3.24A"/>
<attribute name="LSBASE" value="0.18uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196537 "/>
<attribute name="RDCBASE" value="36mOhm"/>
<attribute name="VALUE" value="4.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="83.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196538">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196538.pdf"/>
<attribute name="IRBASE" value="1.35A"/>
<attribute name="ISATBASE" value="2.2A"/>
<attribute name="LSBASE" value="0.24uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196538 "/>
<attribute name="RDCBASE" value="102mOhm"/>
<attribute name="VALUE" value="9.7uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="123.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196547">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196547.pdf"/>
<attribute name="IRBASE" value="2.3A"/>
<attribute name="ISATBASE" value="3.93A"/>
<attribute name="LSBASE" value="0.18uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196547 "/>
<attribute name="RDCBASE" value="36mOhm"/>
<attribute name="VALUE" value="3.4uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="83.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196548">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196548.pdf"/>
<attribute name="IRBASE" value="1.35A"/>
<attribute name="ISATBASE" value="2.98A"/>
<attribute name="LSBASE" value="0.24uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196548 "/>
<attribute name="RDCBASE" value="102mOhm"/>
<attribute name="VALUE" value="7.6uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="123.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_ER14.5/6" prefix="T">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
&lt;br&gt;SEPIC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97648v209%20Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3"&gt;https://katalog.we-online.com/en/pbs/WE-FLEXHV#vs_ct:3&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan 2019-08-19 &lt;br&gt;
&lt;br&gt;20179(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="11"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="9" pad="8"/>
</connects>
<technologies>
<technology name="_749196208">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196208.pdf"/>
<attribute name="IRBASE" value="0.8A"/>
<attribute name="ISATBASE" value="0.07A"/>
<attribute name="LSBASE" value="0.17uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196208 "/>
<attribute name="RDCBASE" value="200mOhm"/>
<attribute name="VALUE" value="140uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="63.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196218">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196218.pdf"/>
<attribute name="IRBASE" value="0.8A"/>
<attribute name="ISATBASE" value="0.48A"/>
<attribute name="LSBASE" value="0.17uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196218 "/>
<attribute name="RDCBASE" value="200mOhm"/>
<attribute name="VALUE" value="21.6uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="63.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196228">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196228.pdf"/>
<attribute name="IRBASE" value="0.8A"/>
<attribute name="ISATBASE" value="0.94A"/>
<attribute name="LSBASE" value="0.17uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196228 "/>
<attribute name="RDCBASE" value="200mOhm"/>
<attribute name="VALUE" value="11.6uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="63.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196238">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196238.pdf"/>
<attribute name="IRBASE" value="0.8A"/>
<attribute name="ISATBASE" value="1.3A"/>
<attribute name="LSBASE" value="0.17uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196238 "/>
<attribute name="RDCBASE" value="200mOhm"/>
<attribute name="VALUE" value="8.3uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="63.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749196248">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749196248.pdf"/>
<attribute name="IRBASE" value="0.8A"/>
<attribute name="ISATBASE" value="1.6A"/>
<attribute name="LSBASE" value="0.17uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749196248 "/>
<attribute name="RDCBASE" value="200mOhm"/>
<attribute name="VALUE" value="6.6uH"/>
<attribute name="VOLTAGE-USECONDBASE" value="63.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
