<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Flexible Transformers for SMPS - WE-FLEX+&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FLEX+_ETD34">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX+ Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;ETD34  THT 14Pin</description>
</package>
<package name="WE-FLEX+_ETD39">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX+ Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;ETD39   THT 16Pin</description>
</package>
<package name="WE-FLEX+_ETD29">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-FLEX+ Flexible Transformer for DC/DC Converter&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;ETD29  THT 14Pin</description>
</package>
</packages>
<symbols>
<symbol name="L_3W:3W_3">
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-FLEX+_ETD34" prefix="T">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS"&gt;https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun, Shan 2019-08-15&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX+_ETD34">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="10" pad="1"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="2"/>
<connect gate="G$1" pin="9" pad="14"/>
</connects>
<technologies>
<technology name="_749197201">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197201.pdf"/>
<attribute name="IRBASE" value="2.5A"/>
<attribute name="ISATBASE" value="0.22A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197201 "/>
<attribute name="RDCBASE" value="51mOhm"/>
<attribute name="VALUE" value="374.4uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197211">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197211.pdf"/>
<attribute name="IRBASE" value="2.5A"/>
<attribute name="ISATBASE" value="0.33A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197211 "/>
<attribute name="RDCBASE" value="51mOhm"/>
<attribute name="VALUE" value="11.38uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197221.pdf"/>
<attribute name="IRBASE" value="2.5A"/>
<attribute name="ISATBASE" value="0.67A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197221 "/>
<attribute name="RDCBASE" value="51mOhm"/>
<attribute name="VALUE" value="69.4uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197231">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197231.pdf"/>
<attribute name="IRBASE" value="2.5A"/>
<attribute name="ISATBASE" value="1.58A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197231 "/>
<attribute name="RDCBASE" value="51mOhm"/>
<attribute name="VALUE" value="36.1uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197241">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197241.pdf"/>
<attribute name="IRBASE" value="2.5A"/>
<attribute name="ISATBASE" value="2.91A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197241 "/>
<attribute name="RDCBASE" value="51mOhm"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX+_ETD39" prefix="T">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS"&gt;https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun, Shan 2019-08-15&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX+_ETD39">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="10" pad="2"/>
<connect gate="G$1" pin="11" pad="10"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="2" pad="13"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="12"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="11"/>
<connect gate="G$1" pin="7" pad="14"/>
<connect gate="G$1" pin="8" pad="3"/>
<connect gate="G$1" pin="9" pad="15"/>
</connects>
<technologies>
<technology name="_749197301">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197301.pdf"/>
<attribute name="IRBASE" value="3.2A"/>
<attribute name="ISATBASE" value="0.2A"/>
<attribute name="LSBASE" value="0.35uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197301 "/>
<attribute name="RDCBASE" value="34mOhm"/>
<attribute name="VALUE" value="326.7uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197311">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197311.pdf"/>
<attribute name="IRBASE" value="3.2A"/>
<attribute name="ISATBASE" value="0.32A"/>
<attribute name="LSBASE" value="0.35uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197311 "/>
<attribute name="RDCBASE" value="34mOhm"/>
<attribute name="VALUE" value="128.5uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197321">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197321.pdf"/>
<attribute name="IRBASE" value="3.2A"/>
<attribute name="ISATBASE" value="0.68A"/>
<attribute name="LSBASE" value="0.35uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197321 "/>
<attribute name="RDCBASE" value="34mOhm"/>
<attribute name="VALUE" value="77.3uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197331.pdf"/>
<attribute name="IRBASE" value="3.2A"/>
<attribute name="ISATBASE" value="1.65A"/>
<attribute name="LSBASE" value="0.35uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197331 "/>
<attribute name="RDCBASE" value="34mOhm"/>
<attribute name="VALUE" value="39.4uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197341">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197341.pdf"/>
<attribute name="IRBASE" value="3.2A"/>
<attribute name="ISATBASE" value="3.25A"/>
<attribute name="LSBASE" value="0.35uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197341 "/>
<attribute name="RDCBASE" value="34mOhm"/>
<attribute name="VALUE" value="223.7uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX+_ETD29" prefix="T">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14788v209%20Family_WE-FLEX_PLUS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS"&gt;https://katalog.we-online.com/en/pbs/WE-FLEX-PLUS&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun, Shan 2019-08-15&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX+_ETD29">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="10" pad="1"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="2"/>
<connect gate="G$1" pin="9" pad="14"/>
</connects>
<technologies>
<technology name="_749197101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197101.pdf"/>
<attribute name="IRBASE" value="2.2A"/>
<attribute name="ISATBASE" value="0.25A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197101 "/>
<attribute name="RDCBASE" value="45mOhm"/>
<attribute name="VALUE" value="284uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197111.pdf"/>
<attribute name="IRBASE" value="2.2A"/>
<attribute name="ISATBASE" value="0.4A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197111 "/>
<attribute name="RDCBASE" value="45mOhm"/>
<attribute name="VALUE" value="75.1uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197121">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197121.pdf"/>
<attribute name="IRBASE" value="2.2A"/>
<attribute name="ISATBASE" value="0.83A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197121 "/>
<attribute name="RDCBASE" value="45mOhm"/>
<attribute name="VALUE" value="46.3uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197131">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197131.pdf"/>
<attribute name="IRBASE" value="2.2A"/>
<attribute name="ISATBASE" value="1.83A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197131 "/>
<attribute name="RDCBASE" value="45mOhm"/>
<attribute name="VALUE" value="24.3uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
<technology name="_749197141">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749197141.pdf"/>
<attribute name="IRBASE" value="2.2A"/>
<attribute name="ISATBASE" value="3.1A"/>
<attribute name="LSBASE" value="0.32uH"/>
<attribute name="N" value="1:1:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 749197141 "/>
<attribute name="RDCBASE" value="45mOhm"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VT" value="500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
