<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-FLYTI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-07-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FLYTI_EFD25_4476">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD25,SMT,12pins
&lt;br&gt;Bobbin: 070-4476</description>
</package>
<package name="WE-FLYTI_EP13_4482">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,SMT,12pins
&lt;br&gt;Bobbin: 070-4482</description>
</package>
<package name="WE-FLYTI_EE16/7/5_5278">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/7/5,THT,10pins
&lt;br&gt;Bobbin: 070-5278</description>
</package>
<package name="WE-FLYTI_EP13_5465">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,SMT,10pins
&lt;br&gt;Bobbin: 070-5465</description>
</package>
<package name="WE-FLYTI_EP7_4436">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,8pins
&lt;br&gt;Bobbin: 070-4436</description>
</package>
<package name="WE-FLYTI_EP7_4390">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,8pins
&lt;br&gt;Bobbin: 070-4390</description>
</package>
<package name="WE-FLYTI_EPQ13_6389_10PINS">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EPQ13,SMT,10pins
&lt;br&gt;Bobbin: 070-6389</description>
</package>
<package name="WE-FLYTI_EP7_5801">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,8pins
&lt;br&gt;Bobbin: 070-5801</description>
</package>
<package name="WE-FLYTI_EPQ13_6389_8PINS">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EPQ13,SMT,8pins
&lt;br&gt;Bobbin: 070-6389</description>
</package>
<package name="WE-FLYTI_EFD15_4265">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD15,SMT,8pins
&lt;br&gt;Bobbin: 070-4265</description>
</package>
<package name="WE-FLYTI_EFD20_5899">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD20,SMT,12pins
&lt;br&gt;Bobbin: 070-5899</description>
</package>
<package name="WE-FLYTI_EFD20_2609">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD20,THT,8pins
&lt;br&gt;Bobbin: 070-2609</description>
</package>
<package name="WE-FLYTI_EFD20_4275">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD20,SMT,12pins
&lt;br&gt;Bobbin: 070-4275</description>
</package>
<package name="WE-FLYTI_EFD25_2710">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD25,THT,10pins
&lt;br&gt;Bobbin: 070-2710</description>
</package>
</packages>
<symbols>
<symbol name="750344050">
<pin name="2" direction="pas"/>
<pin name="7+8" direction="pas"/>
<pin name="9+10" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="750343772">
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="760372002">
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750318701">
<pin name="7+8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5+6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="750319029">
<pin name="3+4" direction="pas"/>
<pin name="1+2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750342985">
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1+2" direction="pas"/>
<pin name="3+4" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="750318704">
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750318525">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750344600">
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="750317605">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7+8" direction="pas"/>
<pin name="5+6" direction="pas"/>
</symbol>
<symbol name="750342984">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="750317933">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750342354">
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750317595">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750317594">
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750316708">
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750313527">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750315623">
<pin name="1" direction="pas"/>
<pin name="11+12" direction="pas"/>
<pin name="7+8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750312791">
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750315778">
<pin name="2" direction="pas"/>
<pin name="7+8+9" direction="pas"/>
<pin name="10+11+12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="750314189">
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750315252">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750313102">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750311805">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750315623" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315623"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD25_4476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11+12" pad="11 12"/>
<connect gate="G$1" pin="2" pad="2 3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315623?ae"/>
<attribute name="IOUT1" value="1250mA"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="L" value="100uH"/>
<attribute name="LS" value="1400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750315623 "/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value=" 750315623 "/>
<attribute name="VAUX" value="24V"/>
<attribute name="VIN" value="25 - 520 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="1772V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750344050" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750344050"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD25_4476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
<connect gate="G$1" pin="9+10" pad="9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750344050?ae"/>
<attribute name="IOUT1" value="2000mA"/>
<attribute name="ISAT" value="7.95A"/>
<attribute name="L" value="65uH"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.85:1:0.54"/>
<attribute name="PART-NUMBER" value=" 750344050 "/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value=" 750344050 "/>
<attribute name="VAUX" value="13V"/>
<attribute name="VIN" value="40 - 180 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="2000V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760372002" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="760372002"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD25_4476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760372002?ae"/>
<attribute name="IOUT1" value="2500mA"/>
<attribute name="IOUT2" value="2500mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="25uH"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1:1"/>
<attribute name="PART-NUMBER" value=" 760372002 "/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value=" 760372002 "/>
<attribute name="VIN" value="9 - 36 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315778" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315778"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD25_4476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10+11+12" pad="10 11 12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7+8+9" pad="7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315778?ae"/>
<attribute name="IOUT1" value="4300mA"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="L" value="62uH"/>
<attribute name="LS" value="836nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.2:1:1"/>
<attribute name="PART-NUMBER" value=" 750315778 "/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value=" 750315778 "/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="42.5 - 57 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342985" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750342985"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP13_4482">
<connects>
<connect gate="G$1" pin="1+2" pad="1 2"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="3+4" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342985?ae"/>
<attribute name="IOUT1" value="500mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L" value="30uH"/>
<attribute name="LS" value="600nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="7.3:4:1:1:4"/>
<attribute name="PART-NUMBER" value=" 750342985 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750342985 "/>
<attribute name="VAUX" value="24V"/>
<attribute name="VIN" value="15 - 36 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="6V"/>
<attribute name="VOUT3" value="6V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343772" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750343772"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EE16/7/5_5278">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750343772?ae"/>
<attribute name="IOUT1" value="125mA"/>
<attribute name="IOUT2" value="125mA"/>
<attribute name="L" value="13uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1:5.5:5.5"/>
<attribute name="PART-NUMBER" value=" 750343772 "/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value=" 750343772 "/>
<attribute name="VIN" value="24 V (DC)"/>
<attribute name="VOUT1" value="100V"/>
<attribute name="VOUT2" value="-100V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342354" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750342354"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP13_5465">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342354?ae"/>
<attribute name="IOUT1" value="2000mA"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="L" value="12uH"/>
<attribute name="LS" value="235nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.2:1"/>
<attribute name="PART-NUMBER" value=" 750342354 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750342354 "/>
<attribute name="VIN" value="8 - 30 V (DC)"/>
<attribute name="VOUT1" value="6V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317594" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750317594"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP13_5465">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317594?ae"/>
<attribute name="IOUT1" value="350mA"/>
<attribute name="ISAT" value="6A"/>
<attribute name="L" value="20uH"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:2:1"/>
<attribute name="PART-NUMBER" value=" 750317594 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750317594 "/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="18 - 30 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="1875V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318704" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750318704"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750318704?ae"/>
<attribute name="IOUT1" value="400mA"/>
<attribute name="IOUT2" value="400mA"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="L" value="7uH"/>
<attribute name="LS" value="150nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.25:1.88:1"/>
<attribute name="PART-NUMBER" value=" 750318704 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750318704 "/>
<attribute name="VIN" value="15 - 42 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="8V"/>
<attribute name="VT" value="500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342984" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750342984"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342984?ae"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="30uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.5:1:1:1"/>
<attribute name="PART-NUMBER" value=" 750342984 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750342984 "/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="9 - 16 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="-15V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318701" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750318701"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4390">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5+6" pad="5 6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750318701?ae"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="6.25A"/>
<attribute name="L" value="8.6uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750318701 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750318701 "/>
<attribute name="VIN" value="12 - 42 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319029" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750319029"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="1+2" pad="1 2"/>
<connect gate="G$1" pin="3+4" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750319029?ae"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="L" value="7uH"/>
<attribute name="LS" value="250nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750319029 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750319029 "/>
<attribute name="VIN" value="15 - 42 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319214" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750318525"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EPQ13_6389_10PINS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750319214?ae"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L" value="65uH"/>
<attribute name="LS" value="600nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:5:2.3"/>
<attribute name="PART-NUMBER" value=" 750319214 "/>
<attribute name="SIZE" value="EPQ13"/>
<attribute name="VALUE" value=" 750319214 "/>
<attribute name="VAUX" value="10.5V"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750344600" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750344600"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750344600?ae"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="IOUT2" value="250mA"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="35uH"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3:3:1"/>
<attribute name="PART-NUMBER" value=" 750344600 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750344600 "/>
<attribute name="VIN" value="20 - 28 V (DC)"/>
<attribute name="VOUT1" value="19V"/>
<attribute name="VOUT2" value="6V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317933" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750317933"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EPQ13_6389_8PINS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317933?ae"/>
<attribute name="IOUT1" value="4000mA"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="L" value="21uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:2"/>
<attribute name="PART-NUMBER" value=" 750317933 "/>
<attribute name="SIZE" value="EPQ13"/>
<attribute name="VALUE" value=" 750317933 "/>
<attribute name="VAUX" value="10V"/>
<attribute name="VIN" value="18 - 36 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318525" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750318525"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EPQ13_6389_10PINS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="9 10"/>
<connect gate="G$1" pin="7" pad="7 8"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750318525?ae"/>
<attribute name="IOUT1" value="2400mA"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:1:2.25"/>
<attribute name="PART-NUMBER" value=" 750318525 "/>
<attribute name="SIZE" value="EPQ13"/>
<attribute name="VALUE" value=" 750318525 "/>
<attribute name="VAUX" value="10.5V"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313527" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313527"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD15_4265">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313527?ae"/>
<attribute name="IOUT1" value="60mA"/>
<attribute name="IOUT2" value="60mA"/>
<attribute name="IOUT3" value="60mA"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="L" value="10uH"/>
<attribute name="LS" value="400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.9:1:1.5:3.8"/>
<attribute name="PART-NUMBER" value=" 750313527 "/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value=" 750313527 "/>
<attribute name="VIN" value="4.5 - 16 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="18V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311805" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311805"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD15_4265">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311805?ae"/>
<attribute name="IOUT1" value="830mA"/>
<attribute name="IOUT2" value="60mA"/>
<attribute name="IOUT3" value="60mA"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="166.5uH"/>
<attribute name="LS" value="2050nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:2:1:2"/>
<attribute name="PART-NUMBER" value=" 750311805 "/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value=" 750311805 "/>
<attribute name="VAUX" value="10V"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="6V"/>
<attribute name="VOUT3" value="18V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314189" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750314189"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314189?ae"/>
<attribute name="IOUT1" value="200mA"/>
<attribute name="L" value="2.5uH"/>
<attribute name="LS" value="650nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.2:1:1"/>
<attribute name="PART-NUMBER" value=" 750314189 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750314189 "/>
<attribute name="VIN" value="3 - 6 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317595" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750317595"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317595?ae"/>
<attribute name="IOUT1" value="200mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="L" value="30uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.82:1.82:1"/>
<attribute name="PART-NUMBER" value=" 750317595 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750317595 "/>
<attribute name="VIN" value="8 - 65 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="8V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317605" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750317605"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5+6" pad="5 6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317605?ae"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L" value="30uH"/>
<attribute name="LS" value="900nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3:1"/>
<attribute name="PART-NUMBER" value=" 750317605 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750317605 "/>
<attribute name="VIN" value="12 - 70 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="625V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313102" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313102"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD20_4275">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313102?ae"/>
<attribute name="IOUT1" value="500mA"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="L" value="12uH"/>
<attribute name="LS" value="540nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 750313102 "/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value=" 750313102 "/>
<attribute name="VIN" value="10 - 32 V (DC)"/>
<attribute name="VOUT1" value="48V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315252" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315252"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD20_2609">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315252?ae"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="L" value="60uH"/>
<attribute name="LS" value="1500nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1:1.33"/>
<attribute name="PART-NUMBER" value=" 750315252 "/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value=" 750315252 "/>
<attribute name="VIN" value="24 - 48 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3000V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312791" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312791"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD20_5899">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312791?ae"/>
<attribute name="IOUT1" value="350mA"/>
<attribute name="ISAT" value="8.75A"/>
<attribute name="L" value="10uH"/>
<attribute name="LS" value="100nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:5:1.13"/>
<attribute name="PART-NUMBER" value=" 750312791 "/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value=" 750312791 "/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="9 - 57 V (DC)"/>
<attribute name="VOUT1" value="56V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316708" prefix="T">
<description>&lt;b&gt;WE-FLYTI Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Low leakage inductance
&lt;br&gt;Multiple package sizes
&lt;br&gt;Wide range input voltages
&lt;br&gt;Different output voltages available
&lt;br&gt;Isolation voltage: up to 3000VAC
&lt;br&gt;Lead free and RoHS compliant
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial and medical power supplies
&lt;br&gt;Auxiliary power supplies
&lt;br&gt;Home automation
&lt;br&gt;Isolated DC/DC power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o795300v209%20FAMILY-MID-FLYTI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-FLYTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750316708"/>
</gates>
<devices>
<device name="" package="WE-FLYTI_EFD25_2710">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316708?ae"/>
<attribute name="IOUT1" value="3000mA"/>
<attribute name="ISAT" value="7A"/>
<attribute name="L" value="42uH"/>
<attribute name="LS" value="750nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="3:1:1"/>
<attribute name="PART-NUMBER" value=" 750316708 "/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value=" 750316708 "/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="12 - 60 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1000V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
