<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Gate Drive Transformers - WE-GDT&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-05-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-GDT_1210_L10.26W12.98H5.64">
<description>&lt;B&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size 1210,  SMT, 8Pins
&lt;BR&gt;LXWXH=10.26X12.98X5.64mm</description>
</package>
<package name="WE-GDT_EP5_L7W8.5H6">
<description>&lt;B&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size EP5, SMT 6pins 
&lt;BR&gt;LXWXH=7X8.5X6mm</description>
</package>
<package name="WE-GDT_ER9.5_L10W12.07H5.97">
<description>&lt;B&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size ER9.5,  SMT, 8Pins
&lt;BR&gt;LXWXH=10X12.07X5.97mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-GDT_1210_2W:2W">
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-GDT_EP5_1W:1W">
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-GDT_EP5_1W:2W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-GDT_ER9.5_2W:1W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750316094" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_1210_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDT_1210_L10.26W12.98H5.64">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="45pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316094?ae"/>
<attribute name="HEIGHT" value="5.64mm"/>
<attribute name="L" value="261uH"/>
<attribute name="LENGTH" value="10.26mm"/>
<attribute name="LS" value="150nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.5:2.5"/>
<attribute name="PART-NUMBER" value=" 750316094 "/>
<attribute name="RDC1" value="148mOhm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value=" 750316094 "/>
<attribute name="VOLTAGE-TIME" value="70uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.98mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316093" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_1210_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDT_1210_L10.26W12.98H5.64">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="70pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316093?ae"/>
<attribute name="HEIGHT" value="5.64mm"/>
<attribute name="L" value="1710uH"/>
<attribute name="LENGTH" value="10.26mm"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1"/>
<attribute name="PART-NUMBER" value=" 750316093 "/>
<attribute name="RDC1" value="649mOhm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value=" 750316093 "/>
<attribute name="VOLTAGE-TIME" value="70uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.98mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301103" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301103?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="2.3uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="2300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.5:1:1"/>
<attribute name="PART-NUMBER" value=" 760301103 "/>
<attribute name="RDC1" value="700mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301103 "/>
<attribute name="VOLTAGE-TIME" value="29.4uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301105" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301105?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="1.7uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="1700nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1"/>
<attribute name="PART-NUMBER" value=" 760301105 "/>
<attribute name="RDC1" value="600mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301105 "/>
<attribute name="VOLTAGE-TIME" value="25.2uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301108" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301108?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="2.3uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="2300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.5:1"/>
<attribute name="PART-NUMBER" value=" 760301108 "/>
<attribute name="RDC1" value="730mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301108 "/>
<attribute name="VOLTAGE-TIME" value="33.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301107" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301107?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="2.9uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="2900nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.5:1"/>
<attribute name="PART-NUMBER" value=" 760301107 "/>
<attribute name="RDC1" value="1200mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301107 "/>
<attribute name="VOLTAGE-TIME" value="40.8uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301104" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301104?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="1.9uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="1900nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 760301104 "/>
<attribute name="RDC1" value="620mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301104 "/>
<attribute name="VOLTAGE-TIME" value="28.6uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="760301106" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_EP5_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-GDT_EP5_L7W8.5H6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760301106?ae"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LS" value="1800nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 760301106 "/>
<attribute name="RDC1" value="520mOhm"/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 760301106 "/>
<attribute name="VOLTAGE-TIME" value="30.2uVs"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311063" prefix="T">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Excellent performances in small package (EP5)
&lt;br&gt;1 or 2 secondary windings
&lt;br&gt;6 different turnsratios
&lt;br&gt;1500VDC insulation test voltage
&lt;br&gt;Operating voltage up to 80 V
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Suitable for signal and power application
&lt;br&gt;Designed for gate drive application high efficient SMPS
&lt;br&gt;Synchronous Flyback
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727400v209%20multi-WE-GDT-76030110x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-GDT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-GDT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-15&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-GDT_ER9.5_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-GDT_ER9.5_L10W12.07H5.97">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CWW" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311063?ae"/>
<attribute name="HEIGHT" value="5.97mm"/>
<attribute name="L" value="600uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="1400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750311063 "/>
<attribute name="RDC1" value="240mOhm"/>
<attribute name="SIZE" value="ER9.5"/>
<attribute name="VALUE" value=" 750311063 "/>
<attribute name="VOLTAGE-TIME" value="70uVs"/>
<attribute name="WIDTH" value="12.07mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
