<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-GFH&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-GFH_3225">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-GFH High Frequency SMD Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;3225</description>
</package>
<package name="WE-GFH_4532">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-GFH High Frequency SMD Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4532</description>
</package>
<package name="WE-GFH_2520">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-GFH High Frequency SMD Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2520</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-GFH_3225" prefix="L">
<description>&lt;b&gt;WE-GFH High Frequency SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;/b&gt;
&lt;br&gt;Chip SMD inductance
&lt;br&gt;Lower RDC for the same type
&lt;br&gt;Higher current supporting than standard form
&lt;br&gt;Small type 2.5 mm x 2.0 mm
&lt;br&gt;Operating temperature: -40°C to +105°C (Size 2520)
&lt;br&gt;Operating Temperature: -40°C to +125°C (Size 3225 and 4532 )

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; HF Circuits
&lt;br&gt;HF Filtering Applications
&lt;br&gt;Acustic Filtering Applications

&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-GFH"&gt;https://katalog.we-online.com/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by  Yingchun,Shan, 2019-07-04&lt;br&gt;
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744764901">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764901.pdf"/>
<attribute name="FRES" value="210MHz"/>
<attribute name="IR" value="1550mA"/>
<attribute name="PART-NUMBER" value=" 744764901 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="156mOhm"/>
<attribute name="RDC-TYP" value="140mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7447649015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649015.pdf"/>
<attribute name="FRES" value="127MHz"/>
<attribute name="IR" value="1400mA"/>
<attribute name="PART-NUMBER" value=" 7447649015 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC-MAX" value="195mOhm"/>
<attribute name="RDC-TYP" value="176mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744764902">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764902.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="1100mA"/>
<attribute name="PART-NUMBER" value=" 744764902 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC-MAX" value="260mOhm"/>
<attribute name="RDC-TYP" value="234mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744764903">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764903.pdf"/>
<attribute name="FRES" value="79MHz"/>
<attribute name="IR" value="1050mA"/>
<attribute name="PART-NUMBER" value=" 744764903 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC-MAX" value="325mOhm"/>
<attribute name="RDC-TYP" value="293mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744764904">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764904.pdf"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="IR" value="800mA"/>
<attribute name="PART-NUMBER" value=" 744764904 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="520mOhm"/>
<attribute name="RDC-TYP" value="468mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744764910">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764910.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="500mA"/>
<attribute name="PART-NUMBER" value=" 744764910 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="1105mOhm"/>
<attribute name="RDC-TYP" value="995mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7447649115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649115.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="450mA"/>
<attribute name="PART-NUMBER" value=" 7447649115 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="1690mOhm"/>
<attribute name="RDC-TYP" value="1521mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7447649122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649122.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="400mA"/>
<attribute name="PART-NUMBER" value=" 7447649122 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="2600mOhm"/>
<attribute name="RDC-TYP" value="2340mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7447649133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649133.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="320mA"/>
<attribute name="PART-NUMBER" value=" 7447649133 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="3640mOhm"/>
<attribute name="RDC-TYP" value="3276mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7447649147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649147.pdf"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="250mA"/>
<attribute name="PART-NUMBER" value=" 7447649147 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="5460mOhm"/>
<attribute name="RDC-TYP" value="4914mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7447649168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447649168.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="225mA"/>
<attribute name="PART-NUMBER" value=" 7447649168 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC-MAX" value="8450mOhm"/>
<attribute name="RDC-TYP" value="7605mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744764920">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744764920.pdf"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="160mA"/>
<attribute name="PART-NUMBER" value=" 744764920 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC-MAX" value="10140mOhm"/>
<attribute name="RDC-TYP" value="9126mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GFH_4532" prefix="L">
<description>&lt;b&gt;WE-GFH High Frequency SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;/b&gt;
&lt;br&gt;Chip SMD inductance
&lt;br&gt;Lower RDC for the same type
&lt;br&gt;Higher current supporting than standard form
&lt;br&gt;Small type 2.5 mm x 2.0 mm
&lt;br&gt;Operating temperature: -40°C to +105°C (Size 2520)
&lt;br&gt;Operating Temperature: -40°C to +125°C (Size 3225 and 4532 )

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; HF Circuits
&lt;br&gt;HF Filtering Applications
&lt;br&gt;Acustic Filtering Applications

&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-GFH"&gt;https://katalog.we-online.com/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by  Yingchun,Shan, 2019-07-04&lt;br&gt;
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744766901">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766901.pdf"/>
<attribute name="FRES" value="254MHz"/>
<attribute name="IR" value="1900mA"/>
<attribute name="PART-NUMBER" value=" 744766901 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC-MAX" value="110mOhm"/>
<attribute name="RDC-TYP" value="81mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7447669012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669012.pdf"/>
<attribute name="FRES" value="182MHz"/>
<attribute name="IR" value="1800mA"/>
<attribute name="PART-NUMBER" value=" 7447669012 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="120mOhm"/>
<attribute name="RDC-TYP" value="93mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744766902">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766902.pdf"/>
<attribute name="FRES" value="79MHz"/>
<attribute name="IR" value="1450mA"/>
<attribute name="PART-NUMBER" value=" 744766902 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="180mOhm"/>
<attribute name="RDC-TYP" value="144mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744766903">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766903.pdf"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="1300mA"/>
<attribute name="PART-NUMBER" value=" 744766903 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="220mOhm"/>
<attribute name="RDC-TYP" value="178mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7447669039">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669039.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1250mA"/>
<attribute name="PART-NUMBER" value=" 7447669039 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="240mOhm"/>
<attribute name="RDC-TYP" value="200mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744766904">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766904.pdf"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="1200mA"/>
<attribute name="PART-NUMBER" value=" 744766904 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="270mOhm"/>
<attribute name="RDC-TYP" value="215mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744766906">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766906.pdf"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="1025mA"/>
<attribute name="PART-NUMBER" value=" 744766906 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="300mOhm"/>
<attribute name="RDC-TYP" value="271mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744766910">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766910.pdf"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="825mA"/>
<attribute name="PART-NUMBER" value=" 744766910 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="500mOhm"/>
<attribute name="RDC-TYP" value="405mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7447669112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669112.pdf"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="810mA"/>
<attribute name="PART-NUMBER" value=" 7447669112 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="600mOhm"/>
<attribute name="RDC-TYP" value="444mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_7447669115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669115.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="800mA"/>
<attribute name="PART-NUMBER" value=" 7447669115 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="700mOhm"/>
<attribute name="RDC-TYP" value="511mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7447669118">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669118.pdf"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="700mA"/>
<attribute name="PART-NUMBER" value=" 7447669118 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="800mOhm"/>
<attribute name="RDC-TYP" value="654mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7447669122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669122.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="650mA"/>
<attribute name="PART-NUMBER" value=" 7447669122 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="900mOhm"/>
<attribute name="RDC-TYP" value="767mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7447669127">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669127.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="575mA"/>
<attribute name="PART-NUMBER" value=" 7447669127 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="1200mOhm"/>
<attribute name="RDC-TYP" value="849mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_7447669133">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669133.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="525mA"/>
<attribute name="PART-NUMBER" value=" 7447669133 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC-MAX" value="1400mOhm"/>
<attribute name="RDC-TYP" value="1030mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7447669139">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669139.pdf"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="460mA"/>
<attribute name="PART-NUMBER" value=" 7447669139 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="1600mOhm"/>
<attribute name="RDC-TYP" value="1320mOhm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_7447669147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669147.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="425mA"/>
<attribute name="PART-NUMBER" value=" 7447669147 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="1900mOhm"/>
<attribute name="RDC-TYP" value="1460mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7447669156">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669156.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="400mA"/>
<attribute name="PART-NUMBER" value=" 7447669156 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="2200mOhm"/>
<attribute name="RDC-TYP" value="1940mOhm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_7447669168">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669168.pdf"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="350mA"/>
<attribute name="PART-NUMBER" value=" 7447669168 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="2600mOhm"/>
<attribute name="RDC-TYP" value="2195mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7447669182">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669182.pdf"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="300mA"/>
<attribute name="PART-NUMBER" value=" 7447669182 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="3500mOhm"/>
<attribute name="RDC-TYP" value="3110mOhm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_744766920">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744766920.pdf"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="275mA"/>
<attribute name="PART-NUMBER" value=" 744766920 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="4000mOhm"/>
<attribute name="RDC-TYP" value="3560mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_7447669212">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669212.pdf"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="235mA"/>
<attribute name="PART-NUMBER" value=" 7447669212 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="4500mOhm"/>
<attribute name="RDC-TYP" value="4185mOhm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_7447669218">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669218.pdf"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="220mA"/>
<attribute name="PART-NUMBER" value=" 7447669218 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="7500mOhm"/>
<attribute name="RDC-TYP" value="6150mOhm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_7447669220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447669220.pdf"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="200mA"/>
<attribute name="PART-NUMBER" value=" 7447669220 "/>
<attribute name="Q" value=" 40 "/>
<attribute name="RDC-MAX" value="9000mOhm"/>
<attribute name="RDC-TYP" value="6940mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GFH_2520" prefix="L">
<description>&lt;b&gt;WE-GFH High Frequency SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;/b&gt;
&lt;br&gt;Chip SMD inductance
&lt;br&gt;Lower RDC for the same type
&lt;br&gt;Higher current supporting than standard form
&lt;br&gt;Small type 2.5 mm x 2.0 mm
&lt;br&gt;Operating temperature: -40°C to +105°C (Size 2520)
&lt;br&gt;Operating Temperature: -40°C to +125°C (Size 3225 and 4532 )

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; HF Circuits
&lt;br&gt;HF Filtering Applications
&lt;br&gt;Acustic Filtering Applications

&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14793v209%20Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-GFH"&gt;https://katalog.we-online.com/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by  Yingchun,Shan, 2019-07-04&lt;br&gt;
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_2520">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447629010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629010.pdf"/>
<attribute name="FRES" value="290MHz"/>
<attribute name="IR" value="850mA"/>
<attribute name="PART-NUMBER" value=" 7447629010 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="408mOhm"/>
<attribute name="RDC-TYP" value="335mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7447629015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629015.pdf"/>
<attribute name="FRES" value="220MHz"/>
<attribute name="IR" value="750mA"/>
<attribute name="PART-NUMBER" value=" 7447629015 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="504mOhm"/>
<attribute name="RDC-TYP" value="393mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7447629022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629022.pdf"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="650mA"/>
<attribute name="PART-NUMBER" value=" 7447629022 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="600mOhm"/>
<attribute name="RDC-TYP" value="510mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7447629033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629033.pdf"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="600mA"/>
<attribute name="PART-NUMBER" value=" 7447629033 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="780mOhm"/>
<attribute name="RDC-TYP" value="625mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7447629047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629047.pdf"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="510mA"/>
<attribute name="PART-NUMBER" value=" 7447629047 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="960mOhm"/>
<attribute name="RDC-TYP" value="750mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7447629068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629068.pdf"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="450mA"/>
<attribute name="PART-NUMBER" value=" 7447629068 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC-MAX" value="1200mOhm"/>
<attribute name="RDC-TYP" value="960mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7447629100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629100.pdf"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="340mA"/>
<attribute name="PART-NUMBER" value=" 7447629100 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="2028mOhm"/>
<attribute name="RDC-TYP" value="1700mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7447629150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629150.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="325mA"/>
<attribute name="PART-NUMBER" value=" 7447629150 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="2640mOhm"/>
<attribute name="RDC-TYP" value="2110mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7447629220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629220.pdf"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="265mA"/>
<attribute name="PART-NUMBER" value=" 7447629220 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="3360mOhm"/>
<attribute name="RDC-TYP" value="2762mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7447629330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447629330.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="210mA"/>
<attribute name="PART-NUMBER" value=" 7447629330 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC-MAX" value="5040mOhm"/>
<attribute name="RDC-TYP" value="4300mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
