<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-HCC&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024b, 2024-12-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCC_8070">
<description>&lt;b&gt; WE-HCC SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8070, SMT, 2pins
&lt;br&gt;LXWXH=8.4X7.9X7.2mm</description>
</package>
<package name="WE-HCC_1090">
<description>&lt;b&gt; WE-HCC SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1090, SMT, 2pins
&lt;br&gt;LXWXH=10.9X10X9.3mm</description>
</package>
<package name="WE-HCC_1210_IRON">
<description>&lt;b&gt; WE-HCC SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1210 iron powder, SMT, 2pins
&lt;br&gt;LXWXH=12.1X11.4X9.5mm</description>
</package>
<package name="WE-HCC_1210_FERRITE">
<description>&lt;b&gt; WE-HCC SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1210 ferrite, SMT, 2pins
&lt;br&gt;LXWXH=12.1X11.4X9.5mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCC_8070" prefix="L">
<description>&lt;b&gt;WE-HCC SMT High Current Cube Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Current capability up to 27 A
&lt;br&gt;Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Filter choke for DC/DC converter
&lt;br&gt;Single and polyphase buck converter
&lt;br&gt;Filter choke for motor electronics
&lt;br&gt;Input filter inductor for DC/DC converter

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCC_8070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443340030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340030?ae"/>
<attribute name="FRES" value="272MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="25.5A"/>
<attribute name="ISAT" value="35.4A@10%"/>
<attribute name="ISAT2" value="40.3A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="0.3uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340030"/>
<attribute name="RDC-MAX" value="2.7mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340047?ae"/>
<attribute name="FRES" value="232MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="22.5A"/>
<attribute name="ISAT" value="28.5A@10%"/>
<attribute name="ISAT2" value="31.3A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="0.47uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340047"/>
<attribute name="RDC-MAX" value="3.1mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340068?ae"/>
<attribute name="FRES" value="181MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="22.5A"/>
<attribute name="ISAT" value="21.2A@10%"/>
<attribute name="ISAT2" value="23A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="0.64uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340068"/>
<attribute name="RDC-MAX" value="3.1mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340100?ae"/>
<attribute name="FRES" value="147MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="18.8A"/>
<attribute name="ISAT" value="22.9A@10%"/>
<attribute name="ISAT2" value="25.1A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="0.97uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340100"/>
<attribute name="RDC-MAX" value="3.9mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340150?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="14.8A"/>
<attribute name="ISAT" value="16.4A@10%"/>
<attribute name="ISAT2" value="18.5A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="1.4uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340150"/>
<attribute name="RDC-MAX" value="5.6mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340220?ae"/>
<attribute name="FRES" value="97MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="14.8A"/>
<attribute name="ISAT" value="11.3A@10%"/>
<attribute name="ISAT2" value="12.9A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="1.4uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340220"/>
<attribute name="RDC-MAX" value="5.6mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340330?ae"/>
<attribute name="FRES" value="81MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="8.4A@10%"/>
<attribute name="ISAT2" value="10.8A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="1.55uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340330"/>
<attribute name="RDC-MAX" value="8.2mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340470?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="8.9A"/>
<attribute name="ISAT" value="7.7A@10%"/>
<attribute name="ISAT2" value="9.5A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="3.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340470"/>
<attribute name="RDC-MAX" value="13.5mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443340680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443340680?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7.4A@10%"/>
<attribute name="ISAT2" value="8.3A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="6.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443340680"/>
<attribute name="RDC-MAX" value="24mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
<technology name="_7443341000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443341000?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="IR" value="4.4A"/>
<attribute name="ISAT" value="7.1A@10%"/>
<attribute name="ISAT2" value="8.3A@30%"/>
<attribute name="LENGTH" value="8.4mm"/>
<attribute name="LR" value="9.8uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443341000"/>
<attribute name="RDC-MAX" value="41mOhm"/>
<attribute name="SIZE" value="8070"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="7.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCC_1090" prefix="L">
<description>&lt;b&gt;WE-HCC SMT High Current Cube Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Current capability up to 27 A
&lt;br&gt;Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Filter choke for DC/DC converter
&lt;br&gt;Single and polyphase buck converter
&lt;br&gt;Filter choke for motor electronics
&lt;br&gt;Input filter inductor for DC/DC converter

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCC_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443330022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330022?ae"/>
<attribute name="FRES" value="300MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="35.2A"/>
<attribute name="ISAT" value="90.5A@10%"/>
<attribute name="ISAT2" value="96A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330022"/>
<attribute name="RDC-MAX" value="1.6mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330033?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="35.2A"/>
<attribute name="ISAT" value="51A@10%"/>
<attribute name="ISAT2" value="59A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.33uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330033"/>
<attribute name="RDC-MAX" value="1.6mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330047?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="31.3A"/>
<attribute name="ISAT" value="46.5A@10%"/>
<attribute name="ISAT2" value="54.9A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.47uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330047"/>
<attribute name="RDC-MAX" value="1.85mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330068?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="27.2A"/>
<attribute name="ISAT" value="41.4A@10%"/>
<attribute name="ISAT2" value="46A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.67uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330068"/>
<attribute name="RDC-MAX" value="2.65mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330082?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="27.2A"/>
<attribute name="ISAT" value="36.8A@10%"/>
<attribute name="ISAT2" value="41.9A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.81uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330082"/>
<attribute name="RDC-MAX" value="2.65mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330100?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="27.2A"/>
<attribute name="ISAT" value="26.5A@10%"/>
<attribute name="ISAT2" value="31.1A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="0.95uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330100"/>
<attribute name="RDC-MAX" value="2.65mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330150?ae"/>
<attribute name="FRES" value="78MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="21.7A"/>
<attribute name="ISAT" value="26.8A@10%"/>
<attribute name="ISAT2" value="31A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="1.45uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330150"/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330220?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="17.4A"/>
<attribute name="ISAT" value="22.5A@10%"/>
<attribute name="ISAT2" value="25.6A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="2.1uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330220"/>
<attribute name="RDC-MAX" value="4.8mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330330?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="14.1A"/>
<attribute name="ISAT" value="19.3A@10%"/>
<attribute name="ISAT2" value="22.8A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="2.6uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330330"/>
<attribute name="RDC-MAX" value="7.15mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330470?ae"/>
<attribute name="FRES" value="49MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="11.3A"/>
<attribute name="ISAT" value="15A@10%"/>
<attribute name="ISAT2" value="17.9A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="3.8uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330470"/>
<attribute name="RDC-MAX" value="9.9mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330680?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="8.9A"/>
<attribute name="ISAT" value="12.4A@10%"/>
<attribute name="ISAT2" value="16.6A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="4.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330680"/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443330820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443330820?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="8.9A"/>
<attribute name="ISAT" value="9.3A@10%"/>
<attribute name="ISAT2" value="12.5A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="2.8uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443330820"/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443331000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443331000?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="9.3mm"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="9.4A@10%"/>
<attribute name="ISAT2" value="11.7A@30%"/>
<attribute name="LENGTH" value="10.9mm"/>
<attribute name="LR" value="5.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443331000"/>
<attribute name="RDC-MAX" value="23.1mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCC_1210" prefix="L">
<description>&lt;b&gt;WE-HCC SMT High Current Cube Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Current capability up to 27 A
&lt;br&gt;Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Filter choke for DC/DC converter
&lt;br&gt;Single and polyphase buck converter
&lt;br&gt;Filter choke for motor electronics
&lt;br&gt;Input filter inductor for DC/DC converter

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14794v209%20family-pic-WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_FERRITE" package="WE-HCC_1210_FERRITE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443320022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320022?ae"/>
<attribute name="FRES" value="280MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="48.2A"/>
<attribute name="ISAT" value="82.9A@10%"/>
<attribute name="ISAT2" value="90.8A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320022"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320033?ae"/>
<attribute name="FRES" value="214MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="48.2A"/>
<attribute name="ISAT" value="56.7A@10%"/>
<attribute name="ISAT2" value="62.1A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.33uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320033"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320047?ae"/>
<attribute name="FRES" value="138MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="40.2A"/>
<attribute name="ISAT" value="49.9A@10%"/>
<attribute name="ISAT2" value="54.7A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.46uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320047"/>
<attribute name="RDC-MAX" value="1.85mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320068?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="40.2A"/>
<attribute name="ISAT" value="35.8A@10%"/>
<attribute name="ISAT2" value="39.1A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.66uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320068"/>
<attribute name="RDC-MAX" value="1.85mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320082?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="32.6A@10%"/>
<attribute name="ISAT2" value="35.8A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.8uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320082"/>
<attribute name="RDC-MAX" value="2.5mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320100?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="30.6A@10%"/>
<attribute name="ISAT2" value="33.5A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.9uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320100"/>
<attribute name="RDC-MAX" value="2.5mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320150?ae"/>
<attribute name="FRES" value="92MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="25.7A"/>
<attribute name="ISAT" value="26.5A@10%"/>
<attribute name="ISAT2" value="29.1A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="1.43uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320150"/>
<attribute name="RDC-MAX" value="3.5mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320220?ae"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="21.6A"/>
<attribute name="ISAT" value="24.8A@10%"/>
<attribute name="ISAT2" value="27.2A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="2uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320220"/>
<attribute name="RDC-MAX" value="4.3mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320330?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="18.2A"/>
<attribute name="ISAT" value="22.4A@10%"/>
<attribute name="ISAT2" value="24.7A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="2.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320330"/>
<attribute name="RDC-MAX" value="5.7mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320470?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="14.9A"/>
<attribute name="ISAT" value="15.6A@10%"/>
<attribute name="ISAT2" value="17.1A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="3.2uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320470"/>
<attribute name="RDC-MAX" value="7.9mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320680?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="12.9A@10%"/>
<attribute name="ISAT2" value="14.2A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="5.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320680"/>
<attribute name="RDC-MAX" value="11mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443320820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443320820?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="11.8A"/>
<attribute name="ISAT" value="12.3A@10%"/>
<attribute name="ISAT2" value="13.5A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="5.1uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443320820"/>
<attribute name="RDC-MAX" value="11.8mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443321000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443321000?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="9.6A"/>
<attribute name="ISAT" value="9.1A@10%"/>
<attribute name="ISAT2" value="11.3A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="7.5uH"/>
<attribute name="MATERIAL" value="Ferrite"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443321000"/>
<attribute name="RDC-MAX" value="16.7mOhm"/>
<attribute name="SIZE" value="1210 ferrite"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
</technologies>
</device>
<device name="_IRON" package="WE-HCC_1210_IRON">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443310022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310022?ae"/>
<attribute name="FRES" value="210MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="48.2A"/>
<attribute name="ISAT" value="49.7A@10%"/>
<attribute name="ISAT2" value="177.2A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.21uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310022"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310033?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="48.2A"/>
<attribute name="ISAT" value="43.6A@10%"/>
<attribute name="ISAT2" value="115.4A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.32uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310033"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310047?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="40.2A"/>
<attribute name="ISAT" value="44.4A@10%"/>
<attribute name="ISAT2" value="116.2A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.46uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310047"/>
<attribute name="RDC-MAX" value="1.85mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310068?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="40.2A"/>
<attribute name="ISAT" value="39.3A@10%"/>
<attribute name="ISAT2" value="63.5A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.66uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310068"/>
<attribute name="RDC-MAX" value="1.85mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310082?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="32.5A"/>
<attribute name="ISAT" value="33.8A@10%"/>
<attribute name="ISAT2" value="67.8A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.78uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310082"/>
<attribute name="RDC-MAX" value="2.5mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310100?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="32.5A"/>
<attribute name="ISAT" value="28.5A@10%"/>
<attribute name="ISAT2" value="55.1A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="0.94uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310100"/>
<attribute name="RDC-MAX" value="2.5mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310150?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="26.9A"/>
<attribute name="ISAT" value="21.9A@10%"/>
<attribute name="ISAT2" value="54.5A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="1.36uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310150"/>
<attribute name="RDC-MAX" value="3.5mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310220?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="22.4A"/>
<attribute name="ISAT" value="20.9A@10%"/>
<attribute name="ISAT2" value="44A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="2.1uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310220"/>
<attribute name="RDC-MAX" value="4.3mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310330?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="15.5A"/>
<attribute name="ISAT" value="19.2A@10%"/>
<attribute name="ISAT2" value="38.9A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="3.2uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310330"/>
<attribute name="RDC-MAX" value="7.7mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310390?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="12.5A"/>
<attribute name="ISAT" value="16.4A@10%"/>
<attribute name="ISAT2" value="35.3A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="3.75uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310390"/>
<attribute name="RDC-MAX" value="11mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="3.9uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_7443310470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443310470?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="IR" value="12.5A"/>
<attribute name="ISAT" value="17.8A@10%"/>
<attribute name="ISAT2" value="35.5A@30%"/>
<attribute name="LENGTH" value="12.1mm"/>
<attribute name="LR" value="4.5uH"/>
<attribute name="MATERIAL" value="Iron Powder"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443310470"/>
<attribute name="RDC-MAX" value="11mOhm"/>
<attribute name="SIZE" value="1210 iron powder"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
