<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-HCI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCI_1365">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1365, SMT, 2pins
&lt;br&gt;LXWXH=12.8X12.8X6.2mm</description>
</package>
<package name="WE-HCI_1335">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1335, SMT, 2pins
&lt;br&gt;LXWXH=12.8X12.8X3.3mm</description>
</package>
<package name="WE-HCI_1350">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1350, SMT, 2pins
&lt;br&gt;LXWXH=12.8X12.8X4.7mm</description>
</package>
<package name="WE-HCI_1030">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1030, SMT, 2pins
&lt;br&gt;LXWXH=10.6X10.6X2.8mm</description>
</package>
<package name="WE-HCI_1890_7443556XXX">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1890 WE-PERM 2, SMT, 2pins
&lt;br&gt;LXWXH=18.2X18.2X8.9mm</description>
</package>
<package name="WE-HCI_1040">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1040, SMT, 2pins
&lt;br&gt;LXWXH=10.2X10.2X4mm</description>
</package>
<package name="WE-HCI_7050">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 7030, SMT, 2pins
&lt;br&gt;LXWXH=6.9X6.9X4.8mm</description>
</package>
<package name="WE-HCI_1890_7443557XXX">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1890 MnZn, SMT, 2pins
&lt;br&gt;LXWXH=18.2X18.2X8.9mm</description>
</package>
<package name="WE-HCI_2212">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 2212 MnZn, SMT, 2pins
&lt;br&gt;LXWXH=22X22.5X12mm</description>
</package>
<package name="WE-HCI_7040">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 7030, SMT, 2pins
&lt;br&gt;LXWXH=6.9X6.9X3.8mm</description>
</package>
<package name="WE-HCI_5040">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 5040, SMT, 2pins
&lt;br&gt;LXWXH=5.3X5.5X4mm</description>
</package>
<package name="WE-HCI_1050">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 1050, SMT, 2pins
&lt;br&gt;LXWXH=10.1X10.1X4.7mm</description>
</package>
<package name="WE-HCI_7030">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size: 7030, SMT, 2pins
&lt;br&gt;LXWXH=6.9X6.9X3mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCI_1365" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443551111">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551111?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="13.1A"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="9.5A@30%"/>
<attribute name="L" value="11.3uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551111"/>
<attribute name="RDC" value="9.1mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="11.3uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551130">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551130?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="32.1A"/>
<attribute name="ISAT1" value="11A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="L" value="1.3uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551130"/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="1.3uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551131">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551131?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="11.9A"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="L" value="13uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551131"/>
<attribute name="RDC" value="11.2mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="13uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551151?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="10A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="L" value="15.4uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551151"/>
<attribute name="RDC" value="14.8mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="15.4uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551181">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551181?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="7.4A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="L" value="18uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551181"/>
<attribute name="RDC" value="22mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551200?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="26.5A"/>
<attribute name="ISAT1" value="9A@10%"/>
<attribute name="ISAT2" value="22A@30%"/>
<attribute name="L" value="2uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551200"/>
<attribute name="RDC" value="2.6mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355122?ae"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="69.7A"/>
<attribute name="ISAT1" value="22A@10%"/>
<attribute name="ISAT2" value="65A@30%"/>
<attribute name="L" value="0.2uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355122"/>
<attribute name="RDC" value="0.35mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="0.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551221?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="7.1A"/>
<attribute name="ISAT1" value="3A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551221"/>
<attribute name="RDC" value="24.7mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551280">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551280?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="22.5A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="17.5A@30%"/>
<attribute name="L" value="2.8uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551280"/>
<attribute name="RDC" value="3.3mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="2.8uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551331?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="6.6A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551331"/>
<attribute name="RDC" value="30.5mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551370">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551370?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="18.3A"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="16A@30%"/>
<attribute name="L" value="3.7uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551370"/>
<attribute name="RDC" value="4.9mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="3.7uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355147?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="54.9A"/>
<attribute name="ISAT1" value="25A@10%"/>
<attribute name="ISAT2" value="50A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355147"/>
<attribute name="RDC" value="0.67mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551470?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="14.9A"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551470"/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551600">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551600?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="13.6A"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="L" value="6uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551600"/>
<attribute name="RDC" value="8.4mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="6uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551730">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551730?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="16.5A"/>
<attribute name="ISAT1" value="5.5A@10%"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="L" value="7.3uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551730"/>
<attribute name="RDC" value="5.9mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="7.3uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355182?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="44.5A"/>
<attribute name="ISAT1" value="15A@10%"/>
<attribute name="ISAT2" value="35A@30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355182"/>
<attribute name="RDC" value="0.9mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443551920">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443551920?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="IRP" value="14.4A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="L" value="9.2uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443551920"/>
<attribute name="RDC" value="7.8mOhm"/>
<attribute name="SIZE" value="1365"/>
<attribute name="VALUE" value="9.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1335" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1335">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744313025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313025?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="61.7A"/>
<attribute name="ISAT1" value="22A@10%"/>
<attribute name="ISAT2" value="60A@30%"/>
<attribute name="L" value="0.25uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313025"/>
<attribute name="RDC" value="0.75mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744313068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313068?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="38.5A"/>
<attribute name="ISAT1" value="13A@10%"/>
<attribute name="ISAT2" value="40A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313068"/>
<attribute name="RDC" value="1.58mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744313120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313120?ae"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="28.8A"/>
<attribute name="ISAT1" value="10A@10%"/>
<attribute name="ISAT2" value="28A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313120"/>
<attribute name="RDC" value="2.85mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744313180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313180?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="19.5A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="22A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313180"/>
<attribute name="RDC" value="5.6mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744313220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313220?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="19.4A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="18A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313220"/>
<attribute name="RDC" value="5.7mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744313330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744313330?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IRP" value="16.3A"/>
<attribute name="ISAT1" value="5.5A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="12.8mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744313330"/>
<attribute name="RDC" value="8.1mOhm"/>
<attribute name="SIZE" value="1335"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1350" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443550101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550101?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="11.1A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="10A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550101"/>
<attribute name="RDC" value="14.1mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550140">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550140?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="29A"/>
<attribute name="ISAT1" value="10A@10%"/>
<attribute name="ISAT2" value="26A@30%"/>
<attribute name="L" value="1.4uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550140"/>
<attribute name="RDC" value="2.4mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="1.4uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355019?ae"/>
<attribute name="FRES" value="225MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="65A"/>
<attribute name="ISAT1" value="28A@10%"/>
<attribute name="ISAT2" value="60A@30%"/>
<attribute name="L" value="0.19uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355019"/>
<attribute name="RDC" value="0.5mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.19uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550230">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550230?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="23.8A"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="17A@30%"/>
<attribute name="L" value="2.3uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550230"/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="2.3uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550320">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550320?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="19.1A"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="3.2uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550320"/>
<attribute name="RDC" value="5.3mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="3.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355047?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="50.1A"/>
<attribute name="ISAT1" value="24A@10%"/>
<attribute name="ISAT2" value="50A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355047"/>
<attribute name="RDC" value="0.9mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550480">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550480?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="12.9A"/>
<attribute name="ISAT1" value="5.5A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="4.8uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550480"/>
<attribute name="RDC" value="10.5mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="4.8uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550600">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550600?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="11.2A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="11.5A@30%"/>
<attribute name="L" value="6uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550600"/>
<attribute name="RDC" value="13.5mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="6uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_7443550820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443550820?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="12.5A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443550820"/>
<attribute name="RDC" value="11.6mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
<technology name="_744355090">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355090?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="36A"/>
<attribute name="ISAT1" value="11A@10%"/>
<attribute name="ISAT2" value="28A@30%"/>
<attribute name="L" value="0.9uH"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355090"/>
<attribute name="RDC" value="1.6mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.9uH"/>
<attribute name="WIDTH" value="12.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1030" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744323020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323020?ae"/>
<attribute name="FRES" value="216MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="52.4A"/>
<attribute name="ISAT1" value="21A@10%"/>
<attribute name="ISAT2" value="50A@30%"/>
<attribute name="L" value="0.2uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323020"/>
<attribute name="RDC" value="0.82mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="0.2uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323033?ae"/>
<attribute name="FRES" value="119MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="30.9A"/>
<attribute name="ISAT1" value="15A@10%"/>
<attribute name="ISAT2" value="36A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323033"/>
<attribute name="RDC" value="2.17mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323056?ae"/>
<attribute name="FRES" value="106MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="30.9A"/>
<attribute name="ISAT1" value="15A@10%"/>
<attribute name="ISAT2" value="33A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323056"/>
<attribute name="RDC" value="2.17mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323068?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="19.4A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="21A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323068"/>
<attribute name="RDC" value="4.79mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323100?ae"/>
<attribute name="FRES" value="69MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="19.4A"/>
<attribute name="ISAT1" value="10A@10%"/>
<attribute name="ISAT2" value="21A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323100"/>
<attribute name="RDC" value="4.79mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323120?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="17.4A"/>
<attribute name="ISAT1" value="6.5A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323120"/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323150?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="17.4A"/>
<attribute name="ISAT1" value="7.5A@10%"/>
<attribute name="ISAT2" value="18A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323150"/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
<technology name="_744323220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744323220?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IRP" value="12.4A"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="10.6mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744323220"/>
<attribute name="RDC" value="11.38mOhm"/>
<attribute name="SIZE" value="1030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1040" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443552100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552100?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="23.1A"/>
<attribute name="ISAT1" value="7.5A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552100"/>
<attribute name="RDC" value="3.3mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744355215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355215?ae"/>
<attribute name="FRES" value="275MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="56.4A"/>
<attribute name="ISAT1" value="20A@10%"/>
<attribute name="ISAT2" value="60A@30%"/>
<attribute name="L" value="0.15uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355215"/>
<attribute name="RDC" value="0.58mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443552150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552150?ae"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="18A"/>
<attribute name="ISAT1" value="6.5A@10%"/>
<attribute name="ISAT2" value="17A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552150"/>
<attribute name="RDC" value="5.3mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443552200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552200?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="14.8A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="2uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552200"/>
<attribute name="RDC" value="7.3mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443552280">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552280?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="12.1A"/>
<attribute name="ISAT1" value="4.8A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="L" value="2.8uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552280"/>
<attribute name="RDC" value="10.6mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="2.8uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744355230">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355230?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="42.2A"/>
<attribute name="ISAT1" value="13A@10%"/>
<attribute name="ISAT2" value="35A@30%"/>
<attribute name="L" value="0.3uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355230"/>
<attribute name="RDC" value="1.1mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443552430">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552430?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="10.9A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="L" value="4.3uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552430"/>
<attribute name="RDC" value="14.1mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="4.3uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744355256">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744355256?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="35.6A"/>
<attribute name="ISAT1" value="12.5A@10%"/>
<attribute name="ISAT2" value="30A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744355256"/>
<attribute name="RDC" value="1.61mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443552560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443552560?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="8.3A"/>
<attribute name="ISAT1" value="3.3A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443552560"/>
<attribute name="RDC" value="20.6mOhm"/>
<attribute name="SIZE" value="1040"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7050" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744314024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314024?ae"/>
<attribute name="FRES" value="320MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="35.4A"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="28A@30%"/>
<attribute name="L" value="0.24uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314024"/>
<attribute name="RDC" value="1mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314047?ae"/>
<attribute name="FRES" value="235MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="31.9A"/>
<attribute name="ISAT1" value="9A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314047"/>
<attribute name="RDC" value="1.35mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314076">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314076?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="22.9A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="0.76uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314076"/>
<attribute name="RDC" value="2.25mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.76uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314101?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="5.3A"/>
<attribute name="ISAT1" value="1.8A@10%"/>
<attribute name="ISAT2" value="4A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314101"/>
<attribute name="RDC" value="33mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314110?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="19.6A"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="1.1uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314110"/>
<attribute name="RDC" value="3.15mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="1.1uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314150?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="16.4A"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314150"/>
<attribute name="RDC" value="4.3mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314200?ae"/>
<attribute name="FRES" value="68MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="13.8A"/>
<attribute name="ISAT1" value="4.5A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="L" value="2uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314200"/>
<attribute name="RDC" value="5.85mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="2uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314330?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="10.9A"/>
<attribute name="ISAT1" value="3.2A@10%"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314330"/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314490">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314490?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="8.3A"/>
<attribute name="ISAT1" value="2.2A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="L" value="4.9uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314490"/>
<attribute name="RDC" value="14.5mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="4.9uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314650">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314650?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="6.6A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="6A@30%"/>
<attribute name="L" value="6.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314650"/>
<attribute name="RDC" value="21.5mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="6.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314760">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314760?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="5.5A"/>
<attribute name="ISAT1" value="2.2A@10%"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="L" value="7.6uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314760"/>
<attribute name="RDC" value="28.2mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="7.6uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744314850">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744314850?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IRP" value="5.3A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="4.5A@30%"/>
<attribute name="L" value="8.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744314850"/>
<attribute name="RDC" value="30.5mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="8.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1890" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_7443556XXX" package="WE-HCI_1890_7443556XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443556082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556082?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="65.3A"/>
<attribute name="ISAT1" value="42A@10%"/>
<attribute name="ISAT2" value="65A@30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556082"/>
<attribute name="RDC" value="0.54mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_74435561100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435561100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="16.5A"/>
<attribute name="ISAT1" value="10A@10%"/>
<attribute name="ISAT2" value="21.5A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435561100"/>
<attribute name="RDC" value="6.9mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556130">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556130?ae"/>
<attribute name="FRES" value="78MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="47.7A"/>
<attribute name="ISAT1" value="31A@10%"/>
<attribute name="ISAT2" value="62A@30%"/>
<attribute name="L" value="1.3uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556130"/>
<attribute name="RDC" value="0.94mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="1.3uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556190">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556190?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="42.1A"/>
<attribute name="ISAT1" value="23A@10%"/>
<attribute name="ISAT2" value="52A@30%"/>
<attribute name="L" value="1.9uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556190"/>
<attribute name="RDC" value="1.2mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="1.9uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556260">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556260?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="36.8A"/>
<attribute name="ISAT1" value="21A@10%"/>
<attribute name="ISAT2" value="50A@30%"/>
<attribute name="L" value="2.6uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556260"/>
<attribute name="RDC" value="1.58mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="2.6uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556350">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556350?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="24.2A"/>
<attribute name="ISAT1" value="17A@10%"/>
<attribute name="ISAT2" value="37A@30%"/>
<attribute name="L" value="3.5uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556350"/>
<attribute name="RDC" value="3.1mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="3.5uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556450">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556450?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="23.5A"/>
<attribute name="ISAT1" value="16A@10%"/>
<attribute name="ISAT2" value="37A@30%"/>
<attribute name="L" value="4.5uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556450"/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="4.5uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556560?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="22.8A"/>
<attribute name="ISAT1" value="15A@10%"/>
<attribute name="ISAT2" value="33A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556560"/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443556680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443556680?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="22A"/>
<attribute name="ISAT1" value="13A@10%"/>
<attribute name="ISAT2" value="27A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443556680"/>
<attribute name="RDC" value="4.1mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
</technologies>
</device>
<device name="_7443557XXX" package="WE-HCI_1890_7443557XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435571100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435571100?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="16.4A"/>
<attribute name="ISAT1" value="8.8A@10%"/>
<attribute name="ISAT2" value="18.5A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435571100"/>
<attribute name="RDC" value="6.9mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_74435571500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435571500?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="14.1A"/>
<attribute name="ISAT1" value="10.75A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435571500"/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_74435572200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435572200?ae"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="10.9A"/>
<attribute name="ISAT1" value="9A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435572200"/>
<attribute name="RDC" value="14.6mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_74435573300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435573300?ae"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="8.7A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435573300"/>
<attribute name="RDC" value="21.7mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_74435574700">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435574700?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="6.4A"/>
<attribute name="ISAT1" value="6.25A@10%"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435574700"/>
<attribute name="RDC" value="33.5mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443557560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443557560?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="27.1A"/>
<attribute name="ISAT1" value="26A@10%"/>
<attribute name="ISAT2" value="29A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443557560"/>
<attribute name="RDC" value="2.82mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
<technology name="_7443557760">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443557760?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IRP" value="22.8A"/>
<attribute name="ISAT1" value="19A@10%"/>
<attribute name="ISAT2" value="22A@30%"/>
<attribute name="L" value="7.6uH"/>
<attribute name="LENGTH" value="18.3mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443557760"/>
<attribute name="RDC" value="3.75mOhm"/>
<attribute name="SIZE" value="1890"/>
<attribute name="VALUE" value="7.6uH"/>
<attribute name="WIDTH" value="18.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_2212" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_2212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435580330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435580330?ae"/>
<attribute name="FRES" value="26.5MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="33.2A"/>
<attribute name="ISAT1" value="27.5A@10%"/>
<attribute name="ISAT2" value="45A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435580330"/>
<attribute name="RDC" value="1.7mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435580680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435580680?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="30.5A"/>
<attribute name="ISAT1" value="9A@10%"/>
<attribute name="ISAT2" value="31A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435580680"/>
<attribute name="RDC" value="2.1mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435580820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435580820?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="26.1A"/>
<attribute name="ISAT1" value="7.5A@10%"/>
<attribute name="ISAT2" value="30A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435580820"/>
<attribute name="RDC" value="2.7mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435581000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435581000?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="22.9A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="26A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435581000"/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435581200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435581200?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="20.1A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435581200"/>
<attribute name="RDC" value="4.3mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435582200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435582200?ae"/>
<attribute name="FRES" value="8.3MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="15.6A"/>
<attribute name="ISAT1" value="5.5A@10%"/>
<attribute name="ISAT2" value="18A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435582200"/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435583300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435583300?ae"/>
<attribute name="FRES" value="6.8MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="10.6A"/>
<attribute name="ISAT1" value="12.5A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435583300"/>
<attribute name="RDC" value="13.2mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435584700">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435584700?ae"/>
<attribute name="FRES" value="6.1MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="8.4A"/>
<attribute name="ISAT1" value="10.25A@10%"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435584700"/>
<attribute name="RDC" value="19.2mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435586800">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435586800?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="6.9A"/>
<attribute name="ISAT1" value="8.25A@10%"/>
<attribute name="ISAT2" value="9.5A@30%"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435586800"/>
<attribute name="RDC" value="27.3mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="68uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_74435588200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435588200?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IRP" value="6.6A"/>
<attribute name="ISAT1" value="7.75A@10%"/>
<attribute name="ISAT2" value="8.5A@30%"/>
<attribute name="L" value="82uH"/>
<attribute name="LENGTH" value="22.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435588200"/>
<attribute name="RDC" value="30.4mOhm"/>
<attribute name="SIZE" value="2212"/>
<attribute name="VALUE" value="82uH"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_5040" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_5040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744316022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316022?ae"/>
<attribute name="FRES" value="507MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="29.9A"/>
<attribute name="ISAT1" value="14A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316022"/>
<attribute name="RDC" value="1.25mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316033?ae"/>
<attribute name="FRES" value="402MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="25.5A"/>
<attribute name="ISAT1" value="9.5A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316033"/>
<attribute name="RDC" value="1.75mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316047?ae"/>
<attribute name="FRES" value="280MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="19.5A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="16A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316047"/>
<attribute name="RDC" value="2.75mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316068?ae"/>
<attribute name="FRES" value="253MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="16A"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="13.5A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316068"/>
<attribute name="RDC" value="4mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316100?ae"/>
<attribute name="FRES" value="158MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="14.8A"/>
<attribute name="ISAT1" value="5.5A@10%"/>
<attribute name="ISAT2" value="11.5A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316100"/>
<attribute name="RDC" value="4.75mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316150?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="11A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316150"/>
<attribute name="RDC" value="8.15mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316220?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="9.2A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316220"/>
<attribute name="RDC" value="11.3mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316330?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="7.1A"/>
<attribute name="ISAT1" value="2.75A@10%"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316330"/>
<attribute name="RDC" value="18.5mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316470?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="6A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="4.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316470"/>
<attribute name="RDC" value="24.5mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
<technology name="_744316560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744316560?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="5.5A"/>
<attribute name="ISAT1" value="2.4A@10%"/>
<attribute name="ISAT2" value="4.6A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744316560"/>
<attribute name="RDC" value="28.5mOhm"/>
<attribute name="SIZE" value="5040"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="5.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7040" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744311022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311022?ae"/>
<attribute name="FRES" value="290MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="36.4A"/>
<attribute name="ISAT1" value="15A@10%"/>
<attribute name="ISAT2" value="32A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311022"/>
<attribute name="RDC" value="1.1mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311047?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="27.9A"/>
<attribute name="ISAT1" value="11A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="L" value="0.4uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311047"/>
<attribute name="RDC" value="1.85mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311068?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="20.9A"/>
<attribute name="ISAT1" value="9.5A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311068"/>
<attribute name="RDC" value="3.1mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311100?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="16.8A"/>
<attribute name="ISAT1" value="8A@10%"/>
<attribute name="ISAT2" value="19A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311100"/>
<attribute name="RDC" value="4.6mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311150?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="13.8A"/>
<attribute name="ISAT1" value="4.5A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311150"/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311220?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="10.2A"/>
<attribute name="ISAT1" value="5.6A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311220"/>
<attribute name="RDC" value="11.4mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311330?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="8.1A"/>
<attribute name="ISAT1" value="4.5A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311330"/>
<attribute name="RDC" value="17.2mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744311470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744311470?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IRP" value="7.8A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744311470"/>
<attribute name="RDC" value="19.5mOhm"/>
<attribute name="SIZE" value="7040"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1050" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744325016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325016?ae"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="57.2A"/>
<attribute name="ISAT1" value="24A@10%"/>
<attribute name="ISAT2" value="58A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325016"/>
<attribute name="RDC" value="0.51mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325040?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="55.7A"/>
<attribute name="ISAT1" value="18A@10%"/>
<attribute name="ISAT2" value="37A@30%"/>
<attribute name="L" value="0.4uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325040"/>
<attribute name="RDC" value="0.67mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325072">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325072?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="37.8A"/>
<attribute name="ISAT1" value="14A@10%"/>
<attribute name="ISAT2" value="35A@30%"/>
<attribute name="L" value="0.72uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325072"/>
<attribute name="RDC" value="1.3mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.72uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443251000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443251000?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="9.5A"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="8.5A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443251000"/>
<attribute name="RDC" value="16.3mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325120?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="32.6A"/>
<attribute name="ISAT1" value="12A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325120"/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_7443251600">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443251600?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="6.25A"/>
<attribute name="ISAT1" value="3.2A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="L" value="16uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443251600"/>
<attribute name="RDC" value="34.5mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="16uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325180?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="22.1A"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="18A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325180"/>
<attribute name="RDC" value="3.5mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325240?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="18.6A"/>
<attribute name="ISAT1" value="6.9A@10%"/>
<attribute name="ISAT2" value="17A@30%"/>
<attribute name="L" value="2.4uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325240"/>
<attribute name="RDC" value="4.75mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="2.4uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325330?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="16.6A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325330"/>
<attribute name="RDC" value="5.9mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325420">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325420?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="15.4A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="L" value="4.2uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325420"/>
<attribute name="RDC" value="7.1mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="4.2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325550">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325550?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="12A"/>
<attribute name="ISAT1" value="4.5A@10%"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="L" value="5.5uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325550"/>
<attribute name="RDC" value="10.3mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="5.5uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325650">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325650?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="11A"/>
<attribute name="ISAT1" value="4.4A@10%"/>
<attribute name="ISAT2" value="10A@30%"/>
<attribute name="L" value="6.5uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325650"/>
<attribute name="RDC" value="12.5mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="6.5uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_744325780">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744325780?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IRP" value="10.7A"/>
<attribute name="ISAT1" value="4.2A@10%"/>
<attribute name="ISAT2" value="9.5A@30%"/>
<attribute name="L" value="7.8uH"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744325780"/>
<attribute name="RDC" value="13.6mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="7.8uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7030" prefix="L">
<description>&lt;b&gt;WE-HCI SMT Flat Wire High Current Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;AECQ 200 qualified
&lt;br&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses at high frequency
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14796v209%20MODEL-WE-HCI.55.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744310013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310013?ae"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="40.75A"/>
<attribute name="ISAT1" value="16A@10%"/>
<attribute name="ISAT2" value="48A@30%"/>
<attribute name="L" value="0.13uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310013"/>
<attribute name="RDC" value="0.91mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="0.13uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310024?ae"/>
<attribute name="FRES" value="220MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="28.8A"/>
<attribute name="ISAT1" value="18A@10%"/>
<attribute name="ISAT2" value="40A@30%"/>
<attribute name="L" value="0.24uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310024"/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310055">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310055?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="19.2A"/>
<attribute name="ISAT1" value="8.5A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="0.52uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310055"/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="0.52uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310095">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310095?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="14.4A"/>
<attribute name="ISAT1" value="5A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="0.95uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310095"/>
<attribute name="RDC" value="6.2mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="0.95uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310115?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="11.8A"/>
<attribute name="ISAT1" value="7.5A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="L" value="1.15uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310115"/>
<attribute name="RDC" value="8.6mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="1.15uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310150?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="9.6A"/>
<attribute name="ISAT1" value="4.75A@10%"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310150"/>
<attribute name="RDC" value="12.7mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_744310200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744310200?ae"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="8.7A"/>
<attribute name="ISAT1" value="3A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="L" value="2uH"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744310200"/>
<attribute name="RDC" value="14.2mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="2uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
